{"text_format":"1","workbook":"xlsx","n_sheets":11,"sheets":["Help and Instructions","Data Entry","Report","NLossCalculations","DropDownLists","NEpreviousCrop","NEcountySoil","NEapplicationTime","NEcountyPrcp","NEmanure","NEfertilizer"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":2,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Help and Instructions","index":0,"n_rows":7,"n_cols":2,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[null,"This excel workbook must have the macro features enabled  to function."]
[]
[null,"Steps required to enable macro features:"]
[null,"1) Locate the Security Warning for the spreadsheet underneath the excel toolbar."]
[null,"2) Click on the options button near the security warning."]
[null,"3) After clicking options, the Security Alert - Macro will appear, next click Enable this content and select OK."]

{"sheet":"Data Entry","index":1,"n_rows":79,"n_cols":15,"rows_kept":79,"cut":false,"hidden":false,"merged":[[7,4,14,4],[7,10,14,10],[17,8,17,9],[19,10,23,10],[8,7,8,8],[16,8,16,13],[17,12,17,13],[9,11,10,13],[13,11,13,12],[12,11,12,12],[9,7,9,8],[11,7,11,8],[12,7,12,8],[13,7,13,8],[10,7,10,8],[19,4,23,4],[15,4,18,4],[26,11,26,13],[31,4,37,4],[24,4,30,4],[34,8,34,10],[33,8,33,10],[78,4,81,15],[71,4,72,15],[47,4,68,4],[45,4,46,4],[26,6,26,8],[55,6,55,8]]}
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Nebraska Nitrogen Loss Assessment Tool (N-LAT)"]
[null,null,null,null,null,null,null,null,null,null,"Please enter the required information in the white drop down lists.  "]
[null,null,null,null,null,null,null,null,null,null,"The light gray boxes are user inputted information."]
[]
[]
[null,null,null,null,"Field Location",null,null,null,null,null,"Production \nMethods"]
[null,null,null,null,null,null,"Date",{"$f":"NOW()","v":"2015-01-06T15:10:02.210"},null,null,null,"Fall Tilled","Spring Tilled","         Tile Drainage"]
[null,null,null,null,null,null,"Scenario Number",1,null,null,null,"Fall or Winter Cover Crop Grown"]
[null,null,null,null,null,null,"County"]
[null,null,null,null,null,null,"Field Name",null,null,null,null,null,"Crop","Yield "]
[null,null,null,null,null,null,"Scenario Name",null,null,null,null,"  Current",null,0,"bu/ac"]
[null,null,null,null,null,null,"Acres",null,null,null,null,"Previous ",null,0,"bu/ac"]
[]
[null,null,null,null,"Soil Unit"]
[null,null,null,null,null,null,null,"Soil unit"]
[null,null,null,null,null,null,null,"Organic matter (%)",null,null,null,"Soil pH"]
[]
[null,null,null,null,"Rainfall",null,null,null,null,null,"Irrigation"]
[null,null,null,null,null,null,"Out of Season","","inches/ac",null,null,null,"Irrigation Type"]
[null,null,null,null,null,null,"In Season","","inches/ac",null,null,null,"Expected Amount Applied"," ","inches/ac"]
[null,null,null,null,null,null,null,null,null,null,null,null,"NO3-N Content"," ","ppm/ac"]
[]
[null,null,null,null,"Nitrogen Application"]
[null,null,null,null,null,null,null,null,null,"N Rate","Time of"]
[null,null,null,null,null,null,"Fertilizer Option",null,null,"lbs/ac","Application","Use of Inhibitor"]
[null,null,null,null,null,null,null,null,null," "]
[]
[]
[]
[null,null,null,null,"Manure Application"]
[null,null,null,null,null,null,null,"Type",null,null,null,null,"Dry matter Content","","percent"]
[null,null,null,null,null,null,null,"Rate of Application",null,null,null,null,"Ammonium N","","lbs/unit"]
[null,null,null,null,null,null,null,"Terms (Unit for Application)","",null,null,null,"Organic N","","lbs/unit"]
[null,null,null,null,null,null,null,"Application Method",null,null,null,null,"Year Applied",""]
[null,null,null,null,null,null,null,"Time of Application",null,null,null,null,"Days to Incorporation"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,"Nebraska Nitrogen Loss Assessment Tool Report (N-LAT)",null,null,null,"Scenario Number"]
[null,null,null,null,null,null,null,null,null,null,"Review summary information below."]
[null,null,null,null,null,null,null,null,null,null,"Click Save Output to save and copy results of a scenario to the Report Tab."]
[null,null,null,null,null,null,null,null,null,null,null,null,null,0]
[]
[]
[null,null,null,null,null,null,null,null,"Scenario number",{"$f":"IF(NLossCalculations!C209<>0,NLossCalculations!C209,\"Select Scenario\")","v":1}]
[null,null,null,null,"Summary Report",null,null,null,"Date",{"$f":"NLossCalculations!C210","v":"2015-01-06T15:10:02.210"}]
[null,null,null,null,null,null,null,null,"Field Name",{"$f":"NLossCalculations!C211","v":"No Field Name"}]
[null,null,null,null,null,null,null,null,"Scenario Name",{"$f":"NLossCalculations!C212","v":"No Scenario Name"}]
[null,null,null,null,null,null,null,null,"County",{"$f":"NLossCalculations!C213","v":"No County Selected"}]
[null,null,null,null,null,null,null,null,"Soil Unit",{"$f":"NLossCalculations!C214","v":"No Soil Selected"}]
[null,null,null,null,null,null,null,null,"Current Crop & Yield",{"$f":"NLossCalculations!C215","v":"No Crop Selected"}]
[null,null,null,null,null,null,null,null,"Previous Crop & Yield",{"$f":"NLossCalculations!C216","v":"No Crop Selected"}]
[null,null,null,null,null,null,null,null,"Cover Crop",{"$f":"NLossCalculations!C217","v":"None"}]
[null,null,null,null,null,null,"Tillage Practice \n(Fall, Spring, or Split Till)",null,null,{"$f":"NLossCalculations!C218","v":"No Till"}]
[null,null,null,null,null,null,null,null,"N Fertilizer",{"$f":"NLossCalculations!C219","v":"UANSuSp# "}]
[null,null,null,null,null,null,null,null,"N Fertilizer",{"$f":"NLossCalculations!C220","v":""}]
[null,null,null,null,null,null,null,null,"N Fertilizer",{"$f":"NLossCalculations!C221","v":""}]
[null,null,null,null,null,null,null,null,"Manure",{"$f":"NLossCalculations!C222","v":"None"}]
[null,null,null,null,null,null,null,null,"Irrigation",{"$f":"NLossCalculations!C223","v":"None"}]
[null,null,null,null,null,null,null,null,"Total N Supply",{"$f":"NLossCalculations!C224","v":0}]
[null,null,null,null,null,null,null,null,"N Uptake",{"$f":"NLossCalculations!C225","v":0}]
[null,null,null,null,null,null,null,null,"Denitrification N lbs/acre",{"$f":"NLossCalculations!C226","v":0}]
[null,null,null,null,null,null,null,null,"Leached NO3-N lbs/acre",{"$f":"NLossCalculations!C227","v":0}]
[null,null,null,null,null,null,null,null,"Volatilized NH3-N lbs/acre",{"$f":"NLossCalculations!C228","v":0}]
[null,null,null,null,null,null,null,null,"N2O-N emission lbs/acre",{"$f":"NLossCalculations!C229","v":0}]
[null,null,null,null,null,null,null,null,"Total N Losses lbs/acre",{"$f":"NLossCalculations!C230","v":0}]
[]
[]
[]
[null,null,null,null,"Credits: Charles Wortmann, Jim Jansen, Michael Van Liew, Richard Ferguson, Gary Hergert, Charles Shapiro, and Tim Shaver  \nof the University of Nebraska-Lincoln."]
[]
[]
[null,null,null,null,"Contact: Charles Wortmann, cwortmann2@unl.edu"]
[]
[null,null,null,null,"© 2014, The Board of Regents of the University of Nebraska. All rights reserved."]
[]
[null,null,null,null,"Extension is a Division of the Institute of Agriculture and Natural Resources at the University of Nebraska–Lincoln cooperating with the Counties and  the United States Department of Agriculture.  University of Nebraska–Lincoln Extension programs abide with the nondiscrimination policies of the University of Nebraska–Lincoln and the United States Department of Agriculture.\n"]

{"sheet":"Report","index":2,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[]}
[]
[]
["Nebraska Nitrogen Loss Assessment Tool (N-LAT) Report"]
[]
["Scenario number",1,2,3,4,5]
["Date"]
["Field Name"]
["Scenario Name"]
["County"]
["Soil Unit"]
["Current Crop & Yield"]
["Previous Crop & Yield"]
["Cover Crop"]
["Tillage Practice \n(Fall, Spring, or Split Till)"]
["N Fertilizer†"]
["N Fertilizer"]
["N Fertilizer"]
["Manure"]
["Irrigation"]
["Total N supply"]
["N uptake"]
["Denitrification N lbs/acre"]
["Leached NO3-N lbs/acre"]
["Volatilized NH3-N lbs/acre"]
["N2O-N emission lbs/acre"]
["Total N Losses lbs/acre"]
[]
[]
[]
["†Abbreviations:"]
["For fertilizer,"]
["·         UreaSuSpUr150: Nitrogen fertilizer type: AmNO3, Ammonium nitrate; Ams, ammonium sulfate; Anh, anhydrous ammonia; Oth, Other incorporated; "]
["       UAN, urea ammonium nitrate; and Ure, urea;"]
["·         UreaSuSpUr150: application method: Fe, fertigation; Ij, injected; In, incorporated; Inc/Ij, incorporated/injected; SIj, sidedress injected; SSu, sidedress surface. "]
["       and Su, surface application."]
["·         UreaSuSpUr150: time of application: Fa, fall; Sp, spring; and In, in-season (split) application. "]
["·         UreaSuSpUr150: inhibitors: Ag/AgU, Agrotain/Agrotain Ultra; Ag+, AgrotrainPlus; ammonium thiosulfate, ATS; CO, controlled release; N-S, N-Serve; "]
["       Nut, Nutrisphere; NI, other nitrification inhibitor; and Ur, other urease inhibitor. "]
["·         UreaSuSpUr150: the rate of N application, lbs/ac."]
["For manure"]
["·         2012FL-Su25ON15AN4: year of application."]
["·         2012FL-Su25ON15AN4: manure types: FL, feedlot solid;  HP, feedlot holding pond;  PO, poultry solid;  SG, swine or dairy solid; SL, swine lagoon;"]
["           and SD, swine or dairy slurry."]
["·         2012FL-Su25ON15AN4: application method: IJ, injected; I7, surface incorporated within 7 days; and Su, not surface incorporated within 7 days."]
["·         2012FL-Su25ON15AN4: Rate in t/ac for solids, ‘000 gal/ac for slurry, and ac-in for holding pond."]
["·         2012FL-Su25ON15AN4: Available organic (ON) and ammonium (AN) N in lb per unit."]
["Irrigation:"]
["·         Pivot-8”-3ppm: Irrigation system."]
["·         Pivot-8”-3ppm: Water applied, in/yr."]
["·         Pivot-8”-3ppm: NO3-N concentration in ppm."]

{"sheet":"NLossCalculations","index":3,"n_rows":230,"n_cols":22,"rows_kept":230,"cut":false,"hidden":true,"merged":[[17,3,17,4],[18,3,18,4],[12,3,12,4],[14,3,14,4],[13,3,13,4],[15,3,15,4],[16,3,16,4],[34,3,34,4],[35,3,35,4],[33,3,33,4],[20,3,20,4],[29,3,29,4],[27,3,27,4],[28,3,28,4],[26,3,26,4],[30,3,30,4],[32,3,32,4],[21,3,21,4],[22,3,22,4],[23,3,23,4],[24,3,24,4],[25,3,25,4],[31,3,31,4]]}
[null,"INTERFACE INPUT"]
[]
[null,null,"Notes: Macro Reference Cell =>"]
[]
[null,"Field Location","List ID","Interface Value",null,null,null,"Production Methods",{"$f":"$C$5","v":"List ID"},"Interface Value"]
[null,"Date",null,{"$f":"'Data Entry'!H9","v":"2015-01-06T15:10:02.210"},null,null,null,"Fall Tilled",null,false]
[null,"Run #",null,{"$f":"'Data Entry'!H10","v":1},null,null,null,"Spring Tilled",null,false]
[null,"County",1,{"$f":"INDEX(DropDownLists!$B$3:$B$96,C8)","v":0},null,null,null,"Tile Drainage",null,false]
[null,"Field name",null,{"$f":"IF('Data Entry'!H12=0,\"No Field Name\",'Data Entry'!H12)","v":"No Field Name"},null,null,null,"Fall or Winter Cover Crop Grown",null,false]
[null,"Scenario name",null,{"$f":"'Data Entry'!H13","v":0},null,null,null,"Current Crop Grown",1,{"$f":"IFERROR(INDEX(DropDownLists!$C$3:$C$5,$I$10), \"No Selection\")","v":0}]
[null,"Acres",null,{"$f":"'Data Entry'!H14","v":0},null,null,null,"Expected Yield (bu/ac)",{"$f":"IFERROR(VLOOKUP($J$10,NEpreviousCrop!$A$3:$C$4,2,FALSE),0)","v":0},{"$f":"IF(I11<>\"\",'Data Entry'!N13,\"\")","v":0}]
[null,null,null,null,null,null,null,"Previous Crop Grown",1,{"$f":"IFERROR(INDEX(DropDownLists!$C$3:$C$5,$I$12), \"No Selection\")","v":0}]
[null,"Soil Unit",{"$f":"$C$5","v":"List ID"},"Interface Value",null,null,null,"Previous Yield (bu/acre)",{"$f":"IFERROR(VLOOKUP($J$12,NEpreviousCrop!$A$3:$C$4,3,FALSE),0)","v":0},{"$f":"IF(I13<>\"\",'Data Entry'!N14,\"\")","v":0}]
[null,"Soil unit",1,{"$f":"IF(INDEX(SoilList,$C$14,)<>0, INDEX(SoilList,$C$14,),\"No Soil Selected\")","v":"No Soil Selected"}]
[null,"Drainage Class",null,{"$f":"INDEX(OFFSET(SoilList,0,1),$C$14)","v":0},null,null,null,"Rainfall","List ID","Interface Value"]
[null,"Hydrology Group",null,{"$f":"INDEX(OFFSET(SoilList,0,2),$C$14)","v":0},null,null,null,{"$f":"'Data Entry'!G21","v":"Out of Season"},{"$f":"IFERROR(VLOOKUP($D$8,NEcountyPrcp!$A$2:$C$94,2,FALSE),\"\")","v":""},{"$f":"IF(I16<>\"\",'Data Entry'!H21,\"\")","v":""}]
[null,"Organic Matter (%)",{"$f":"IF($C$14<>1,INDEX(OFFSET(SoilList,0,3),$C$14),\"\")","v":""},{"$f":"IF(C17<>\"\",'Data Entry'!I18,\"\")","v":""},null,null,null,{"$f":"'Data Entry'!G22","v":"In Season"},{"$f":"IFERROR(VLOOKUP($D$8,NEcountyPrcp!$A$2:$C$94,3,FALSE),\"\")","v":""},{"$f":"IF(I17<>\"\",'Data Entry'!H22,\"\")","v":""}]
[null,"Sand Total",null,{"$f":"INDEX(OFFSET(SoilList,0,4),$C$14)","v":0}]
[null,"Soil pH",{"$f":"IF(C14<>1,INDEX(OFFSET(SoilList,0,5),$C$14),\"\")","v":""},{"$f":"IF(C19<>\"\",'Data Entry'!M18,\"\")","v":""}]
[null,null,null,null,null,null,null,"Irrigation",{"$f":"$C$5","v":"List ID"},"Interface Value","Abbreviation"]
[null,"Nitrogen Application",{"$f":"$C$5","v":"List ID"},"Interface Value",null,"Abbreviation",null,"List Number",1,{"$f":"IFERROR(INDEX(DropDownLists!$D$3:$D$7,$I$21), \"No Selection\")","v":0},{"$f":"IFERROR(INDEX(DropDownLists!$D$19:$D$23,$I$21), \"No Selection\")","v":0}]
[null,"Fertilizer Option 1",11,{"$f":"INDEX(DropDownLists!$E$3:$E$16,NLossCalculations!$C$22)","v":"UAN surface"},null,{"$f":"INDEX(DropDownLists!$E$19:$E$32,NLossCalculations!$C$22)","v":"UANSu"},null,"Expected Amount Applied (inches/acre)",null,{"$f":"'Data Entry'!N22","v":" "}]
[null,"Fertilizer Option 2",1,{"$f":"INDEX(DropDownLists!$E$3:$E$16,NLossCalculations!$C$23)","v":0},null,{"$f":"INDEX(DropDownLists!$E$19:$E$32,NLossCalculations!$C$23)","v":0},null,"NO3-N Content (ppm)",null,{"$f":"'Data Entry'!N23","v":" "}]
[null,"Fertilizer Option 3",1,{"$f":"INDEX(DropDownLists!$E$3:$E$16,NLossCalculations!$C$24)","v":0},null,{"$f":"INDEX(DropDownLists!$E$19:$E$32,NLossCalculations!$C$24)","v":0}]
[null,"N rate lbs/acre 1",null,{"$f":"'Data Entry'!J28","v":" "},null,{"$f":"D25","v":" "}]
[null,"N rate lbs/acre 2",null,{"$f":"'Data Entry'!J29","v":0},null,{"$f":"D26","v":0},null,"Manure Application",{"$f":"$C$5","v":"List ID"},"Interface Value","Abbreviation"]
[null,"N rate lbs/acre 3",null,{"$f":"'Data Entry'!J30","v":0},null,{"$f":"D27","v":0},null,"Manure Type",1,{"$f":"INDEX(DropDownLists!$H$3:$H$9,NLossCalculations!$I$27)","v":0},{"$f":"INDEX(DropDownLists!$H$19:$H$25,NLossCalculations!$I$27)","v":0}]
[null,"Default Time of Application 1",{"$f":"IFERROR(VLOOKUP($D$22,NEapplicationTime!$A$3:$C$16,3,FALSE),1)","v":3},null,null,null,null,"Rate of Application",null,{"$f":"'Data Entry'!I34","v":0}]
[null,"Default Time of Application 2",{"$f":"IFERROR(VLOOKUP($D$23,NEapplicationTime!$A$3:$C$16,3,FALSE),1)","v":1},null,null,null,null,"Terms (unit for application)",null,{"$f":"IFERROR(VLOOKUP($J$27,NEmanure!$A$1:$I$8,2,FALSE),\"\")","v":""}]
[null,"Default Time of Application 3",{"$f":"IFERROR(VLOOKUP($D$24,NEapplicationTime!$A$3:$C$16,3,FALSE),1)","v":1},null,null,null,null,"Application method",1,{"$f":"INDEX(DropDownLists!$I$3:$I$6,NLossCalculations!$I$30)","v":0},{"$f":"INDEX(DropDownLists!$I$19:$I$22,NLossCalculations!$I$30)","v":0}]
[null,"Time of Application 1",3,{"$f":"INDEX(DropDownLists!$F$3:$F$6,NLossCalculations!$C$31)","v":"Spring "},null,{"$f":"INDEX(DropDownLists!$F$19:$F$23,NLossCalculations!$C$31)","v":"Sp"},null,"Time of Application",1,{"$f":"INDEX(DropDownLists!$J$3:$J$5,NLossCalculations!I31)","v":0}]
[null,"Time of Application 2",1,{"$f":"INDEX(DropDownLists!$F$3:$F$6,NLossCalculations!$C$32)","v":0},null,{"$f":"INDEX(DropDownLists!$F$19:$F$23,NLossCalculations!$C$32)","v":0},null,"Dry matter content",{"$f":"IFERROR(VLOOKUP($J$27,NEmanure!$A$1:$I$8,4,FALSE),\"\")","v":""},{"$f":"IF(I32<>\"\",'Data Entry'!N33,\"\")","v":""}]
[null,"Time of Application 3",1,{"$f":"INDEX(DropDownLists!$F$3:$F$6,NLossCalculations!$C$33)","v":0},null,{"$f":"INDEX(DropDownLists!$F$19:$F$23,NLossCalculations!$C$33)","v":0},null,"Ammonium N (lbs/unit)",{"$f":"IFERROR(VLOOKUP($J$27,NEmanure!$A$1:$I$8,6,FALSE),\"\")","v":""},{"$f":"IF(I33<>\"\",'Data Entry'!N34,\"\")","v":""}]
[null,"Use of Inhibitor 1",1,{"$f":"INDEX(DropDownLists!$G$3:$G$11,NLossCalculations!$C$34)","v":0},null,{"$f":"INDEX(DropDownLists!$G$19:$G$27,NLossCalculations!$C$34)","v":0},null,"Organic N (lbs/unit)",{"$f":"IFERROR(VLOOKUP($J$27,NEmanure!$A$1:$I$8,7,FALSE),\"\")","v":""},{"$f":"IF(I34<>\"\",'Data Entry'!N35,\"\")","v":""}]
[null,"Use of Inhibitor 2",1,{"$f":"INDEX(DropDownLists!$G$3:$G$11,NLossCalculations!$C$35)","v":0},null,{"$f":"INDEX(DropDownLists!$G$19:$G$27,NLossCalculations!$C$35)","v":0},null,"Year applied",{"$f":"IF(J27<>0,'Data Entry'!N36,\"\")","v":""},{"$f":"IF(I35<>\"\",'Data Entry'!N36,\"\")","v":""}]
[null,"Use of Inhibitor 3",1,{"$f":"INDEX(DropDownLists!$G$3:$G$11,NLossCalculations!$C$36)","v":0},null,{"$f":"INDEX(DropDownLists!$G$19:$G$27,NLossCalculations!$C$36)","v":0},null,"Days to incorporation",{"$f":"NEmanure!B11","v":""},{"$f":"IF(I36<>\"\",'Data Entry'!N37,\"\")","v":""}]
[null,null,null,null,null,null,null,"Days to incorp default adj",null,{"$f":"NEmanure!C11","v":""}]
[]
[null,"N Availability and Fertilizer Sum Calculations"]
[]
[null,null,null,null,null,null,null,"Dentrification Fertilzier Calculations"]
[null,"N Fertilizers","Applied N","Crop Available N","Percent Fert N",null,null,"N Fertilizers",null,"Side-Dress/Fertigation in Season Fertilzier Application"]
[null,"N rate lb/ac 1",{"$f":"$D$25","v":" "},{"$f":"C43","v":" "},{"$f":"IFERROR(D43/$D$46,0)","v":0},null,null,"N rate lb/ac 1",null,{"$f":"IF(AND($C$31=4,OR($C$22=8,$C$22=10,$C$22=12)),$D$43,0)","v":0}]
[null,"N rate lb/ac 2",{"$f":"$D$26","v":0},{"$f":"C44","v":0},{"$f":"IFERROR(D44/$D$46,0)","v":0},null,null,"N rate lb/ac 2",null,{"$f":"IF(AND($C$32=4,OR($C$23=8,$C$23=10,$C$23=12)),$D$44,0)","v":0}]
[null,"N rate lb/ac 3",{"$f":"$D$27","v":0},{"$f":"C45","v":0},{"$f":"IFERROR(D45/$D$46,0)","v":0},null,null,"N rate lb/ac 3",null,{"$f":"IF(AND($C$33=4,OR($C$24=8,$C$24=10,$C$24=12)),$D$45,0)","v":0}]
[null,"Total Fertilizer ",{"$f":"SUM(C43:C45)","v":0},{"$f":"SUM(D43:D45)","v":0},0,null,null,"Total Fertilizer ",null,{"$f":"$C$79","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,"Percent N side-dress/fertigation in season ",null,{"$f":"IFERROR(SUM(J43:J45)/J46,0)","v":0}]
[null,"N Fertilizers","Applied N","% N AmN","AmN N"]
[null,"N rate lb/ac 1",{"$f":"$D$25","v":" "},{"$f":"IFERROR(VLOOKUP(D22,NEfertilizer!$A$2:$E$15,5,FALSE),0)","v":0.75},{"$f":"C49*D49","v":{"$error":"#VALUE!"}},null,null,"Volitization Fertilzier Calculations"]
[null,"N rate lb/ac 2",{"$f":"$D$26","v":0},{"$f":"IFERROR(VLOOKUP(D23,NEfertilizer!$A$2:$E$15,5,FALSE),0)","v":0},{"$f":"C50*D50","v":0},null,null,"Fertilizer or Manure","Crop Available N","% Urea N","% Ammonium N","Urea N","Ammonium N"]
[null,"N rate lb/ac 3",{"$f":"$D$27","v":0},{"$f":"IFERROR(VLOOKUP(D24,NEfertilizer!$A$2:$E$15,5,FALSE),0)","v":0},{"$f":"C51*D51","v":0},null,null,"N Fertilizers"]
[null,"Total Fertilizer ",{"$f":"SUM(C49:C51)","v":0},null,{"$f":"SUM(E49:E51)","v":{"$error":"#VALUE!"}},null,null,"N rate lb/ac 1",{"$f":"D43","v":" "},{"$f":"IFERROR(VLOOKUP($D$22,NEfertilizer!$A$2:$C$15,2,FALSE),0)","v":0.5},{"$f":"IFERROR(VLOOKUP($D$22,NEfertilizer!$A$2:$C$15,3,FALSE),0)","v":0.25},{"$f":"$I52*J52","v":{"$error":"#VALUE!"}},{"$error":"#VALUE!"}]
[null,null,null,null,null,null,null,"N rate lb/ac 2",{"$f":"D44","v":0},{"$f":"IFERROR(VLOOKUP($D$23,NEfertilizer!$A$2:$C$15,2,FALSE),0)","v":0},{"$f":"IFERROR(VLOOKUP($D$23,NEfertilizer!$A$2:$C$15,3,FALSE),0)","v":0},0,0]
[null,"Manure N Availability","Applied N","% N Available","Crop Available N",null,null,"N rate lb/ac 3",{"$f":"D45","v":0},{"$f":"IFERROR(VLOOKUP($D$24,NEfertilizer!$A$2:$C$15,2,FALSE),0)","v":0},{"$f":"IFERROR(VLOOKUP($D$24,NEfertilizer!$A$2:$C$15,3,FALSE),0)","v":0},0,0]
[null,"Ammonium N (lb/unit)",{"$f":"IF(NEmanure!B74<>NEmanure!A77,0,1)*IFERROR($J$33*$J$28,0)","v":0},{"$f":"IFERROR(VLOOKUP($J$27,NEmanure!$A$3:$I$8,8,FALSE),0)","v":0},{"$f":"C55*D55","v":0},null,null,"Manure"]
[null,"Organic N (lb/unit)",{"$f":"IFERROR($J$34*$J$28,0)","v":0},{"$f":"IFERROR(VLOOKUP($J$27,NEmanure!$A$3:$I$8,9,FALSE),0)","v":0},{"$f":"C56*D56","v":0},null,null,"Ammonium N (lb/unit)",null,null,null,{"$f":"E55","v":0},{"$f":"C55","v":0}]
[null,"Total N Available from Manure",null,null,{"$f":"E55+E56","v":0},null,null,"Total AmN",null,null,null,{"$f":"SUM(L52:L54)","v":{"$error":"#VALUE!"}},{"$f":"SUM(M52:M54)","v":{"$error":"#VALUE!"}}]
[]
[null,"Manure Application  Amount",null,"Units",null,null,null,"Leaching  Fertilizer Calculations"]
[null,{"$f":"\"Rate of Application: \"&J29","v":"Rate of Application: "},null,{"$f":"J28","v":0},null,null,null,"Individual Fertilizer Multiplier Adjustments",null,"Condition Fert Sum","Fertilizer Total","Percent of Total","Reduction Amount","Adjusted Multipler "]
[null,"Conversion Factor: Unit for App to t/ac",null,{"$f":"IFERROR(VLOOKUP($J$27,NEmanure!$A$1:$I$8,5,FALSE),\"\")","v":""},null,null,null,"Nitrif inhib or controlled release fert used with spring app",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{5,6,8},$C$31:$C$33,{3}))","v":0},{"$f":"$C$75","v":0},{"$f":"IFERROR(J61/K61,0)","v":0},{"$f":"(1-0.75)*L61","v":0},{"$f":"1-M61","v":1}]
[null,"Dry matter Content",null,{"$f":"J32","v":""},null,null,null,"Nitrif inhib or controlled release fert used with fall app",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{5,6,8},$C$31:$C$33,{2}))","v":0},0,0,{"$f":"(1-0.9)*L62","v":0},1]
[null,"Ton per Acre of Dry Weight of Manure",null,{"$f":"IFERROR(D60*D61*D62,0)","v":0},null,null,null,"AgrotainPlus used with fert application in spring app",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{3},$C$22:$C$24,{2,3,4,5,7,8,9,10,11,12,13,14},$C$31:$C$33,{3}))","v":0},0,0,{"$f":"(1-0.75)*L63","v":0},1]
[null,null,null,null,null,null,null,"AgrotainPlus used with fert application in fall app",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{3},$C$22:$C$24,{2,3,4,5,7,8,9,10,11,12,13,14},$C$31:$C$33,{2}))","v":0},0,0,{"$f":"(1-0.9)*L64","v":0},1]
[null,"Irrigation N Availability",null,"Crop Available N",null,null,null,"N inhibitor is nutrisphere",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{7}))","v":0},0,0,{"$f":"(1-0.96)*L65","v":0},1]
[null,"Expected Amount Applied (inches/acre)",null,{"$f":"J22","v":" "},null,null,null,"N Fertilizer is ammonium thiosulfate",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{4}))","v":0},0,0,{"$f":"(1-0.96)*L66","v":0},1]
[null,"NO3-N Content (ppm)",null,{"$f":"J23","v":" "},null,null,null,"N fertilizer incorporated ",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$22:$C$24,{2,4,6,7,9,13}))","v":0},0,0,{"$f":"(1-1.1)*L67","v":0},1]
[null,"Pounds of N each PPM per acre-inch",null,2.25,null,null,null,"Fall applied fertilizer or manure",null,{"$f":"SUM(SUMIFS($D$43:$D$45,$C$31:$C$33,{2}))+SUM(SUMIFS($C$76,$I$31,{3}))","v":0},{"$f":"$C$75+$C$76","v":0},0,{"$f":"(1-1.2)*L68","v":0},1]
[null,"Total N from Irrigation",null,{"$f":"D66*D67*D68","v":{"$error":"#VALUE!"}}]
[null,null,null,null,null,null,null,"Leaching Fertilizer Calculations"]
[null,"Other N Availabity",null,"Crop Available N",null,null,null,"Total Fertilizer Multiplier Calculations",null,"Condition Fert Sum","Fertilizer Total","Percent of Total"]
[null,"N availaible from other sources than fertilizer or manure",null,{"$f":"SUM(D90:D95)","v":109.1},null,null,null,"> 40% of N applied in June or July",null,{"$f":"SUM(SUMIFS($D$43:$D$45,$C$31:$C$33,4))","v":0},{"$f":"$C$75+$C$76","v":0},{"$f":"IFERROR(J72/K72,0)","v":0}]
[null,null,null,null,null,null,null,"> 50% of N applied from manure surface app or incorp",null,{"$f":"SUM(SUMIFS($C$76,$I$30,{2,3}))","v":0},{"$f":"$C$75+$C$76","v":0},{"$f":"IFERROR(J73/K73,0)","v":0}]
[null,"N Application Totals","Crop Available N","Percent"]
[null,{"$f":"B46","v":"Total Fertilizer "},{"$f":"D46","v":0},{"$f":"IFERROR(C75/$C$79,0)","v":0},null,null,null,"Nitrious Oxide Fertilizer Calculations"]
[null,{"$f":"B57","v":"Total N Available from Manure"},{"$f":"E57","v":0},{"$f":"IFERROR(C76/$C$79,0)","v":0},null,null,null,"Individual Fertilzier Multiplier Adjustments",null,"Condition Fert Sum","Fertilizer Total","Percent of Total","Reduction Amount","Adjusted Multipler "]
[null,{"$f":"B69","v":"Total N from Irrigation"},{"$f":"D69","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(C77/$C$79,0)","v":0},null,null,null,"Nitrification or urease inhibitor used",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{6,8,9},$C$22:$C$24,{11}),SUMIFS($E$49:$E$51,$C$34:$C$36,{6,8,9},$C$22:$C$24,{14}))","v":0},{"$f":"$C$75","v":0},{"$f":"IFERROR(J77/K77,0)","v":0},{"$f":"(1-0.85)*L77","v":0},{"$f":"1-M77","v":1}]
[null,null,null,null,null,null,null,"Agrotain/Agrotain Ultra or AgrotrainPlus used with urea or UAN",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{2},$C$22:$C$24,{7,8,9,10,11,12}),SUMIFS($E$49:$E$51,$C$34:$C$36,{3},$C$22:$C$24,{7,8,9,10,11,12}))","v":0},0,{"$f":"IFERROR(J78/K78,0)","v":0},{"$f":"(1-0.85)*L78","v":0},1]
[null,"Total N Applied",{"$f":"SUM(C75:C77)","v":{"$error":"#VALUE!"}},{"$f":"IFERROR(C79/$C$79,0)","v":0},null,null,null,"N inhibitor is nutrisphere",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{7}))","v":0},0,{"$f":"IFERROR(J79/K79,0)","v":0},{"$f":"(1-0.95)*L79","v":0},1]
[null,null,null,null,null,null,null,"N fertilizer is anhydrous ammonia",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$22:$C$24,{6}))","v":0},0,{"$f":"IFERROR(J80/K80,0)","v":0},{"$f":"(1-1.25)*L80","v":0},1]
[null,null,null,null,null,null,null,"N fertilizer is urea",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$22:$C$24,{13,14}))","v":0},0,{"$f":"IFERROR(J81/K81,0)","v":0},{"$f":"(1-1.1)*L81","v":0},1]
[null,null,null,null,null,null,null,"UAN injected",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$22:$C$24,{7,9}))","v":0},0,{"$f":"IFERROR(J82/K82,0)","v":0},{"$f":"(1-1.1)*L82","v":0},1]
[null,null,null,null,null,null,null,"N applied as controlled released fertilizer ",null,{"$f":"SUM(SUMIFS($E$49:$E$51,$C$34:$C$36,{5}))","v":0},0,{"$f":"IFERROR(J83/K83,0)","v":0},{"$f":"(1-0.75)*L83","v":0},1]
[]
[]
[null,"N LOSS CALCULATIONS"]
[]
[]
[null,"Total N availability (TN)",null,"Value"]
[null,"Constant",null,56]
[null,"%SOM * 40",null,{"$f":"IFERROR(D17*40,0)","v":0}]
[null,"17.7 * SoilNo ",null,{"$f":"17.7*3","v":53.099999999999994}]
[null,"IrrN (ac-in * ppm*0.225) ",null,{"$f":"IF(OR(I21=1,I21=2),0,(J22*J23*0.225))","v":0}]
[null,"0.11 * bu of previous corn crop",null,{"$f":"IF(I12=2,(0.11*J13),0)","v":0}]
[null,"0.97 * bu of previous soybean crop",null,{"$f":"IF(I12=3,(0.11*J13),0)","v":0}]
[null,"FertilizerN ",null,{"$f":"C75","v":0}]
[null,"ManureN ",null,{"$f":"C76","v":0}]
[null,"minsus volatilization loss ",null,{"$f":"-SUM(K143:M143)","v":0}]
[null,"minsus denitrification loss",null,{"$f":"-E144","v":0}]
[null,null,"TN  =",{"$f":"SUM(D90:D99)","v":109.1}]
[null,"Crop N Uptake (Nu)"]
[null,"Current Crop"]
[null,"Corn",null,{"$f":"IF($I$10=2,(1.2*$J$11),\"\")","v":""}]
[null,"Soybean",null,{"$f":"IF($I$10=3,(5*$J$11),\"\")","v":""}]
[null,null,"Nu = ",{"$f":"IF(SUM(D103:D104)<>0,SUM(D103:D104),0)","v":0}]
[null,"Difference TN - NU"]
[null,"Value","TN - Nu =",{"$f":"MAX(D100-D105,0)","v":109.1}]
[]
[]
[null,"Denitrification",null,null,"Value",null,null,null,"Volatilization",null,null,"Value"]
[null,"Other N Sources",null,null,null,null,null,null,"Other N Sources"]
[null,"N availaible from other sources than fertilizer or manure",null,null,{"$f":"IF($D$72=0,\"\",$D$72)","v":109.1},null,null,null,"N availaible from other sources than fertilizer or manure",null,null,{"$f":"IF($D$72=0,\"\",$D$72)","v":109.1}]
[null,"Base Percent",null,null,{"$f":"IF(E112>0,0.03,\"\")","v":0.03},null,null,null,"Base Percent"]
[null,null,null,"Denitrification Value ",null,null,null,null,"Other N sources",null,null,{"$f":"IF(L112>0,0.06,\"\")","v":0.06}]
[null,null,null,"from Other N Sources =",{"$f":"E112*E113","v":3.2729999999999997},null,null,null,"Base Volatilization Value",null,null,{"$f":"L112*L114","v":6.5459999999999994}]
[null,"Fertilzier or Manure N Sources",null,"Fertilizer 1","Fertilizer 2","Fertilizer 3","Manure",null,"Multiplier Adjustments"]
[null,"Fertilizer or Manure",null,{"$f":"IF($F$22=0,\"\",$F$22)","v":"UANSu"},{"$f":"IF($F$23=0,\"\",$F$23)","v":""},{"$f":"IF($F$24=0,\"\",$F$24)","v":""},{"$f":"IF($K$27=0,\"\",$K$27)","v":""},null,"Soil pH > 7.2",null,null,{"$f":"IF($D$19=\"\",\"\",IF($D$19>=7.2,2,\"\"))","v":""}]
[null,"Available N",null,{"$f":"IF(D43>0,D43,0)","v":" "},{"$f":"IF(D44>0,D44,0)","v":0},{"$f":"IF(D45>0,D45,0)","v":0},{"$f":"IF(E57>0,E57,0)","v":0},null,null,null,"Volatization Value "]
[null,"Base Percent",null,null,null,null,null,null,null,null,"from Other N Sources =",{"$f":"IF(L117=\"\",L115,L115*L117)","v":6.5459999999999994}]
[null,"UAN surface applied and incorporated/injected",null,{"$f":"IF(OR($C$22=8,$C$22=9,$C$22=10,$C$22=11,$C$22=12,),0.06,\"\")","v":0.06},{"$f":"IF(OR($C$23=8,$C$23=9,$C$23=10,$C$23=11,$C$23=12,),0.06,\"\")","v":""},{"$f":"IF(OR($C$24=8,$C$24=9,$C$24=10,$C$24=11,$C$24=12,),0.06,\"\")","v":""},null,null,"Fertilzier or Manure N Sources",null,"Fertilizer 1","Fertilizer 2","Fertilizer 3","Manure"]
[null,"Urea surface applied and incorporated/injected",null,{"$f":"IF(OR($C$22=13,$C$22=14),0.07,\"\")","v":""},{"$f":"IF(OR($C$23=13,$C$23=14),0.07,\"\")","v":""},{"$f":"IF(OR($C$24=13,$C$24=14),0.07,\"\")","v":""},null,null,"Fertilizer or Manure",null,{"$f":"IF($F$22=0,\"\",$F$22)","v":"UANSu"},{"$f":"IF($F$23=0,\"\",$F$23)","v":""},{"$f":"IF($F$24=0,\"\",$F$24)","v":""},{"$f":"IF($K$27=0,\"\",$K$27)","v":""}]
[null,"Ammonium sulfate or Ammonium nitrate applied",null,{"$f":"IF(OR($C$22=2,$C$22=3,$C$22=4,$C$22=5,$C$22=7),0.055,\"\")","v":""},{"$f":"IF(OR($C$23=2,$C$23=3,$C$23=4,$C$23=5,$C$23=7),0.03,\"\")","v":""},{"$f":"IF(OR($C$24=2,$C$24=3,$C$24=4,$C$24=5,$C$24=7),0.03,\"\")","v":""},null,null,"Urea N",null,{"$f":"IF($L$52>0,$L$52,0)","v":{"$error":"#VALUE!"}},{"$f":"IF($L$53>0,$L$53,0)","v":0},{"$f":"IF($L$54>0,$L$54,0)","v":0},{"$f":"IF($L$56>0,$L$56,0)","v":0}]
[null,"NH3 injected",null,{"$f":"IF(OR($C$22=6),0.06,\"\")","v":""},{"$f":"IF(OR($C$23=6),0.06,\"\")","v":""},{"$f":"IF(OR($C$24=6),0.06,\"\")","v":""},null,null,"Ammonium N",null,{"$f":"IF($M$52>0,$M$52,0)","v":{"$error":"#VALUE!"}},{"$f":"IF($M$53>0,$M$53,0)","v":0},{"$f":"IF($M$54>0,$M$54,0)","v":0},{"$f":"M56","v":0}]
[null,"Manure Adjustment",null,null,null,null,null,null,"Adjustment Equation: NH3 - Nv"]
[null,"Spring applied manure, surface/incorporated",null,null,null,null,{"$f":"IF(AND($I$31=2,$I$27<>1),0.06*(1+0.48*$D$63/25)*$E$57,\"\")","v":""},null,"Individual Adjustment Equations"]
[null,"Fall applied manure, surface/incorporated",null,null,null,null,{"$f":"IF(AND($I$31=3,$I$27<>1),0.06*(1+0.54*$D$63/25)*$E$57,\"\")","v":""},null,"Urea N surface applied",null,{"$f":"IF(OR($C$22=10,$C$22=11,$C$22=14),0.05,\"\")","v":0.05},{"$f":"IF(OR($C$22=10,$C$23=11,$C$23=14),0.05,\"\")","v":""},{"$f":"IF(OR($C$22=10,$C$24=11,$C$24=14),0.05,\"\")","v":""}]
[null,"Base Denitrification Values",null,{"$f":"IFERROR($D$118*PRODUCT($D$120:$D$123),\"\")","v":""},{"$f":"IFERROR($E$118*PRODUCT($E$120:$E$123),\"\")","v":0},{"$f":"IFERROR($F$118*PRODUCT($F$120:$F$123),\"\")","v":0},{"$f":"MAX(G125:G126)","v":0},null,"Urea N incorporated/injected",null,{"$f":"IF(OR($C$22=8,$C$22=9,$C$22=12,$C$22=13),0.01,\"\")","v":""},{"$f":"IF(OR($C$23=8,$C$23=9,$C$23=12,$C$23=13),0.01,\"\")","v":""},{"$f":"IF(OR($C$23=8,$C$23=9,$C$23=12,$C$23=13),0.01,\"\")","v":""}]
[null,"N Fert other than NH3 incorporated",null,{"$f":"IF($C$22<>1,IF($C$22<>6,1.1,1),\"\")","v":1.1000000000000001},{"$f":"IF($C$23<>1,IF($C$23<>6,1.1,1),\"\")","v":""},{"$f":"IF($C$24<>1,IF($C$24<>6,1.1,1),\"\")","v":""},null,null,"Ammonium N surface applied",null,{"$f":"IF(OR($C$22=3,$C$22=5,$C$22=10,$C$22=11,$C$22=14),0.025,\"\")","v":2.5000000000000001E-2},{"$f":"IF(OR($C$23=3,$C$23=5,$C$23=10,$C$23=11,$C$23=14),0.025,\"\")","v":""},{"$f":"IF(OR($C$24=3,$C$24=5,$C$24=10,$C$24=11,$C$24=14),0.025,\"\")","v":""}]
[null,"NH3 Base Adjustments",null,{"$f":"IF(D128=1.1,D127*D128,D127)","v":{"$error":"#VALUE!"}},{"$f":"IF(E128=1.1,E127*E128,E127)","v":0},{"$f":"IF(F128=1.1,F127*F128,F127)","v":0},{"$f":"G127","v":0},null,"Ammonium N incorporated/injected",null,{"$f":"IF(OR($C$22=2,$C$22=4,$C$22=7,$C$22=8,$C$22=9,$C$22=12,$C$22=13),0.0015,\"\")","v":""},{"$f":"IF(OR($C$23=2,$C$23=4,$C$23=7,$C$23=8,$C$23=9,$C$23=12,$C$23=13),0.0015,\"\")","v":""},{"$f":"IF(OR($C$24=2,$C$24=4,$C$24=7,$C$24=8,$C$24=9,$C$24=12,$C$24=13),0.0015,\"\")","v":""}]
[null,null,null,"Denitrification Values from",null,null,null,null,"NH3 injected",null,{"$f":"IF($C$22=6,0.004,\"\")","v":""},{"$f":"IF($C$23=6,0.004,\"\")","v":""},{"$f":"IF($C$24=6,0.004,\"\")","v":""}]
[null,null,null,"Fertilizer and Manure N Sources =",{"$f":"SUM(D129:G129)","v":{"$error":"#VALUE!"}},null,null,null,"Manure-solid/slurry surface applied",null,null,null,null,{"$f":"IF(OR($I$27=3,$I$27=4,$I$27=5, $I$27=6, $I$27=7),1-(0.985*POWER(0.65,$J$37)),\"\")","v":""}]
[null,"Denitrification Value",null,null,null,null,null,null,"Manure-injected/incorporated",null,null,null,null,{"$f":"IF($I$27=2,0.008,\"\")","v":""}]
[null,"Total Base Denitrification Value = ",null,null,{"$f":"E115+E131","v":{"$error":"#VALUE!"}},null,null,null,"Base NH3 - Nv Values",null,{"$f":"IFERROR(K123*PRODUCT(K128:K129),0)+IFERROR(K122*PRODUCT(K126:K127),0)+IFERROR(K123*K130,0)","v":0},{"$f":"IFERROR(L123*PRODUCT(L128:L129),0)+IFERROR(L122*PRODUCT(L126:L127),0)+IFERROR(L123*L130,0)","v":0},0,{"$f":"IFERROR(N123*PRODUCT(N131:N132),0)","v":0}]
[null,"Multiplier Adjustments",null,null,null,null,null,null,"Multiplier Adjustments"]
[null,"Equation adjustment for SOM",null,null,{"$f":"IF($E$131>0,0.33+0.65*($C$17/2.5),\"\")","v":{"$error":"#VALUE!"}},null,null,null,"Individual Multiplier Adjustments"]
[null,"Adjustment drainage rating",null,null,{"$f":"IF(E131>0,IF($J$8=TRUE,1,IF($D$15=\"Somewhat poorly drained\",2,IF(OR($D$15=\"Poorly drained\",$D$15=\"Very poorly drained\"),3,1))),\"\")","v":{"$error":"#VALUE!"}},null,null,null,"Urease inhibitor used",null,{"$f":"IF(AND(OR($C$22={11,14}),OR($C$34={2,3,5,9})),0.6,\"\")","v":""},{"$f":"IF(AND(OR($C$23={11,14}),OR($C$35={2,3,5,9})),0.6,\"\")","v":""},{"$f":"IF(AND(OR($C$24={11,14}),OR($C$36={2,3,5,9})),0.6,\"\")","v":""}]
[null,"Side-dress/fertigation in season on >40% N applied",null,null,{"$f":"IF($J$47>0.4,0.9,\"\")","v":""},null,null,null,"Ammonium Thiosulfate Applied",null,{"$f":"IF(AND(OR($C$22={11,14}),OR($C$34={4})),0.9,\"\")","v":""},{"$f":"IF(AND(OR($C$23={11,14}),OR($C$35={4})),0.9,\"\")","v":""},{"$f":"IF(AND(OR($C$24={11,14}),OR($C$36={4})),0.9,\"\")","v":""}]
[null,"Fall or Spring Tillage",null,null,{"$f":"IF(OR($J$6=TRUE,$J$7=TRUE),0.9,\"\")","v":""},null,null,null,"Nutrisphere Applied",null,{"$f":"IF(AND(OR($C$22={11,14}),OR($C$34={7})),0.85,\"\")","v":""},{"$f":"IF(AND(OR($C$23={11,14}),OR($C$35={7})),0.85,\"\")","v":""},{"$f":"IF(AND(OR($C$24={11,14}),OR($C$36={7})),0.85,\"\")","v":""}]
[null,null,null,"Multiplier Adjustment =",{"$f":"IFERROR(PRODUCT(E135:E138),\"\")","v":""},null,null,null,"N-Serve or Other Nitrification Inhibitor Applied",null,{"$f":"IF(OR($C$34=6,$C$34=8),1,\"\")","v":""},{"$f":"IF(OR($C$35=6,$C$35=8),1,\"\")","v":""},{"$f":"IF(OR($C$36=6,$C$36=8),1,\"\")","v":""}]
[null,"Denitrification Loss",null,null,null,null,null,null,"Split (Inseason) or Fertigation Application",null,{"$f":"IF(OR($C$31=4,$C$22=8),0.75,\"\")","v":""},{"$f":"IF(OR($C$32=4,$C$23=8),0.75,\"\")","v":""},{"$f":"IF(OR($C$33=4,$C$24=8),0.75,\"\")","v":""}]
[null,"Loss from Denitrification",null,"Loss (lbs/acre/year) =",{"$f":"E133*E139","v":{"$error":"#VALUE!"}},null,null,null,"Soil pH > 7.2",null,{"$f":"IF($D$19=\"\",\"\",IF($D$19>=7.2,2,\"\"))","v":""},{"$f":"IF($D$19=\"\",\"\",IF($D$19>=7.2,2,\"\"))","v":""},"",1]
[null,"Soil Adjustment",null,null,null,null,null,null,"Multiplier Adjustment ",null,{"$f":"IF(PRODUCT(K136:K141)=0,\"\",PRODUCT(K136:K141))","v":""},{"$f":"IF(PRODUCT(L136:L141)=0,\"\",PRODUCT(L136:L141))","v":""},{"$f":"IF(PRODUCT(M136:M141)=0,\"\",PRODUCT(M136:M141))","v":""},{"$f":"IF(PRODUCT(N141)=0,\"\",PRODUCT(N141))","v":1}]
[null,"Sand Content",null,null,{"$f":"IF(E131>0,((($D$18/100)-10)*-0.06),\"\")","v":{"$error":"#VALUE!"}},null,null,null,"Adjusted Base NH3 - Nv Values",null,{"$f":"IFERROR(IF(K142=\"\",K133,K133*K142),0)","v":0},{"$f":"IFERROR(IF(L142=\"\",L133,L133*L142),0)","v":0},{"$f":"IFERROR(IF(M142=\"\",M133,M133*M142),0)","v":0},{"$f":"IFERROR(IF(N142=\"\",N133,N133*N142),0)","v":0}]
[null,null,null,"Net Denitrification Loss (lbs/acre/year) = ",{"$f":"IFERROR(E141*E143,0)","v":0},null,null,null,null,null,"Volatization Value "]
[null,null,null,null,null,null,null,null,null,null,"from Other N Sources =",{"$f":"SUM(K143:N143)","v":0}]
[null,null,null,null,null,null,null,null,"Volatilization Loss"]
[null,"Leaching",null,"Value",null,null,null,null,"Loss from Volatilization",null,"Loss (lbs/acre/year) =",{"$f":"L119+L145","v":6.5459999999999994}]
[null,"Base Value"]
[null,"Constant",null,5.0000000000000002E-5,null,null,null,null,null,null,null,null,null,null,null,null,"Manure Type",null,null,null,null,"Inhibitors"]
[null,"Water from precipitation and irrigation (TW)",null,{"$f":"(SUM($J$16,$J$17,$J$22))^2","v":0},null,null,null,null,"Nitrous Oxide",null,"Value",null,null,null,null,1,null,null,null,null,1]
[null,"Difference total available N and N uptake",null,{"$f":"IFERROR(D107,0)","v":109.1},null,null,null,null,"Base Value",null,null,null,null,null,null,2,"Effluent Pond",null,null,null,2,"Agrotain/Agrotain Ultra"]
[null,null,"Base Value =",{"$f":"D149*D150*D151","v":0},null,null,null,null,"Constant",null,0.94,null,null,null,null,3,"Feedlot solid",null,null,null,3,"AgrotrainPlus"]
[null,"Multiplier Adjustments",null,null,null,null,null,null,"0.015*N",null,{"$f":"0.015*($C$75+$C$76)","v":0},null,null,null,null,4,"Poultry solid",null,null,null,4,"Ammonium thiosulfate"]
[null,"Individual multiplier adjustments",null,null,null,null,null,null,"0.15*Det",null,{"$f":"0.15*E144","v":0},null,null,null,null,5,"Swine lagoon",null,null,null,5,"Controlled release N Fertilizer"]
[null,"Nitrif inhib or controlled release fert used with spring app",null,{"$f":"IF(N61<>1,N61,\"\")","v":""},null,null,null,null,"minus 0.00039 * N * Det",null,{"$f":"0.00039*($C$75+$C$76)*$E$144","v":0},null,null,null,null,6,"Swine or dairy slurry",null,null,null,6,"N-Serve"]
[null,"Nitrif inhib or controlled release fert used with fall app",null,"",null,null,null,null,null,"Base Value =",{"$f":"$K$152+$K$153+$K$154-$K$155","v":0.94},null,null,null,null,7,"Swine or dairy solid",null,null,null,7,"Nutrisphere"]
[null,"AgrotainPlus used with fert application in spring app",null,"",null,null,null,null,"Water Adjustment",null,null,null,null,null,null,null,null,null,null,null,8,"Other nitrification inhibitor"]
[null,"AgrotainPlus used with fert application in fall app",null,"",null,null,null,null,"Water from precipitation and irrigation (TW)",null,{"$f":"0.01*(SUM($J$16,$J$17,$J$22))","v":0},null,null,null,null,null,null,null,null,null,9,"Other urease inhibitor"]
[null,"N inhibitor is nutrisphere",null,"",null,null,null,null,null,"Adjusted Base Value =",{"$f":"$K$156+$K$158","v":0.94},null,null,null,null,null,"Application"]
[null,"N Fertilizer is ammonium thiosulfate",null,"",null,null,null,null,"Multiplier Adjustments",null,null,null,null,null,null,1,null,null,null,null,null,"Application Method"]
[null,"N fertilizer incorporated ",null,"",null,null,null,null,"Individual multiplier adjustments",null,null,null,null,null,null,2,"Ammonium nitrate incorporated  ",null,null,null,1]
[null,"Fall applied fertilizer or manure",null,"",null,null,null,null,"Nitrification or urease inhibitor used",null,{"$f":"IF(N77<>1,N77,\"\")","v":""},null,null,null,null,3,"Ammonium nitrate surface applied",null,null,null,2,"Injected"]
[null,"Total multiplier adjustments ",null,null,null,null,null,null,"Agrotain/Agrotain Ultra or AgrotrainPlus used with urea or UAN",null,"",null,null,null,null,4,"Ammonium sulfate incorporated",null,null,null,3,"Incorporated within 7 days"]
[null,"Corn crop was preceded by a fall or winter cover crop",null,{"$f":"IF(AND(I10=2,J9=TRUE),0.8,\"\")","v":""},null,null,null,null,"N inhibitor is nutrisphere",null,"",null,null,null,null,5,"Ammonium sulfate surface applied",null,null,null,4,"Not incorporated within 7 days"]
[null,"> 40% of N applied in June or July",null,{"$f":"IF(L72>0.4,0.75,\"\")","v":""},null,null,null,null,"N fertilizer is anhydrous ammonia",null,"",null,null,null,null,6,"Anhydrous ammonia injected"]
[null,"> 50% of N applied from manure surface app or incorp",null,{"$f":"IF(L73>0.5,0.85,\"\")","v":""},null,null,null,null,"N fertilizer is urea",null,"",null,null,null,null,7,"Other incorporated/injected",null,null,null,null,"Time of Application"]
[null,"Tile drained, but only if somewhat poor or poor drainage",null,{"$f":"IF(AND($J$8=TRUE,OR($D$15=\"Somewhat poorly drained\",$D$15=\"Poorly drained\",$D$15=\"Very poorly drained\")),1.1,\"\")","v":""},null,null,null,null,"UAN injected",null,"",null,null,null,null,8,"UAN fertigation",null,null,null,1]
[null,"Fall Tilled",null,{"$f":"IF($J$6=TRUE,1.2,\"\")","v":""},null,null,null,null,"N applied as controlled released fertilizer ",null,"",null,null,null,null,9,"UAN incorporated/injected",null,null,null,2,"Fall"]
[null,"Spring Tilled",null,{"$f":"IF($J$7=TRUE,1.1,\"\")","v":""},null,null,null,null,"Total multiplier adjustments ",null,null,null,null,null,null,10,"UAN sidedress surface",null,null,null,3,"Spring "]
[null,"Hydrology class  A, B, C, or D adjustments",null,{"$f":"IF(LEFT($D$16,1)=\"A\",1.7,IF(LEFT($D$16,1)=\"B\",1,IF(LEFT($D$16,1)=\"C\",0.6,IF(LEFT($D$16,1)=\"D\",0.4,\"\"))))","v":""},null,null,null,null,"Hydrology class  A, B, C, or D adjustments",null,{"$f":"IF(LEFT($D$16,1)=\"A\",0.7,IF(LEFT($D$16,1)=\"B\",1,IF(LEFT($D$16,1)=\"C\",1.25,IF(LEFT($D$16,1)=\"D\",1.35,\"\"))))","v":""},null,null,null,null,11,"UAN surface",null,null,null,4,"In-season (spilt)"]
[null,null,"Multiplier Adjustment =",{"$f":"IFERROR(PRODUCT(D155:D170),\"\")","v":0},null,null,null,null,"Drainage is somewhat poor or worse",null,{"$f":"IF(OR($D$15=\"Somewhat poorly drained\",$D$15=\"Poorly drained\",$D$15=\"Very poorly drained\"),2,\"\")","v":""},null,null,null,null,12,"UAN sidedress injected"]
[null,"Leaching Loss",null,null,null,null,null,null,null,"Multiplier Adjustment =",{"$f":"IFERROR(PRODUCT(K162:K171),\"\")","v":0},null,null,null,null,13,"Urea incorporated"]
[null,"Loss from Leaching","Loss (lbs/acre/year) =",{"$f":"D171*D152","v":0},null,null,null,null,"Leaching Loss",null,null,null,null,null,null,14,"Urea surface"]
[null,null,null,null,null,null,null,null,"Loss from Leaching","Loss (lbs/acre/year) =",{"$f":"$K$159*$K$172","v":0}]
[]
[]
[null,"N Loss Output Formatting"]
[]
[]
[null,"N Fertilizers","N fertilizer\n Acronym 1","N fertilizer \nAcronym 2","N fertilizer \nAcronym 3"]
[null,"Fertilizer \nAcronym",{"$f":"IF(F22=0,\"#\",F22)","v":"UANSu"},{"$f":"IF(F23=0,\"#\",F23)","v":"#"},{"$f":"IF(F24=0,\"#\",F24)","v":"#"}]
[null,"Time of \nApplication Acronym",{"$f":"IF(F31=0,\"#\",F31)","v":"Sp"},{"$f":"IF(F32=0,\"#\",F32)","v":"#"},{"$f":"IF(F33=0,\"#\",F33)","v":"#"}]
[null,"Inhibitor \nAcronym",{"$f":"IF(F34=0,\"#\",F34)","v":"#"},{"$f":"IF(F35=0,\"#\",F35)","v":"#"},{"$f":"IF(F36=0,\"#\",F36)","v":"#"}]
[null,"Crop \nAvailable N",{"$f":"IF(D43=0,\"#\",D43)","v":" "},{"$f":"IF(D44=0,\"#\",D44)","v":"#"},{"$f":"IF(D45=0,\"#\",D45)","v":"#"}]
[null,"Summary ",{"$f":"IF(C181=\"#\",\"None\",C181&C182&C183&C184)","v":"UANSuSp# "},{"$f":"IF(D181=\"#\",\"\",D181&D182&D183&D184)","v":""},{"$f":"IF(E181=\"#\",\"\",E181&E182&E183&E184)","v":""}]
[]
[null,"Manure","Manure \nAcronym"]
[null,"Year applied",{"$f":"IF(OR(J35=\"\",J35=0),\"#\",J35)","v":"#"}]
[null,"Manure Type",{"$f":"IF(OR(K27=\"\",K27=0),\"#\",K27)","v":"#"}]
[null,"Application Method",{"$f":"IF(OR(K30=\"\",K30=0),\"#\",K30)","v":"#"}]
[null,"Rate of Application",{"$f":"IF(OR(J28=\"\",J28=0),\"#\",J28)","v":"#"}]
[null,"Organic N",{"$f":"IF(OR(E56=\"\",E56=0),\"#\",E56)","v":"#"}]
[null,"Ammonium N",{"$f":"IF(OR(E55=\"\",E55=0),\"#\",E55)","v":"#"}]
[null,"Summary ",{"$f":"IF(C189=\"#\",\"None\",C188&C189&\"-\"&C190&C191&\"ON\"&C192&\"AN\"&C193)","v":"None"}]
[]
[null,"Irrigation","Irrigation\nAcronym"]
[null,"Type",{"$f":"IF(K21=0,\"#\",K21)","v":"#"}]
[null,"Expected Amount Applied (inches/acre)",{"$f":"IF(D66=0,\"#\",D66)","v":" "}]
[null,"NO3-N Content (ppm)",{"$f":"IF(D67=0,\"#\",D67)","v":" "}]
[null,"Summary ",{"$f":"IF(OR(C197=\"#\",C197=\"None\"),\"None\",C197&\"-\"&C198&\"\"\"-\"&C199&\"ppm\")","v":"None"}]
[]
[]
[null,"N Loss Interface"]
[]
[]
[null,"Scenario Drop Down List",{"$f":"$C$5","v":"List ID"}]
[null,null,2]
[null,"NE Loss Assessment Tool Report",{"$f":"$D$5","v":"Interface Value"}]
[null,"Scenario number",{"$f":"INDEX(DropDownLists!K3:K8,NLossCalculations!C207)","v":1}]
[null,"Date",{"$f":"D6","v":"2015-01-06T15:10:02.210"}]
[null,"Field",{"$f":"IF(D9=0,\"No Field Name\",D9)","v":"No Field Name"}]
[null,"Scenario Name",{"$f":"IF(D10=0,\"No Scenario Name\",D10)","v":"No Scenario Name"}]
[null,"County",{"$f":"IF(D8=0,\"No County Selected\",D8)","v":"No County Selected"}]
[null,"Soil Unit",{"$f":"IF(D14=0,\"No soil selected\",D14)","v":"No Soil Selected"}]
[null,"Current Crop & Yield",{"$f":"IF($J$10=0,\"No Crop Selected\",$J$10&\": \"&$J$11&\" bu\")","v":"No Crop Selected"}]
[null,"Previous Crop",{"$f":"IF($J$12=0,\"No Crop Selected\",$J$12&\": \"&$J$13&\" bu\")","v":"No Crop Selected"}]
[null,"Cover Crop",{"$f":"IF(J9=FALSE,\"None\",\"Cover Crop Grown\")","v":"None"}]
[null,"Tillage Practice \n(Fall, Spring, or Split Till)",{"$f":"IF(AND(J6=TRUE,J7=TRUE),\"Split Till\",IF(J6=TRUE,\"Fall Till\",IF(J7=TRUE,\"Spring Till\",\"No Till\")))","v":"No Till"}]
[null,"N Fertilizer",{"$f":"C185","v":"UANSuSp# "}]
[null,"N Fertilizer",{"$f":"D185","v":""}]
[null,"N Fertilizer",{"$f":"E185","v":""}]
[null,"Manure",{"$f":"C194","v":"None"}]
[null,"Irrigation",{"$f":"C200","v":"None"}]
[null,"Total N Supply",{"$f":"IF(C14<>1,IFERROR(D100,0),0)","v":0}]
[null,"N Uptake",{"$f":"IF(D105>=0,D105,0)","v":0}]
[null,"Denitrification N lbs/acre",{"$f":"IF(E144>=0,E144,\"\")","v":0}]
[null,"Leached NO3-N lbs/acre",{"$f":"IF(C14>1,D173,0)","v":0}]
[null,"Volatilized NH3-N lbs/acre",{"$f":"IF($C$14<>1,IF(L147>=0,L147,0),0)","v":0}]
[null,"N2O-N emission N lbs/acre",{"$f":"IF(K174>=0,K174,\"\")","v":0}]
[null,"Total N Losses lbs/acre",{"$f":"C226+C227+C228+C229","v":0}]

{"sheet":"DropDownLists","index":4,"n_rows":96,"n_cols":11,"rows_kept":96,"cut":false,"hidden":true,"merged":[]}
[]
[null,"County","Previous Crop","Irrigation Type","Application","Time of Application","Inhibitors","Manure Type","Application Method","Application Timming","Scenario Number"]
[]
[null,"Adams","Corn","None","Ammonium nitrate incorporated  ","Fall","Agrotain/Agrotain Ultra","Effluent Pond","Injected","Spring ",1]
[null,"Antelope","Soybeans","Pivot","Ammonium nitrate surface applied","Spring ","AgrotrainPlus","Feedlot solid","Incorporated within 7 days","Fall",2]
[null,"Arthur",null,"Furrow","Ammonium sulfate incorporated","In-season (spilt)","Ammonium thiosulfate","Poultry solid","Not incorporated within 7 days",null,3]
[null,"Banner",null,"Drip","Ammonium sulfate surface applied",null,"Controlled release N Fertilizer","Swine lagoon",null,null,4]
[null,"Blaine",null,null,"Anhydrous ammonia injected",null,"N-Serve/Instinct","Swine or dairy slurry",null,null,5]
[null,"Boone",null,null,"Other incorporated/injected",null,"Nutrisphere","Swine or dairy solid"]
[null,"Box Butte",null,null,"UAN fertigation",null,"Other nitrification inhibitor"]
[null,"Boyd",null,null,"UAN incorporated/injected",null,"Other urease inhibitor"]
[null,"Brown",null,null,"UAN sidedress surface"]
[null,"Buffalo",null,null,"UAN surface"]
[null,"Burt",null,null,"UAN sidedress injected"]
[null,"Butler",null,null,"Urea incorporated"]
[null,"Cass",null,null,"Urea surface"]
[null,"Cedar"]
[null,"Chase",null,"Summary Abbrev.","Summary Abbrev.","Summary Abbrev.","Summary Abbrev.","Summary Abbrev.","Summary Abbrev."]
[null,"Cherry"]
[null,"Cheyenne",null,"None","AmNO3In","Fa","Ag/AgU","HP","Ij"]
[null,"Clay",null,"Pivot","AmNO3Su","Sp","Ag+","FL","I7"]
[null,"Colfax",null,"Furrow","AmSIn","Is","ATS","PO","Su"]
[null,"Cuming",null,"Drip","AmSSu",null,"CO","SG"]
[null,"Custer",null,null,"AnhIj",null,"N-S/I","SL"]
[null,"Dakota",null,null,"OthInc/Ij",null,"Nut","SD"]
[null,"Dawes",null,null,"UANFe",null,"NI"]
[null,"Dawson",null,null,"UANInc/Ij",null,"Ur"]
[null,"Deuel",null,null,"UANSSu"]
[null,"Dixon",null,null,"UANSu"]
[null,"Dodge",null,null,"UANSIj"]
[null,"Douglas",null,null,"UreaIn"]
[null,"Dundy",null,null,"UreaSu"]
[null,"Fillmore"]
[null,"Franklin"]
[null,"Frontier"]
[null,"Furnas"]
[null,"Gage"]
[null,"Garden"]
[null,"Garfield"]
[null,"Gosper"]
[null,"Grant"]
[null,"Greeley"]
[null,"Hall"]
[null,"Hamilton"]
[null,"Harlan"]
[null,"Hayes"]
[null,"Hitchcock"]
[null,"Holt"]
[null,"Hooker"]
[null,"Howard"]
[null,"Jefferson"]
[null,"Johnson"]
[null,"Kearney"]
[null,"Keith"]
[null,"Keya Paha"]
[null,"Kimball"]
[null,"Knox"]
[null,"Lancaster"]
[null,"Lincoln"]
[null,"Logan"]
[null,"Loup"]
[null,"McPherson"]
[null,"Madison"]
[null,"Merrick"]
[null,"Morrill"]
[null,"Nance"]
[null,"Nemaha"]
[null,"Nuckolls"]
[null,"Otoe"]
[null,"Pawnee"]
[null,"Perkins"]
[null,"Phelps"]
[null,"Pierce"]
[null,"Platte"]
[null,"Polk"]
[null,"Red Willow"]
[null,"Richardson"]
[null,"Rock"]
[null,"Saline"]
[null,"Sarpy"]
[null,"Saunders"]
[null,"Scotts Bluff"]
[null,"Seward"]
[null,"Sheridan"]
[null,"Sherman"]
[null,"Sioux"]
[null,"Stanton"]
[null,"Thayer"]
[null,"Thomas"]
[null,"Thurston"]
[null,"Valley"]
[null,"Washington"]
[null,"Wayne"]
[null,"Webster"]
[null,"Wheeler"]
[null,"York"]

{"sheet":"NEpreviousCrop","index":5,"n_rows":4,"n_cols":3,"rows_kept":4,"cut":false,"hidden":true,"merged":[]}
[null,"Default Current","Default Previous"]
["Crop","Yield","Yield"]
["Corn",200,200]
["Soybeans",60,60]

{"sheet":"NEcountySoil","index":6,"n_rows":7285,"n_cols":8,"rows_kept":7285,"cut":false,"hidden":true,"merged":[]}
["areasymbol","county","muname","drainagecl","hydgrp","om_r","sandtotal_r","ph1to1h2o_r"]
["NE001","Adams",null,"",""]
["NE001","Adams","Anselmo fine sandy loam, terrace, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE001","Adams","Anselmo fine sandy loam, terrace, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE001","Adams","Boel fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.25,84.3,7.8]
["NE001","Adams","Bolent loam, occasionally flooded","Somewhat poorly drained","C",0.25,62.8,7.9]
["NE001","Adams","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE001","Adams","Calamus loamy fine sand, rarely flooded","Moderately well drained","A",0.25,92.5,7]
["NE001","Adams","Cass fine sandy loam, overwash, occasionally flooded","Well drained","A",1.25,67.599999999999994,7.3]
["NE001","Adams","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE001","Adams","Cass loam, occasionally flooded","Well drained","C",0.75,62,7.3]
["NE001","Adams","Cass loam, rarely flooded","Well drained","B",0.75,62,7.3]
["NE001","Adams","Cass silt loam, occasionally flooded","Well drained","B",0.75,85.4,7.3]
["NE001","Adams","Coly silt loam, 11 to 30 percent slopes","Somewhat excessively drained","B",1.125,11.3,7.9]
["NE001","Adams","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE001","Adams","Coly silt loam, 6 to 11 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE001","Adams","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE001","Adams","Coly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",1.125,11.3,7.7]
["NE001","Adams","Coly-Uly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.8]
["NE001","Adams","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE001","Adams","Cozad loam, sand substratum, 0 to 3 percent slopes","Well drained","B",1.375,47.45,6.35]
["NE001","Adams","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE001","Adams","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE001","Adams","Deroin soils, 6 to 11 percent slopes, severely eroded","Well drained","C",0.5,6.7,7]
["NE001","Adams","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE001","Adams","Gates fine sandy loam, 0 to 3 percent slopes, hummocky","Well drained","B",0.5,52.95,6.3000000000000007]
["NE001","Adams","Gates silt loam, 0 to 1 percent slopes","Well drained","B",0.375,37.85,7.7]
["NE001","Adams","Gates silt loam, 1 to 3 percent slopes","Well drained","B",0.5,13.9,7.5]
["NE001","Adams","Geary silt loam, 11 to 30 percent slopes","Somewhat excessively drained","C",1.25,7.4,6.7]
["NE001","Adams","Geary silt loam, 3 to 7 percent slopes","Well drained","C",1.25,6.9,6.7]
["NE001","Adams","Geary silt loam, 7 to 11 percent slopes","Well drained","C",1.25,6.9,6.7]
["NE001","Adams","Geary silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE001","Adams","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE001","Adams","Geary-Hobbs silt loams, 0 to 30 percent slopes","Well drained","C",0.75,9.5,7]
["NE001","Adams","Gothenburg loam, frequently flooded","Poorly drained","B/D",0.5,81,7.2]
["NE001","Adams","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,91.9,7.3]
["NE001","Adams","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE001","Adams","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE001","Adams","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE001","Adams","Hastings silt loam, thin solum variant","Well drained","C",0.75,8,6.5]
["NE001","Adams","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE001","Adams","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.5]
["NE001","Adams","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.25,66.099999999999994,7.2]
["NE001","Adams","Hersh-Kenesaw complex, undulating","Well drained","A",0.5,37.5,7.2]
["NE001","Adams","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE001","Adams","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE001","Adams","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,7.5,7]
["NE001","Adams","Holder loam, 0 to 3 percent slopes, overblown","Well drained","C",1.625,9.0500000000000007,7]
["NE001","Adams","Holder silt loam, 0 to 1 percent slopes","Well drained","C",0.75,10,6.6]
["NE001","Adams","Holder silt loam, 1 to 3 percent slopes","Well drained","C",0.75,10,6.6]
["NE001","Adams","Holder silt loam, 3 to 7 percent slopes","Well drained","C",0.25,9.4,7]
["NE001","Adams","Holder silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.25,9.4,7]
["NE001","Adams","Holder silt loam, 7 to 11 percent slopes","Well drained","C",0.25,9.4,7]
["NE001","Adams","Holder silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1,9.1,7]
["NE001","Adams","Holder silty clay loam, 3 to 7 percent slopes, severely eroded","Well drained","C",0.25,7.4,7]
["NE001","Adams","Holder silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.25,9.1,7]
["NE001","Adams","Holder silty clay loam, 7 to 11 percent slopes, severely eroded","Well drained","C",0.25,7.4,7]
["NE001","Adams","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE001","Adams","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE001","Adams","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE001","Adams","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.25,7.2]
["NE001","Adams","Holdrege silt loam, 7 to 11 percent slopes","Well drained","C",1.25,7,7.2]
["NE001","Adams","Holdrege soils, 3 to 7 percent slopes, severely eroded","Well drained","C",0.75,6.3,7.2]
["NE001","Adams","Holdrege soils, 7 to 11 percent slopes, severely eroded","Well drained","C",0.75,6.3,7.2]
["NE001","Adams","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,11.2,7]
["NE001","Adams","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE001","Adams","Hord silt loam, rarely flooded","Well drained","B",0.75,9.3000000000000007,7]
["NE001","Adams","Inavale fine sandy loam, occasionally flooded","Excessively drained","A",0.25,77.699999999999989,6.7]
["NE001","Adams","Inavale loamy fine sand, occasionally flooded","Excessively drained","A",0.25,87.3,6.7]
["NE001","Adams","Inavale loamy fine sand, rarely flooded","Excessively drained","A",0.25,87.3,6.7]
["NE001","Adams","Kenesaw silt loam, 0 to 1 percent slopes","Well drained","B",0.75,11.5,7.5]
["NE001","Adams","Kenesaw silt loam, 1 to 3 percent slopes","Well drained","B",0.75,6,7.5]
["NE001","Adams","Kenesaw silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14,7.5]
["NE001","Adams","Lex silt loam, rarely flooded","Somewhat poorly drained","C",1.375,41.6,8.1999999999999993]
["NE001","Adams","Massie silt loam, frequently ponded","Very poorly drained","D",3.125,16.75,6.25]
["NE001","Adams","Massie silty clay loam, frequently ponded","Very poorly drained","D",1.25,6,6.4]
["NE001","Adams","Meadin sandy loam, 0 to 2 percent slopes","Excessively drained","A",0.875,84.05,6.45]
["NE001","Adams","Ortello loam, 0 to 1 percent slopes","Well drained","B",0.75,69.599999999999994,6.8]
["NE001","Adams","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,63.2,7.5]
["NE001","Adams","Platte-Bolent complex, occasionally flooded","Somewhat poorly drained","B",0.25,66.900000000000006,7.45]
["NE001","Adams","Rusco silt loam, 0 to 1 percent slopes","Moderately well drained","C/D",0.75,11.2,7.5]
["NE001","Adams","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE001","Adams","Simeon sandy loam, 0 to 3 percent slopes","Excessively drained","A",0.5,79.25,6.75]
["NE001","Adams","Spoil banks","Well drained","B",0.75,6.8,7.9]
["NE001","Adams","Thurman-Valentine loamy fine sands, undulating","Somewhat excessively drained","A",0.25,87.3,6.5]
["NE001","Adams","Uly-Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.8]
["NE001","Adams","Uly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,10.35,7]
["NE001","Adams","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,7]
["NE001","Adams","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,7]
["NE001","Adams","Valentine loamy fine sand, rolling","Excessively drained","A",0.25,87.3,6.5]
["NE003","Antelope",null,"",""]
["NE003","Antelope","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE003","Antelope","Alcester silty clay loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE003","Antelope","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE003","Antelope","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE003","Antelope","Anselmo loam, 0 to 1 percent slopes","Well drained","B",0.75,66.099999999999994,6.7]
["NE003","Antelope","Barney-Boel-Calamus complex, channeled","Poorly drained","B/D",0.25,92.1,7.2]
["NE003","Antelope","Bazile complex, 0 to 3 percent slopes","Well drained","C",0.75,58,6.75]
["NE003","Antelope","Bazile complex, 3 to 6 percent slopes","Well drained","C",0.75,58,6.75]
["NE003","Antelope","Bazile complex, 6 to 11 percent slopes","Well drained","C",0.75,58,6.75]
["NE003","Antelope","Bazile loam, 0 to 2 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE003","Antelope","Bazile loam, 2 to 6 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE003","Antelope","Bazile loam, 6 to 11 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE003","Antelope","Bazile loamy fine sand, 0 to 2 percent slopes","Well drained","C",0.75,87.3,6.5]
["NE003","Antelope","Bazile loamy fine sand, 2 to 6 percent slopes","Well drained","C",0.75,87.3,6.5]
["NE003","Antelope","Bazile silt loam, 0 to 2 percent slopes","Well drained","C",0.75,19.95,7]
["NE003","Antelope","Blackloup loam, occasionally flooded","Very poorly drained","B/D",0.5,72.55,7.4]
["NE003","Antelope","Blackloup loam, rarely flooded","Poorly drained","B/D",0.75,65.900000000000006,7.4]
["NE003","Antelope","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.125,66.699999999999989,6.5]
["NE003","Antelope","Blendon fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.125,66.699999999999989,6.85]
["NE003","Antelope","Boelus fine sand, 0 to 6 percent slopes","Well drained","B",0.5,55.2,6.65]
["NE003","Antelope","Boelus loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.5,55.2,6.65]
["NE003","Antelope","Boelus loamy fine sand, 2 to 6 percent slopes","Well drained","B",0.5,55.2,6.65]
["NE003","Antelope","Boelus loamy sand, 0 to 3 percent slopes","Well drained","B",0.5,51.849999999999994,7.15]
["NE003","Antelope","Boelus loamy sand, 3 to 6 percent slopes","Well drained","B",0.5,53.9,7.15]
["NE003","Antelope","Boelus loamy sand, 6 to 11 percent slopes","Well drained","B",0.5,53.9,7.15]
["NE003","Antelope","Brunswick-Paka complex, 11 to 30 percent slopes","Well drained","B",0.5,23.55,6.6]
["NE003","Antelope","Brunswick-Paka complex, 17 to 30 percent slopes","Well drained","B",0.5,32.1,6.6]
["NE003","Antelope","Brunswick-Pivot complex, 11 to 30 percent slopes","Well drained","B",0.25,81.75,6.5]
["NE003","Antelope","Calamus-Boel complex, channeled, rarely flooded","Somewhat poorly drained","A",0.25,96.3,7.5]
["NE003","Antelope","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE003","Antelope","Cass loam, occasionally flooded","Well drained","B",0.75,63.5,7.3]
["NE003","Antelope","Cass loam, rarely flooded","Well drained","A",0.75,63.5,7.3]
["NE003","Antelope","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,11.2,7]
["NE003","Antelope","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE003","Antelope","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE003","Antelope","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE003","Antelope","Crofton silt loam, coarse, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE003","Antelope","Crofton soils, 30 to 60 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE003","Antelope","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE003","Antelope","Crofton-Nora silt loams, 11 to 17 percent slopes, eroded","Well drained","B",1.25,9.4,7.9]
["NE003","Antelope","Crofton-Nora silt loams, 17 to 30 percent slopes","Well drained","B",0.75,9.4,7.5]
["NE003","Antelope","Crofton-Nora silt loams, 2 to 6 percent slopes, eroded","Well drained","B",1.25,9.4,7.9]
["NE003","Antelope","Crofton-Nora silt loams, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.4,7.9]
["NE003","Antelope","Doger fine sand, 0 to 6 percent slopes","Somewhat excessively drained","A",1,95.85,6.75]
["NE003","Antelope","Doger loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",1.25,91.35,6.85]
["NE003","Antelope","Doger loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",1.25,91.35,6.85]
["NE003","Antelope","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE003","Antelope","Dunday loamy fine sand, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE003","Antelope","Dunday loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,89.6,6.85]
["NE003","Antelope","Dunday loamy sand, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,89.6,6.85]
["NE003","Antelope","Elsmere fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.875,96.8,6.6]
["NE003","Antelope","Elsmere fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.25,79.400000000000006,7]
["NE003","Antelope","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.875,91.35,6.7]
["NE003","Antelope","Elsmere-Ipage loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,94.9,7]
["NE003","Antelope","Fillmore silt loam, occasionally ponded","Somewhat poorly drained","D",1.5,7.5,6.7]
["NE003","Antelope","Fluvaquents, frequently flooded","Very poorly drained","A/D",5,12,7.5]
["NE003","Antelope","Fluvaquents, sandy-Fluvaquents, loamy complex, frequently flooded","Very poorly drained","A/D",0.5,78.95,7.55]
["NE003","Antelope","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE003","Antelope","Gibbon silt loam, saline, occasionally flooded","Somewhat poorly drained","C",0.75,7.8,7.9]
["NE003","Antelope","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE003","Antelope","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE003","Antelope","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE003","Antelope","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,8,7]
["NE003","Antelope","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE003","Antelope","Inavale fine sand, channeled, frequently flooded","Excessively drained","A",0.25,92.2,6.7]
["NE003","Antelope","Inavale fine sand, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE003","Antelope","Inavale fine sandy loam, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE003","Antelope","Inglewood-Boel complex, channeled, occasionally flooded","Somewhat poorly drained","A",0.25,92.9,7.25]
["NE003","Antelope","Kezan silt loam, occasionally flooded","Poorly drained","C",1.875,7.85,7.35]
["NE003","Antelope","Lawet silt loam, occasionally flooded","Poorly drained","C/D",2.875,40.35,8.0500000000000007]
["NE003","Antelope","Lawet soils, wet, occasionally flooded","Very poorly drained","C/D",2.875,40.35,8.0500000000000007]
["NE003","Antelope","Lawet-Saltine complex, occasionally flooded","Poorly drained","B/D",0.25,11.3,8.5]
["NE003","Antelope","Longford complex, 1 to 7 percent slopes","Well drained","C",0.5,22.7,6.7]
["NE003","Antelope","Longford loam, 1 to 7 percent slopes","Well drained","C",1.25,24,6.7]
["NE003","Antelope","Loretto fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE003","Antelope","Loretto fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE003","Antelope","Loretto loam, 0 to 2 percent slopes","Well drained","B",1.125,39.1,6.75]
["NE003","Antelope","Loretto loam, 2 to 6 percent slopes","Well drained","B",1.125,39.1,6.75]
["NE003","Antelope","Loretto sandy loam, 0 to 3 percent slopes","Well drained","B",1.5,39.1,6.5]
["NE003","Antelope","Loretto sandy loam, 3 to 6 percent slopes","Well drained","B",1.5,39.1,6.5]
["NE003","Antelope","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,63.5,7.5]
["NE003","Antelope","Loup fine sandy loam, drained, 0 to 3 percent slopes","Poorly drained","A/D",1.5,85.9,7.3]
["NE003","Antelope","Loup fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,79.2,7.5]
["NE003","Antelope","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,78.2,7.5]
["NE003","Antelope","Meadin sandy loam, 0 to 2 percent slopes","Excessively drained","A",0.75,85.7,6.2]
["NE003","Antelope","Meadin sandy loam, 2 to 30 percent slopes","Excessively drained","A",0.75,85.7,6.2]
["NE003","Antelope","Meadin-O'Neill complex, 2 to 30 percent slopes","Excessively drained","B",0.75,68.150000000000006,6.35]
["NE003","Antelope","Moody loam, 0 to 2 percent slopes","Well drained","C",3,9.4,6.5]
["NE003","Antelope","Moody loam, 2 to 6 percent slopes","Well drained","C",3,9.4,6.5]
["NE003","Antelope","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE003","Antelope","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE003","Antelope","Nenzel loamy fine sand, very rarely flooded","Moderately well drained","A",1.375,89.550000000000011,6.7]
["NE003","Antelope","Nora silt loam, 0 to 2 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE003","Antelope","Nora silt loam, 11 to 17 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE003","Antelope","Nora silt loam, 2 to 6 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE003","Antelope","Nora silt loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,9.1,6.5]
["NE003","Antelope","Nora silt loam, 6 to 11 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE003","Antelope","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,8,6.5]
["NE003","Antelope","Nora silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,8.9,7]
["NE003","Antelope","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE003","Antelope","Nora-Crofton complex, 2 to 6 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE003","Antelope","Obert silt loam, occasionally flooded","Very poorly drained","C/D",1.5,7.3,7.9]
["NE003","Antelope","O'Neill loam, 0 to 2 percent slopes","Well drained","B",0.75,67.599999999999994,6.5]
["NE003","Antelope","O'Neill sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,68.5,6.5]
["NE003","Antelope","O'Neill sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,68.5,6.5]
["NE003","Antelope","Ord fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE003","Antelope","Ord loam, rarely flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE003","Antelope","Ortello fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE003","Antelope","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE003","Antelope","Ortello fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE003","Antelope","Ortello loam, 0 to 1 percent slopes","Well drained","B",0.75,63.5,6.7]
["NE003","Antelope","Ortello loam, 1 to 6 percent slopes","Well drained","B",0.75,63.5,6.7]
["NE003","Antelope","Orwet loam, rarely flooded","Poorly drained","B/D",0.75,63.5,7.5]
["NE003","Antelope","Ovina loamy fine sand, rarely flooded","Somewhat poorly drained","B",1.125,75.2,7.7]
["NE003","Antelope","Paka complex, 0 to 2 percent slopes","Well drained","C",0.75,27.1,6.5]
["NE003","Antelope","Paka complex, 2 to 6 percent slopes","Well drained","C",0.75,27.1,6.5]
["NE003","Antelope","Paka complex, 6 to 11 percent slopes","Well drained","C",0.75,27.1,6.5]
["NE003","Antelope","Paka fine sandy loam, 0 to 2 percent slopes","Well drained","B",1.125,9.1,7.1]
["NE003","Antelope","Paka fine sandy loam, 2 to 6 percent slopes","Well drained","B",1.125,9.1,7.45]
["NE003","Antelope","Paka loam, 0 to 2 percent slopes","Well drained","C",1.125,20.149999999999999,7.1]
["NE003","Antelope","Paka loam, 2 to 6 percent slopes","Well drained","C",1.125,20.149999999999999,7.1]
["NE003","Antelope","Paka loam, 6 to 11 percent slopes, eroded","Well drained","C",1.125,8.25,7.1]
["NE003","Antelope","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE003","Antelope","Simeon sand, 6 to 30 percent slopes, eroded","Excessively drained","A",0.5,91.85,7]
["NE003","Antelope","Simeon sandy loam, 0 to 6 percent slopes","Excessively drained","A",0.5,80.199999999999989,7]
["NE003","Antelope","Thurman fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,94.9,6.5]
["NE003","Antelope","Thurman fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,94.9,6.5]
["NE003","Antelope","Thurman fine sand, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,94.9,6.5]
["NE003","Antelope","Thurman fine sandy loam, 2 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE003","Antelope","Thurman loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE003","Antelope","Thurman loamy fine sand, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE003","Antelope","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE003","Antelope","Thurman-Crofton complex, 11 to 30 percent slopes","Well drained","B",0.25,84.9,6.5]
["NE003","Antelope","Thurman-Valentine complex, undulating","Somewhat excessively drained","A",0.25,94,6.5]
["NE003","Antelope","Trent silt loam, 0 to 2 percent slopes","Moderately well drained","C",2.5,9.1,6.7]
["NE003","Antelope","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE003","Antelope","Valentine fine sand, 0 to 6 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE003","Antelope","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE003","Antelope","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE003","Antelope","Valentine-Dunday loamy fine sands, 0 to 3 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE003","Antelope","Valentine-Dunday loamy fine sands, 3 to 9 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE003","Antelope","Valentine-Simeon complex, 0 to 3 percent slopes","Excessively drained","A",0.5,94.199999999999989,6.75]
["NE003","Antelope","Valentine-Simeon complex, 3 to 6 percent slopes","Excessively drained","A",0.5,94.199999999999989,6.75]
["NE003","Antelope","Valentine-Simeon complex, 6 to 11 percent slopes","Excessively drained","A",0.5,94.199999999999989,6.75]
["NE003","Antelope","Valentine-Simeon sands, 3 to 9 percent slopes","Excessively drained","A",0.5,93.8,6.6]
["NE005","Arthur",null,"",""]
["NE005","Arthur","Clawhammer-Ord complex, 0 to 3 percent slopes","Poorly drained","B/D",1.5,70,8]
["NE005","Arthur","Crowther loam, 0 to 1 percent slopes","Poorly drained","B/D",6.75,42.2,7.7]
["NE005","Arthur","Crowther mucky peat","Very poorly drained","B/D",6.75,38.5,7.7]
["NE005","Arthur","Cullison loam, 0 to 1 percent slopes","Poorly drained","B/D",3,33.5,7.9]
["NE005","Arthur","Cullison mucky peat","Very poorly drained","B/D",12,33.5,7.9]
["NE005","Arthur","Cutcomb mucky peat","Very poorly drained","A/D",55,0,5.8]
["NE005","Arthur","Doughboy fine sandy loam, 0 to 3 percent slopes","Moderately well drained","A",2,50,7.9]
["NE005","Arthur","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.75,86.8,6.7]
["NE005","Arthur","Els calcareous-Hoffland complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.625,94.1,7.9]
["NE005","Arthur","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.7]
["NE005","Arthur","Elsmere loamy fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,79.400000000000006,7.9]
["NE005","Arthur","Gannett mucky peat","Very poorly drained","A/D",6.375,41.9,6.55]
["NE005","Arthur","Gus mucky peat","Very poorly drained","B/D",9.5,35.200000000000003,7]
["NE005","Arthur","Ipage calcareous-Hoffland complex, 0 to 3 percent slopes","Very poorly drained","A/D",0.625,94.1,8]
["NE005","Arthur","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.95]
["NE005","Arthur","Ipage-Els complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,95.4,6.5]
["NE005","Arthur","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","B",0.75,72.900000000000006,7.4]
["NE005","Arthur","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,94.9,6.7]
["NE005","Arthur","Loup mucky peat","Very poorly drained","A/D",4,63.5,6.6]
["NE005","Arthur","Marlake mucky peat","Very poorly drained","A/D",3.375,76.449999999999989,6.5500000000000007]
["NE005","Arthur","Medihemists","Very poorly drained","A/D",40,0,5.8]
["NE005","Arthur","Nenzel loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",1.25,86.8,6.7]
["NE005","Arthur","Nenzel loamy fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",1.375,91.4,7.9]
["NE005","Arthur","Ord loam, 0 to 3 percent slopes","Somewhat poorly drained","B",1.5,67,7.4]
["NE005","Arthur","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,6.5]
["NE005","Arthur","Valentine fine sand, hilly","Excessively drained","A",0.5,94.9,6.5]
["NE005","Arthur","Valentine fine sand, rolling","Excessively drained","A",0.5,94.9,6.5]
["NE005","Arthur","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,94.9,6.5]
["NE005","Arthur","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.75,86.8,6.7]
["NE005","Arthur","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.625,95.4,6.5]
["NE005","Arthur","Valentine-Hoffland, complex, 0 to 24 percent slopes","Very poorly drained","A/D",0.625,94.1,7.15]
["NE005","Arthur","Valentine-Libory complex, 0 to 9 percent slopes","Moderately well drained","B",0.625,90.05,6.55]
["NE005","Arthur","Valentine-Tryon complex, 0 to 24 percent slopes","Very poorly drained","A/D",0.625,94.1,6.5]
["NE005","Arthur","Wildhorse-Hoffland complex, 0 to 3 percent slopes","Poorly drained","A/D",2,94.9,9.1]
["NE007","Banner",null,"",""]
["NE007","Banner","Albinas-Cheyenne loams, rarely flooded","Well drained","C",1.25,41.4,7.2]
["NE007","Banner","Alice fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.9]
["NE007","Banner","Alice fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,62.5,7.9]
["NE007","Banner","Alice fine sandy loam, 6 to 9 percent slopes, eroded","Well drained","A",0.75,62.5,7.9]
["NE007","Banner","Alliance loam, 0 to 1 percent slopes","Well drained","B",0.75,31.9,7.2]
["NE007","Banner","Alliance loam, 1 to 3 percent slopes","Well drained","B",0.75,31.9,7.2]
["NE007","Banner","Alliance loam, 3 to 6 percent slopes","Well drained","B",0.75,31.9,7.2]
["NE007","Banner","Alliance loam, 6 to 9 percent slopes, eroded","Well drained","B",0.75,32.15,7.2]
["NE007","Banner","Altvan fine sandy loam, 1 to 3 percent slopes","Well drained","C",0.75,54.5,7.5]
["NE007","Banner","Altvan loam, 3 to 6 percent slopes","Well drained","B",0.75,41.75,7.7]
["NE007","Banner","Altvan-Eckley complex, 3 to 9 percent slopes","Well drained","B",0.75,55.1,7.2]
["NE007","Banner","Altvan-Satanta fine sandy loams, 1 to 3 percent slopes","Well drained","C",0.75,40.549999999999997,7.5]
["NE007","Banner","Altvan-Satanta loams, 0 to 1 percent slopes","Well drained","C",0.75,40,7.5]
["NE007","Banner","Bankard fine sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,94.75,7.9]
["NE007","Banner","Bankard loamy fine sand, occasionally flooded","Somewhat excessively drained","A",0.75,90.449999999999989,8.0500000000000007]
["NE007","Banner","Bayard fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.125,65.400000000000006,6.85]
["NE007","Banner","Bayard fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.125,65.400000000000006,6.85]
["NE007","Banner","Bayard very fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE007","Banner","Bayard very fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE007","Banner","Bayard very fine sandy loam, 6 to 9 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE007","Banner","Bayard very fine sandy loam, 9 to 20 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE007","Banner","Bayard-Dix complex, 3 to 9 percent slopes","Well drained","A",1.125,62.9,7.35]
["NE007","Banner","Bayard-Dix complex, 9 to 20 percent slopes","Well drained","A",1.125,62.9,7.35]
["NE007","Banner","Bridget very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE007","Banner","Bridget very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE007","Banner","Bridget very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE007","Banner","Bridget very fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE007","Banner","Bridget very fine sandy loam, 9 to 20 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE007","Banner","Broadwater loamy sand, channeled, occasionally flooded","Excessively drained","A",0.25,91.9,7.2]
["NE007","Banner","Busher-Tassel complex, 9 to 20 percent slopes","Well drained","A",0.5,64.05,7.25]
["NE007","Banner","Busher-Tassel loamy very fine sands, 9 to 20 percent slopes","Well drained","A",1,79.3,7.25]
["NE007","Banner","Canyon fine sandy loam, 6 to 30 percent slopes","Well drained","D",1.25,60.9,7.9]
["NE007","Banner","Canyon loam, 9 to 30 percent slopes","Well drained","D",1.25,43,7.9]
["NE007","Banner","Canyon-Rock outcrop complex, 20 to 60 percent slopes","Well drained","D",0.625,21.9,3.95]
["NE007","Banner","Canyon-Sidney loams, 9 to 20 percent slopes, eroded","Well drained","D",1,43.4,7.9]
["NE007","Banner","Creighton very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE007","Banner","Creighton very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE007","Banner","Dix sandy loam, 0 to 3 percent slopes","Excessively drained","A",1.125,79.900000000000006,7.25]
["NE007","Banner","Duroc loam, 0 to 1 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE007","Banner","Duroc loam, 1 to 3 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE007","Banner","Eckley and Altvan soils, 9 to 50 percent slopes","Well drained","C",1,69,7.2]
["NE007","Banner","Eckley gravelly sandy loam, 3 to 30 percent slopes","Well drained","B",1.25,67.900000000000006,7]
["NE007","Banner","Epping silt loam, 9 to 30 percent slopes","Well drained","D",0.75,26.7,7.5]
["NE007","Banner","Glenberg very fine sandy loam, 0 to 2 percent slopes","Well drained","B",0.5,73.099999999999994,8.0500000000000007]
["NE007","Banner","Goshen loam, 0 to 1 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE007","Banner","Janise loam, occasionally flooded","Somewhat poorly drained","C",0.75,42.2,9.4]
["NE007","Banner","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,67.599999999999994,7.2]
["NE007","Banner","Keith loam, 0 to 1 percent slopes","Well drained","B",0.75,38,7]
["NE007","Banner","Keith loam, 1 to 3 percent slopes","Well drained","B",0.75,38,7]
["NE007","Banner","Keith loam, 3 to 6 percent slopes","Well drained","B",0.75,38,7]
["NE007","Banner","Lisco fine sandy loam, 0 to 2 percent slopes","Somewhat poorly drained","C",0.25,63.5,8.8000000000000007]
["NE007","Banner","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",1.375,26.55,7.25]
["NE007","Banner","Mitchell very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1,60.5,7.9]
["NE007","Banner","Mitchell very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1,60.5,7.9]
["NE007","Banner","Mitchell very fine sandy loam, 3 to 6 percent slopes","Well drained","B",1,60.5,7.9]
["NE007","Banner","Mitchell very fine sandy loam, 6 to 9 percent slopes","Well drained","B",1,60.5,7.9]
["NE007","Banner","Mitchell-Epping complex, 3 to 9 percent slopes","Well drained","D",0.75,30.1,7.9]
["NE007","Banner","Mitchell-Epping complex, 9 to 30 percent slopes","Well drained","D",0.75,30.1,7.9]
["NE007","Banner","Otero loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.75,80.3,7.9]
["NE007","Banner","Otero loamy very fine sand, 3 to 9 percent slopes","Well drained","A",0.75,80.3,7.9]
["NE007","Banner","Otero loamy very fine sand, 9 to 20 percent slopes","Well drained","A",0.75,80.3,7.9]
["NE007","Banner","Otero-Epping complex, 9 to 60 percent slopes","Well drained","D",0.75,30.1,7.9]
["NE007","Banner","Rock outcrop-Epping complex, 20 to 60 percent slopes","Well drained","D",0.375,15.05,3.95]
["NE007","Banner","Rosebud loam, 1 to 3 percent slopes","Well drained","C",0.75,38,7.35]
["NE007","Banner","Rosebud-Blanche complex , 1 to 3 percent slopes","Well drained","B",0.5,38,7.6]
["NE007","Banner","Rosebud-Canyon loams, 1 to 3 percent slopes","Well drained","D",0.75,37,7.2]
["NE007","Banner","Rosebud-Canyon loams, 3 to 6 percent slopes","Well drained","D",0.75,42,7.5]
["NE007","Banner","Sarben loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.25,84,7.2]
["NE007","Banner","Sarben loamy very fine sand, 3 to 9 percent slopes","Well drained","A",0.25,84,7.2]
["NE007","Banner","Sarben very fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,62,7.2]
["NE007","Banner","Satanta fine sandy loam, 1 to 3 percent slopes","Well drained","C",1,65.400000000000006,7.7]
["NE007","Banner","Satanta loam, gravelly substratum, 3 to 6 percent slopes","Well drained","C",1,43,7.5500000000000007]
["NE007","Banner","Satanta-Altvan complex, 3 to 6 percent slopes","Well drained","B",1,59.3,7.5]
["NE007","Banner","Sidney-Canyon complex, 3 to 9 percent slopes","Well drained","D",0.75,44.3,7.9]
["NE007","Banner","Sidney-Canyon loams, 3 to 6 percent slopes","Well drained","D",1,43.4,7.9]
["NE007","Banner","Sidney-Canyon loams, 6 to 9 percent slopes, eroded","Well drained","D",1,43.4,7.9]
["NE007","Banner","Tassel-Ashollow-Rock outcrop complex, 20 to 60 percent slopes","Well drained","B",0.75,63.3,7.9]
["NE007","Banner","Tassel-Blanche complex, 9 to 30 percent slopes","Well drained","B",0.25,62.5,7.75]
["NE007","Banner","Tassel-Blanche sandy loams, 3 to 9 percent slopes","Well drained","B",0.25,62.5,7.6]
["NE007","Banner","Tassel-Busher-Rock outcrop complex, 20 to 60 percent slopes","Well drained","A",1,79.3,7.25]
["NE007","Banner","Tassel-Busher-Rock outcrop complex, 9 to 60 percent slopes","Well drained","A",0.75,63.6,7]
["NE007","Banner","Tripp loamy very fine sand, overblown, 0 to 3 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE007","Banner","Tripp loamy very fine sand, overblown, 3 to 6 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE007","Banner","Tripp very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE007","Banner","Tripp very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE007","Banner","Tripp very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE007","Banner","Tripp very fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE007","Banner","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE007","Banner","Valent fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE007","Banner","Valent loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,89.45,7.2]
["NE007","Banner","Valent loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,89.45,7.2]
["NE007","Banner","Vetal fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE007","Banner","Vetal very fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,62,7]
["NE007","Banner","Yockey loam, alkali, occasionally flooded","Somewhat poorly drained","C",0.625,49.5,8.75]
["NE009","Blaine",null,"",""]
["NE009","Blaine","Almeria fine sandy loam, occasionally flooded","Poorly drained","A/D",3.375,77.75,6.9]
["NE009","Blaine","Almeria loamy fine sand, channeled, frequently flooded","Very poorly drained","A/D",1.25,75.349999999999994,6.9]
["NE009","Blaine","Almeria loamy fine sand, occasionally flooded","Poorly drained","A/D",0.25,92.9,6.5]
["NE009","Blaine","Almeria loamy fine sand, wet, occasionally flooded","Poorly drained","A/D",0.25,75.349999999999994,6.5]
["NE009","Blaine","Bolent loamy sand, occasionally flooded","Somewhat poorly drained","A",0.5,88.6,7.7]
["NE009","Blaine","Bolent-Calamus loamy sands, rarely flooded","Somewhat poorly drained","B",0.27500000000000002,91,7.25]
["NE009","Blaine","Calamus loamy sand, rarely flooded","Moderately well drained","A",0.75,90.7,7]
["NE009","Blaine","Dunn loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,85.3,6.5]
["NE009","Blaine","Dunn loamy fine sand, 9 to 20 percent slopes","Moderately well drained","A",0.75,85.3,6.5]
["NE009","Blaine","Dunn-Josburg loamy fine sands, 3 to 9 percent slopes","Moderately well drained","A",0.5,68.400000000000006,6.5]
["NE009","Blaine","Els loamy sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,89.85,6.6]
["NE009","Blaine","Els-Ipage complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,95.15,6.35]
["NE009","Blaine","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,95.15,6.35]
["NE009","Blaine","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,40.85,3.75]
["NE009","Blaine","Gates very fine sandy loam, 11 to 17 percent slopes","Well drained","B",0.5,58.6,7.5]
["NE009","Blaine","Gates very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.5,58.6,7.5]
["NE009","Blaine","Gates-Hersh complex, 20 to 60 percent slopes","Well drained","B",0.625,62.849999999999994,7.35]
["NE009","Blaine","Hersh loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.75,84,6.7]
["NE009","Blaine","Hersh-Gates complex, 0 to 3 percent slopes","Well drained","B",0.625,62.849999999999994,7.35]
["NE009","Blaine","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE009","Blaine","Ipage fine sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,96.8,6.5]
["NE009","Blaine","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE009","Blaine","Ipage loamy fine sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,94.4,6.5]
["NE009","Blaine","Ipage sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,96,6.5]
["NE009","Blaine","Ipage-Tryon complex, 0 to 3 percent slopes","Moderately well drained","A",0.75,95.15,6.45]
["NE009","Blaine","Jansen fine sandy loam, 0 to 2 percent slopes","Well drained","B",0.75,67,6.2]
["NE009","Blaine","Jansen loamy fine sand, 0 to 2 percent slopes","Well drained","B",0.75,78.599999999999994,6.2]
["NE009","Blaine","Josburg-Dunn loamy fine sands, 0 to 2 percent slopes","Moderately well drained","A",0.5,68.400000000000006,6.5]
["NE009","Blaine","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,72.150000000000006,7.15]
["NE009","Blaine","Marlake loamy fine sand, frequently ponded","Very poorly drained","A/D",0.75,93.2,7.5]
["NE009","Blaine","Meadin loamy sand, 2 to 30 percent slopes","Excessively drained","A",0.75,84.3,6.2]
["NE009","Blaine","Natick sand, 0 to 3 percent slopes","Moderately well drained","A",0.57499999999999996,93.5,6.4]
["NE009","Blaine","Sandose loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,79.400000000000006,6.7]
["NE009","Blaine","Simeon sand, 0 to 3 percent slopes","Excessively drained","A",0.5,90.9,7]
["NE009","Blaine","Simeon sand, 3 to 30 percent slopes","Excessively drained","A",0.5,90.9,7]
["NE009","Blaine","Simeon-Valentine complex, 0 to 9 percent slopes","Excessively drained","A",0.5,93.75,6.75]
["NE009","Blaine","Tryon loamy fine sand, 0 to 3 percent slopes","Poorly drained","A/D",0.75,94.9,6.7]
["NE009","Blaine","Tryon loamy fine sand, frequently ponded","Very poorly drained","A/D",0.75,94.9,6.7]
["NE009","Blaine","Tryon-Els complex, 0 to 3 percent slopes","Somewhat poorly drained","A",1,94.65,6.7]
["NE009","Blaine","Tryon-Els loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,94.9,6.7]
["NE009","Blaine","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.5,6.5]
["NE009","Blaine","Valentine fine sand, rolling","Excessively drained","A",0.5,94.5,6.5]
["NE009","Blaine","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,94.5,6.5]
["NE009","Blaine","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,90,6.5]
["NE009","Blaine","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,90,6.5]
["NE009","Blaine","Valentine-Dunday complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.625,94,6.6]
["NE009","Blaine","Valentine-Els complex, 0 to 9 percent slopes","Somewhat poorly drained","A",0.5,94.050000000000011,6.5]
["NE009","Blaine","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.5,94.7,6.5]
["NE009","Blaine","Valentine-Libory complex, 0 to 9 percent slopes","Moderately well drained","B",0.625,90.05,6.55]
["NE009","Blaine","Valentine-Sandose loamy fine sands, 0 to 9 percent slopes","Well drained","A",0.75,87.3,6.5]
["NE009","Blaine","Valentine-Simeon complex, 0 to 9 percent slopes","Excessively drained","A",0.5,92.15,6.75]
["NE009","Blaine","Vetal loamy fine sand, 3 to 6 percent slopes","Well drained","A",2,85.9,7.2]
["NE009","Blaine","Vetal very fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,62,7]
["NE011","Boone",null,"",""]
["NE011","Boone","Alcester silty clay loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE011","Boone","Barney silt loam, channeled, frequently flooded","Very poorly drained","B/D",0.25,86.5,7.35]
["NE011","Boone","Belfore silt loam, 0 to 1 percent slopes","Well drained","C",0.75,8,6.5]
["NE011","Boone","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE011","Boone","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,73,7.5]
["NE011","Boone","Boelus loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.75,80,7]
["NE011","Boone","Cass silt loam, occasionally flooded","Well drained","B",0.75,63.5,7.3]
["NE011","Boone","Cass soils, rarely flooded","Well drained","B",0.75,60,7.3]
["NE011","Boone","Coly silt loam, 17 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE011","Boone","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE011","Boone","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE011","Boone","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE011","Boone","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,9.25,7.9]
["NE011","Boone","Crofton silt loam, 30 to 60 percent slopes","Well drained","B",0.75,8,7.9]
["NE011","Boone","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE011","Boone","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE011","Boone","Crofton-Nora silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,8.5,7.5]
["NE011","Boone","Crofton-Nora silt loams, 17 to 30 percent slopes","Well drained","B",0.75,8.5,7.5]
["NE011","Boone","Crofton-Nora silt loams, 6 to 11 percent slopes, eroded","Well drained","B",1.25,10,7.9]
["NE011","Boone","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE011","Boone","Dunday loamy fine sand, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE011","Boone","Elsmere fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.5,6.5]
["NE011","Boone","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,82,6.5]
["NE011","Boone","Fillmore silt loam, occasionally ponded","Somewhat poorly drained","D",1.5,8,6.7]
["NE011","Boone","Fluvaquents, frequently flooded","Very poorly drained","A/D",5,12,7.5]
["NE011","Boone","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.75,90.15,7.5]
["NE011","Boone","Gannett fine sandy loam, 0 to 1 percent slopes","Very poorly drained","A/D",0.75,65.5,6.5]
["NE011","Boone","Gates very fine sandy loam, 6 to 11 percent slopes, eroded","Well drained","B",0.5,58.6,7.5]
["NE011","Boone","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE011","Boone","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,95.35,7.2]
["NE011","Boone","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,10,7]
["NE011","Boone","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.5,8.5,7]
["NE011","Boone","Hall silt loam, 3 to 6 percent slopes, eroded","Well drained","C",1.5,9.5,7]
["NE011","Boone","Hall-Gayville complex, 1 to 3 percent slopes","Somewhat poorly drained","D",1.5,8.5,7.35]
["NE011","Boone","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE011","Boone","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE011","Boone","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,39.5,7.25]
["NE011","Boone","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",1.25,8,7.2]
["NE011","Boone","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",1.25,8,7.2]
["NE011","Boone","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.5,7.1,7.2]
["NE011","Boone","Hord and Ortello fine sandy loams, 1 to 3 percent slopes","Well drained","B",0.5,36.5,6.7]
["NE011","Boone","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,8,7]
["NE011","Boone","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,8,7]
["NE011","Boone","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,8,7]
["NE011","Boone","Hord-Uly complex, 0 to 6 percent slopes","Well drained","B",0.75,9,6.7]
["NE011","Boone","Inavale fine sand, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE011","Boone","Inavale soils, 0 to 3 percent slopes","Excessively drained","A",0.25,80,6.7]
["NE011","Boone","Inavale soils, frequently flooded","Excessively drained","A",0.25,80,6.7]
["NE011","Boone","Inglewood-Boel complex, channeled, occasionally flooded","Somewhat poorly drained","A",0.25,92.9,7.25]
["NE011","Boone","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,8,7.9]
["NE011","Boone","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,8.5,7.5]
["NE011","Boone","Loretto fine sandy loam, 0 to 2 percent slopes, eroded","Well drained","A",1.5,12,6.5]
["NE011","Boone","Loretto fine sandy loam, 3 to 6 percent slopes, eroded","Well drained","A",1.5,40,6.5]
["NE011","Boone","Loretto loam, 3 to 6 percent slopes, eroded","Well drained","B",1.5,12,6.5]
["NE011","Boone","Loretto sandy loam, 3 to 6 percent slopes","Well drained","B",1.5,39.1,6.5]
["NE011","Boone","Loretto-Nora fine sandy loams, 6 to 12 percent slopes, eroded","Well drained","A",1.5,12,6.5]
["NE011","Boone","Loup fine sandy loam, rarely flooded","Poorly drained","A/D",3.375,79.2,6.6]
["NE011","Boone","Loup loam, occasionally flooded","Very poorly drained","B/D",3.375,63.75,6.6]
["NE011","Boone","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE011","Boone","Moody silty clay loam, 1 to 3 percent slopes","Well drained","C",3,8,6.5]
["NE011","Boone","Moody silty clay loam, 1 to 3 percent slopes, eroded","Well drained","C",3,8,6.5]
["NE011","Boone","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE011","Boone","Moody silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",3,8,6.5]
["NE011","Boone","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE011","Boone","Nora silt loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,9.1,6.5]
["NE011","Boone","Nora silt loam, 6 to 11 percent slopes","Well drained","B",0.75,8,7]
["NE011","Boone","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,8,6.5]
["NE011","Boone","Nora silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE011","Boone","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE011","Boone","Nora-Crofton complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE011","Boone","Nora-Crofton complex, 2 to 6 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE011","Boone","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE011","Boone","Nora-Crofton silt loams, 11 to 17 percent slopes","Well drained","B",0.75,8,7.5]
["NE011","Boone","Nora-Moody complex, 2 to 6 percent slopes, eroded","Well drained","C",1.875,8,6.85]
["NE011","Boone","Ord loam, rarely flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE011","Boone","Ortello fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE011","Boone","Ortello fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE011","Boone","Scott silty clay loam, frequently ponded","Poorly drained","D",1.125,14.35,7.1]
["NE011","Boone","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE011","Boone","Shell silt loam, rarely flooded","Well drained","B",0.75,9.1,6.5]
["NE011","Boone","Shell silty clay loam, 0 to 1 percent slopes","Well drained","C",0.75,9.1,6.5]
["NE011","Boone","Thurman loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,78,6.5]
["NE011","Boone","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,78.5,6.5]
["NE011","Boone","Thurman loamy fine sand, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,78.5,6.5]
["NE011","Boone","Thurman loamy fine sand, terrace, 0 to 3 percent slopes","Somewhat excessively drained","A",0.25,69,6.5]
["NE011","Boone","Thurman-Valentine complex, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,85.5,6.5]
["NE011","Boone","Uly silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.5,7]
["NE011","Boone","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE011","Boone","Uly, eroded-Hersh complex, 11 to 60 percent slopes","Well drained","A",0.81499999999999995,50,6.8]
["NE011","Boone","Uly-Coly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.73,24.5,7.9]
["NE011","Boone","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE011","Boone","Uly-Coly silt loams, 17 to 30 percent slopes, eroded, moist","Well drained","B",1,24,7.5]
["NE011","Boone","Uly-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE011","Boone","Uly-Holdrege silt loams, 7 to 11 percent slopes, eroded","Well drained","C",0.5,9.4,7.6]
["NE011","Boone","Valentine fine sand, 0 to 6 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE011","Boone","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE011","Boone","Valentine fine sand, rolling","Excessively drained","A",0.25,87,6.5]
["NE011","Boone","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,96.3,6.5]
["NE011","Boone","Valentine loamy fine sand, undulating","Excessively drained","A",0.25,84,6.5]
["NE011","Boone","Valentine-Dunday loamy fine sands, 3 to 9 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE011","Boone","Wann loam, occasionally flooded","Somewhat poorly drained","C",0.75,63,8.1999999999999993]
["NE013","Box Butte",null,"",""]
["NE013","Box Butte","Alliance loam, 0 to 1 percent slopes","Well drained","C",0.75,11.4,7.2]
["NE013","Box Butte","Alliance loam, 1 to 3 percent slopes","Well drained","C",0.75,11.4,7.2]
["NE013","Box Butte","Alliance loam, 3 to 6 percent slopes","Well drained","C",0.75,11.4,7.2]
["NE013","Box Butte","Alliance-Rosebud loams, 1 to 3 percent slopes","Well drained","C",0.75,34,7.2]
["NE013","Box Butte","Alliance-Rosebud loams, 3 to 6 percent slopes","Well drained","C",0.75,34,7.2]
["NE013","Box Butte","Alliance-Rosebud loams, 6 to 11 percent slopes","Well drained","C",0.75,34,7.2]
["NE013","Box Butte","Bankard fine sand, channeled, frequently flooded","Somewhat excessively drained","A",1,94.5,7.9]
["NE013","Box Butte","Bankard loamy coarse sand, frequently flooded","Somewhat excessively drained","A",1,80.900000000000006,7.9]
["NE013","Box Butte","Bankard loamy fine sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,78.599999999999994,7.9]
["NE013","Box Butte","Bankard very fine sandy loam, 0 to 3 percent slopes","Somewhat excessively drained","A",1.125,76.95,7.9]
["NE013","Box Butte","Beckton silt loam, 0 to 2 percent slopes","Moderately well drained","C",0.5,23.8,8]
["NE013","Box Butte","Bigwinder fine sandy loam, frequently flooded","Poorly drained","C",2,66.8,7.9]
["NE013","Box Butte","Bridget very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,59,7.9]
["NE013","Box Butte","Bridget very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,59,7.9]
["NE013","Box Butte","Bridget very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,59,7.9]
["NE013","Box Butte","Busher fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,63.5,7]
["NE013","Box Butte","Busher fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,7]
["NE013","Box Butte","Busher fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,63.5,7]
["NE013","Box Butte","Busher loamy very fine sand, 1 to 6 percent slopes","Well drained","A",0.75,79.5,7]
["NE013","Box Butte","Busher-Jayem loamy very fine sands, 0 to 3 percent slopes","Well drained","A",0.52500000000000002,79.75,7.2]
["NE013","Box Butte","Busher-Jayem loamy very fine sands, 3 to 6 percent slopes","Well drained","A",0.52500000000000002,80,7.2]
["NE013","Box Butte","Busher-Jayem loamy very fine sands, 6 to 9 percent slopes","Well drained","A",0.52500000000000002,80,7.2]
["NE013","Box Butte","Busher-Tassel complex, 0 to 6 percent slopes","Well drained","A",1,72.05,7.25]
["NE013","Box Butte","Busher-Tassel complex, 6 to 30 percent slopes","Well drained","A",1,72.05,7.25]
["NE013","Box Butte","Busher-Tassel loamy very fine sand, 3 to 9 percent slopes","Well drained","A",1,79.5,7.25]
["NE013","Box Butte","Busher-Tassel loamy very fine sands, 0 to 6 percent slopes","Well drained","A",1,79.5,7.25]
["NE013","Box Butte","Busher-Tassel loamy very fine sands, 6 to 30 percent slopes","Well drained","A",1,79.5,7.25]
["NE013","Box Butte","Canyon very fine sandy loam, 3 to 30 percent slopes","Well drained","D",1.25,60.9,7.9]
["NE013","Box Butte","Craft very fine sandy loam, occasionally flooded","Well drained","A",0.75,59,7.9]
["NE013","Box Butte","Creighton very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,61.2,7.2]
["NE013","Box Butte","Creighton very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,61.2,7.2]
["NE013","Box Butte","Creighton very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,61.2,7.2]
["NE013","Box Butte","Creighton very fine sandy loam, 6 to 11 percent slopes","Well drained","B",0.75,61.2,7.2]
["NE013","Box Butte","Creighton-Norrest complex, 11 to 30 percent slopes","Well drained","B",0.625,50.35,7.5500000000000007]
["NE013","Box Butte","Creighton-Norrest complex, 6 to 11 percent slopes","Well drained","B",0.625,50.35,7.5500000000000007]
["NE013","Box Butte","Crowther mucky peat","Very poorly drained","B/D",6.75,36,7.7]
["NE013","Box Butte","Dailey loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1.375,79.800000000000011,7.25]
["NE013","Box Butte","Dailey loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",1.375,79.800000000000011,7.25]
["NE013","Box Butte","Dailey loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1.375,80.400000000000006,7.25]
["NE013","Box Butte","Dailey loamy sand, 3 to 9 percent slopes","Somewhat excessively drained","A",1.375,80.400000000000006,7.25]
["NE013","Box Butte","Duroc loam, 1 to 3 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE013","Box Butte","Duroc loam, occasionally flooded","Well drained","B",1.875,38.200000000000003,7.7]
["NE013","Box Butte","Els fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,94.9,6.7]
["NE013","Box Butte","Goshen loam, 0 to 1 percent slopes","Well drained","B",0.75,37.6,7.5]
["NE013","Box Butte","Hemingford loam, 0 to 1 percent slopes","Well drained","C",0.5,38.35,7.35]
["NE013","Box Butte","Hemingford loam, 1 to 3 percent slopes","Well drained","C",0.5,38.35,7.35]
["NE013","Box Butte","Hemingford loam, 3 to 6 percent slopes","Well drained","C",0.5,38.35,7.35]
["NE013","Box Butte","Hoffland fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7.5]
["NE013","Box Butte","Hoffland fine sandy loam, occasionally flooded","Poorly drained","A/D",0.75,93.2,7.5]
["NE013","Box Butte","Imlay-Rock outcrop complex, 9 to 60 percent slopes","Well drained","D",0.25,0,0]
["NE013","Box Butte","Ipage loamy fine sand, alkali substratum, 0 to 3 percent slopes","Moderately well drained","A",0.5,79,8]
["NE013","Box Butte","Janise loam, drained, 0 to 3 percent slopes","Moderately well drained","C",0.75,38.200000000000003,9.1999999999999993]
["NE013","Box Butte","Janise loam, occasionally flooded","Somewhat poorly drained","C",1.75,38.200000000000003,9.1]
["NE013","Box Butte","Janise loamy fine sand, drained, overblown, 0 to 3 percent slopes","Moderately well drained","C",0.25,59,9.1]
["NE013","Box Butte","Janise loamy fine sand, overblown, 0 to 3 percent slopes","Somewhat poorly drained","C",0.75,38.200000000000003,9.1]
["NE013","Box Butte","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,63.3,7.2]
["NE013","Box Butte","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,7.2]
["NE013","Box Butte","Jayem loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.52500000000000002,70.5,7.2]
["NE013","Box Butte","Jayem loamy sand, overblown, 0 to 3 percent slopes","Well drained","B",0.75,61.2,7.5]
["NE013","Box Butte","Jayem loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.5,62.5,7.2]
["NE013","Box Butte","Keith loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE013","Box Butte","Keith loam, 1 to 3 percent slopes","Well drained","B",0.75,38.200000000000003,7]
["NE013","Box Butte","Keith loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7]
["NE013","Box Butte","Lamo variant loam, 0 to 1 percent slopes","Poorly drained","B/D",1.25,43.2,7.9]
["NE013","Box Butte","Las Animas-Lisco complex, occasionally flooded","Somewhat poorly drained","B",0.25,63.5,8.5]
["NE013","Box Butte","Las Animas-Lisco very fine sandy loams, occasionally flooded","Somewhat poorly drained","B",0.25,81.5,8.5]
["NE013","Box Butte","Lisco very fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.25,65.900000000000006,9.1]
["NE013","Box Butte","Lisco very fine sandy loam, wet, occasionally flooded","Poorly drained","A/D",0.25,64.400000000000006,8.8000000000000007]
["NE013","Box Butte","Lodgepole loam, frequently ponded","Somewhat poorly drained","C/D",1.375,17.95,7]
["NE013","Box Butte","Lute loam, 0 to 2 percent slopes","Somewhat poorly drained","D",0.5,59.9,8.6]
["NE013","Box Butte","Manter-Satanta fine sandy loams, 0 to 3 percent slopes","Well drained","A",1.125,64.45,7.5500000000000007]
["NE013","Box Butte","Manter-Satanta fine sandy loams, 3 to 6 percent slopes","Well drained","A",1.125,63.5,7.5500000000000007]
["NE013","Box Butte","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7.5]
["NE013","Box Butte","Marlake very fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7]
["NE013","Box Butte","McCook loam, occasionally flooded","Well drained","B",1.75,38.200000000000003,7.9]
["NE013","Box Butte","Norrest loam, 6 to 11 percent slopes","Well drained","C",0.5,29,7.9]
["NE013","Box Butte","Norrest loam, 9 to 30 percent slopes","Well drained","C",0.5,29,7.9]
["NE013","Box Butte","Norrest-Canyon complex, 9 to 30 percent slopes","Well drained","D",0.875,34.25,7.9]
["NE013","Box Butte","Oglala-Canyon complex, 3 to 9 percent slopes","Well drained","D",1,52.2,7.1]
["NE013","Box Butte","Oglala-Canyon complex, 9 to 30 percent slopes","Well drained","D",1,52.2,7.1]
["NE013","Box Butte","Oglala-Canyon very fine sandy loams, 3 to 9 percent slopes","Well drained","D",1,59,7.45]
["NE013","Box Butte","Oglala-Canyon very fine sandy loams, 9 to 30 percent slopes","Well drained","D",1,59,7.45]
["NE013","Box Butte","Otero loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.625,73.25,7.9]
["NE013","Box Butte","Richfield loam, 0 to 1 percent slopes","Well drained","C",0.75,38,7.5]
["NE013","Box Butte","Rosebud loam, 0 to 1 percent slopes","Well drained","C",0.75,38.6,7.35]
["NE013","Box Butte","Rosebud loam, 1 to 3 percent slopes","Well drained","C",0.75,38.6,7.35]
["NE013","Box Butte","Rosebud-Canyon complex, 3 to 9 percent slopes","Well drained","D",0.75,43.2,7.5]
["NE013","Box Butte","Rosebud-Canyon complex, 9 to 30 percent slopes","Well drained","D",0.75,43.2,7.5]
["NE013","Box Butte","Sarben-Busher complex, 0 to 3 percent slopes","Well drained","A",0.75,79.75,7.1]
["NE013","Box Butte","Sarben-Busher complex, 3 to 9 percent slopes","Well drained","A",0.75,79.75,7.1]
["NE013","Box Butte","Sarben-Busher loamy very fine sands, 0 to 3 percent slopes","Well drained","A",0.75,81.5,7.2]
["NE013","Box Butte","Sarben-Busher loamy very fine sands, 3 to 9 percent slopes","Well drained","A",0.75,81.5,7.2]
["NE013","Box Butte","Satanta fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,62,7.9]
["NE013","Box Butte","Satanta fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,62,7.9]
["NE013","Box Butte","Satanta fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.75,62,7.9]
["NE013","Box Butte","Tassel loamy very fine sand, 3 to 30 percent slopes","Well drained","D",1.25,64.599999999999994,7.9]
["NE013","Box Butte","Tassel-Ashollow-Rock outcrop complex, 9 to 60 percent slopes","Well drained","A",1,73.199999999999989,7.9]
["NE013","Box Butte","Tassel-Busher loamy very fine sands, 3 to 30 percent slopes","Well drained","A",1,79.5,7.25]
["NE013","Box Butte","Tassel-Busher-Rock outcrop complex, 6 to 30 percent slopes","Well drained","A",0.75,64.599999999999994,7]
["NE013","Box Butte","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE013","Box Butte","Valent fine sand, 9 to 20 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE013","Box Butte","Valent fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE013","Box Butte","Valent loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE013","Box Butte","Valent loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE013","Box Butte","Valent loamy fine sand, 9 to 20 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE013","Box Butte","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,95.85,6.5]
["NE013","Box Butte","Valentine fine sand, 9 to 17 percent slopes","Excessively drained","A",0.5,95.85,6.5]
["NE013","Box Butte","Valentine fine sand, hilly","Excessively drained","A",0.5,95.85,6.5]
["NE013","Box Butte","Valentine fine sand, rolling","Excessively drained","A",0.5,95.85,6.5]
["NE013","Box Butte","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,95.85,6.5]
["NE013","Box Butte","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,83.35,6.5]
["NE013","Box Butte","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,91.35,6.5]
["NE013","Box Butte","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE013","Box Butte","Vetal fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE013","Box Butte","Wildhorse loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,88.85,9.1499999999999986]
["NE013","Box Butte","Wildhorse-Hoffland complex, 0 to 3 percent slopes","Poorly drained","A/D",1.25,92.95,8.6499999999999986]
["NE013","Box Butte","Wildhorse-Ipage, calcareous complex, 0 to 3 percent slopes","Moderately well drained","A",0.5,94.050000000000011,8.3000000000000007]
["NE015","Boyd",null,"",""]
["NE015","Boyd","Albaton silty clay, occasionally flooded","Poorly drained","D",2.29,2.4,7.9]
["NE015","Boyd","Anselmo fine sandy loam, 11 to 20 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE015","Boyd","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE015","Boyd","Anselmo fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE015","Boyd","Anselmo-Rock outcrop complex, 11 to 17 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE015","Boyd","Aowa silt loam, channeled, frequently flooded","Well drained","B",1.625,10.149999999999999,7.9]
["NE015","Boyd","Aowa silt loam, channeled, frequently flooded, wet","Well drained","B",1.625,9.0500000000000007,7.9]
["NE015","Boyd","Aowa silt loam, occasionally flooded","Well drained","B",1.625,9.0500000000000007,7.9]
["NE015","Boyd","Aowa silt loam, occasionally flooded, wet","Well drained","B",1.625,9.0500000000000007,7.9]
["NE015","Boyd","Barney loam, frequently flooded","Poorly drained","B/D",1.625,67.650000000000006,7.35]
["NE015","Boyd","Barney loam, frequently flooded, wet","Very poorly drained","B/D",1.625,67.650000000000006,7.35]
["NE015","Boyd","Barney silt loam, channeled, frequently flooded","Very poorly drained","B/D",0.25,55,7.5]
["NE015","Boyd","Bazile loam, 2 to 6 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE015","Boyd","Bazile loam, 6 to 11 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE015","Boyd","Blake silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.5,7.1,7.9]
["NE015","Boyd","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,66.099999999999994,7.3]
["NE015","Boyd","Blendon fine sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7.3]
["NE015","Boyd","Boel-Inavale complex, channeled, frequently flooded","Somewhat poorly drained","A",0.25,96.3,7.5]
["NE015","Boyd","Boyd silty clay, 6 to 11 percent slopes","Well drained","D",2,9.8500000000000014,7.5]
["NE015","Boyd","Bristow silty clay, 20 to 40 percent slopes","Well drained","D",0.25,2.6,7.9]
["NE015","Boyd","Bristow silty clay, 30 to 60 percent slopes","Well drained","D",0.25,2.6,7.9]
["NE015","Boyd","Brocksburg fine sandy loam, 0 to 2 percent slopes","Well drained","C",1.5,63.5,7.2]
["NE015","Boyd","Brocksburg loam, 0 to 2 percent slopes","Well drained","C",1.5,44.3,7.2]
["NE015","Boyd","Cass fine sandy loam, occasionally flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE015","Boyd","Cass loam, rarely flooded","Well drained","B",0.75,66.900000000000006,7.3]
["NE015","Boyd","Crofton silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE015","Boyd","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE015","Boyd","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE015","Boyd","Dunday loamy fine sand, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE015","Boyd","Dunday loamy fine sand, 6 to 11 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE015","Boyd","Dunday loamy fine sand, loamy substratum, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,81.75,7.15]
["NE015","Boyd","Eltree silt loam, 0 to 3 percent slopes","Well drained","B",1,9.5,7.9]
["NE015","Boyd","Fluvaquents, frequently flooded, wet","Very poorly drained","B/D",5,19.2,7.5]
["NE015","Boyd","Grigston silt loam, occasionally flooded","Well drained","B",1.5,9.4,7.9]
["NE015","Boyd","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.125,9.1999999999999993,7.1]
["NE015","Boyd","Haynie silt loam, occasionally flooded","Well drained","B",1.25,12.600000000000001,7.7]
["NE015","Boyd","Inavale fine sand, 3 to 11 percent slopes","Excessively drained","A",0.25,92.2,6.7]
["NE015","Boyd","Inavale fine sand, channeled, frequently flooded","Excessively drained","A",0.25,92.2,6.7]
["NE015","Boyd","Inavale fine sand, channeled, frequently flooded, wet","Excessively drained","A",0.25,92.2,6.7]
["NE015","Boyd","Inavale fine sandy loam, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE015","Boyd","Inavale loamy fine sand, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE015","Boyd","Inavale loamy fine sand, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE015","Boyd","Inavale loamy fine sand, rarely flooded, wet","Excessively drained","A",0.25,92.2,7.5]
["NE015","Boyd","Jansen loam, 0 to 2 percent slopes","Well drained","C",1.25,43.3,6.2]
["NE015","Boyd","Jansen loam, 2 to 6 percent slopes","Well drained","C",1.25,43.3,6.2]
["NE015","Boyd","Jansen loam, 6 to 11 percent slopes","Well drained","C",1.25,43.3,6.2]
["NE015","Boyd","Labu silty clay, 6 to 11 percent slopes","Well drained","D",0.75,2.6,7.5]
["NE015","Boyd","Labu-Sansarc complex, 11 to 30 percent slopes","Well drained","D",0.65,1.3,7.7]
["NE015","Boyd","Labu-Sansarc silty clays, 11 to 30 percent slopes","Well drained","D",0.65,3.8,7.5]
["NE015","Boyd","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,11.3,7.5]
["NE015","Boyd","Lynch silty clay, 2 to 6 percent slopes","Well drained","D",0.75,2.5499999999999998,7.9]
["NE015","Boyd","Lynch silty clay, 6 to 11 percent slopes","Well drained","D",0.75,2.5499999999999998,7.9]
["NE015","Boyd","Lynch-Bristow complex, 11 to 30 percent slopes","Well drained","D",0.5,2.5499999999999998,7.9]
["NE015","Boyd","Lynch-Bristow silty clays, 11 to 30 percent slopes","Well drained","D",0.75,2.6,7.9]
["NE015","Boyd","Lynch-Bristow silty clays, 6 to 11 percent slopes","Well drained","D",0.75,2.6,7.9]
["NE015","Boyd","Lynch-Verdel complex, 6 to 11 percent slopes","Well drained","D",0.75,5.3,7.8]
["NE015","Boyd","Mariaville-Paka loams, 11 to 40 percent slopes","Well drained","D",0.75,19.899999999999999,7.2]
["NE015","Boyd","Meadin gravelly sandy loam, 2 to 30 percent slopes","Excessively drained","A",0.25,84.3,6.2]
["NE015","Boyd","Meadin sandy loam, 2 to 20 percent slopes","Excessively drained","A",0.75,67.8,6.2]
["NE015","Boyd","Nora silt loam, 2 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE015","Boyd","Nora silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE015","Boyd","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE015","Boyd","O'Neill fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,67.599999999999994,6.5]
["NE015","Boyd","O'Neill fine sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,67.599999999999994,6.5]
["NE015","Boyd","O'Neill-Meadin fine sandy loams, 2 to 11 percent slopes","Excessively drained","A",0.75,66.449999999999989,6.35]
["NE015","Boyd","Onita silt loam, 0 to 1 percent slopes","Well drained","C",1,19.7,6.7]
["NE015","Boyd","Ord fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE015","Boyd","Paka fine sandy loam, 2 to 6 percent slopes","Well drained","C",1.125,18.05,7.1]
["NE015","Boyd","Paka loam, 0 to 2 percent slopes","Well drained","C",1.125,8.25,7.1]
["NE015","Boyd","Paka loam, 2 to 6 percent slopes","Well drained","C",1.125,8.25,7.1]
["NE015","Boyd","Paka loam, 6 to 11 percent slopes, eroded","Well drained","C",1.125,8.25,7.1]
["NE015","Boyd","Promise silty clay, 2 to 6 percent slopes","Well drained","D",2,11.4,8.1999999999999993]
["NE015","Boyd","Ree silt loam, 11 to 20 percent slopes","Well drained","C",1.25,54.6,7.5]
["NE015","Boyd","Ree silt loam, 2 to 6 percent slopes","Well drained","C",1.25,35.4,7.5]
["NE015","Boyd","Ree silt loam, 6 to 11 percent slopes","Well drained","C",1.25,35.4,7.5]
["NE015","Boyd","Reliance silt loam, 2 to 6 percent slopes","Well drained","C",1.25,19.7,7]
["NE015","Boyd","Reliance silt loam, 6 to 11 percent slopes","Well drained","C",1.25,19.7,7]
["NE015","Boyd","Reliance silty clay loam, 2 to 6 percent slopes","Well drained","C",1.25,19.7,7]
["NE015","Boyd","Riverwash","Very poorly drained","A/D",0.15000000000000002,95.95,7.9]
["NE015","Boyd","Ronson-Anselmo fine sandy loams, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE015","Boyd","Ronson-Anselmo fine sandy loams, 6 to 30 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE015","Boyd","Sansarc silty clay, 20 to 40 percent slopes","Well drained","D",0.55000000000000004,5,7.5]
["NE015","Boyd","Sansarc silty clay, 30 to 60 percent slopes","Well drained","D",0.55000000000000004,0,7.9]
["NE015","Boyd","Sardak loamy fine sand, 2 to 11 percent slopes, very rare flooding, wet","Excessively drained","A",0.5,87.9,7.5]
["NE015","Boyd","Scott silt loam, frequently ponded","Poorly drained","D",1.125,21.1,7.1]
["NE015","Boyd","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,87.8,7]
["NE015","Boyd","Simeon-Valentine complex, 3 to 30 percent slopes, eroded","Excessively drained","A",0.25,92.7,6.5]
["NE015","Boyd","Simeon-Valentine loamy sands, 0 to 6 percent slopes","Excessively drained","A",0.25,92.1,6.5]
["NE015","Boyd","Thurman fine sandy loam, 2 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE015","Boyd","Trent silt loam, 0 to 2 percent slopes","Well drained","B",2.5,8.8000000000000007,6.7]
["NE015","Boyd","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE015","Boyd","Valentine fine sand, 9 to 17 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE015","Boyd","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE015","Boyd","Valentine loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE015","Boyd","Verdel silty clay, 0 to 2 percent slopes","Well drained","D",1.375,5.3,7.4]
["NE015","Boyd","Verdel silty clay, 2 to 6 percent slopes","Well drained","C",1.375,5.3,7.4]
["NE015","Boyd","Wewela fine sandy loam, 2 to 6 percent slopes","Well drained","D",1.25,38.799999999999997,6.7]
["NE017","Brown",null,"",""]
["NE017","Brown","Almeria fine sandy loam, occasionally flooded","Poorly drained","A/D",3.375,77.75,6.9]
["NE017","Brown","Almeria loamy fine sand, channeled, frequently flooded","Very poorly drained","A/D",1.25,89.85,6.9]
["NE017","Brown","Almeria loamy fine sand, occasionally flooded","Poorly drained","A/D",1.25,89.4,6.9]
["NE017","Brown","Almeria-Histosols complex, channeled, frequently flooded","Very poorly drained","A/D",3.375,77.75,3.25]
["NE017","Brown","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE017","Brown","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE017","Brown","Anselmo fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE017","Brown","Anselmo-Brunswick fine sandy loams, 11 to 30 percent slopes","Well drained","A",0.5,66.099999999999994,6.6]
["NE017","Brown","Barney fine sandy loam, frequently flooded","Very poorly drained","A/D",0.25,91,7.5]
["NE017","Brown","Bolent fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,80.75,7.7]
["NE017","Brown","Brocksburg loam, 0 to 2 percent slopes","Well drained","B",1.5,44.3,7.2]
["NE017","Brown","Brunswick fine sandy loam, 3 to 11 percent slopes","Well drained","B",0.25,66.900000000000006,6.5]
["NE017","Brown","Calamus loamy fine sand, calcareous, rarely flooded","Moderately well drained","A",0.3,93.2,7.5]
["NE017","Brown","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE017","Brown","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE017","Brown","Els fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.7]
["NE017","Brown","Els loamy sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,89.85,6.6]
["NE017","Brown","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,95.15,6.35]
["NE017","Brown","Elsmere loamy fine sand, rarely flooded","Somewhat poorly drained","A",1.125,91.8,6.6]
["NE017","Brown","Elsmere-Loup complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,94.9,6.5]
["NE017","Brown","Els-Tryon complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,95.4,6.7]
["NE017","Brown","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",5,87.3,7.5]
["NE017","Brown","Gannett fine sandy loam, 0 to 1 percent slopes","Poorly drained","B/D",0.75,62.5,7.5]
["NE017","Brown","Inavale loamy fine sand, rarely flooded","Excessively drained","A",0.5,89.75,6.7]
["NE017","Brown","Inavale sand, channeled, occasionally flooded","Excessively drained","A",0.5,93.85,6.7]
["NE017","Brown","Inavale-Barney complex, channeled, occasionally flooded","Very poorly drained","A/D",0.25,91,7.2]
["NE017","Brown","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE017","Brown","Ipage fine sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,96.8,6.5]
["NE017","Brown","Ipage loamy sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,89.6,6.2]
["NE017","Brown","Jansen fine sandy loam, 0 to 2 percent slopes","Well drained","B",1.25,66.900000000000006,6.2]
["NE017","Brown","Jansen fine sandy loam, 2 to 6 percent slopes","Well drained","B",1.25,66.900000000000006,6.2]
["NE017","Brown","Jansen loam, 0 to 2 percent slopes","Well drained","B",1.25,43.3,6.2]
["NE017","Brown","Jansen loam, 2 to 6 percent slopes","Well drained","C",1.25,43.3,6.2]
["NE017","Brown","Jansen-Meadin complex, 0 to 2 percent slopes","Well drained","C",1,73.900000000000006,6.2]
["NE017","Brown","Jansen-Sandose complex, 0 to 2 percent slopes","Well drained","C",1,73.150000000000006,6.35]
["NE017","Brown","Johnstown fine sandy loam, 0 to 2 percent slopes","Well drained","C",0.75,47.2,7.1]
["NE017","Brown","Johnstown loam, 0 to 2 percent slopes","Well drained","C",0.75,34.150000000000006,7.1]
["NE017","Brown","Johnstown loam, 2 to 6 percent slopes","Well drained","C",0.75,34.150000000000006,7.1]
["NE017","Brown","Labu-Sansarc silty clays, 11 to 40 percent slopes","Well drained","D",0.65,2.6,7.7]
["NE017","Brown","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,86.4,6.5]
["NE017","Brown","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",3.375,79.2,6.6]
["NE017","Brown","Loup fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,79.2,6.6]
["NE017","Brown","Loup-Els complex, 0 to 3 percent slopes","Somewhat poorly drained","A",1.25,90.85,6.6]
["NE017","Brown","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,72.150000000000006,7.15]
["NE017","Brown","McKelvie-Fishberry-Rock outcrop complex, 11 to 60 percent slopes","Excessively drained","D",0.375,83.55,7.25]
["NE017","Brown","McKelvie-Longpine-Ronson complex, 17 to 70 percent slopes","Well drained","D",0.75,64.599999999999994,7.5]
["NE017","Brown","Meadin sandy loam, 0 to 2 percent slopes","Excessively drained","A",0.75,84.3,6.2]
["NE017","Brown","Meadin sandy loam, 2 to 30 percent slopes","Excessively drained","A",0.75,67.8,6.2]
["NE017","Brown","O'Neill fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,67.3,6.5]
["NE017","Brown","O'Neill loam, 0 to 2 percent slopes","Well drained","B",0.75,67.3,6.5]
["NE017","Brown","O'Neill-Meadin sandy loams, 2 to 6 percent slopes","Excessively drained","A",0.75,75.949999999999989,6.35]
["NE017","Brown","O'Neill-Meadin sandy loams, 6 to 11 percent slopes","Excessively drained","A",0.75,75.949999999999989,6.35]
["NE017","Brown","Pivot loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,84.9,6.5]
["NE017","Brown","Ronson-Longpine fine sandy loams, 0 to 2 percent slopes","Well drained","D",0.75,64.599999999999994,7.4]
["NE017","Brown","Ronson-Longpine fine sandy loams, 2 to 6 percent slopes","Well drained","D",0.75,64.25,7.4]
["NE017","Brown","Ronson-Longpine fine sandy loams, 6 to 11 percent slopes","Well drained","D",0.75,64.25,7.4]
["NE017","Brown","Sandose loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.75,72.949999999999989,6.95]
["NE017","Brown","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,86.35,7]
["NE017","Brown","Simeon loamy sand, 3 to 11 percent slopes","Excessively drained","A",0.5,86.35,7]
["NE017","Brown","Simeon-Valentine complex, 0 to 9 percent slopes","Excessively drained","A",0.5,93.75,6.75]
["NE017","Brown","Simeon-Valentine fine sands, 0 to 11 percent slopes","Excessively drained","A",0.5,93.6,6.75]
["NE017","Brown","Tryon fine sandy loam, 0 to 3 percent slopes","Poorly drained","A/D",3.375,79.45,6.85]
["NE017","Brown","Tryon fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,63.5,6.7]
["NE017","Brown","Tryon loamy fine sand, 0 to 3 percent slopes","Poorly drained","A/D",3.125,90.85,6.85]
["NE017","Brown","Tryon loamy fine sand, frequently ponded","Very poorly drained","A/D",3.125,90.85,6.85]
["NE017","Brown","Tryon-Els complex, 0 to 3 percent slopes","Somewhat poorly drained","A",1,94.65,6.7]
["NE017","Brown","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,95.5,6.5]
["NE017","Brown","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,95.85,6.5]
["NE017","Brown","Valentine fine sand, rolling","Excessively drained","A",0.5,94.5,6.5]
["NE017","Brown","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,94.5,6.5]
["NE017","Brown","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE017","Brown","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE017","Brown","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.5,94.7,6.5]
["NE017","Brown","Valentine-Libory complex, 0 to 9 percent slopes","Moderately well drained","A",0.75,86.4,6.5]
["NE017","Brown","Valentine-Longpine complex, 3 to 17 percent slopes","Well drained","D",0.75,64.599999999999994,6.5]
["NE017","Brown","Valentine-Pivot complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.75,91.5,6.5]
["NE017","Brown","Valentine-Sandose complex, 0 to 9 percent slopes","Well drained","B",0.75,87.4,6.6]
["NE017","Brown","Valentine-Sandose loamy fine sands, 0 to 9 percent slopes","Well drained","C",0.75,79.400000000000006,6.5]
["NE017","Brown","Valentine-Simeon complex, 9 to 40 percent slopes, eroded","Excessively drained","A",0.5,92.6,6.75]
["NE017","Brown","Valentine-Tryon complex, 0 to 17 percent slopes","Very poorly drained","A/D",0.5,94.45,6.6]
["NE017","Brown","Valentine-Tryon fine sands, 0 to 24 percent slopes","Very poorly drained","A/D",0.75,95.85,6.6]
["NE017","Brown","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,65.75,7.15]
["NE017","Brown","Vetal loam, 1 to 3 percent slopes","Well drained","A",1.25,43.2,7.15]
["NE019","Buffalo",null,"",""]
["NE019","Buffalo","Alda fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,66,7.5]
["NE019","Buffalo","Alda loam, rarely flooded","Somewhat poorly drained","C",0.75,66,7.5]
["NE019","Buffalo","Anselmo fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.5,66.099999999999994,6.95]
["NE019","Buffalo","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE019","Buffalo","Anselmo fine sandy loam, 3 to 6 percent slopes, eroded","Well drained","A",0.5,66.099999999999994,6.95]
["NE019","Buffalo","Anselmo fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.5,66.099999999999994,6.95]
["NE019","Buffalo","Anselmo loam, 1 to 3 percent slopes","Well drained","B",0.75,66.099999999999994,7.1]
["NE019","Buffalo","Barney loam, frequently flooded","Very poorly drained","B/D",1.625,59.800000000000004,7.35]
["NE019","Buffalo","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.5,76.150000000000006,7.5]
["NE019","Buffalo","Blendon loam, 0 to 2 percent slopes","Well drained","B",1.125,66.349999999999994,7.25]
["NE019","Buffalo","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.599999999999994,7.5]
["NE019","Buffalo","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE019","Buffalo","Bolent fine sandy loam, occasionally flooded","Somewhat poorly drained","A",0.5,93.3,7.7]
["NE019","Buffalo","Bolent loamy sand, occasionally flooded","Somewhat poorly drained","A",1,95.4,6.9]
["NE019","Buffalo","Calamus loamy fine sand, rarely flooded","Moderately well drained","A",0.25,92.5,7]
["NE019","Buffalo","Caruso loam, rarely flooded","Somewhat poorly drained","C",0.5,51,7.3]
["NE019","Buffalo","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE019","Buffalo","Cass loam, rarely flooded","Well drained","B",0.75,63.5,7.3]
["NE019","Buffalo","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE019","Buffalo","Coly silt loam, 11 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE019","Buffalo","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE019","Buffalo","Coly silt loam, 6 to 11 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE019","Buffalo","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE019","Buffalo","Coly, Uly, and Hobbs soils, 3 to 30 percent slopes","Well drained","B",0.75,11.2,7.5]
["NE019","Buffalo","Coly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",1.125,11.3,7.7]
["NE019","Buffalo","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE019","Buffalo","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE019","Buffalo","Coly-Uly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE019","Buffalo","Cozad fine sandy loam, calcareous variant, 0 to 1 percent slopes","Well drained","B",0.75,65.7,7]
["NE019","Buffalo","Cozad loam, 0 to 1 percent slopes","Well drained","B",0.75,42.7,7]
["NE019","Buffalo","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,41,7]
["NE019","Buffalo","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,41,7]
["NE019","Buffalo","Cozad silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,41,7]
["NE019","Buffalo","Cozad silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,14.2,7.3]
["NE019","Buffalo","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,9.3000000000000007,7.2]
["NE019","Buffalo","Dunday fine sandy loam, terrace, 0 to 2 percent slopes","Somewhat excessively drained","A",0.875,78.849999999999994,6.85]
["NE019","Buffalo","Dunday-Valentine loamy fine sands, loamy substratum, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,87.3,6.5]
["NE019","Buffalo","Fluvaquents, frequently flooded","Very poorly drained","A/D",0.75,79,6.5]
["NE019","Buffalo","Gates silt loam, 1 to 3 percent slopes","Well drained","B",0.5,13.9,7.5]
["NE019","Buffalo","Gates silt loam, 3 to 6 percent slopes","Well drained","B",0.25,37.950000000000003,7.7]
["NE019","Buffalo","Gibbon loam, rarely flooded","Somewhat poorly drained","C",0.5,51.75,7.9]
["NE019","Buffalo","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE019","Buffalo","Gibbon silt loam, rarely flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE019","Buffalo","Gibbon silt loam, saline, rarely flooded","Somewhat poorly drained","C",0.75,9.1,7.9]
["NE019","Buffalo","Gothenburg loam, frequently flooded","Poorly drained","B/D",0.5,81,7.2]
["NE019","Buffalo","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,91.9,7.3]
["NE019","Buffalo","Gothenburg soils, frequently flooded","Poorly drained","B/D",0.5,70.900000000000006,7.35]
["NE019","Buffalo","Grigston silt loam","Well drained","B",0.75,37.6,7.5]
["NE019","Buffalo","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE019","Buffalo","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.5,9.5,7]
["NE019","Buffalo","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE019","Buffalo","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.75,11.4,7.5]
["NE019","Buffalo","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE019","Buffalo","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",1.25,9.3000000000000007,7.2]
["NE019","Buffalo","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.3500000000000014,7.2]
["NE019","Buffalo","Holdrege silt loam, 1 to 3 percent slopes, overblown","Well drained","C",2,7,7.2]
["NE019","Buffalo","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.3500000000000014,7.2]
["NE019","Buffalo","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,9.3000000000000007,7.2]
["NE019","Buffalo","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,7,7.2]
["NE019","Buffalo","Holdrege silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.75,6.8,7.2]
["NE019","Buffalo","Holdrege-Hall silt loams, 0 to 1 percent slopes","Well drained","C",1.25,9.4,7.2]
["NE019","Buffalo","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE019","Buffalo","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE019","Buffalo","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE019","Buffalo","Hord silt loam, rarely flooded","Well drained","B",0.75,9.3000000000000007,7]
["NE019","Buffalo","Inavale fine sandy loam, 0 to 3 percent slopes","Excessively drained","A",0.5,76.150000000000006,6.7]
["NE019","Buffalo","Inavale loamy fine sand, very rarely flooded","Excessively drained","A",0.25,87.3,7]
["NE019","Buffalo","Inavale loamy sand, 3 to 11 percent slopes, very rarely flooded","Excessively drained","A",0.25,87.3,7.2]
["NE019","Buffalo","Janude loam, calcareous, rarely flooded","Moderately well drained","B",0.9,66.599999999999994,7.6]
["NE019","Buffalo","Kenesaw silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.3,7.5]
["NE019","Buffalo","Kenesaw silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.3,7.5]
["NE019","Buffalo","Kenesaw silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.3,7.5]
["NE019","Buffalo","Kenesaw-Coly silt loams, 3 to 6 percent slopes","Well drained","B",0.75,11.3,7.9]
["NE019","Buffalo","Lamo silt loam, sand substratum, 0 to 1 percent slope","Poorly drained","C",1.5,9.4,7.6]
["NE019","Buffalo","Leshara and Gibbon silt loams","Somewhat poorly drained","C",0.75,11.350000000000001,7.7]
["NE019","Buffalo","Leshara fine sandy loam","Somewhat poorly drained","C",0.75,62.8,7.5]
["NE019","Buffalo","Lex silt loam, rarely flooded","Somewhat poorly drained","C",0.75,43.150000000000006,7.4]
["NE019","Buffalo","Loup loam, 0 to 3 percent slopes","Very poorly drained","B/D",0.75,79,6.5]
["NE019","Buffalo","O'Neill and Pivot loams, 0 to 2 percent slopes","Well drained","B",0.75,70,6.8]
["NE019","Buffalo","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,63.2,7.5]
["NE019","Buffalo","Platte soils, occasionally flooded","Somewhat poorly drained","C",0.25,66.599999999999994,7.5]
["NE019","Buffalo","Platte-Alda complex, occasionally flooded","Somewhat poorly drained","B",0.5,66.3,7.5]
["NE019","Buffalo","Platte-Bolent complex, occasionally flooded","Somewhat poorly drained","B",0.25,66.900000000000006,7.45]
["NE019","Buffalo","Platte-Wann complex, channeled, occasionally flooded","Somewhat poorly drained","C",0.5,64.7,8.1]
["NE019","Buffalo","Riverwash","Very poorly drained","A/D",0.15000000000000002,94.05,7.9]
["NE019","Buffalo","Rusco silt loam, 0 to 1 percent slopes","Moderately well drained","C/D",0.75,11.2,7.5]
["NE019","Buffalo","Scott silt loam, drained, frequently ponded","Poorly drained","D",1.125,21.1,7.1]
["NE019","Buffalo","Scott silt loam, frequently ponded","Poorly drained","D",1.125,21.1,7.1]
["NE019","Buffalo","Silver Creek silt loam, rarely flooded","Somewhat poorly drained","D",0.75,26,8.1999999999999993]
["NE019","Buffalo","Simeon sandy loam, 0 to 3 percent slopes","Excessively drained","A",0.5,80.199999999999989,7]
["NE019","Buffalo","Thurman-Valentine loamy fine sands, 0 to 2 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE019","Buffalo","Thurman-Valentine loamy fine sands, 2 to 6 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE019","Buffalo","Thurman-Valentine loamy fine sands, terrace, 0 to 2 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE019","Buffalo","Uly and Holdrege silt loams, 6 to 11 percent slopes","Well drained","C",0.75,9.4,7.2]
["NE019","Buffalo","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE019","Buffalo","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE019","Buffalo","Uly, eroded-Coly silt loams, 11 to 17 percent slopes","Well drained","B",0.75,21.25,7.9]
["NE019","Buffalo","Uly, eroded-Coly silt loams, 6 to 11 percent slopes","Well drained","B",1.25,21.3,7.9]
["NE019","Buffalo","Uly, eroded-Hobbs silt loams, 2 to 40 percent slopes","Well drained","B",2,17.049999999999997,7]
["NE019","Buffalo","Uly, Holdrege, and Coly soils, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.4,7.2]
["NE019","Buffalo","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE019","Buffalo","Uly-Holdrege silt loams, 6 to 11 percent slopes","Well drained","C",1,9.25,7.1]
["NE019","Buffalo","Uly-Holdrege-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","C",1,9.25,7.1]
["NE019","Buffalo","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.2]
["NE019","Buffalo","Valentine fine sand, rolling","Excessively drained","A",0.25,96.3,5.9499999999999993]
["NE019","Buffalo","Valentine fine sand, rolling and hilly","Excessively drained","A",0.25,96.3,6.3]
["NE019","Buffalo","Valentine loamy fine sand, 3 to 17 percent slopes","Excessively drained","A",0.5,91.8,6.5]
["NE019","Buffalo","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.4]
["NE019","Buffalo","Valentine loamy fine sand, rolling","Excessively drained","A",0.25,96.3,6.35]
["NE019","Buffalo","Wann fine sandy loam, rarely flooded","Somewhat poorly drained","B",1.375,63.3,7.85]
["NE019","Buffalo","Wann loam, rarely flooded","Somewhat poorly drained","C",1.375,53.05,7.85]
["NE019","Buffalo","Wood River silt loam, 0 to 1 percent slopes","Moderately well drained","C",0.75,22.9,8.1999999999999993]
["NE019","Buffalo","Wood River silt loam, 1 to 3 percent slopes","Moderately well drained","C",0.75,20,8.1999999999999993]
["NE019","Buffalo","Wood River-Gayville complex, 0 to 1 percent slopes","Moderately well drained","D",1.375,18,8.35]
["NE019","Buffalo","Wood River-Gayville variant complex, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,21.9,8.5]
["NE021","Burt",null,"",""]
["NE021","Burt","Albaton silty clay, frequently flooded","Very poorly drained","D",2.5,2.2999999999999998,7.9]
["NE021","Burt","Albaton silty clay, occasionally flooded","Poorly drained","D",1.5,3.9,7.9]
["NE021","Burt","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",1.5,6,7]
["NE021","Burt","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE021","Burt","Belfore silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE021","Burt","Blencoe silty clay loam, rarely flooded","Somewhat poorly drained","D",2,7.6,7.2]
["NE021","Burt","Blencoe silty clay, rarely flooded","Somewhat poorly drained","D",2,6.8,7.2]
["NE021","Burt","Blyburg silt loam, rarely flooded","Well drained","A",0.875,14,7.85]
["NE021","Burt","Boone-Rock outcrop complex, 20 to 60 percent slopes","Excessively drained","A",0.25,87.45,5.4]
["NE021","Burt","Burchard clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.75,36.5,6.7]
["NE021","Burt","Burchard clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,36.5,6.7]
["NE021","Burt","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE021","Burt","Calco silty clay loam, occasionally flooded","Poorly drained","C/D",5,6.8000000000000007,7.9]
["NE021","Burt","Calco silty clay loam, wet, occasionally flooded","Poorly drained","C/D",5,6.8000000000000007,7.9]
["NE021","Burt","Carr silt loam, occasionally flooded","Well drained","B",0.25,68.5,7.9]
["NE021","Burt","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE021","Burt","Colo silt loam, overwash, occasionally flooded","Poorly drained","C/D",3.75,8.1,6.5]
["NE021","Burt","Colo silty clay loam, occasionally flooded","Poorly drained","C/D",4.75,6.85,6.5]
["NE021","Burt","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE021","Burt","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE021","Burt","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1.5,6.8,6.7]
["NE021","Burt","Forney silty clay, rarely flooded","Poorly drained","D",2.25,3.9,7]
["NE021","Burt","Grable silt loam, occasionally flooded","Well drained","B",0.5,14.2,7.9]
["NE021","Burt","Haynie silt loam, occasionally flooded","Well drained","B",1.25,12.600000000000001,7.65]
["NE021","Burt","Haynie silt loam, rarely flooded","Well drained","B",1.25,12.600000000000001,7.7]
["NE021","Burt","Haynie variant silt loam, rarely flooded","Moderately well drained","C",1.125,8.35,7.7]
["NE021","Burt","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,10.4,7.25]
["NE021","Burt","Holly Springs silty clay loam, occasionally flooded","Poorly drained","C/D",3.5,18.7,7.9]
["NE021","Burt","Ida silt loam, 11 to 17 percent slopes","Well drained","B",1.375,11.2,7.7]
["NE021","Burt","Ida silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.375,11.2,7.7]
["NE021","Burt","Ida silt loam, 17 to 30 percent slopes","Well drained","B",1.375,11.2,7.7]
["NE021","Burt","Ida silt loam, 17 to 30 percent slopes, eroded","Well drained","B",1.375,11.2,7.7]
["NE021","Burt","Ida silt loam, 30 to 60 percent slopes","Well drained","B",1.375,11.2,7.7]
["NE021","Burt","Ida silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.375,11.2,7.7]
["NE021","Burt","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3.5,7.9,6.5]
["NE021","Burt","Judson silty clay loam, 2 to 6 percent slopes","Well drained","C",3.5,6.85,6.5]
["NE021","Burt","Kennebec silt loam, occasionally flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE021","Burt","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE021","Burt","Kezan silt loam, occasionally flooded","Poorly drained","B/D",2,9.1,7.2]
["NE021","Burt","Kezan-Kennebec silt loams, drained, occasionally flooded","Moderately well drained","B",2,9.1,7.2]
["NE021","Burt","Luton silty clay, rarely flooded","Poorly drained","D",0.5,5.3,7.2]
["NE021","Burt","Marshall silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,6.9,6.5]
["NE021","Burt","Marshall silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,6.9,6.5]
["NE021","Burt","Marshall silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.75,6.9,6.5]
["NE021","Burt","Marshall silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",0.75,6.9,6.5]
["NE021","Burt","Marshall-Pohocco silty clay loams, 6 to 11 percent slopes, eroded","Well drained","C",0.75,4.75,7]
["NE021","Burt","Modale silt loam, occasionally flooded","Somewhat poorly drained","C",1.375,8.35,8.0500000000000007]
["NE021","Burt","Monona silt loam, 11 to 17 percent slopes","Well drained","B",1.25,9.4,6.7]
["NE021","Burt","Monona silt loam, 17 to 30 percent slopes","Well drained","B",1.25,9.4,7]
["NE021","Burt","Monona silt loam, 6 to 11 percent slopes","Well drained","B",1.25,9.4,6.7]
["NE021","Burt","Monona silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.4,7]
["NE021","Burt","Monona silt loam, bench, 0 to 2 percent slopes","Well drained","B",1.125,3.5,6.65]
["NE021","Burt","Monona-Pohocco complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,4.75,7]
["NE021","Burt","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE021","Burt","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE021","Burt","Moody silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",2,7,6.5]
["NE021","Burt","Moody silty clay loam, 6 to 11 percent slopes","Well drained","C",3,6.9,6.5]
["NE021","Burt","Moody silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE021","Burt","Moody silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE021","Burt","Napier-Nodaway-Gullied land complex, 0 to 60 percent slopes","Well drained","B",1,3.5,7.3]
["NE021","Burt","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.4,6.7]
["NE021","Burt","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,9.1,8]
["NE021","Burt","Nora silty clay loam, 11 to 17 percent slopes","Well drained","C",0.75,8.9,7]
["NE021","Burt","Nora silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE021","Burt","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE021","Burt","Nora silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE021","Burt","Nora variant silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE021","Burt","Nora variant silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE021","Burt","Omadi silt loam, rarely flooded","Moderately well drained","B",1.125,10.45,7.7]
["NE021","Burt","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE021","Burt","Owego silty clay, occasionally flooded","Poorly drained","D",0.5,7.2,7.9]
["NE021","Burt","Percival silty clay, occasionally flooded","Somewhat poorly drained","D",1.125,44.4,7.9]
["NE021","Burt","Pohocco silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.4,7.2]
["NE021","Burt","Pohocco silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.4,7.2]
["NE021","Burt","Pohocco-Ida complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.6]
["NE021","Burt","Pohocco-Monona complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,4.75,7]
["NE021","Burt","Salix silty clay loam, rarely flooded","Moderately well drained","C",1.5,7.1,7]
["NE021","Burt","Sarpy fine sand, 0 to 6 percent slopes, occasionally flooded","Excessively drained","A",0.75,95.9,7.5]
["NE021","Burt","Sarpy-Grable variant complex, occasionally flooded","Somewhat poorly drained","C",0.75,95.4,7.6]
["NE021","Burt","Solomon silty clay, occasionally flooded","Poorly drained","D",1.75,5.5,8.1999999999999993]
["NE021","Burt","Steinauer clay loam, 11 to 30 percent slopes, eroded","Well drained","C",0.75,33.6,7.9]
["NE021","Burt","Steinauer soils, 11 to 30 percent slopes","Well drained","C",0.75,33.6,8.1999999999999993]
["NE021","Burt","Udorthents silt loam, channeled, occasionally flooded","Well drained","B",0.75,13.8,7.8]
["NE021","Burt","Wathena fine sandy loam, occasionally flooded","Moderately well drained","B",0.25,75.349999999999994,7.3000000000000007]
["NE021","Burt","Woodbury silty clay, occasionally flooded","Somewhat poorly drained","D",2,13.600000000000001,6.95]
["NE021","Burt","Zook silt loam, overwash, occasionally flooded","Poorly drained","D",3,16.25,6.6]
["NE021","Burt","Zook silty clay loam, occasionally flooded","Poorly drained","D",4.5,7.75,6.6]
["NE021","Burt","Zook silty clay, occasionally flooded","Poorly drained","D",4.5,7.85,6.6]
["NE023","Butler",null,"",""]
["NE023","Butler","Aksarben silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,3,6.5]
["NE023","Butler","Aksarben silty clay loam, 2 to 6 percent slopes","Well drained","C",1.5,18.2,5.8]
["NE023","Butler","Aksarben silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.5,18.2,5.8]
["NE023","Butler","Alda fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,66,7.5]
["NE023","Butler","Barney loam, frequently flooded","Poorly drained","B/D",0.25,47.9,7.5]
["NE023","Butler","Barney silty clay loam, frequently flooded","Poorly drained","B/D",1.625,67.449999999999989,7.35]
["NE023","Butler","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,66.099999999999994,6.7]
["NE023","Butler","Blendon fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.5,66.099999999999994,6.7]
["NE023","Butler","Blendon-Muir complex, 0 to 2 percent slopes","Well drained","A",1.75,37.450000000000003,6.7]
["NE023","Butler","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE023","Butler","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE023","Butler","Boel-Alda complex, occasionally flooded","Somewhat poorly drained","B",0.75,66,7.5]
["NE023","Butler","Brocksburg sandy loam, 0 to 2 percent slopes","Well drained","B",1.5,63.5,7.2]
["NE023","Butler","Burchard loam, 11 to 17 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE023","Butler","Burchard loam, 6 to 11 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE023","Butler","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.5,7.9]
["NE023","Butler","Burchard-Steinauer clay loams, 6 to 11 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE023","Butler","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE023","Butler","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE023","Butler","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE023","Butler","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE023","Butler","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE023","Butler","Crofton silt loam, 30 to 60 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE023","Butler","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE023","Butler","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE023","Butler","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE023","Butler","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE023","Butler","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.4,7.9]
["NE023","Butler","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.5,83.6,7.35]
["NE023","Butler","Grigston silt loam, rarely flooded","Well drained","B",1.5,9.1,7.9]
["NE023","Butler","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE023","Butler","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE023","Butler","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE023","Butler","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",0.75,18.5,6.5]
["NE023","Butler","Hastings silt loam, 7 to 11 percent slopes","Well drained","C",0.75,18.5,6.5]
["NE023","Butler","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE023","Butler","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE023","Butler","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE023","Butler","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE023","Butler","Ida-Steinauer complex, 17 to 60 percent slopes","Well drained","B",0.5,22.35,7.9]
["NE023","Butler","Inavale loamy sand, 3 to 6 percent slopes, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE023","Butler","Inavale-Boel complex, 0 to 6 percent slopes, occasionally flooded","Somewhat poorly drained","B",0.25,92.2,7.5]
["NE023","Butler","Inglewood loamy fine sand, rarely flooded","Moderately well drained","A",0.25,87.55,7]
["NE023","Butler","Judson silt loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE023","Butler","Judson silt loam, 2 to 6 percent slopes","Well drained","C",2.5,7.1,6.5]
["NE023","Butler","Kenridge silty clay loam, occasionally flooded","Moderately well drained","C",2.75,6.8000000000000007,6.4]
["NE023","Butler","Kezan silt loam, frequently flooded","Poorly drained","C",0.75,8.6999999999999993,7.2]
["NE023","Butler","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE023","Butler","Leshara silt loam, drained, rarely flooded","Well drained","B",0.75,11.6,7.5]
["NE023","Butler","Lex loam, occasionally flooded","Somewhat poorly drained","C",2,39.1,7.9]
["NE023","Butler","Longford silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,19.899999999999999,6.5]
["NE023","Butler","Longford silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,19.899999999999999,6.5]
["NE023","Butler","Malmo clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE023","Butler","Monona silt loam, 11 to 17 percent slopes","Well drained","B",1.25,9.4,6.7]
["NE023","Butler","Monona silt loam, 17 to 30 percent slopes","Well drained","B",1.25,9.4,6.7]
["NE023","Butler","Monona silt loam, 2 to 6 percent slopes","Well drained","B",1.25,9.4,6.7]
["NE023","Butler","Muir silt loam, 1 to 3 percent slopes","Well drained","B",2,9,6.7]
["NE023","Butler","Muir silt loam, 3 to 7 percent slopes","Well drained","B",2,9,6.7]
["NE023","Butler","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE023","Butler","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.4,6.3]
["NE023","Butler","Nodaway silt loam, channeled, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE023","Butler","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE023","Butler","Olbut-Butler silt loams, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.25,6,7.5]
["NE023","Butler","Ovina loamy fine sand, rarely flooded","Somewhat poorly drained","B",1.5,66.900000000000006,7.5]
["NE023","Butler","Ovina-Thurman complex, 0 to 6 percent slopes","Somewhat poorly drained","B",1.125,84.9,7]
["NE023","Butler","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE023","Butler","Pawnee clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,33.5,6.5]
["NE023","Butler","Platte fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.25,73.900000000000006,7.5]
["NE023","Butler","Platte-Barney complex, channeled, frequently flooded","Poorly drained","C/D",2,64.400000000000006,7.2]
["NE023","Butler","Platte-Inavale complex, channeled, frequently flooded","Excessively drained","A",0.25,87.3,7.5]
["NE023","Butler","Pohocco silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.4,7.2]
["NE023","Butler","Pohocco silty clay loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,8.9,7.2]
["NE023","Butler","Pohocco silty clay loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,8.9,7.2]
["NE023","Butler","Pohocco silty clay loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,8.9,7.2]
["NE023","Butler","Pohocco, eroded-Crofton complex, 11 to 17 percent slopes","Well drained","B",0.75,9.4,7.2]
["NE023","Butler","Pohocco, eroded-Crofton complex, 17 to 30 percent slopes","Well drained","B",0.75,9.4,7.2]
["NE023","Butler","Pohocco, eroded-Crofton complex, 6 to 11 percent slopes","Well drained","B",0.75,9.4,7.2]
["NE023","Butler","Saltine-Gibbon silt loams, occasionally flooded","Somewhat poorly drained","C",0.75,9.4499999999999993,8.35]
["NE023","Butler","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE023","Butler","Silver Creek complex, rarely flooded","Somewhat poorly drained","C",0.5,44.15,8.0500000000000007]
["NE023","Butler","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,86.35,7]
["NE023","Butler","Steinauer clay loam, 11 to 30 percent slopes","Well drained","C",0.75,33.6,7.9]
["NE023","Butler","Steinauer clay loam, 30 to 50 percent slopes","Well drained","C",0.75,33.6,7.9]
["NE023","Butler","Steinauer clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,33.6,7.9]
["NE023","Butler","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE023","Butler","Thurman-Monona complex, 6 to 11 percent slopes","Well drained","B",0.75,84.9,6.5]
["NE023","Butler","Tomek silt loam, 0 to 2 percent slopes","Well drained","C",2.5,18.850000000000001,6.95]
["NE023","Butler","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE023","Butler","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE023","Butler","Uly variant silty clay loam, 3 to 6 percent slopes, eroded","Somewhat poorly drained","C",0.75,20,7.9]
["NE023","Butler","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE023","Butler","Uly-Hobbs silt loams, 0 to 30 percent slopes, eroded","Well drained","B",0.75,10.35,7]
["NE023","Butler","Wood River silt loam, 1 to 3 percent slopes","Moderately well drained","C",0.75,22.9,8.5]
["NE023","Butler","Yutan silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.5,7.5,6.7]
["NE023","Butler","Yutan silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.75,7.6,6.5]
["NE023","Butler","Yutan silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,7.6,6.5]
["NE023","Butler","Yutan, eroded-Aksarben silty clay loams, 2 to 6 percent slopes","Well drained","C",0.75,7.5,6.5]
["NE023","Butler","Yutan, eroded-Judson complex, 6 to 11 percent slopes","Well drained","C",0.875,7.2,6.6]
["NE023","Butler","Zook silt loam, overwash, occasionally flooded","Poorly drained","C/D",3,16.25,6.6]
["NE023","Butler","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.75,6.6]
["NE025","Cass",null,"",""]
["NE025","Cass","Aksarben silty clay loam, 0 to 2 percent slopes","Well drained","C",1.5,18.2,6.3]
["NE025","Cass","Aksarben silty clay loam, 2 to 6 percent slopes","Well drained","C",1.5,18.2,6.3]
["NE025","Cass","Aksarben silty clay loam, 6 to 11 percent slopes","Well drained","C",1.5,18.2,6.3]
["NE025","Cass","Aksarben silty clay loam, terrace, 0 to 1 percent slopes","Well drained","C",1.5,18.2,6.3]
["NE025","Cass","Aksarben silty clay loam, terrace, 1 to 3 percent slopes","Well drained","C",1.5,18.2,6.3]
["NE025","Cass","Albaton silty clay, occasionally flooded","Poorly drained","D",1.5,3.9,7.6]
["NE025","Cass","Alda-Platte complex, occasionally flooded","Somewhat poorly drained","C",0.75,65.7,7.9]
["NE025","Cass","Burchard-Morrill clay loams, 6 to 11 percent slopes","Well drained","C",0.75,36.5,6.55]
["NE025","Cass","Cass-Novina complex, occasionally flooded","Well drained","B",0.75,64.599999999999994,6.8]
["NE025","Cass","Colo silty clay loam, occasionally flooded","Poorly drained","C/D",3.5,6.8,6.3]
["NE025","Cass","Colo-Nodaway complex, frequently flooded","Poorly drained","C/D",3,6.85,6.3]
["NE025","Cass","Filbert silt loam, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,8.75,6.4]
["NE025","Cass","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1.5,18.5,6.7]
["NE025","Cass","Fillmore silt loam, terrace, occasionally ponded","Somewhat poorly drained","D",1.5,10,5.8]
["NE025","Cass","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",2,7.1,6.1]
["NE025","Cass","Haynie silt loam, occasionally flooded","Well drained","B",1.25,12.600000000000001,7.5]
["NE025","Cass","Hedville sandy loam, 7 to 20 percent slopes","Somewhat excessively drained","D",2.5,43.2,5.8]
["NE025","Cass","Ida silt loam, 17 to 30 percent slopes","Well drained","B",2.5,11.2,7.5]
["NE025","Cass","Ida-Steinauer complex, 17 to 60 percent slopes","Well drained","B",0.5,22.35,7.9]
["NE025","Cass","Inglewood-Novina complex, occasionally flooded","Moderately well drained","B",0.25,66.599999999999994,7]
["NE025","Cass","Judson silt loam, 0 to 2 percent slopes","Well drained","C",3.5,7.9,6.25]
["NE025","Cass","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3.5,7.9,6.25]
["NE025","Cass","Kennebec silt loam, occasionally flooded","Moderately well drained","C",2,5,6.35]
["NE025","Cass","Lex-Platte complex, occasionally flooded","Somewhat poorly drained","C",2,60,7.9]
["NE025","Cass","Marshall silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.5,6.9,6.5]
["NE025","Cass","Marshall silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,6.9,6.5]
["NE025","Cass","Marshall silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.75,6.9,6.5]
["NE025","Cass","Marshall silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,6.9,6.5]
["NE025","Cass","Marshall silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,6.9,6.5]
["NE025","Cass","Mayberry silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.75,26.1,6.5]
["NE025","Cass","Monona silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1,9.4,6.3]
["NE025","Cass","Monona silt loam, 17 to 30 percent slopes","Well drained","B",1,9.4,6.3]
["NE025","Cass","Monona silt loam, 2 to 6 percent slopes","Well drained","B",1,9.4,6.3]
["NE025","Cass","Monona silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.3,6.8]
["NE025","Cass","Monona-Ida silt loams, 11 to 17 percent slopes, eroded","Well drained","B",1.75,10.3,6.65]
["NE025","Cass","Monona-Ida silt loams, 30 to 60 percent slopes","Well drained","B",1.75,10.3,6.65]
["NE025","Cass","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.6,55.8,6.1]
["NE025","Cass","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",3,9.5,6.7]
["NE025","Cass","Nodaway silt loam, channeled, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE025","Cass","Nodaway silt loam, occasionally flooded","Moderately well drained","B",2.5,9.5,6.7]
["NE025","Cass","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.6]
["NE025","Cass","Otoe silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE025","Cass","Pawnee clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",2,33.5,7]
["NE025","Cass","Pohocco silty clay loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.1,7.35]
["NE025","Cass","Pohocco silty clay loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,8.9,7.2]
["NE025","Cass","Pohocco-Pahuk complex, 11 to 17 percent slopes, eroded","Excessively drained","A",0.75,9.3000000000000007,7.2]
["NE025","Cass","Pohocco-Pahuk complex, 6 to 11 percent slopes, eroded","Excessively drained","A",0.75,9.3000000000000007,7.2]
["NE025","Cass","Sarpy loamy fine sand, frequently flooded","Excessively drained","A",0.5,87.9,7.25]
["NE025","Cass","Sarpy-Haynie complex, occasionally flooded","Well drained","B",0.75,69.599999999999994,7.5]
["NE025","Cass","Sharpsburg variant silty clay loam, 1 to 3 percent slopes","Moderately well drained","D",0.75,8.4,8.1999999999999993]
["NE025","Cass","Thurman loamy fine sand, 11 to 20 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE025","Cass","Tomek silt loam, 0 to 2 percent slopes","Well drained","C",2.5,18.850000000000001,6.95]
["NE025","Cass","Udorthents, silty","Well drained","B",0.375,10,3.9]
["NE025","Cass","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE025","Cass","Wymore silty clay loam, 2 to 6 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE025","Cass","Wymore silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",1.5,17.3,6.5]
["NE025","Cass","Yutan silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.75,7.6,6.3]
["NE025","Cass","Yutan silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.75,7.6,6.3]
["NE025","Cass","Yutan silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,7.6,6.3]
["NE025","Cass","Yutan, eroded-Aksarben silty clay loams, 2 to 6 percent slopes","Well drained","C",0.75,7.5,6.5]
["NE025","Cass","Yutan, eroded-Judson complex, 6 to 11 percent slopes","Well drained","C",0.875,7.2,6.6]
["NE025","Cass","Zook silty clay loam, occasionally flooded","Poorly drained","D",4.5,7.75,6.05]
["NE025","Cass","Zook silty clay, occasionally flooded","Poorly drained","D",4.5,7.85,6.05]
["NE027","Cedar",null,"",""]
["NE027","Cedar","Albaton silty clay, frequently flooded","Very poorly drained","D",1.5,2.4,7.9]
["NE027","Cedar","Albaton silty clay, rarely flooded","Poorly drained","D",1.5,3.9,7.9]
["NE027","Cedar","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE027","Cedar","Alcester silt loam, 6 to 11 percent slopes","Well drained","B",2.5,7.4,7]
["NE027","Cedar","Aowa silt loam, channeled, frequently flooded","Well drained","B",1.625,21.15,7.9]
["NE027","Cedar","Aowa silt loam, occasionally flooded","Well drained","B",1.625,21.15,7.9]
["NE027","Cedar","Baltic silty clay loam, occasionally flooded","Poorly drained","C/D",3,8,7.9]
["NE027","Cedar","Barney variant fine sand, frequently flooded","Very poorly drained","A/D",0.5,92.7,7.9]
["NE027","Cedar","Bazile loam, 0 to 2 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE027","Cedar","Betts clay loam, 15 to 30 percent slopes","Somewhat excessively drained","C",0.5,35.4,7.9]
["NE027","Cedar","Betts clay loam, 6 to 15 percent slopes","Well drained","C",1.75,20.85,7.55]
["NE027","Cedar","Blake silty clay loam, rarely flooded","Somewhat poorly drained","C",0.5,7.1,7.9]
["NE027","Cedar","Blendon fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.125,66.699999999999989,6.85]
["NE027","Cedar","Blendon loam, 0 to 2 percent slopes","Well drained","B",0.875,63.95,6.85]
["NE027","Cedar","Boyd silty clay, 11 to 15 percent slopes","Well drained","D",2,2.5499999999999998,7.5]
["NE027","Cedar","Boyd silty clay, 6 to 11 percent slopes","Well drained","D",2,2.5499999999999998,7.5]
["NE027","Cedar","Coleridge silt loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE027","Cedar","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE027","Cedar","Crofton silt loam, 17 to 30 percent slopes","Somewhat excessively drained","B",0.75,10.350000000000001,7.9]
["NE027","Cedar","Crofton silt loam, 30 to 60 percent slopes","Excessively drained","B",0.75,10.350000000000001,7.9]
["NE027","Cedar","Crofton-Alcester silt loams, 20 to 60 percent slopes","Well drained","B",1.25,9.4,7.5]
["NE027","Cedar","Crofton-Gavins silt loams, 30 to 60 percent slopes","Excessively drained","B",0.5,11.3,7.5]
["NE027","Cedar","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE027","Cedar","Crofton-Nora complex, 2 to 6 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE027","Cedar","Crofton-Nora complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE027","Cedar","Crofton-Nora silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE027","Cedar","Crofton-Nora silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE027","Cedar","Dudley-Moody complex, 0 to 2 percent slopes","Moderately well drained","C",2,26.1,7.3]
["NE027","Cedar","Eltree silt loam, 0 to 3 percent slopes","Well drained","B",1,9.5,7.9]
["NE027","Cedar","Eltree silt loam, 3 to 6 percent slopes","Well drained","B",1,9.5,7.9]
["NE027","Cedar","Eltree silt loam, 6 to 11 percent slopes","Well drained","B",1,9.5,7.9]
["NE027","Cedar","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1.5,15.4,6.7]
["NE027","Cedar","Gavins silt loam, 17 to 30 percent slopes","Somewhat excessively drained","D",0.5,24,7.5]
["NE027","Cedar","Gavins silt loam, 30 to 60 percent slopes","Well drained","D",0.5,24,7.5]
["NE027","Cedar","Gavins silt loam, 6 to 17 percent slopes","Well drained","D",0.5,24,7.5]
["NE027","Cedar","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE027","Cedar","Grable silt loam, rarely flooded","Well drained","B",0.5,14.2,7.9]
["NE027","Cedar","Hobbs silt loam, frequently flooded","Well drained","B",1.875,11.3,7]
["NE027","Cedar","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE027","Cedar","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE027","Cedar","Hord silt loam, bedrock substratum, 0 to 1 percent slopes","Well drained","B",0.75,8.9499999999999993,7.2]
["NE027","Cedar","Hord silt loam, rarely flooded","Well drained","B",0.75,9.3000000000000007,7]
["NE027","Cedar","Inavale coarse sand, channeled, frequently flooded","Excessively drained","A",0.25,92.2,6.7]
["NE027","Cedar","Kezan silt loam, frequently flooded","Poorly drained","C",1.875,9.0500000000000007,7.2]
["NE027","Cedar","Kezan silt loam, occasionally flooded","Poorly drained","C",1.875,7.85,7.35]
["NE027","Cedar","Labu silty clay, 6 to 11 percent slopes","Well drained","D",0.75,2.6,7.5]
["NE027","Cedar","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE027","Cedar","Loretto loam, sand substratum, 2 to 6 percent slopes","Well drained","B",1.5,44.3,6.5]
["NE027","Cedar","Loretto loam, sand substratum, 6 to 11 percent slopes","Well drained","B",1.5,44.3,6.5]
["NE027","Cedar","Maskell loam, 0 to 2 percent slopes","Well drained","B",0.5,39.799999999999997,7]
["NE027","Cedar","Maskell loam, 2 to 6 percent slopes","Well drained","B",0.5,39.799999999999997,7]
["NE027","Cedar","Modale silt loam, rarely flooded","Moderately well drained","C",1.375,8.35,7.9]
["NE027","Cedar","Moody loam, 2 to 6 percent slopes","Well drained","C",3,9.4,6.5]
["NE027","Cedar","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE027","Cedar","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE027","Cedar","Moody silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE027","Cedar","Moody silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE027","Cedar","Nimbro silt loam, occasionally flooded","Well drained","B",1.75,30.900000000000002,7.9]
["NE027","Cedar","Nora silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE027","Cedar","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE027","Cedar","Nora silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,8.9,7]
["NE027","Cedar","Obert silt loam, occasionally flooded","Very poorly drained","C/D",1.5,7.3,7.9]
["NE027","Cedar","Obert silty clay loam, occasionally flooded","Poorly drained","C/D",1.5,7.3,7.9]
["NE027","Cedar","Onawa silty clay, rarely flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE027","Cedar","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE027","Cedar","Ortello sandy loam, 11 to 17 percent slopes","Well drained","A",0.75,66.599999999999994,6.7]
["NE027","Cedar","Ortello sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,66.599999999999994,6.7]
["NE027","Cedar","Ortello sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.599999999999994,6.7]
["NE027","Cedar","Percival silty clay, rarely flooded","Somewhat poorly drained","D",1.125,48.5,7.9]
["NE027","Cedar","Redstoe silt loam, 0 to 2 percent slopes","Well drained","C",2,9,7.5]
["NE027","Cedar","Redstoe silt loam, 2 to 6 percent slopes","Well drained","C",2,9,7.5]
["NE027","Cedar","Redstoe silt loam, 6 to 11 percent slopes","Well drained","C",2,9,7.5]
["NE027","Cedar","Redstoe-Gavins complex, 11 to 30 percent slopes","Well drained","D",1.25,10.1,7.5]
["NE027","Cedar","Sarpy fine sand, 3 to 11 percent slopes","Excessively drained","A",0.75,95.9,7.7]
["NE027","Cedar","Sarpy loamy fine sand, rarely flooded","Excessively drained","A",0.5,87.9,7.5]
["NE027","Cedar","Sarpy-Riverwash complex, frequently flooded","Very poorly drained","A/D",0.5,92.95,7.7]
["NE027","Cedar","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE027","Cedar","Simeon sand, 6 to 30 percent slopes, eroded","Excessively drained","A",0.5,91.85,7]
["NE027","Cedar","Simeon-Talmo-Ortello complex, 11 to 30 percent slopes","Well drained","A",0.75,67.449999999999989,7]
["NE027","Cedar","Talmo-Loretto complex, 3 to 11 percent slopes","Well drained","B",1.5,65.900000000000006,7.2]
["NE027","Cedar","Thurman fine sandy loam, 2 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE027","Cedar","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.875,89.9,6.5]
["NE027","Cedar","Thurman-Loretto complex, 2 to 6 percent slopes","Well drained","B",0.875,83.7,6.5]
["NE027","Cedar","Thurman-Ortello complex, 6 to 11 percent slopes","Well drained","A",0.75,82.5,6.5]
["NE029","Chase",null,"",""]
["NE029","Chase","Alliance silt loam, 0 to 1 percent slopes","Well drained","B",0.75,11.4,7.2]
["NE029","Chase","Altvan loam, 0 to 1 percent slopes","Well drained","C",0.875,41.9,7.85]
["NE029","Chase","Altvan loam, 1 to 3 percent slopes","Well drained","C",0.875,41.9,7.85]
["NE029","Chase","Altvan loam, 3 to 6 percent slopes","Well drained","C",0.875,41.9,7.85]
["NE029","Chase","Ascalon fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.875,60.6,7.5500000000000007]
["NE029","Chase","Ascalon fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.875,62.9,7.5500000000000007]
["NE029","Chase","Blackwood loam, 0 to 1 percent slopes","Well drained","B",1.5,33.299999999999997,8.1999999999999993]
["NE029","Chase","Blackwood loam, 1 to 3 percent slopes","Well drained","B",1.5,33.299999999999997,8.1999999999999993]
["NE029","Chase","Blackwood silt loam, 0 to 1 percent slopes","Well drained","B",1.5,9.1,7.6]
["NE029","Chase","Blackwood silt loam, 1 to 3 percent slopes","Well drained","B",1.5,9.5,7.6]
["NE029","Chase","Blackwood silt loam, 3 to 6 percent slopes","Well drained","B",1.5,9.1,7.6]
["NE029","Chase","Blanche fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,62.8,7.2]
["NE029","Chase","Blanche very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,65.05,7.35]
["NE029","Chase","Bridget silt loam, 0 to 1 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE029","Chase","Bridget silt loam, 1 to 3 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE029","Chase","Bushman very fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.125,62,7.9]
["NE029","Chase","Canyon-Sulco-Rock outcrop complex, 17 to 60 percent slopes","Excessively drained","D",0.75,43.3,7.9]
["NE029","Chase","Caruso loam, occasionally flooded","Somewhat poorly drained","C",1.375,38.849999999999994,8.1999999999999993]
["NE029","Chase","Creighton very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE029","Chase","Creighton very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE029","Chase","Creighton very fine sandy loam, 6 to 11 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE029","Chase","Dailey loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1.375,80.400000000000006,7.25]
["NE029","Chase","Duda-Tassel complex, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,63.3,6.85]
["NE029","Chase","Duda-Tassel loamy sands, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,71.900000000000006,6.85]
["NE029","Chase","Duroc loam, 0 to 1 percent slopes","Well drained","B",1.25,33.299999999999997,7.3]
["NE029","Chase","Fluvaquents, silty, frequently flooded","Very poorly drained","B/D",2.5,11.75,3.75]
["NE029","Chase","Gannett silt loam, overwash, frequently ponded","Very poorly drained","B/D",4.375,47.4,7.5]
["NE029","Chase","Gannett variant silt loam, occasionally flooded","Very poorly drained","B/D",2.875,51.15,6.6]
["NE029","Chase","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE029","Chase","Goshen silt loam, 0 to 1 percent slopes","Well drained","C",0.75,11.3,7.5]
["NE029","Chase","Haxtun fine sandy loam, 0 to 3 percent slopes","Well drained","B",1.5,64.05,7.45]
["NE029","Chase","Haxtun loamy fine sand, 0 to 3 percent slopes","Well drained","B",1.75,63.599999999999994,7]
["NE029","Chase","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.52500000000000002,63,7.2]
["NE029","Chase","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.52500000000000002,63,7.2]
["NE029","Chase","Jayem loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE029","Chase","Jayem loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE029","Chase","Jayem loamy sand, 0 to 3 percent slopes","Well drained","A",1,62.5,7]
["NE029","Chase","Jayem loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.75,80,7.2]
["NE029","Chase","Jayem loamy very fine sand, 3 to 6 percent slopes","Well drained","A",1.1499999999999999,80.75,7.2]
["NE029","Chase","Keith silt loam, 1 to 3 percent slopes","Well drained","C",0.75,13.7,7]
["NE029","Chase","Keith silt loam, 3 to 6 percent slopes, eroded","Well drained","C",0.75,13.7,7]
["NE029","Chase","Kuma silt loam, 0 to 1 percent slopes","Well drained","B",2,13.7,7.5]
["NE029","Chase","Kuma silt loam, 1 to 3 percent slopes","Well drained","B",2,13.7,7.5]
["NE029","Chase","Kuma silt loam, 3 to 6 percent slopes","Well drained","B",2,13.7,7.5]
["NE029","Chase","Laird fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,62.8,8.5]
["NE029","Chase","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",2,26.4,7]
["NE029","Chase","Lodgepole silty clay loam, frequently ponded","Poorly drained","C/D",1.75,13.149999999999999,6.65]
["NE029","Chase","Mace silt loam, 0 to 1 percent slopes","Well drained","C",1.25,9.5,7.2]
["NE029","Chase","Mace silt loam, 1 to 3 percent slopes","Well drained","C",1.25,9.5,7.2]
["NE029","Chase","Mace-Alliance silt loams, 0 to 1 percent slopes","Well drained","C",0.75,10.45,7.2]
["NE029","Chase","Mace-Alliance silt loams, 1 to 3 percent slopes","Well drained","C",0.75,10.45,7.2]
["NE029","Chase","McCash very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.25,60.3,7]
["NE029","Chase","McCook silt loam, channeled, occasionally flooded","Well drained","B",1.75,12.75,7.9]
["NE029","Chase","McCook silt loam, occasionally flooded","Well drained","B",1.75,12.75,7.9]
["NE029","Chase","McCook silt loam, rarely flooded","Well drained","B",1.875,12.95,7.9]
["NE029","Chase","Otero-Canyon loams, 6 to 20 percent slopes","Well drained","D",0.75,44.3,7.9]
["NE029","Chase","Overlake sand, 0 to 3 percent slopes","Well drained","B",0.25,81.150000000000006,8.5]
["NE029","Chase","Rosebud loam, 0 to 1 percent slopes","Well drained","C",0.75,38,7.35]
["NE029","Chase","Rosebud loam, 1 to 3 percent slopes","Well drained","C",0.75,39.4,7.35]
["NE029","Chase","Rosebud-Canyon loams, 0 to 1 percent slopes","Well drained","D",0.75,43,7.5]
["NE029","Chase","Rosebud-Canyon loams, 1 to 3 percent slopes","Well drained","D",0.75,43,7.5]
["NE029","Chase","Rosebud-Canyon loams, 3 to 6 percent slopes","Well drained","D",0.75,43,7.5]
["NE029","Chase","Rosebud-Canyon loams, 6 to 12 percent slopes, eroded","Well drained","D",0.75,43,7.5]
["NE029","Chase","Sarben loamy sand, 3 to 6 percent slopes","Well drained","A",0.25,62.5,7]
["NE029","Chase","Sarben loamy very fine sand, 3 to 6 percent slopes","Well drained","A",0.5,79.099999999999994,7.2]
["NE029","Chase","Sarben loamy very fine sand, 6 to 9 percent slopes","Well drained","A",0.5,79.099999999999994,7.2]
["NE029","Chase","Satanta fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,39.799999999999997,7.3]
["NE029","Chase","Satanta loam, 1 to 3 percent slopes","Well drained","C",0.75,43,7.5]
["NE029","Chase","Satanta loam, 3 to 6 percent slopes","Well drained","C",0.75,43,7.5]
["NE029","Chase","Satanta very fine sandy loam, 1 to 3 percent slopes","Well drained","C",1.25,63.5,7.5]
["NE029","Chase","Satanta very fine sandy loam, 3 to 6 percent slopes","Well drained","C",1.25,63.5,7.5]
["NE029","Chase","Sulco complex, 9 to 60 percent slopes","Well drained","B",0.25,43.6,8.1999999999999993]
["NE029","Chase","Sulco fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.25,52.400000000000006,8.1999999999999993]
["NE029","Chase","Sulco loam, 9 to 30 percent slopes","Well drained","B",0.25,43.6,8.1999999999999993]
["NE029","Chase","Sulco silt loam, 30 to 60 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE029","Chase","Sulco silt loam, 6 to 9 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE029","Chase","Sulco silt loam, 9 to 30 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE029","Chase","Sulco-Canyon loams, 20 to 45 percent slopes","Well drained","D",1.25,43.6,7.9]
["NE029","Chase","Sulco-Ulysses silt loams, 9 to 30 percent slopes, eroded","Well drained","B",1.25,13.6,7.9]
["NE029","Chase","Tassel-Duda loamy sands, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,71.900000000000006,6.85]
["NE029","Chase","Tassel-Duda loamy sands, 3 to 30 percent slopes","Somewhat excessively drained","A",0.875,71.900000000000006,6.85]
["NE029","Chase","Tassel-Duda loamy sands, 6 to 30 percent slopes","Somewhat excessively drained","A",0.875,71.900000000000006,6.85]
["NE029","Chase","Ulysses loam, 1 to 3 percent slopes","Well drained","B",1,37.15,7.8999999999999995]
["NE029","Chase","Ulysses loam, 3 to 6 percent slopes","Well drained","B",0.9,33.299999999999997,7.6]
["NE029","Chase","Ulysses silt loam, 3 to 6 percent slopes, eroded","Well drained","B",1.5,9.5,7.9]
["NE029","Chase","Ulysses silt loam, 6 to 9 percent slopes, eroded","Well drained","B",1.5,9.5,7.9]
["NE029","Chase","Ulysses-Sulco silt loams, 6 to 9 percent slopes, eroded","Well drained","B",1,13.6,7.9]
["NE029","Chase","Valent complex, rolling and hilly","Excessively drained","A",0.375,95,7]
["NE029","Chase","Valent loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,88.6,7]
["NE029","Chase","Valent loamy sand, 3 to 9 percent slopes","Excessively drained","A",0.5,88.6,7]
["NE029","Chase","Valent sand, 0 to 3 percent slopes","Excessively drained","A",0.25,95,7]
["NE029","Chase","Valent sand, 3 to 9 percent slopes","Excessively drained","A",0.25,95,7]
["NE029","Chase","Valent sand, rolling","Excessively drained","A",0.5,95,7]
["NE029","Chase","Valent sand, rolling and hilly","Excessively drained","A",0.5,95,7]
["NE029","Chase","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE029","Chase","Wann fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,63.2,8.1999999999999993]
["NE029","Chase","Woodly fine sandy loam, 0 to 3 percent slopes","Well drained","B",0.5,65.400000000000006,7]
["NE029","Chase","Woodly loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.5,65.400000000000006,7]
["NE031","Cherry",null,"",""]
["NE031","Cherry","Almeria fine sandy loam, occasionally flooded","Poorly drained","A/D",3.375,78.2,6.9]
["NE031","Cherry","Almeria fine sandy loam, wet, occasionally flooded","Very poorly drained","A/D",0.25,63.5,6.5]
["NE031","Cherry","Almeria loamy fine sand, channeled, frequently flooded","Very poorly drained","A/D",1.25,89.85,6.9]
["NE031","Cherry","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE031","Cherry","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE031","Cherry","Anselmo fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE031","Cherry","Anselmo loamy fine sand, 0 to 3 percent slopes","Well drained","A",1.125,76.55,7.1]
["NE031","Cherry","Anselmo loamy fine sand, 3 to 6 percent slopes","Well drained","A",1.125,76.55,7.1]
["NE031","Cherry","Anselmo-Longpine fine sandy loams, 9 to 30 percent slopes","Well drained","A",0.75,66.099999999999994,7.2]
["NE031","Cherry","Bolent fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.875,65.2,7.7]
["NE031","Cherry","Bolent loamy fine sand, channeled, occasionally flooded","Somewhat poorly drained","A",0.5,75.349999999999994,7.7]
["NE031","Cherry","Bolent-Almeria complex, channeled, frequently flooded","Very poorly drained","B/D",0.52500000000000002,89.5,7.4]
["NE031","Cherry","Bolent-Calamus, calcareous loamy fine sands, occasionally flooded","Somewhat poorly drained","A",0.3,86.8,7.5]
["NE031","Cherry","Busher fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,63.5,7]
["NE031","Cherry","Busher-Tassel fine sandy loams, 9 to 30 percent slopes","Well drained","A",0.75,64.5,7.25]
["NE031","Cherry","Calamus fine sand, calcareous","Moderately well drained","A",0.3,92.2,7.5]
["NE031","Cherry","Calamus loamy fine sand, calcareous, rarely flooded","Moderately well drained","A",0.3,93.2,7.5]
["NE031","Cherry","Calamus-Bolent loamy fine sands, channeled, occasionally flooded","Somewhat poorly drained","A",0.375,89.5,6.8]
["NE031","Cherry","Crowther loam, 0 to 1 percent slopes","Poorly drained","B/D",1.125,37.200000000000003,7.7]
["NE031","Cherry","Crowther mucky peat","Very poorly drained","B/D",1.125,37.200000000000003,7.7]
["NE031","Cherry","Cullison loam, 0 to 1 percent slopes","Poorly drained","B/D",3,33.5,7.9]
["NE031","Cherry","Cullison mucky peat","Very poorly drained","B/D",8.5,34.700000000000003,7.9]
["NE031","Cherry","Cutcomb mucky peat","Very poorly drained","A/D",29,0,0]
["NE031","Cherry","Dailey loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1.375,79.900000000000006,7.25]
["NE031","Cherry","Dailey loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",1.375,79.900000000000006,7.25]
["NE031","Cherry","Doughboy fine sandy loam, 0 to 3 percent slopes","Moderately well drained","A",2,63.5,7.9]
["NE031","Cherry","Doughboy loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",2,86,7.9]
["NE031","Cherry","Duda-Fishberry loamy fine sands, 0 to 3 percent slopes","Somewhat excessively drained","A",0.5,80.099999999999994,6.85]
["NE031","Cherry","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE031","Cherry","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE031","Cherry","Els calcareous-Hoffland complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.625,94.1,7.9]
["NE031","Cherry","Els fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.7]
["NE031","Cherry","Els, calcareous-Hoffland complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,93.2,7.9]
["NE031","Cherry","Els, calcareous-Selia fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,93.2,8.1]
["NE031","Cherry","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE031","Cherry","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.5]
["NE031","Cherry","Elsmere loamy fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,7.9]
["NE031","Cherry","Elsmere-Loup complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,94.9,6.5]
["NE031","Cherry","Els-Tryon complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,95.4,6.7]
["NE031","Cherry","Fishberry fine sandy loam, 0 to 6 percent slopes","Excessively drained","D",0.5,60.5,7.5]
["NE031","Cherry","Fishberry-Duda loamy fine sands, 6 to 30 percent slopes","Somewhat excessively drained","A",0.5,70.400000000000006,6.85]
["NE031","Cherry","Fishberry-Rock outcrop complex, 30 to 60 percent slopes","Excessively drained","D",0.25,30.25,3.75]
["NE031","Cherry","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,44.85,3.75]
["NE031","Cherry","Gannett loam, 0 to 1 percent slopes","Poorly drained","B/D",0.75,45.3,6.5]
["NE031","Cherry","Gannett mucky peat","Very poorly drained","B/D",0.5,42.55,6.5]
["NE031","Cherry","Gus clay loam, 0 to 1 percent slopes","Poorly drained","B/D",3.125,45.5,7]
["NE031","Cherry","Gus mucky peat","Very poorly drained","B/D",9.25,36.549999999999997,7]
["NE031","Cherry","Hennings fine sandy loam, 0 to 3 percent slopes","Well drained","B",0.25,67.3,7.2]
["NE031","Cherry","Hennings fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.25,67.3,7.2]
["NE031","Cherry","Hennings fine sandy loam, 6 to 11 percent slopes","Well drained","B",0.25,67.3,7.2]
["NE031","Cherry","Hennings-Anselmo fine sandy loams, 11 to 20 percent slopes","Well drained","A",0.75,66.099999999999994,7.2]
["NE031","Cherry","Hoffland fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,93.2,7.5]
["NE031","Cherry","Hoffland fine sandy loam, frequently ponded","Very poorly drained","A/D",0.5,70.650000000000006,7.35]
["NE031","Cherry","Holt fine sandy loam, 0 to 2 percent slopes","Well drained","B",1,62.65,7.1]
["NE031","Cherry","Holt-Longpine fine sandy loams, 2 to 6 percent slopes","Well drained","B",0.75,66.099999999999994,7.2]
["NE031","Cherry","Holt-Longpine fine sandy loams, 6 to 11 percent slopes","Well drained","B",0.75,62.8,7.2]
["NE031","Cherry","Holt-Vetal fine sandy loams, 0 to 6 percent slopes","Well drained","B",1.125,65.75,7.1]
["NE031","Cherry","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE031","Cherry","Ipage fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,7.5]
["NE031","Cherry","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE031","Cherry","Ipage-Tryon complex, 0 to 3 percent slopes","Moderately well drained","A",0.75,95.15,6.45]
["NE031","Cherry","Jansen fine sandy loam, 0 to 2 percent slopes","Well drained","B",1.25,66.900000000000006,6.2]
["NE031","Cherry","Keya loam, 0 to 2 percent slopes","Well drained","B",1.25,39.5,7.2]
["NE031","Cherry","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,86.4,6.5]
["NE031","Cherry","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",2,26.4,7]
["NE031","Cherry","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",3.375,79.2,6.6]
["NE031","Cherry","Loup mucky peat","Very poorly drained","A/D",0.75,63.5,6.5]
["NE031","Cherry","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",0.5,72.150000000000006,6.85]
["NE031","Cherry","McKelvie loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,92.9,7]
["NE031","Cherry","McKelvie loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,92.9,7]
["NE031","Cherry","McKelvie loamy fine sand, 9 to 30 percent slopes","Excessively drained","A",0.25,92.9,7]
["NE031","Cherry","McKelvie-Fishberry loamy fine sands, 9 to 30 percent slopes","Excessively drained","D",0.375,83.55,7.25]
["NE031","Cherry","McKelvie-Fishberry-Rock outcrop complex, 11 to 60 percent slopes","Excessively drained","D",0.375,83.55,7.25]
["NE031","Cherry","McKelvie-Rock outcrop complex, 30 to 60 percent slopes","Excessively drained","A",0.25,89.85,7]
["NE031","Cherry","McKelvie-Ustorthents complex, 30 to 60 percent slopes","Excessively drained","A",0.25,86.8,7]
["NE031","Cherry","Meadin loamy sand, 0 to 2 percent slopes","Excessively drained","A",0.75,84.3,6.2]
["NE031","Cherry","Meadin loamy sand, 2 to 30 percent slopes","Excessively drained","A",0.75,89.9,6.2]
["NE031","Cherry","Medihemists","Very poorly drained","A/D",59.5,0,6.5]
["NE031","Cherry","Natick sand, 0 to 3 percent slopes","Moderately well drained","A",0.57499999999999996,93.5,6.4]
["NE031","Cherry","Nenzel loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",1.25,85.9,6.7]
["NE031","Cherry","Nenzel loamy fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",1.25,85.9,7.9]
["NE031","Cherry","Ord loam, rarely flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE031","Cherry","Orpha loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,94.4,7.2]
["NE031","Cherry","Orpha-Niobrara loamy fine sands, 9 to 30 percent slopes","Excessively drained","D",0.375,83.15,7.35]
["NE031","Cherry","Orpha-Rock outcrop complex, 30 to 60 percent slopes","Excessively drained","A",0.25,90.4,7.2]
["NE031","Cherry","Pivot loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.5,80.449999999999989,6.5]
["NE031","Cherry","Sandose loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.75,67.599999999999994,6.95]
["NE031","Cherry","Sandose-Hennings loamy fine sands, 0 to 3 percent slopes","Well drained","B",0.75,67.3,7.2]
["NE031","Cherry","Sandose-Hennings loamy fine sands, 3 to 6 percent slopes","Well drained","B",0.75,67.3,7.2]
["NE031","Cherry","Sandose-Hennings loamy fine sands, 6 to 11 percent slopes","Well drained","B",0.75,67.3,7.2]
["NE031","Cherry","Satanta fine sandy loam, 1 to 3 percent slopes","Well drained","C",1,63.95,7.7]
["NE031","Cherry","Simeon sand, 0 to 3 percent slopes","Excessively drained","A",0.5,91.85,7]
["NE031","Cherry","Simeon-Valentine complex, 0 to 9 percent slopes","Excessively drained","A",0.5,93.75,6.75]
["NE031","Cherry","Simeon-Valentine complex, 11 to 30 percent slopes","Excessively drained","A",0.5,93.75,6.75]
["NE031","Cherry","Tryon fine sandy loam, 0 to 3 percent slopes","Poorly drained","A/D",3.375,79.45,6.85]
["NE031","Cherry","Tryon fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,63.5,6.7]
["NE031","Cherry","Tuthill fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.625,75.650000000000006,7.45]
["NE031","Cherry","Tuthill fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.625,75.650000000000006,7.45]
["NE031","Cherry","Valentine complex, rolling and hilly","Excessively drained","A",0.5,96.3,6.1]
["NE031","Cherry","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,96.3,6.1]
["NE031","Cherry","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.1]
["NE031","Cherry","Valentine fine sand, hilly","Excessively drained","A",0.5,96.3,6.1]
["NE031","Cherry","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.1]
["NE031","Cherry","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,95.85,6.5]
["NE031","Cherry","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,83.35,6.5]
["NE031","Cherry","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,91.35,6.5]
["NE031","Cherry","Valentine-Birdwood complex, 9 to 80 percent slopes","Well drained","A",0.625,85.8,6.5]
["NE031","Cherry","Valentine-Duda complex, 3 to 9 percent slopes","Somewhat excessively drained","A",0.5,86.8,6.4]
["NE031","Cherry","Valentine-Duda complex, 9 to 24 percent slopes","Somewhat excessively drained","A",0.5,92.2,6.4]
["NE031","Cherry","Valentine-Dunday complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.625,94,6.6]
["NE031","Cherry","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.625,95.4,6.5]
["NE031","Cherry","Valentine-Libory complex, 0 to 9 percent slopes","Moderately well drained","A",0.75,91.7,6.5]
["NE031","Cherry","Valentine-Mullen complex, 0 to 9 percent slopes","Well drained","B",0.75,86,6.7]
["NE031","Cherry","Valentine-Sandose complex, 0 to 9 percent slopes","Well drained","B",0.75,87.4,6.6]
["NE031","Cherry","Valentine-Tryon fine sands, 0 to 24 percent slopes","Very poorly drained","A/D",0.75,95.85,6.6]
["NE031","Cherry","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,65.75,7.15]
["NE031","Cherry","Vetal loamy fine sand, 0 to 3 percent slopes","Well drained","A",1.125,74.45,7.5500000000000007]
["NE031","Cherry","Wildhorse fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,92.95,9.1499999999999986]
["NE033","Cheyenne",null,"",""]
["NE033","Cheyenne","Alliance loam, 0 to 1 percent slopes","Well drained","B",0.75,9.15,7.2]
["NE033","Cheyenne","Alliance loam, 1 to 3 percent slopes","Well drained","B",0.75,9.15,7.2]
["NE033","Cheyenne","Alliance loam, 3 to 6 percent slopes","Well drained","B",0.75,9.15,7.2]
["NE033","Cheyenne","Alliance-Rosebud loams, 1 to 3 percent slopes","Well drained","C",0.75,35.450000000000003,7.2]
["NE033","Cheyenne","Altvan fine sandy loam, 1 to 3 percent slopes","Well drained","C",0.75,54.5,7.5]
["NE033","Cheyenne","Altvan loam, 1 to 3 percent slopes","Well drained","B",0.75,42.4,7.9]
["NE033","Cheyenne","Altvan loam, 3 to 6 percent slopes","Well drained","B",0.75,42.4,7.9]
["NE033","Cheyenne","Altvan-Dix complex, 3 to 9 percent slopes","Well drained","B",0.75,62.5,7.5]
["NE033","Cheyenne","Altvan-Eckley complex, 3 to 9 percent slopes","Well drained","C",0.75,68,7.2]
["NE033","Cheyenne","Altvan-Eckley-Satanta complex, 3 to 9 percent slopes","Well drained","C",0.75,62,7.2]
["NE033","Cheyenne","Altvan-Eckley-Tassel complex, 3 to 9 percent slopes","Well drained","C",0.75,64.599999999999994,7.2]
["NE033","Cheyenne","Ashollow-Tassel complex, 9 to 30 percent slopes","Well drained","B",0.75,63.3,7.9]
["NE033","Cheyenne","Bankard loamy fine sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,78.599999999999994,7.9]
["NE033","Cheyenne","Bankard loamy sand, occasionally flooded","Somewhat excessively drained","A",0.625,81.75,8.0500000000000007]
["NE033","Cheyenne","Bayard fine sandy loam, 0 to 1 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE033","Cheyenne","Bayard fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.125,65.400000000000006,6.85]
["NE033","Cheyenne","Bayard fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE033","Cheyenne","Bayard fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE033","Cheyenne","Bayard fine sandy loam, 6 to 9 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE033","Cheyenne","Bayard fine sandy loam, 9 to 20 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE033","Cheyenne","Blueridge-Altvan complex, 6 to 30 percent slopes","Well drained","C",0.75,83.5,7.2]
["NE033","Cheyenne","Bridget very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE033","Cheyenne","Bridget very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE033","Cheyenne","Bridget very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE033","Cheyenne","Bridget very fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE033","Cheyenne","Broadwater loamy sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,84.3,7.2]
["NE033","Cheyenne","Broadwater loamy sand, channeled, occasionally flooded","Excessively drained","A",0.25,91.9,7.2]
["NE033","Cheyenne","Broadwater loamy sand, frequently flooded","Somewhat excessively drained","A",0.5,88.800000000000011,7.2]
["NE033","Cheyenne","Busher fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,7]
["NE033","Cheyenne","Busher-Tassel complex, 3 to 9 percent slopes","Well drained","A",1,64.05,7.25]
["NE033","Cheyenne","Busher-Tassel complex, 9 to 20 percent slopes","Well drained","A",1,64.05,7.25]
["NE033","Cheyenne","Canyon fine sandy loam, 6 to 30 percent slopes","Well drained","D",1.25,60.9,7.9]
["NE033","Cheyenne","Canyon-Bayard complex, 6 to 20 percent slopes","Well drained","A",1.25,62.5,7.9]
["NE033","Cheyenne","Canyon-Rock outcrop complex, 12 to 60 percent slopes","Well drained","D",0.625,30.45,3.95]
["NE033","Cheyenne","Chappell-Alice-Broadwater complex, 0 to 3 percent slopes","Well drained","A",0.75,66.599999999999994,7.2]
["NE033","Cheyenne","Chappell-Bayard-Broadwater complex, 0 to 2 percent slopes","Well drained","A",0.75,68,7.2]
["NE033","Cheyenne","Creighton very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE033","Cheyenne","Creighton very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE033","Cheyenne","Dix gravelly loam, 3 to 9 percent slopes","Excessively drained","B",0.75,83.2,7.5]
["NE033","Cheyenne","Dix gravelly loam, 9 to 50 percent slopes","Excessively drained","B",1.125,68.800000000000011,7.25]
["NE033","Cheyenne","Duroc loam, 0 to 1 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE033","Cheyenne","Duroc loam, 1 to 3 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE033","Cheyenne","Duroc loam, terrace, gravelly substratum, 0 to 1 percent slopes","Well drained","B",1.5,39.200000000000003,7.6999999999999993]
["NE033","Cheyenne","Duroc silt loam, terrace, 0 to 1 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE033","Cheyenne","Dwyer loamy fine sand, 9 to 17 percent slopes","Excessively drained","A",1.125,78.900000000000006,7.7]
["NE033","Cheyenne","Eckley and Altvan soils, 9 to 50 percent slopes","Well drained","C",1,69,7.2]
["NE033","Cheyenne","Epping-Mitchell complex, 3 to 20 percent slopes","Well drained","D",0.75,44.3,7.9]
["NE033","Cheyenne","Glenberg fine sandy loam, 0 to 2 percent slopes","Well drained","A",1,55.699999999999996,7.9]
["NE033","Cheyenne","Goshen silt loam, 0 to 1 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE033","Cheyenne","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE033","Cheyenne","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE033","Cheyenne","Johnstown loam, 0 to 2 percent slopes","Well drained","B",0.75,34.150000000000006,7.1]
["NE033","Cheyenne","Keith loam, 0 to 1 percent slopes","Well drained","B",0.75,25,7]
["NE033","Cheyenne","Keith loam, 1 to 3 percent slopes","Well drained","B",0.75,25,7]
["NE033","Cheyenne","Keith loam, 3 to 6 percent slopes","Well drained","B",0.75,25,7]
["NE033","Cheyenne","Kuma loam, 0 to 1 percent slopes","Well drained","C",2,36.9,7.5]
["NE033","Cheyenne","Las Animas loam, channeled, frequently flooded","Poorly drained","B/D",0.75,67.150000000000006,7.9]
["NE033","Cheyenne","Las Animas loam, frequently flooded","Poorly drained","B/D",1,52.8,7.9]
["NE033","Cheyenne","Las loam, occasionally flooded","Somewhat poorly drained","C",0.5,38.400000000000006,7.9]
["NE033","Cheyenne","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",1.375,27.75,7.25]
["NE033","Cheyenne","McCook very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.375,59.6,7.7]
["NE033","Cheyenne","Mitchell very fine sandy loam, 3 to 6 percent slopes","Well drained","B",1,51.1,7.9]
["NE033","Cheyenne","Mitchell very fine sandy loam, 6 to 9 percent slopes","Well drained","B",1,51.1,7.9]
["NE033","Cheyenne","Mitchell very fine sandy loam, 9 to 20 percent slopes","Well drained","B",1,51.1,7.9]
["NE033","Cheyenne","Ralton loam, very rarely flooded","Moderately well drained","B",0.5,41.7,7.9]
["NE033","Cheyenne","Rock outcrop-Epping complex, 9 to 60 percent slopes","Well drained","D",0.375,22.15,3.95]
["NE033","Cheyenne","Rosebud loam, 0 to 1 percent slopes","Well drained","C",0.75,39.4,7.35]
["NE033","Cheyenne","Rosebud loam, 1 to 3 percent slopes","Well drained","C",0.75,39.4,7.35]
["NE033","Cheyenne","Rosebud loam, 3 to 6 percent slopes","Well drained","C",0.75,39.4,7.35]
["NE033","Cheyenne","Rosebud-Canyon complex, 3 to 9 percent slopes","Well drained","D",0.75,44.3,7.5]
["NE033","Cheyenne","Rosebud-Canyon loams, 1 to 3 percent slopes","Well drained","D",0.75,37,7.2]
["NE033","Cheyenne","Rosebud-Hemingford loams, 0 to 1 percent slopes","Well drained","C",0.75,38,7.2]
["NE033","Cheyenne","Sarben loamy very fine sand, 3 to 9 percent slopes","Well drained","A",0.25,84,7.2]
["NE033","Cheyenne","Satanta loam, gravelly substratum, 0 to 1 percent slopes","Well drained","C",1,43,7.5500000000000007]
["NE033","Cheyenne","Satanta loam, gravelly substratum, 1 to 3 percent slopes","Well drained","C",1,43,7.5500000000000007]
["NE033","Cheyenne","Satanta loam, gravelly substratum, 3 to 6 percent slopes","Well drained","C",1,43,7.5500000000000007]
["NE033","Cheyenne","Satanta-Altvan complex, 3 to 6 percent slopes","Well drained","B",1,59.3,7.5]
["NE033","Cheyenne","Satanta-Johnstown-Altvan loams, 1 to 3 percent slopes","Well drained","C",1,42.1,7.35]
["NE033","Cheyenne","Sidney loam, 3 to 6 percent slopes","Well drained","B",0.75,45,7.9]
["NE033","Cheyenne","Sidney-Canyon complex, 3 to 9 percent slopes","Well drained","D",0.75,44.3,7.9]
["NE033","Cheyenne","Sidney-Canyon loams, 3 to 9 percent slopes","Well drained","D",0.75,43.2,7.5500000000000007]
["NE033","Cheyenne","Tassel-Ashollow-Rock outcrop complex, 20 to 60 percent slopes","Well drained","B",0.75,63.3,7.9]
["NE033","Cheyenne","Tassel-Blanche complex, 9 to 30 percent slopes","Well drained","B",0.25,62.5,7.75]
["NE033","Cheyenne","Tassel-Blanche sandy loams, 3 to 9 percent slopes","Well drained","B",0.25,62.5,7.6]
["NE033","Cheyenne","Tassel-Busher complex, 3 to 30 percent slopes","Well drained","A",1,64.05,7.25]
["NE033","Cheyenne","Tassel-Busher-Rock outcrop complex, 9 to 60 percent slopes","Well drained","A",0.75,63.5,7]
["NE033","Cheyenne","Ulysses loam, 1 to 3 percent slopes","Well drained","B",1.5,33.299999999999997,7.9]
["NE033","Cheyenne","Ulysses loam, 3 to 6 percent slopes","Well drained","B",1.5,33.299999999999997,7.9]
["NE033","Cheyenne","Valent loamy fine sand, 6 to 9 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE035","Clay",null,"",""]
["NE035","Clay","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE035","Clay","Cass fine sandy loam, overwash, occasionally flooded","Well drained","A",1.25,67.599999999999994,7.3]
["NE035","Clay","Cass loam, occasionally flooded","Well drained","C",0.75,62,7.3]
["NE035","Clay","Cass silt loam, occasionally flooded","Well drained","B",0.75,85.4,7.3]
["NE035","Clay","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE035","Clay","Crete silt loam, 1 to 3 percent slopes","Moderately well drained","C",1.625,17.149999999999999,6.25]
["NE035","Clay","Crete silt loam, thick solum, 0 to 1 percent slopes","Moderately well drained","C",1.625,18.149999999999999,6.25]
["NE035","Clay","Fillmore silt loam, drained, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,15,7.1]
["NE035","Clay","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE035","Clay","Geary silt loam, 11 to 30 percent slopes","Somewhat excessively drained","C",1.25,7.4,6.7]
["NE035","Clay","Geary silt loam, 3 to 7 percent slopes","Well drained","C",1.25,6.9,6.7]
["NE035","Clay","Geary silt loam, 7 to 11 percent slopes","Well drained","C",1.25,6.9,6.7]
["NE035","Clay","Geary silty clay loam, 11 to 17 percent slopes, eroded","Somewhat excessively drained","C",0.25,6.7,7]
["NE035","Clay","Geary silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE035","Clay","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE035","Clay","Geary-Hobbs silt loams, 0 to 30 percent slopes","Well drained","C",0.75,9.5,7]
["NE035","Clay","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,7.8,7]
["NE035","Clay","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE035","Clay","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE035","Clay","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",0.5,18.5,6.5]
["NE035","Clay","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE035","Clay","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE035","Clay","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE035","Clay","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE035","Clay","Holder silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.1,7]
["NE035","Clay","Holder silt loam, 7 to 11 percent slopes","Well drained","C",0.75,9.1,7]
["NE035","Clay","Holder silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1,9.1,7]
["NE035","Clay","Holder silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.25,9.1,7]
["NE035","Clay","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",1.25,7,7.2]
["NE035","Clay","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE035","Clay","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE035","Clay","Massie silty clay loam, frequently ponded","Very poorly drained","D",1.25,6,6.4]
["NE035","Clay","Meadin sandy loam, 2 to 30 percent slopes","Excessively drained","B",0.75,86.3,6.2]
["NE035","Clay","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE035","Clay","Uly silt loam, 11 to 17 percent slopes, eroded","Somewhat excessively drained","B",0.75,9.5,7]
["NE035","Clay","Uly silt loam, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE035","Clay","Uly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,10.35,7]
["NE037","Colfax",null,"",""]
["NE037","Colfax","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",3.25,8.4499999999999993,7.1]
["NE037","Colfax","Alcester silty clay loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE037","Colfax","Alda fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,66,7.5]
["NE037","Colfax","Alda loam, occasionally flooded","Somewhat poorly drained","C",0.75,66,7.5]
["NE037","Colfax","Barney loam, frequently flooded","Poorly drained","B/D",0.25,80,7.5]
["NE037","Colfax","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE037","Colfax","Belfore silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",1.125,19.25,6.6]
["NE037","Colfax","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,66.099999999999994,6.7]
["NE037","Colfax","Blendon loam, 2 to 6 percent slopes","Well drained","B",1.5,65.400000000000006,6.7]
["NE037","Colfax","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.599999999999994,7.5]
["NE037","Colfax","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE037","Colfax","Coleridge silt loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE037","Colfax","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE037","Colfax","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE037","Colfax","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE037","Colfax","Crofton silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE037","Colfax","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE037","Colfax","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE037","Colfax","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE037","Colfax","Crofton-Nora complex, 2 to 6 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE037","Colfax","Eudora loam, rarely flooded","Moderately well drained","B",1.5,61,7.3]
["NE037","Colfax","Fillmore silt loam, frequently ponded","Poorly drained","D",1.625,15.75,6.1]
["NE037","Colfax","Fillmore silt loam, occasionally ponded","Somewhat poorly drained","D",1.125,11.100000000000001,7.1]
["NE037","Colfax","Gayville variant silty clay loam, rarely flooded","Moderately well drained","D",2,17.3,8.1999999999999993]
["NE037","Colfax","Geary silty clay loam, 11 to 17 percent slopes, eroded","Well drained","B",2,7.4,6.1]
["NE037","Colfax","Geary silty clay loam, 11 to 30 percent slopes","Well drained","B",2,7.4,6.1]
["NE037","Colfax","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE037","Colfax","Geary variant silty clay loam, 11 to 30 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE037","Colfax","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.5,79.849999999999994,7.35]
["NE037","Colfax","Hall silty clay loam, sandy substratum, 0 to 1 percent slopes","Well drained","C",1.5,6.9,6.3]
["NE037","Colfax","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,10.4,7.25]
["NE037","Colfax","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,10.4,7.25]
["NE037","Colfax","Inavale loamy fine sand, 3 to 11 percent slopes, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE037","Colfax","Inavale loamy fine sand, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE037","Colfax","Inavale loamy fine sand, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE037","Colfax","Kezan silt loam, frequently flooded","Poorly drained","C",1.875,9.0500000000000007,7.2]
["NE037","Colfax","Lawet silt loam, occasionally flooded","Somewhat poorly drained","B/D",1.25,54.4,7.9]
["NE037","Colfax","Lawet silt loam, rarely flooded","Somewhat poorly drained","B/D",1.25,54.4,7.9]
["NE037","Colfax","Lawet silty clay loam, occasionally flooded","Somewhat poorly drained","B/D",1.25,54.4,7.9]
["NE037","Colfax","Luton silty clay, occasionally flooded","Poorly drained","D",0.5,5.3,7.2]
["NE037","Colfax","Moody silty clay loam, 0 to 1 percent slopes","Well drained","C",3,6.9,6.5]
["NE037","Colfax","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE037","Colfax","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE037","Colfax","Moody silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE037","Colfax","Moody silty clay loam, 6 to 11 percent slopes","Well drained","C",3,6.9,6.5]
["NE037","Colfax","Moody silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE037","Colfax","Moody silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE037","Colfax","Moody-Thurman complex, 2 to 6 percent slopes, eroded","Well drained","C",1,47.15,6.5]
["NE037","Colfax","Napa-Luton complex, occasionally flooded","Poorly drained","D",1.75,5.3,7.5]
["NE037","Colfax","Nora silty clay loam, 11 to 17 percent slopes","Well drained","C",0.75,8.9,7]
["NE037","Colfax","Nora silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,8.9,7]
["NE037","Colfax","Nora silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE037","Colfax","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE037","Colfax","Nora variant silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE037","Colfax","Nora variant silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE037","Colfax","Nora-Crofton complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE037","Colfax","Nora-Crofton complex, 2 to 6 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE037","Colfax","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE037","Colfax","Ord fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE037","Colfax","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,63.2,7.5]
["NE037","Colfax","Platte-Inavale complex, channeled, frequently flooded","Excessively drained","A",0.25,87.3,7.5]
["NE037","Colfax","Shell silt loam, clayey substratum, occasionally flooded","Moderately well drained","C",0.75,11.2,7]
["NE037","Colfax","Shell silt loam, occasionally flooded","Well drained","B",1.625,10.199999999999999,6.75]
["NE037","Colfax","Steinauer clay loam, 11 to 30 percent slopes, eroded","Well drained","C",0.75,33.6,7.9]
["NE037","Colfax","Steinauer clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,33.6,7.9]
["NE037","Colfax","Thurman-Moody complex, 2 to 6 percent slopes, eroded","Well drained","C",1,47.000000000000007,6.5]
["NE037","Colfax","Thurman-Moody complex, 6 to 11 percent slopes, eroded","Well drained","C",1,47.000000000000007,6.5]
["NE037","Colfax","Wann loam, occasionally flooded","Somewhat poorly drained","C",0.75,66.2,8.1999999999999993]
["NE037","Colfax","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.75,6.6]
["NE039","Cuming",null,"",""]
["NE039","Cuming","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",3.25,8.4499999999999993,7.1]
["NE039","Cuming","Alcester silty clay loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE039","Cuming","Barney sandy loam, frequently flooded","Very poorly drained","A/D",1.125,78.8,7.35]
["NE039","Cuming","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE039","Cuming","Belfore silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",0.75,20,6.5]
["NE039","Cuming","Belfore-Moody silty clay loams, 1 to 3 percent slopes","Well drained","C",1.875,10.1,6.5]
["NE039","Cuming","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE039","Cuming","Calco silty clay loam, occasionally flooded","Somewhat poorly drained","B/D",4,6.9,7.9]
["NE039","Cuming","Calco silty clay loam, wet, occasionally flooded","Poorly drained","B/D",4,6.9,7.9]
["NE039","Cuming","Cass fine sandy loam, occasionally flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE039","Cuming","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE039","Cuming","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE039","Cuming","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE039","Cuming","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE039","Cuming","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE039","Cuming","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE039","Cuming","Fluvaquents, frequently flooded","Very poorly drained","A/D",5,23.5,7.5]
["NE039","Cuming","Gibbon loam, occasionally flooded","Somewhat poorly drained","C",0.75,41.5,7.9]
["NE039","Cuming","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.4,7.9]
["NE039","Cuming","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE039","Cuming","Inavale loamy fine sand, 3 to 6 percent slopes, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE039","Cuming","Inavale loamy fine sand, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE039","Cuming","Inavale-Boel complex, channeled, occasionally flooded","Somewhat poorly drained","C",0.25,92.2,7.5]
["NE039","Cuming","Judson silt loam, 2 to 6 percent slopes","Well drained","C",2.5,7,6.5]
["NE039","Cuming","Judson silty clay loam, 2 to 6 percent slopes","Well drained","C",2.5,7,6.5]
["NE039","Cuming","Kennebec silt loam, occasionally flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE039","Cuming","Kennebec silt loam, overwash, occasionally flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE039","Cuming","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE039","Cuming","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE039","Cuming","Lamo-Saltine complex, occasionally flooded","Somewhat poorly drained","C",0.5,6.9,8.5]
["NE039","Cuming","Leisy fine sandy loam, 2 to 6 percent slopes","Well drained","C",0.75,39.200000000000003,6.5]
["NE039","Cuming","Leisy fine sandy loam, 6 to 11 percent slopes","Well drained","C",0.75,39.200000000000003,6.5]
["NE039","Cuming","Leisy loam, 2 to 6 percent slopes","Well drained","C",0.75,39.200000000000003,6.5]
["NE039","Cuming","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.5,11.45,7.5]
["NE039","Cuming","Loretto fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE039","Cuming","Moody silty clay loam, 0 to 1 percent slopes","Well drained","C",3,6.9,6.5]
["NE039","Cuming","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE039","Cuming","Moody silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE039","Cuming","Moody silty clay loam, 6 to 11 percent slopes","Well drained","C",3,6.9,6.5]
["NE039","Cuming","Moody silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE039","Cuming","Moody silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE039","Cuming","Nora silt loam, 11 to 17 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE039","Cuming","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE039","Cuming","Nora silty clay loam, 11 to 17 percent slopes","Well drained","C",0.75,8.9,7]
["NE039","Cuming","Nora silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.75,8.9,7]
["NE039","Cuming","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE039","Cuming","Nora silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,8.9,7]
["NE039","Cuming","Nora variant silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE039","Cuming","Nora variant silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE039","Cuming","Nora-Crofton complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE039","Cuming","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE039","Cuming","Nora-Moody silty clay loams, 6 to 11 percent slopes","Well drained","C",1.875,7,6.85]
["NE039","Cuming","Obert silt loam, frequently ponded","Very poorly drained","C/D",2.25,9.3000000000000007,7.9]
["NE039","Cuming","Obert silty clay loam, frequently ponded","Very poorly drained","C/D",1.875,7.1,7.9]
["NE039","Cuming","Platte-Inavale complex, channeled, occasionally flooded","Excessively drained","A",0.25,89.6,7.5]
["NE039","Cuming","Saltine-Gibbon complex, occasionally flooded","Somewhat poorly drained","C",0.75,7,8.5]
["NE039","Cuming","Shell silt loam, occasionally flooded","Well drained","B",1.625,10.199999999999999,6.75]
["NE039","Cuming","Shell silty clay loam, 0 to 1 percent slopes","Well drained","C",0.75,9.1,6.5]
["NE039","Cuming","Thurman and Valentine loamy fine sands, 6 to 11 percent slopes","Somewhat excessively drained","A",0.5,86.1,6.5]
["NE039","Cuming","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE039","Cuming","Thurman-Valentine loamy fine sands, 0 to 2 percent slopes","Somewhat excessively drained","A",0.5,86.1,6.5]
["NE039","Cuming","Thurman-Valentine loamy fine sands, 2 to 6 percent slopes","Somewhat excessively drained","A",0.5,86.1,6.5]
["NE039","Cuming","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,87.3,6.5]
["NE039","Cuming","Wann loam, occasionally flooded","Somewhat poorly drained","B/D",0.75,66.2,8.1999999999999993]
["NE039","Cuming","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.75,6.6]
["NE039","Cuming","Zook silty clay, occasionally flooded","Poorly drained","C/D",4.5,7.85,6.6]
["NE041","Custer",null,"",""]
["NE041","Custer","Almeria loamy fine sand, channeled, frequently flooded","Very poorly drained","A/D",1.25,75.349999999999994,6.9]
["NE041","Custer","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE041","Custer","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE041","Custer","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE041","Custer","Anselmo fine sandy loam, terrace, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE041","Custer","Anselmo loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE041","Custer","Anselmo very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,66.099999999999994,7]
["NE041","Custer","Anselmo very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,66.099999999999994,7]
["NE041","Custer","Barney fine sandy loam, frequently flooded","Poorly drained","A/D",0.25,63.5,7.5]
["NE041","Custer","Barney loam, channeled, frequently flooded","Very poorly drained","B/D",1.625,69.5,7.35]
["NE041","Custer","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.599999999999994,7.5]
["NE041","Custer","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE041","Custer","Boel soils, channeled, frequently flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE041","Custer","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE041","Custer","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE041","Custer","Coly silt loam, 11 to 30 percent slopes","Well drained","B",1.125,8,7.9]
["NE041","Custer","Coly silt loam, 6 to 11 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE041","Custer","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE041","Custer","Coly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE041","Custer","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE041","Custer","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE041","Custer","Coly-Uly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE041","Custer","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE041","Custer","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7.3]
["NE041","Custer","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE041","Custer","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7.3]
["NE041","Custer","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE041","Custer","Els fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.7]
["NE041","Custer","Els-Ipage complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,95.15,6.35]
["NE041","Custer","Fillmore silt loam, frequently ponded","Somewhat poorly drained","C/D",1.125,12.649999999999999,7.1]
["NE041","Custer","Fillmore variant silt loam, frequently ponded","Somewhat poorly drained","B/D",1.375,10.1,7]
["NE041","Custer","Fluvaquents, frequently flooded","Very poorly drained","A/D",2.5,18.95,3.75]
["NE041","Custer","Gannett and Loup loams, occasionally flooded","Poorly drained","B/D",0.75,66.099999999999994,6.7]
["NE041","Custer","Gannett loam, 0 to 1 percent slopes","Very poorly drained","B/D",6.625,67.349999999999994,6.6]
["NE041","Custer","Gates silt loam, 1 to 3 percent slopes","Well drained","B",0.5,13.9,7.5]
["NE041","Custer","Gates silt loam, 11 to 30 percent slopes","Well drained","B",0.5,13.9,7.5]
["NE041","Custer","Gates silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.5,13.9,7.5]
["NE041","Custer","Gates silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.5,13.9,7.5]
["NE041","Custer","Gates very fine sandy loam, 11 to 17 percent slopes","Well drained","B",0.5,58.6,7.5]
["NE041","Custer","Gates very fine sandy loam, 17 to 30 percent slopes","Well drained","B",0.5,58.6,7.5]
["NE041","Custer","Gates very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.5,58.6,7.5]
["NE041","Custer","Gates very fine sandy loam, 6 to 11 percent slopes, eroded","Well drained","B",0.5,58.6,7.5]
["NE041","Custer","Gates-Hersh complex, 20 to 60 percent slopes","Well drained","B",0.625,62.849999999999994,7.35]
["NE041","Custer","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE041","Custer","Graybert very fine sandy loam, 0 to 1 percent slopes","Well drained","B",2.25,36,7.75]
["NE041","Custer","Graybert very fine sandy loam, 1 to 3 percent slopes","Well drained","B",2.25,36,7.75]
["NE041","Custer","Graybert very fine sandy loam, 3 to 6 percent slopes","Well drained","B",2.25,36,7.75]
["NE041","Custer","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.125,10.4,7.1]
["NE041","Custer","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.125,10.4,7.1]
["NE041","Custer","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE041","Custer","Hersh fine sandy loam, 11 to 17 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE041","Custer","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE041","Custer","Hersh fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE041","Custer","Hersh loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.75,84,6.7]
["NE041","Custer","Hersh-Valentine complex, 11 to 24 percent slopes","Well drained","A",0.5,77.099999999999994,6.6]
["NE041","Custer","Hersh-Valentine complex, 15 to 30 percent slopes","Well drained","A",0.5,77.099999999999994,6.6]
["NE041","Custer","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE041","Custer","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE041","Custer","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",1.25,9.4,7.2]
["NE041","Custer","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",1.25,9.4,7.2]
["NE041","Custer","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.875,9.4,6.85]
["NE041","Custer","Holdrege silt loam, 7 to 11 percent slopes","Well drained","C",1.25,9.4,7.2]
["NE041","Custer","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,6.8,7.2]
["NE041","Custer","Holdrege silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.75,6.8,7.2]
["NE041","Custer","Hord fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE041","Custer","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE041","Custer","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE041","Custer","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE041","Custer","Inavale loamy fine sand, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE041","Custer","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE041","Custer","Ipage sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,96,6.5]
["NE041","Custer","Kenesaw very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,60.3,7.5]
["NE041","Custer","Kenesaw very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,60.3,7.5]
["NE041","Custer","Ord fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE041","Custer","Ord very fine sandy loam, occasionally flooded","Somewhat poorly drained","C",0.75,63.3,7.5]
["NE041","Custer","Ovina loam, 0 to 1 percent slopes","Somewhat poorly drained","C",1.75,56.25,7.5]
["NE041","Custer","Rusco silty clay loam, 0 to 1 percent slopes","Moderately well drained","C/D",0.75,6.8,7.5]
["NE041","Custer","Scott silty clay loam, frequently ponded","Poorly drained","D",1.125,19.350000000000001,7.1]
["NE041","Custer","Uly and Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE041","Custer","Uly silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.3,7.9]
["NE041","Custer","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE041","Custer","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE041","Custer","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE041","Custer","Uly-Holdrege silt loams, 6 to 11 percent slopes","Well drained","C",0.75,13.6,7.2]
["NE041","Custer","Uly-Holdrege-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","C",1,9.25,7.1]
["NE041","Custer","Uly-Sully silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.5,40.75,7.9]
["NE041","Custer","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE041","Custer","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE041","Custer","Valentine fine sand, rolling","Excessively drained","A",0.25,96.3,6.5]
["NE041","Custer","Valentine fine sand, rolling and hilly","Excessively drained","A",0.25,96.3,6.5]
["NE041","Custer","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE041","Custer","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE041","Custer","Valentine loamy fine sand, rolling","Excessively drained","A",0.25,87.3,6.5]
["NE043","Dakota",null,"",""]
["NE043","Dakota","Albaton silty clay loam, occasionally flooded","Poorly drained","D",1.5,10.6,7.9]
["NE043","Dakota","Albaton silty clay, frequently flooded","Very poorly drained","D",2.5,2.2999999999999998,7.9]
["NE043","Dakota","Albaton silty clay, occasionally flooded","Poorly drained","D",1.5,3.9,7.9]
["NE043","Dakota","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE043","Dakota","Alcester silt loam, 6 to 11 percent slopes","Well drained","B",2.5,7.4,7]
["NE043","Dakota","Aowa silt loam, occasionally flooded","Well drained","B",1.625,21.15,7.9]
["NE043","Dakota","Barney fine sandy loam, occasionally flooded","Poorly drained","A/D",1.125,77.25,7.35]
["NE043","Dakota","Blake silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.5,7.1,8.1999999999999993]
["NE043","Dakota","Blencoe silty clay, rarely flooded","Somewhat poorly drained","D",2,6.8,7.2]
["NE043","Dakota","Blyburg silt loam, 2 to 6 percent slopes, rarely flooded","Well drained","B",0.875,14,7.75]
["NE043","Dakota","Blyburg silt loam, rarely flooded","Well drained","B",0.875,14,7.75]
["NE043","Dakota","Blyburg silty clay loam, rarely flooded","Well drained","C",1.125,10.45,7.75]
["NE043","Dakota","Blyburg silty clay, overwash, rarely flooded","Well drained","D",0.875,9.75,8.0500000000000007]
["NE043","Dakota","Burchard clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.75,35.4,6.7]
["NE043","Dakota","Calco silt loam, overwash, occasionally flooded","Poorly drained","C/D",4,7.1,7.9]
["NE043","Dakota","Calco silty clay loam, occasionally flooded","Poorly drained","C/D",4,6.9,7.9]
["NE043","Dakota","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE043","Dakota","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE043","Dakota","Crofton silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE043","Dakota","Crofton silt loam, 30 to 60 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE043","Dakota","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE043","Dakota","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE043","Dakota","Fluvaquents, frequently flooded","Very poorly drained","A/D",5,23.5,7.5]
["NE043","Dakota","Forney silt loam, overwash, rarely flooded","Poorly drained","D",2,13.5,7.9]
["NE043","Dakota","Forney silty clay, rarely flooded","Poorly drained","D",2.25,3.9,7.45]
["NE043","Dakota","Forney soils, swales, rarely flooded","Poorly drained","D",2.25,3.9,7.45]
["NE043","Dakota","Grable very fine sandy loam, occasionally flooded","Well drained","A",0.5,59,7.9]
["NE043","Dakota","Grable very fine sandy loam, rarely flooded","Well drained","B",0.5,59,7.9]
["NE043","Dakota","Gullied land-Ida complex, 30 to 60 percent slopes","Well drained","B",0.5,10.35,7.7]
["NE043","Dakota","Haynie silt loam, occasionally flooded","Well drained","B",1.25,12.600000000000001,7.9]
["NE043","Dakota","Haynie silt loam, rarely flooded","Well drained","B",1.25,12.600000000000001,7.7]
["NE043","Dakota","Hobbs silt loam, frequently flooded","Well drained","B",1.875,11.3,7]
["NE043","Dakota","Ida silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.375,11.2,7.7]
["NE043","Dakota","Ida silt loam, 17 to 30 percent slopes","Well drained","B",1.375,11.2,7.7]
["NE043","Dakota","Ida silt loam, 17 to 30 percent slopes, eroded","Well drained","B",1.375,11.2,7.7]
["NE043","Dakota","Ida soils, 30 to 60 percent slopes","Well drained","B",1.375,11.2,7.7]
["NE043","Dakota","Judson silty clay loam, 0 to 2 percent slopes","Well drained","C",2.5,7,7]
["NE043","Dakota","Judson silty clay loam, 2 to 6 percent slopes","Well drained","C",2.5,7,7]
["NE043","Dakota","Kennebec silt loam, overwash, occasionally flooded","Moderately well drained","B",3.5,9.1499999999999986,7.4]
["NE043","Dakota","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,9.1499999999999986,7.4]
["NE043","Dakota","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,8.1999999999999993]
["NE043","Dakota","Luton silty clay, thin surface, rarely flooded","Poorly drained","D",0.5,5.3,7.9]
["NE043","Dakota","Modale silt loam, occasionally flooded","Somewhat poorly drained","C",1.375,8.35,8.0500000000000007]
["NE043","Dakota","Monona silt loam, 11 to 17 percent slopes","Well drained","B",1.25,9.4,7.4]
["NE043","Dakota","Monona silt loam, 17 to 30 percent slopes","Well drained","B",1.25,9.4,7.4]
["NE043","Dakota","Monona silt loam, 6 to 11 percent slopes","Well drained","B",1.25,9.4,7.4]
["NE043","Dakota","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.6]
["NE043","Dakota","Moody silty clay loam, 6 to 11 percent slopes","Well drained","C",3,6.9,6.6]
["NE043","Dakota","Moody silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",3,6.9,6.6]
["NE043","Dakota","Moody-Nora silty clay loams, 11 to 17 percent slopes","Well drained","C",1.875,7.9,6.85]
["NE043","Dakota","Napier silt loam, 11 to 17 percent slopes","Well drained","B",2.5,9.4,7]
["NE043","Dakota","Napier silt loam, 2 to 6 percent slopes","Well drained","B",2.5,9.4,7]
["NE043","Dakota","Napier silt loam, 6 to 11 percent slopes","Well drained","B",2.5,9.4,7]
["NE043","Dakota","Napier-Gullied land complex, 2 to 11 percent slopes","Well drained","B",1.5,9.4,7.3]
["NE043","Dakota","Nora silt loam, 11 to 17 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE043","Dakota","Nora silt loam, 11 to 17 percent slopes, eroded","Well drained","C",1.25,9.1,6.6]
["NE043","Dakota","Nora silt loam, 17 to 30 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE043","Dakota","Nora silt loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,9.1,6.6]
["NE043","Dakota","Nora silt loam, 6 to 11 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE043","Dakota","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,9.1,6.6]
["NE043","Dakota","Nora silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,8.9,7]
["NE043","Dakota","Nora silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE043","Dakota","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE043","Dakota","Nora silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE043","Dakota","Nora variant silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE043","Dakota","Nora-Alcester silt loams, 11 to 17 percent slopes","Well drained","B",1.625,9.1000000000000014,7]
["NE043","Dakota","Omadi silt loam, rarely flooded","Moderately well drained","B",1.125,10.45,7.6]
["NE043","Dakota","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE043","Dakota","Owego silty clay, occasionally flooded","Poorly drained","D",0.5,7.2,7.9]
["NE043","Dakota","Percival silty clay, occasionally flooded","Somewhat poorly drained","D",1,5.3,7.9]
["NE043","Dakota","Sansarc-Nora complex, 11 to 30 percent slopes","Well drained","B",0.65,9.3500000000000014,7.5]
["NE043","Dakota","Sarpy fine sand, 3 to 11 percent slopes","Excessively drained","A",0.5,95.9,8]
["NE043","Dakota","Sarpy loamy fine sand, occasionally flooded","Excessively drained","A",0.5,87.9,8]
["NE043","Dakota","Sarpy silty clay, overwash, occasionally flooded","Excessively drained","D",0.5,42.6,8]
["NE043","Dakota","Waubonsie very fine sandy loam, loamy substratum, occasionally flooded","Moderately well drained","B",0.5,61.3,8.1999999999999993]
["NE045","Dawes",null,"",""]
["NE045","Dawes","Alliance loam, 1 to 3 percent slopes","Well drained","B",0.75,11.4,7.2]
["NE045","Dawes","Alliance loam, 3 to 6 percent slopes","Well drained","B",0.75,11.4,7.2]
["NE045","Dawes","Alliance silt loam, 1 to 3 percent slopes","Well drained","B",0.75,12.5,7.35]
["NE045","Dawes","Alliance silt loam, 3 to 9 percent slopes","Well drained","B",0.75,12.5,7.35]
["NE045","Dawes","Alliance silt loam, 3 to 9 percent slopes, eroded","Well drained","B",0.75,12.5,7.35]
["NE045","Dawes","Bankard fine sand, channeled, frequently flooded","Somewhat excessively drained","A",1,94.5,7.9]
["NE045","Dawes","Bankard loamy coarse sand, frequently flooded","Somewhat excessively drained","A",1,80.900000000000006,7.9]
["NE045","Dawes","Bankard loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.75,87.3,7.9]
["NE045","Dawes","Bankard loamy fine sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,78.599999999999994,7.9]
["NE045","Dawes","Bankard loamy fine sand, frequently flooded","Somewhat excessively drained","A",0.25,89.699999999999989,7.9]
["NE045","Dawes","Bankard loamy fine sand, occasionally flooded","Somewhat excessively drained","A",0.75,78.599999999999994,7.9]
["NE045","Dawes","Bankard loamy fine sand, wet variant","Somewhat poorly drained","A",0.625,82.6,7.9]
["NE045","Dawes","Bankard very fine sandy loam, 0 to 3 percent slopes","Somewhat excessively drained","A",1.125,76.95,7.9]
["NE045","Dawes","Bigwinder fine sandy loam, frequently flooded","Poorly drained","C",2,66.8,7.9]
["NE045","Dawes","Bolent loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.5,75.349999999999994,7.7]
["NE045","Dawes","Bridget loam, 0 to 1 percent slopes","Well drained","B",1.375,52.45,7.5500000000000007]
["NE045","Dawes","Bridget silt loam, 0 to 1 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE045","Dawes","Bridget silt loam, 1 to 3 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE045","Dawes","Bridget silt loam, 3 to 6 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE045","Dawes","Bridget silt loam, 9 to 20 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE045","Dawes","Bridget very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.375,61.7,7.5500000000000007]
["NE045","Dawes","Bridget very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.375,61.7,7.5500000000000007]
["NE045","Dawes","Bridget very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE045","Dawes","Bridget very fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE045","Dawes","Buffington silty clay, 0 to 1 percent slopes","Well drained","C",0.25,22.1,7.9]
["NE045","Dawes","Bufton clay loam, 1 to 3 percent slopes","Well drained","C",0.75,29,8.1999999999999993]
["NE045","Dawes","Bufton clay loam, 3 to 9 percent slopes","Well drained","C",0.75,29,8.1999999999999993]
["NE045","Dawes","Bufton silty clay loam, 0 to 1 percent slopes","Well drained","C",0.75,17.3,8.1999999999999993]
["NE045","Dawes","Bufton silty clay loam, 1 to 3 percent slopes","Well drained","C",0.75,17.3,8.1999999999999993]
["NE045","Dawes","Bufton silty clay loam, 3 to 9 percent slopes","Well drained","C",0.75,17.3,8.1999999999999993]
["NE045","Dawes","Bufton silty clay loam, 9 to 20 percent slopes","Well drained","C",0.75,17.3,8.1999999999999993]
["NE045","Dawes","Bufton-Hisle complex, 0 to 9 percent slopes","Well drained","C",1,17.3,7.85]
["NE045","Dawes","Busher and tassel loamy very fine sands, 6 to 20 percent slopes","Well drained","A",1,72.05,7.25]
["NE045","Dawes","Busher loamy very fine sand, 1 to 6 percent slopes","Well drained","A",0.75,79.5,7]
["NE045","Dawes","Busher loamy very fine sand, 1 to 6 percent slopes, eroded","Well drained","A",0.75,79.5,7]
["NE045","Dawes","Busher loamy very fine sand, 3 to 6 percent slopes","Well drained","A",0.75,79.5,7]
["NE045","Dawes","Busher loamy very fine sand, 6 to 9 percent slopes","Well drained","A",0.75,79.5,7]
["NE045","Dawes","Busher loamy very fine sand, 6 to 9 percent slopes, eroded","Well drained","A",0.75,79.5,7]
["NE045","Dawes","Busher loamy very fine sand, 9 to 20 percent slopes","Well drained","A",0.75,79.5,7]
["NE045","Dawes","Busher-Jayem loamy very fine sands, 0 to 3 percent slopes","Well drained","A",0.52500000000000002,79.75,7.2]
["NE045","Dawes","Busher-Jayem loamy very fine sands, 3 to 6 percent slopes","Well drained","A",0.52500000000000002,80,7.2]
["NE045","Dawes","Busher-Jayem loamy very fine sands, 6 to 9 percent slopes","Well drained","A",0.52500000000000002,80,7.2]
["NE045","Dawes","Busher-Tassel complex, 6 to 30 percent slopes","Well drained","A",1,72.05,7.25]
["NE045","Dawes","Busher-Tassel loamy very fine sands, 6 to 30 percent slopes","Well drained","A",1,79.5,7.25]
["NE045","Dawes","Canyon soils, 3 to 30 percent slopes","Well drained","D",1.25,44.3,7.9]
["NE045","Dawes","Canyon soils, 30 to 50 percent slopes","Well drained","D",1.25,44.3,7.9]
["NE045","Dawes","Craft loam, channeled, frequently flooded","Well drained","B",0.75,66.849999999999994,7.9]
["NE045","Dawes","Duroc loam, 1 to 3 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE045","Dawes","Duroc very fine sandy loam, 1 to 3 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE045","Dawes","Els fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",1,94.050000000000011,7.9]
["NE045","Dawes","Enning and Minnequa silty clay loams, 6 to 20 percent slopes","Well drained","D",0.375,7.9,7.9]
["NE045","Dawes","Enning-Minnequa complex, 6 to 20 percent slopes","Well drained","D",0.375,6.8,7.7]
["NE045","Dawes","Enning-Rock outcrop complex, 11 to 40 percent slopes","Well drained","D",0.25,9.6,3.75]
["NE045","Dawes","Enning-Shale outcrop complex, 11 to 50 percent slopes","Well drained","D",0.375,9.65,7.7]
["NE045","Dawes","Epping silt loam, 3 to 30 percent slopes","Well drained","D",0.75,34.950000000000003,7.7]
["NE045","Dawes","Glenberg fine sandy loam, 0 to 2 percent slopes","Well drained","A",1,68.05,7.9]
["NE045","Dawes","Glenberg fine sandy loam, channeled, frequently flooded","Well drained","A",1,68.05,7.9]
["NE045","Dawes","Glenberg loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.75,82.5,7.9]
["NE045","Dawes","Glenberg loamy very fine sand, occasionally flooded, 0 to 3 percent slopes","Well drained","A",0.75,82.5,7.9]
["NE045","Dawes","Haverson loam, frequently flooded","Well drained","B",1,51.5,7.9]
["NE045","Dawes","Haverson silt loam, 0 to 3 percent slopes","Well drained","B",1,44.3,7.9]
["NE045","Dawes","Haverson silt loam, occasionally flooded","Well drained","B",1,44.3,7.9]
["NE045","Dawes","Haverson silty clay loam, occasionally flooded","Well drained","B",1,42.55,7.9]
["NE045","Dawes","Hisle-Slickspots complex, 0 to 6 percent slopes","Well drained","D",0.875,17.100000000000001,7.6]
["NE045","Dawes","Hoffland fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7.5]
["NE045","Dawes","Ipage loamy fine sand, alkali substratum, 0 to 3 percent slopes","Moderately well drained","A",0.5,79,8]
["NE045","Dawes","Jayem and Vetal loamy very fine sands, 6 to 9 percent slopes","Well drained","A",1,65.75,7.2]
["NE045","Dawes","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,67.5,7.2]
["NE045","Dawes","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,67.5,7.2]
["NE045","Dawes","Jayem loamy very fine sand, 1 to 6 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE045","Dawes","Jayem loamy very fine sand, 3 to 6 percent slopes","Well drained","A",0.5,62.5,7.2]
["NE045","Dawes","Jayem loamy very fine sand, 6 to 9 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE045","Dawes","Keith and Ulysses silt loams, 3 to 9 percent slopes","Well drained","B",1.125,13.95,7.5500000000000007]
["NE045","Dawes","Keith loam, 1 to 3 percent slopes","Well drained","C",0.5,14.2,7.45]
["NE045","Dawes","Keith loam, 3 to 6 percent slopes","Well drained","C",0.5,14.2,7.45]
["NE045","Dawes","Keith silt loam, 1 to 3 percent slopes","Well drained","B",0.75,13.7,7]
["NE045","Dawes","Keith silt loam, 3 to 9 percent slopes","Well drained","B",0.75,13.7,7]
["NE045","Dawes","Keota silt loam, 1 to 3 percent slopes","Well drained","C",0.25,14.3,7.9]
["NE045","Dawes","Keota-Epping silt loams, 3 to 9 percent slopes","Well drained","D",0.5,17.55,7.7]
["NE045","Dawes","Keya loam, 0 to 2 percent slopes","Well drained","B",1.25,39.5,7.2]
["NE045","Dawes","Kyle silty clay, 0 to 1 percent slopes","Well drained","D",0.75,11.4,7.9]
["NE045","Dawes","Kyle silty clay, 1 to 6 percent slopes","Well drained","D",0.75,11.4,7.9]
["NE045","Dawes","Kyle-Hisle complex, 0 to 2 percent slopes","Well drained","D",1,11.4,7.5500000000000007]
["NE045","Dawes","Las Animas soils, 0 to 2 percent slopes","Somewhat poorly drained","C",0.25,63.5,7.9]
["NE045","Dawes","Lisco very fine sandy loam, wet, occasionally flooded","Poorly drained","A/D",0.25,64.400000000000006,8.8000000000000007]
["NE045","Dawes","Lohmiller silty clay loam, frequently flooded","Well drained","C",1,12.05,7.7]
["NE045","Dawes","Manvel silty clay loam, 3 to 6 percent slopes","Well drained","C",0.875,6.8,8.1999999999999993]
["NE045","Dawes","Minnequa silty clay loam, 1 to 6 percent slopes","Well drained","C",0.25,6.8,7.9]
["NE045","Dawes","Minnequa silty clay loam, 6 to 12 percent slopes","Well drained","C",0.25,6.8,7.9]
["NE045","Dawes","Mitchell silt loam, 0 to 1 percent slopes","Well drained","B",1,27.25,7.9]
["NE045","Dawes","Mitchell silt loam, 1 to 6 percent slopes","Well drained","B",1,27.25,7.9]
["NE045","Dawes","Mitchell silt loam, 6 to 9 percent slopes","Well drained","B",1,27.25,7.9]
["NE045","Dawes","Mitchell silt loam, 9 to 20 percent slopes","Well drained","B",1,27.25,7.9]
["NE045","Dawes","Mitchell-Epping complex, 9 to 30 percent slopes","Well drained","D",0.75,34.950000000000003,7.9]
["NE045","Dawes","Munjor fine sandy loam, channeled, frequently flooded","Well drained","A",0.5,56.1,7.9]
["NE045","Dawes","Munjor fine sandy loam, rarely flooded","Well drained","A",0.5,56.1,7.9]
["NE045","Dawes","Norrest clay loam, 1 to 3 percent slopes","Well drained","C",0.75,7.1,7.9]
["NE045","Dawes","Norrest clay loam, 3 to 9 percent slopes","Well drained","C",0.75,7.1,7.9]
["NE045","Dawes","Norrest silty clay loam, 1 to 3 percent slopes","Well drained","C",0.5,7.1,7.9]
["NE045","Dawes","Norrest silty clay loam, 3 to 9 percent slopes","Well drained","C",0.5,7.1,7.9]
["NE045","Dawes","Norrest silty clay loam, 9 to 20 percent slopes","Well drained","C",0.5,7.1,7.9]
["NE045","Dawes","Oglala loam, 9 to 30 percent slopes","Well drained","B",0.75,42.7,7]
["NE045","Dawes","Oglala-Canyon complex, 3 to 9 percent slopes","Well drained","D",1,52.2,7.1]
["NE045","Dawes","Oglala-Canyon complex, 6 to 9 percent slopes","Well drained","D",1,43.400000000000006,7.1]
["NE045","Dawes","Oglala-Canyon complex, 9 to 30 percent slopes","Well drained","D",1,52.2,7.1]
["NE045","Dawes","Oglala-Canyon loams, 9 to 20 percent slopes","Well drained","D",1,43.400000000000006,7.1]
["NE045","Dawes","Oglala-Canyon very fine sandy loams, 9 to 30 percent slopes","Well drained","D",1,59,7.45]
["NE045","Dawes","Orella clay, 1 to 30 percent slopes","Well drained","D",0.75,21.6,7.9]
["NE045","Dawes","Orella silty clay loam, 3 to 30 percent slopes","Well drained","D",0.75,18.7,7.9]
["NE045","Dawes","Orpha loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,86.4,7.2]
["NE045","Dawes","Orpha-Niobrara complex, 9 to 30 percent slopes","Excessively drained","D",0.375,83.15,7.35]
["NE045","Dawes","Pierre clay, 1 to 6 percent slopes","Well drained","D",0.5,17.100000000000001,7]
["NE045","Dawes","Pierre clay, 6 to 20 percent slopes","Well drained","D",0.5,17.100000000000001,7]
["NE045","Dawes","Pierre-Slickspots complex, 3 to 9 percent slopes","Well drained","D",0.875,9.8000000000000007,7]
["NE045","Dawes","Ponderosa loamy very fine sand, 6 to 9 percent slopes","Well drained","A",0.75,63.3,7.2]
["NE045","Dawes","Ponderosa loamy very fine sand, 9 to 20 percent slopes","Well drained","A",0.75,63.3,7.2]
["NE045","Dawes","Ponderosa-Tassel-Vetal complex, 6 to 30 percent slopes","Well drained","A",1.25,63.949999999999996,7.1]
["NE045","Dawes","Richfield silt loam, 1 to 3 percent slopes","Well drained","C",0.75,20,7.5]
["NE045","Dawes","Rock outcrop-Canyon complex, 30 to 60 percent slopes","Well drained","D",0.625,22.15,3.95]
["NE045","Dawes","Rosebud loam, 1 to 3 percent slopes","Well drained","C",0.75,39.4,7.35]
["NE045","Dawes","Rosebud silt loam, 1 to 3 percent slopes","Well drained","C",0.75,32.049999999999997,7.35]
["NE045","Dawes","Rosebud-Canyon complex, 3 to 9 percent slopes","Well drained","D",0.75,43.2,7.5]
["NE045","Dawes","Rosebud-Canyon loams, 3 to 9 percent slopes","Well drained","D",0.75,44.3,7.5]
["NE045","Dawes","Samsil silty clay, 3 to 30 percent slopes","Well drained","D",0.5,9.4,7.25]
["NE045","Dawes","Samsil-Pierre complex, 3 to 30 percent slopes","Well drained","D",0.5,16.649999999999999,7.25]
["NE045","Dawes","Sarben and Vetal loamy very fine sands, 9 to 30 percent slopes","Well drained","A",1,72.8,7.1]
["NE045","Dawes","Sarben fine sandy loam, 1 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7.2]
["NE045","Dawes","Sarben fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,66.099999999999994,7.2]
["NE045","Dawes","Sarben fine sandy loam, 9 to 30 percent slopes","Well drained","A",0.75,66.099999999999994,7.2]
["NE045","Dawes","Sarben loamy very fine sand, 9 to 30 percent slopes","Well drained","A",1,82.75,6.95]
["NE045","Dawes","Satanta fine sandy loam, 3 to 6 percent slopes","Well drained","B",1.25,63.5,7.5]
["NE045","Dawes","Satanta fine sandy loam, 6 to 9 percent slopes","Well drained","B",1.25,63.5,7.5]
["NE045","Dawes","Satanta-Canyon complex, 12 to 20 percent slopes","Well drained","D",1.25,58.6,7.9]
["NE045","Dawes","Satanta-Canyon complex, 6 to 12 percent slopes","Well drained","D",1.25,51.45,7.7]
["NE045","Dawes","Schamber soils, 3 to 30 percent slopes","Somewhat excessively drained","A",0.875,75.349999999999994,7.6]
["NE045","Dawes","Skilak silty clay loam, 0 to 5 percent slopes","Well drained","B",0.25,7.3,8.5]
["NE045","Dawes","Sulco-Haverson loams, 0 to 50 percent slopes","Well drained","B",1,41.099999999999994,7.9]
["NE045","Dawes","Tassel loamy very fine sand, 3 to 30 percent slopes","Well drained","D",1.25,64.599999999999994,7.9]
["NE045","Dawes","Tassel soils, 3 to 30 percent slopes","Well drained","D",1.25,64.599999999999994,7.9]
["NE045","Dawes","Tassel-Ashollow-Rock outcrop complex, 9 to 60 percent slopes","Well drained","A",1,73.199999999999989,7.9]
["NE045","Dawes","Tassel-Busher-Rock outcrop complex, 6 to 30 percent slopes","Well drained","A",0.75,64.599999999999994,7]
["NE045","Dawes","Tassel-Ponderosa-Rock outcrop association, 9 to 70 percent slopes","Well drained","A",0.75,63.3,7.2]
["NE045","Dawes","Thirtynine loam, 1 to 3 percent slopes","Well drained","B",0.5,9.5,7.9]
["NE045","Dawes","Thirtynine loam, 3 to 6 percent slopes","Well drained","B",0.5,9.5,7.9]
["NE045","Dawes","Thirtynine loam, 6 to 9 percent slopes","Well drained","B",0.5,9.5,7.9]
["NE045","Dawes","Thirtynine silt loam, 0 to 2 percent slopes","Well drained","B",0.5,9.5,7.9]
["NE045","Dawes","Thirtynine silt loam, 2 to 11 percent slopes","Well drained","B",0.5,9.5,7.9]
["NE045","Dawes","Thirtynine silt loam, 2 to 11 percent slopes, eroded","Well drained","B",0.5,9.5,7.9]
["NE045","Dawes","Tripp silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7.5]
["NE045","Dawes","Tripp silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7.5]
["NE045","Dawes","Tripp silt loam, saline-alkali, 0 to 2 percent slopes","Well drained","B",0.75,14.2,8.5]
["NE045","Dawes","Ulysses silt loam, 9 to 20 percent slopes","Well drained","B",1.5,33.299999999999997,7.9]
["NE045","Dawes","Valent and Dwyer loamy fine sands, 0 to 3 percent slopes","Excessively drained","A",0.75,83.199999999999989,7.35]
["NE045","Dawes","Valent and Dwyer loamy fine sands, 3 to 20 percent slopes","Excessively drained","A",0.75,83.199999999999989,7.35]
["NE045","Dawes","Valent complex, rolling and hilly","Excessively drained","A",0.5,94.9,7.2]
["NE045","Dawes","Valent fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE045","Dawes","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE045","Dawes","Valent loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE045","Dawes","Valent loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,89.45,7.2]
["NE045","Dawes","Valent loamy fine sand, 9 to 20 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE045","Dawes","Vetal and Bayard soils, 1 to 6 percent slopes","Well drained","A",1.25,65.900000000000006,7.2]
["NE045","Dawes","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7.3]
["NE045","Dawes","Vetal fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE045","Dawes","Vetal loamy fine sand, 0 to 3 percent slopes","Well drained","A",2,83.1,7.2]
["NE045","Dawes","Vetal very fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.25,65.900000000000006,7.3]
["NE045","Dawes","Vetal very fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.25,65.900000000000006,7.3]
["NE047","Dawson",null,"",""]
["NE047","Dawson","Alda loam, rarely flooded","Somewhat poorly drained","C",0.25,61.7,7.5]
["NE047","Dawson","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE047","Dawson","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE047","Dawson","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE047","Dawson","Anselmo fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE047","Dawson","Anselmo loam, 0 to 1 percent slopes","Well drained","B",0.75,66.099999999999994,7.1]
["NE047","Dawson","Coly and Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE047","Dawson","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE047","Dawson","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE047","Dawson","Coly, Uly, and Hobbs soils, 3 to 30 percent slopes","Well drained","B",0.75,11.2,7.5]
["NE047","Dawson","Coly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE047","Dawson","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE047","Dawson","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE047","Dawson","Cozad fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,14.3,7]
["NE047","Dawson","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE047","Dawson","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE047","Dawson","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7]
["NE047","Dawson","Cozad silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,14.2,7.3]
["NE047","Dawson","Cozad silt loam, saline-alkali, 0 to 1 percent slopes","Moderately well drained","B",0.75,11.4,8.8000000000000007]
["NE047","Dawson","Cozad silt loam, wet substratum, 0 to 1 percent slopes","Moderately well drained","C",1.5,11.7,7.5]
["NE047","Dawson","Cozad silt loam, wet substratum, 1 to 3 percent slopes","Moderately well drained","C",1.5,11.7,7.5]
["NE047","Dawson","Cozad silty clay loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE047","Dawson","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,82.9,6.85]
["NE047","Dawson","Elsmere loamy fine sand, loamy substratum, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,79.400000000000006,6.7]
["NE047","Dawson","Fillmore silt loam, drained, occasionally ponded","Somewhat poorly drained","D",1.125,12.649999999999999,7.1]
["NE047","Dawson","Fillmore silt loam, frequently ponded","Somewhat poorly drained","C/D",1.125,12.649999999999999,7.1]
["NE047","Dawson","Fillmore silt loam, occasionally ponded","Somewhat poorly drained","D",1.125,12.649999999999999,6.4]
["NE047","Dawson","Gibbon loam, rarely flooded","Somewhat poorly drained","C",0.5,51.75,7.9]
["NE047","Dawson","Gosper fine sandy loam, 0 to 1 percent slopes","Moderately well drained","C",0.75,64.5,7.7]
["NE047","Dawson","Gosper loam, 0 to 1 percent slopes","Moderately well drained","C",0.75,53.800000000000004,7.7]
["NE047","Dawson","Gosper loam, saline-alkali, 0 to 1 percent slopes","Moderately well drained","C",0.75,43.2,7.9]
["NE047","Dawson","Gothenburg soils, frequently flooded","Poorly drained","B/D",0.25,96,7.2]
["NE047","Dawson","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE047","Dawson","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.5,9.5,7]
["NE047","Dawson","Hall silt loam, wet substratum, 0 to 1 percent slopes","Somewhat poorly drained","C",0.75,9.3000000000000007,7.9]
["NE047","Dawson","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE047","Dawson","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,10.4,7.25]
["NE047","Dawson","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",1.25,9.3000000000000007,7.2]
["NE047","Dawson","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",1.25,9.3000000000000007,7.2]
["NE047","Dawson","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",1.25,9.3000000000000007,7.2]
["NE047","Dawson","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,9.3000000000000007,7.2]
["NE047","Dawson","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,6.8,7.2]
["NE047","Dawson","Holdrege-Uly silt loams, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.4,7.2]
["NE047","Dawson","Hord fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,46,7]
["NE047","Dawson","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE047","Dawson","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE047","Dawson","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE047","Dawson","Hord silt loam, wet substratum, 0 to 1 percent slopes","Somewhat poorly drained","C",0.75,9.3000000000000007,7.9]
["NE047","Dawson","Hord silty clay loam, 0 to 1 percent slopes","Well drained","C",0.75,8.9,7]
["NE047","Dawson","Hord silty clay loam, wet substratum, 0 to 1 percent slopes","Somewhat poorly drained","C",0.75,9.1,7.9]
["NE047","Dawson","Lawet loam, ponded, rarely flooded","Poorly drained","B/D",0.75,39.799999999999997,7.9]
["NE047","Dawson","Lawet silt loam, drained, rarely flooded","Somewhat poorly drained","B/D",0.75,46.95,7.85]
["NE047","Dawson","Lawet silt loam, saline-alkali, rarely flooded","Somewhat poorly drained","B/D",0.75,41.55,8.3500000000000014]
["NE047","Dawson","Lex loam, rarely flooded","Somewhat poorly drained","C",0.75,56,7.8]
["NE047","Dawson","Lex loam, saline-alkali, rarely flooded","Somewhat poorly drained","C",0.75,56,8.1999999999999993]
["NE047","Dawson","Ovina fine sandy loam","Somewhat poorly drained","B",1.125,66.900000000000006,6.5]
["NE047","Dawson","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,63.2,7.5]
["NE047","Dawson","Platte-Alda complex, occasionally flooded","Somewhat poorly drained","C",0.5,66,7.5]
["NE047","Dawson","Rusco silt loam, 0 to 1 percent slopes","Moderately well drained","C/D",0.75,11.2,7.5]
["NE047","Dawson","Selia loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,84.45,8]
["NE047","Dawson","Silver Creek complex, rarely flooded","Somewhat poorly drained","D",0.5,36.950000000000003,8.0500000000000007]
["NE047","Dawson","Silver Creek silt loam, rarely flooded","Somewhat poorly drained","D",0.5,36.950000000000003,8.0500000000000007]
["NE047","Dawson","Silver Creek silty clay loam, rarely flooded","Somewhat poorly drained","D",0.75,20,7.9]
["NE047","Dawson","Spoil banks","Well drained","B",0.75,6.8,7.9]
["NE047","Dawson","Uly and Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE047","Dawson","Uly and Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.6]
["NE047","Dawson","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE047","Dawson","Uly-Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE047","Dawson","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE047","Dawson","Uly-Holdrege silt loams, 6 to 11 percent slopes","Well drained","C",1,9.25,7.1]
["NE047","Dawson","Uly-Holdrege-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","C",1,9.25,7.1]
["NE047","Dawson","Ustorthents, 17 to 60 percent slopes","Well drained","B",0.75,6.8,7.9]
["NE047","Dawson","Valentine fine sand, rolling","Excessively drained","A",0.5,95.85,6.5]
["NE047","Dawson","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE047","Dawson","Valentine loamy fine sand, 3 to 6 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE047","Dawson","Valentine loamy fine sand, rolling","Excessively drained","A",0.25,87.3,6.5]
["NE047","Dawson","Wann fine sandy loam, saline-alkali, rarely flooded","Somewhat poorly drained","B",0.5,66.650000000000006,8.8000000000000007]
["NE047","Dawson","Wann loam, rarely flooded","Somewhat poorly drained","C",0.75,63.1,8.1999999999999993]
["NE047","Dawson","Wood River silt loam, 0 to 1 percent slopes","Moderately well drained","C",0.75,22.9,8.1999999999999993]
["NE047","Dawson","Wood River-Gayville complex, 0 to 1 percent slopes","Moderately well drained","D",1.375,18,8.35]
["NE049","Deuel",null,"",""]
["NE049","Deuel","Alliance loam, 0 to 1 percent slopes","Well drained","C",0.75,42.2,7.2]
["NE049","Deuel","Alliance-Rosebud loams, 1 to 3 percent slopes","Well drained","C",0.75,35.450000000000003,7.2]
["NE049","Deuel","Altvan-Eckley-Satanta complex, 3 to 9 percent slopes","Well drained","C",0.75,62,7.2]
["NE049","Deuel","Ashollow-Tassel complex, 9 to 30 percent slopes","Well drained","B",0.75,63.3,7.9]
["NE049","Deuel","Blueridge-Altvan complex, 6 to 30 percent slopes","Well drained","C",0.75,83.5,7.2]
["NE049","Deuel","Broadwater loamy sand, frequently flooded","Somewhat excessively drained","A",0.5,88.800000000000011,7.2]
["NE049","Deuel","Calamus sand, very rarely flooded","Moderately well drained","A",0.75,93.55,7]
["NE049","Deuel","Chappell-Alice-Broadwater complex, 0 to 3 percent slopes","Well drained","A",0.75,66.599999999999994,7.2]
["NE049","Deuel","Duroc loam, 0 to 1 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE049","Deuel","Duroc loam, terrace, 0 to 1 percent slopes","Well drained","B",1.375,33.299999999999997,7.2]
["NE049","Deuel","Duroc loam, terrace, 1 to 3 percent slopes","Well drained","B",1.375,33.299999999999997,7.2]
["NE049","Deuel","Duroc silt loam, 1 to 3 percent slopes","Well drained","B",1.375,9.5,7.2]
["NE049","Deuel","Glenberg fine sandy loam, rarely flooded","Well drained","A",1,66.95,7.9]
["NE049","Deuel","Gothenburg soils, occasionally flooded","Poorly drained","A/D",0.25,91.9,7.5]
["NE049","Deuel","Jankosh loam, rarely flooded","Somewhat poorly drained","C",0.5,48.400000000000006,8.5]
["NE049","Deuel","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,67.599999999999994,7.2]
["NE049","Deuel","Johnstown-Satanta-Richfield loams, 0 to 2 percent slopes","Well drained","C",1,42.1,7.25]
["NE049","Deuel","Keith loam, 1 to 3 percent slopes","Well drained","C",0.75,23.35,7]
["NE049","Deuel","Keith loam, 3 to 6 percent slopes","Well drained","C",0.75,37.4,7]
["NE049","Deuel","Kuma loam, 0 to 1 percent slopes","Well drained","C",2,36.9,7.5]
["NE049","Deuel","Kuma loam, 1 to 3 percent slopes","Well drained","C",2,36.9,7.5]
["NE049","Deuel","Las Animas loam, channeled, frequently flooded","Poorly drained","B/D",0.75,67.150000000000006,7.9]
["NE049","Deuel","Las Animas loam, occasionally flooded","Somewhat poorly drained","C",0.75,65.2,7.9]
["NE049","Deuel","Lexsworth loam, very rarely flooded","Moderately well drained","C",0.25,91.9,8]
["NE049","Deuel","Lodgepole silt loam, occasionally ponded","Somewhat poorly drained","C/D",2,21,7]
["NE049","Deuel","Merrick sandy clay loam, very rarely flooded","Moderately well drained","C",0.75,41.1,7.9]
["NE049","Deuel","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,67.599999999999994,7.5]
["NE049","Deuel","Ralton loam, very rarely flooded","Moderately well drained","B",0.5,41.7,7.9]
["NE049","Deuel","Sarben loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.5,66.099999999999994,6.95]
["NE049","Deuel","Sarben loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.5,66.099999999999994,6.95]
["NE049","Deuel","Satanta-Altvan complex, 3 to 6 percent slopes","Well drained","C",0.75,62,7.7]
["NE049","Deuel","Satanta-Ascalon complex, 0 to 1 percent slopes","Well drained","C",0.75,63.7,7.35]
["NE049","Deuel","Satanta-Johnstown-Altvan loams, 1 to 3 percent slopes","Well drained","C",1,42.1,7.35]
["NE049","Deuel","Scoville loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.25,83.5,7.2]
["NE049","Deuel","Sidney loam, 3 to 6 percent slopes","Well drained","B",0.75,43.2,7.2]
["NE049","Deuel","Sidney-Canyon complex, 3 to 9 percent slopes","Well drained","D",0.75,44.3,7.9]
["NE049","Deuel","Sidney-Canyon loams, 3 to 9 percent slopes","Well drained","D",0.75,43.2,7.5500000000000007]
["NE049","Deuel","Sulco-McConaughy complex, 3 to 6 percent slopes, eroded","Well drained","B",0.75,43.6,7.9]
["NE049","Deuel","Sulco-McConaughy loams, 3 to 6 percent slopes, eroded","Well drained","B",0.75,42.2,7.9]
["NE049","Deuel","Sulco-McConaughy loams, 6 to 9 percent slopes, eroded","Well drained","B",0.75,42.2,7.9]
["NE049","Deuel","Sulco-McConaughy loams, 9 to 30 percent slopes","Well drained","B",0.75,43.6,7.9]
["NE049","Deuel","Valent complex, rolling and hilly","Excessively drained","A",0.5,94.9,7.2]
["NE049","Deuel","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE049","Deuel","Valent fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE051","Dixon",null,"",""]
["NE051","Dixon","Albaton silty clay, occasionally flooded","Poorly drained","D",1.5,3.9,7.9]
["NE051","Dixon","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE051","Dixon","Alcester silt loam, 6 to 11 percent slopes","Well drained","B",2.5,7.4,7]
["NE051","Dixon","Alcester silt loam, gullied, 11 to 60 percent slopes","Well drained","B",2.5,7.4,7]
["NE051","Dixon","Aowa silt loam, channeled, frequently flooded","Well drained","B",1.625,21.15,7.9]
["NE051","Dixon","Aowa silt loam, occasionally flooded","Well drained","B",1.625,21.15,7.9]
["NE051","Dixon","Baltic silty clay loam, occasionally flooded","Poorly drained","C/D",3,8,7.9]
["NE051","Dixon","Baltic silty clay, occasionally flooded","Poorly drained","C/D",3,5.5,7.9]
["NE051","Dixon","Bazile silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,7.1,6.5]
["NE051","Dixon","Belfore-Moody silty clay loams, 1 to 3 percent slopes","Well drained","C",1.875,10.1,6.5]
["NE051","Dixon","Blake silty clay loam, rarely flooded","Somewhat poorly drained","C",0.5,7.1,7.9]
["NE051","Dixon","Blendon sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,67.3,7]
["NE051","Dixon","Calco silt loam, overwash, occasionally flooded","Poorly drained","B/D",5,6.8000000000000007,7.9]
["NE051","Dixon","Calco silty clay loam, occasionally flooded","Poorly drained","B/D",5,6.8000000000000007,7.9]
["NE051","Dixon","Calco silty clay loam, wet, occasionally flooded","Very poorly drained","B/D",5,6.8000000000000007,7.9]
["NE051","Dixon","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE051","Dixon","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE051","Dixon","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE051","Dixon","Crofton silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE051","Dixon","Crofton silt loam, 30 to 60 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE051","Dixon","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE051","Dixon","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE051","Dixon","Crofton-Alcester silt loams, 20 to 60 percent slopes","Well drained","B",1.25,9.4,7.5]
["NE051","Dixon","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE051","Dixon","Crofton-Nora complex, 2 to 6 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE051","Dixon","Crofton-Nora complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE051","Dixon","Grable very fine sandy loam, rarely flooded","Well drained","B",0.5,59,7.9]
["NE051","Dixon","Haynie silt loam, rarely flooded","Well drained","B",1.25,12.600000000000001,7.7]
["NE051","Dixon","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE051","Dixon","Lamo silt loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.95,7.9]
["NE051","Dixon","Lamo silt loam, overwash, occasionally flooded","Somewhat poorly drained","C",1.375,7.95,8.1999999999999993]
["NE051","Dixon","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE051","Dixon","Leisy loam, 0 to 6 percent slopes","Well drained","B",0.75,39.200000000000003,6.5]
["NE051","Dixon","Loretto fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,37.200000000000003,6.5]
["NE051","Dixon","Loretto loam, sand substratum, 6 to 11 percent slopes","Well drained","B",1.5,44.3,6.5]
["NE051","Dixon","Maskell loam, 0 to 2 percent slopes","Well drained","B",0.5,39.799999999999997,7]
["NE051","Dixon","Maskell loam, 2 to 6 percent slopes","Well drained","B",0.5,39.799999999999997,7]
["NE051","Dixon","Modale very fine sandy loam, rarely flooded","Moderately well drained","C",1.375,31.05,7.9]
["NE051","Dixon","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE051","Dixon","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE051","Dixon","Moody silty clay loam, 6 to 11 percent slopes","Well drained","C",3,6.9,6.5]
["NE051","Dixon","Moody silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE051","Dixon","Moody-Leisy complex, 2 to 6 percent slopes","Well drained","B",1.875,14.7,6.5]
["NE051","Dixon","Moody-Leisy complex, 6 to 11 percent slopes","Well drained","B",1.875,14.7,6.5]
["NE051","Dixon","Nora silt loam, 11 to 17 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE051","Dixon","Nora silt loam, 11 to 17 percent slopes, eroded","Well drained","C",1.25,9.1,6.5]
["NE051","Dixon","Nora silt loam, 17 to 30 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE051","Dixon","Nora silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE051","Dixon","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE051","Dixon","Nora silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,8.9,7]
["NE051","Dixon","Nora silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE051","Dixon","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE051","Dixon","Nora silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE051","Dixon","Nora variant silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE051","Dixon","Nora variant silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE051","Dixon","Nora-Alcester silt loams, 11 to 17 percent slopes","Well drained","B",1.625,9.1000000000000014,7]
["NE051","Dixon","Nora-Alcester silt loams, 17 to 30 percent slopes","Well drained","B",1.625,9.1000000000000014,7]
["NE051","Dixon","Nora-Moody silty clay loams, 6 to 11 percent slopes","Well drained","C",1.875,7,6.85]
["NE051","Dixon","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE051","Dixon","Onawa silty clay, rarely flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE051","Dixon","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE051","Dixon","Ortello sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,66.599999999999994,6.7]
["NE051","Dixon","Percival silty clay, occasionally flooded","Somewhat poorly drained","D",1.125,48.5,7.9]
["NE051","Dixon","Sarpy fine sand, 3 to 11 percent slopes","Excessively drained","A",0.75,95.9,7.7]
["NE051","Dixon","Sarpy loamy fine sand, occasionally flooded","Excessively drained","A",0.75,87.9,7.5]
["NE051","Dixon","Sarpy silty clay, overwash, occasionally flooded","Excessively drained","C",0.5,42.6,7.7]
["NE051","Dixon","Sarpy-Riverwash complex, frequently flooded","Very poorly drained","A/D",0.5,92.95,7.7]
["NE051","Dixon","Sarpy-Ustorthents complex, 0 to 4 percent slopes","Excessively drained","A",0.75,91.35,7.25]
["NE051","Dixon","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE051","Dixon","Thurman loamy sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE051","Dixon","Thurman loamy sand, 2 to 6 percent slopes, eroded","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE051","Dixon","Thurman loamy sand, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE051","Dixon","Thurman loamy sand, 6 to 11 percent slopes, eroded","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE051","Dixon","Thurman sand, 2 to 20 percent slopes","Somewhat excessively drained","A",0.25,94.1,6.5]
["NE051","Dixon","Thurman-Leisy complex, 2 to 6 percent slopes","Well drained","B",0.5,75.2,6.5]
["NE051","Dixon","Thurman-Leisy complex, 6 to 11 percent slopes","Well drained","B",0.5,75.2,6.5]
["NE051","Dixon","Thurman-Loretto complex, 2 to 6 percent slopes","Well drained","B",0.875,83.7,6.5]
["NE051","Dixon","Thurman-Ortello complex, 6 to 11 percent slopes","Well drained","A",0.75,82.5,6.5]
["NE051","Dixon","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.75,6.6]
["NE051","Dixon","Zook silty clay, occasionally flooded","Poorly drained","C/D",4.5,7.85,6.6]
["NE053","Dodge",null,"",""]
["NE053","Dodge","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",3.25,8.4499999999999993,7.1]
["NE053","Dodge","Alda fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,66,7.5]
["NE053","Dodge","Alda loam, occasionally flooded","Somewhat poorly drained","C",0.75,66,7.5]
["NE053","Dodge","Barney silty clay loam, frequently flooded","Poorly drained","B/D",1.625,67.449999999999989,7.35]
["NE053","Dodge","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE053","Dodge","Belfore silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",1.125,19.25,6.6]
["NE053","Dodge","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE053","Dodge","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE053","Dodge","Calco silty clay loam, frequently flooded","Poorly drained","B/D",5,6.8000000000000007,7.9]
["NE053","Dodge","Calco silty clay loam, occasionally flooded","Somewhat poorly drained","B/D",4,6.9,7.9]
["NE053","Dodge","Calco silty clay loam, wet, occasionally flooded","Poorly drained","B/D",5,6.8000000000000007,7.9]
["NE053","Dodge","Cass fine sandy loam, clayey substratum, rarely flooded","Well drained","A",0.5,67.150000000000006,7]
["NE053","Dodge","Cass fine sandy loam, occasionally flooded","Well drained","A",0.75,66.900000000000006,6.8]
["NE053","Dodge","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE053","Dodge","Cass loam, clayey substratum, rarely flooded","Well drained","B",0.5,55.85,7]
["NE053","Dodge","Cass loam, occasionally flooded","Well drained","B",0.75,63.5,6.8]
["NE053","Dodge","Cass loam, rarely flooded","Well drained","B",0.75,63.5,7.3]
["NE053","Dodge","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2.5,6.85,6.5]
["NE053","Dodge","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE053","Dodge","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE053","Dodge","Crofton silt loam, 30 to 60 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE053","Dodge","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE053","Dodge","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE053","Dodge","Fillmore silt loam, frequently ponded","Poorly drained","D",1.625,15.75,6.1]
["NE053","Dodge","Fillmore silt loam, occasionally ponded","Poorly drained","D",1.5,18.5,6.1]
["NE053","Dodge","Fluvaquents sandy and Aquolls silty, frequently flooded","Very poorly drained","B/D",1.375,76.5,7.5]
["NE053","Dodge","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",0.05,94.1,7.9]
["NE053","Dodge","Fontanelle silty clay loam, frequently flooded","Very poorly drained","C/D",0.75,15,7.6]
["NE053","Dodge","Gibbon loam, occasionally flooded","Somewhat poorly drained","C",0.75,41.5,7.9]
["NE053","Dodge","Gibbon loamy sand, overwash, occasionally flooded","Somewhat poorly drained","B",0.75,83.8,6.7]
["NE053","Dodge","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.4,7.9]
["NE053","Dodge","Gibbon variant soils, frequently flooded","Poorly drained","C/D",2,6.9,8.1999999999999993]
["NE053","Dodge","Gibbon-Wann complex, occasionally flooded","Somewhat poorly drained","C",1.375,39.75,8.1999999999999993]
["NE053","Dodge","Gilliam-Eudora silt loams, occasionally flooded","Well drained","A",1.1499999999999999,29,7.65]
["NE053","Dodge","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,10.4,7.25]
["NE053","Dodge","Ida-Steinauer complex, 17 to 60 percent slopes","Well drained","B",0.5,22.35,7.9]
["NE053","Dodge","Inavale loamy fine sand, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE053","Dodge","Inglewood loamy fine sand, occasionally flooded","Moderately well drained","A",0.25,87.55,7]
["NE053","Dodge","Inglewood loamy fine sand, rarely flooded","Moderately well drained","A",0.25,87.55,7]
["NE053","Dodge","Inglewood-Novina complex, occasionally flooded","Moderately well drained","B",0.25,66.599999999999994,7]
["NE053","Dodge","Janude loam, clayey substratum, rarely flooded","Moderately well drained","B",0.75,44.3,7.5]
["NE053","Dodge","Janude loam, rarely flooded","Moderately well drained","B",1.25,45,7.5]
["NE053","Dodge","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3.5,7.9,6.5]
["NE053","Dodge","Kennebec and Colo soils, channeled, frequently flooded","Poorly drained","B/D",4.5,8.0500000000000007,6.5]
["NE053","Dodge","Kennebec silt loam, occasionally flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE053","Dodge","Kezan silt loam, frequently flooded","Poorly drained","C",1.875,9.0500000000000007,7.2]
["NE053","Dodge","Leisy fine sandy loam, 2 to 6 percent slopes","Well drained","C",0.75,39.200000000000003,6.5]
["NE053","Dodge","Luton silty clay, occasionally flooded","Poorly drained","D",2.25,5.3,7.35]
["NE053","Dodge","Monona silt loam, terrace, 0 to 2 percent slopes","Well drained","B",1.25,9.4,6.7]
["NE053","Dodge","Monona silt loam, terrace, 2 to 6 percent slopes","Well drained","B",1.25,9.4,6.7]
["NE053","Dodge","Moody silty clay loam, 0 to 2 percent slopes","Somewhat poorly drained","D",2.25,8.15,6.6]
["NE053","Dodge","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE053","Dodge","Moody silty clay loam, 6 to 11 percent slopes","Well drained","C",3,6.9,6.5]
["NE053","Dodge","Moody silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE053","Dodge","Napa-Luton complex, occasionally flooded","Poorly drained","D",1.75,5.3,7.5]
["NE053","Dodge","Nora silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.75,8.9,7]
["NE053","Dodge","Nora silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE053","Dodge","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE053","Dodge","Nora silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE053","Dodge","Nora variant silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE053","Dodge","Nora variant silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE053","Dodge","Nora-Crofton complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE053","Dodge","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE053","Dodge","Platte fine sandy loam, occasionally flooded","Somewhat poorly drained","B",2,64.400000000000006,7.2]
["NE053","Dodge","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,63.2,7.5]
["NE053","Dodge","Platte-Barney complex, channeled, frequently flooded","Poorly drained","C/D",2,64.400000000000006,7.2]
["NE053","Dodge","Platte-Inavale complex, channeled, frequently flooded","Excessively drained","A",0.25,87.3,7.5]
["NE053","Dodge","Platte-Inavale complex, channeled, occasionally flooded","Excessively drained","A",0.25,89.6,7.5]
["NE053","Dodge","Saltine-Gibbon complex, occasionally flooded","Somewhat poorly drained","C",0.75,7,8.5]
["NE053","Dodge","Shell silt loam, occasionally flooded","Well drained","B",1.625,10.199999999999999,6.75]
["NE053","Dodge","Steinauer clay loam, 11 to 30 percent slopes, eroded","Well drained","C",0.75,33.6,7.9]
["NE053","Dodge","Thurman and Valentine loamy fine sands, 6 to 11 percent slopes","Somewhat excessively drained","A",0.5,86.1,6.5]
["NE053","Dodge","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE053","Dodge","Thurman loamy fine sand, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE053","Dodge","Thurman-Moody complex, 11 to 30 percent slopes, eroded","Well drained","C",1,47.15,6.5]
["NE053","Dodge","Thurman-Moody complex, 6 to 11 percent slopes, eroded","Well drained","C",1,47.000000000000007,6.5]
["NE053","Dodge","Thurman-Valentine loamy fine sands, 2 to 6 percent slopes","Somewhat excessively drained","A",0.5,86.1,6.5]
["NE053","Dodge","Wann fine sandy loam, occasionally flooded","Somewhat poorly drained","B",1.375,64.849999999999994,7.85]
["NE053","Dodge","Wann loam, occasionally flooded","Somewhat poorly drained","C",1.375,54.6,7.85]
["NE053","Dodge","Zook silt loam, overwash, occasionally flooded","Poorly drained","C/D",3,16.25,6.6]
["NE053","Dodge","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.75,6.6]
["NE053","Dodge","Zook silty clay, occasionally flooded","Poorly drained","C/D",4.5,7.85,6.6]
["NE055","Douglas",null,"",""]
["NE055","Douglas","Alda loam, occasionally flooded","Somewhat poorly drained","C",0.75,66,7.5]
["NE055","Douglas","Alda-Platte complex, occasionally flooded","Somewhat poorly drained","C",0.75,65.7,7.9]
["NE055","Douglas","Alda-Platte fine sandy loams, occasionally flooded","Somewhat poorly drained","B",0.75,65.7,7.9]
["NE055","Douglas","Alda-Platte-Lex complex, occasionally flooded","Somewhat poorly drained","C",0.75,60.7,7.9]
["NE055","Douglas","Burchard-Contrary-Steinauer complex, 7 to 16 percent slopes","Well drained","C",0.75,33.5,7.45]
["NE055","Douglas","Carr-Ticonic-Scroll complex, occasionally flooded","Well drained","B",0.25,45,7.9]
["NE055","Douglas","Cass-Novina complex, occasionally flooded","Well drained","B",0.75,64.599999999999994,6.8]
["NE055","Douglas","Cass-Wann fine sandy loams, occasionally flooded","Well drained","A",0.75,65.7,8.1999999999999993]
["NE055","Douglas","Clamo-Zook-Kezan silty clay loams, occasionally flooded","Poorly drained","D",3.5,7.6,6.7]
["NE055","Douglas","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE055","Douglas","Contrary-Marshall silty clay loams, 6 to 11 percent slopes","Well drained","C",1,3.5,6.3]
["NE055","Douglas","Contrary-Monona silty clay loams, 6 to 11 percent slopes","Well drained","C",1,3.5,6.3]
["NE055","Douglas","Contrary-Monona-Ida complex, 6 to 17 percent slopes","Well drained","B",1,3.5,7]
["NE055","Douglas","Fluvaquents sandy and Aquolls silty, frequently flooded","Very poorly drained","B/D",1.375,76.5,7.5]
["NE055","Douglas","Gibbon loamy fine sand, overwash, occasionally flooded","Somewhat poorly drained","A",0.75,27.6,7.9]
["NE055","Douglas","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,16.899999999999999,7.9]
["NE055","Douglas","Gibbon-Wann complex, occasionally flooded","Somewhat poorly drained","C",1.375,39.75,8.1999999999999993]
["NE055","Douglas","Gilliam-Eudora silt loams, occasionally flooded","Well drained","A",1.1499999999999999,29,7.65]
["NE055","Douglas","Gilliam-Onawa complex, occasionally flooded","Somewhat poorly drained","C",1.25,7.85,7.6]
["NE055","Douglas","Haynie silt loam, occasionally flooded","Well drained","B",1.25,12.600000000000001,7.5]
["NE055","Douglas","Ida-Pohocco-Monona silt loams, 11 to 30 percent slopes","Well drained","B",0.75,3.5,7.5]
["NE055","Douglas","Inavale loamy fine sand, hummocky, rarely flooded","Excessively drained","A",0.75,87.3,6.8]
["NE055","Douglas","Inglewood-Novina complex, occasionally flooded","Moderately well drained","B",0.25,66.599999999999994,7]
["NE055","Douglas","Judson silty clay loam, 2 to 6 percent slopes","Well drained","C",1.75,3.5,6.3]
["NE055","Douglas","Judson-Nodaway channeled-Contrary complex, 3 to 10 percent slopes","Well drained","B",1,3.5,6.3]
["NE055","Douglas","Kennebec silt loam, occasionally flooded","Moderately well drained","B",2,9.1999999999999993,6.3]
["NE055","Douglas","Kezan-Kennebec silt loams, drained, occasionally flooded","Moderately well drained","B",2,9.1,7.2]
["NE055","Douglas","Lex-Platte complex, occasionally flooded","Somewhat poorly drained","C",2,60,7.9]
["NE055","Douglas","Luton silty clay, occasionally flooded","Poorly drained","D",2.25,5.3,7.35]
["NE055","Douglas","Marshall silty clay loam, 0 to 2 percent slopes","Well drained","C",1.375,3.5,6.05]
["NE055","Douglas","Marshall-Contrary silty clay loams, 2 to 7 percent slopes","Well drained","C",1,3.5,6.3]
["NE055","Douglas","Melia silty clay loam, 0 to 2 percent slopes","Well drained","C",1.25,3.5,6.65]
["NE055","Douglas","Monona-Pohocco-Ida silt loams, 17 to 33 percent slopes","Well drained","B",0.75,3.5,7.5]
["NE055","Douglas","Muscotah silty clay loam, occasionally flooded","Somewhat poorly drained","C",2.25,4,6.8]
["NE055","Douglas","Nishna silty clay loam, occasionally flooded","Poorly drained","C/D",2.25,7.65,7.9]
["NE055","Douglas","Novina-Gibbon complex, occasionally flooded","Somewhat poorly drained","C",0.75,16,7.9]
["NE055","Douglas","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,8.1999999999999993,7.6]
["NE055","Douglas","Platte and Alda soils, frequently flooded","Somewhat poorly drained","C",0.75,65.7,7.9]
["NE055","Douglas","Platte, Inglewood, and Barney soils, frequently flooded","Poorly drained","C/D",0.25,74.5,7.5]
["NE055","Douglas","Platte-Barney complex, channeled, frequently flooded","Poorly drained","C/D",2,64.400000000000006,7.2]
["NE055","Douglas","Platte-Inavale complex, channeled, occasionally flooded","Excessively drained","A",0.25,89.6,7.5]
["NE055","Douglas","Pohocco-Ida complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.6]
["NE055","Douglas","Pohocco-Ida-Monona complex, 6 to 17 percent slopes","Well drained","B",0.75,3.5,7.5]
["NE055","Douglas","Pohocco-Judson silt loams, 11 to 40 percent slopes","Well drained","C",0.75,4.75,6.65]
["NE055","Douglas","Pohocco-Monona silt loams, 11 to 54 percent slopes","Well drained","B",0.75,4.75,7]
["NE055","Douglas","Saltine-Gibbon silty clay loams, occasionally flooded","Somewhat poorly drained","C",0.75,7,8.5]
["NE055","Douglas","Smithland-Kenridge silty clay loams, occasionally flooded","Moderately well drained","C",2.5,6.7,6.5]
["NE055","Douglas","Ticonic-Sarpy-Carr complex, occasionally flooded","Well drained","B",0.25,73.400000000000006,7.9]
["NE055","Douglas","Udorthents-Urban land-Pohocco complex, 0 to 39 percent slopes","Well drained","B",0.5,6,7]
["NE055","Douglas","Urban land-Udorthents-Judson complex, 0 to 11 percent slopes","Well drained","C",0.75,3.5,6.05]
["NE055","Douglas","Urban land-Udorthents-Marshall complex, 0 to 9 percent slopes","Well drained","C",0.47500000000000003,3.5,5.8]
["NE055","Douglas","Urban land-Udorthents-Pohocco complex, 0 to 16 percent slopes","Well drained","B",0.5,6,7]
["NE055","Douglas","Wann-Caruso-Ingelwood complex, occasionally flooded","Somewhat poorly drained","C",0.75,63.15,7.2]
["NE057","Dundy",null,"",""]
["NE057","Dundy","Bankard sand, occasionally flooded","Somewhat excessively drained","A",0.375,88.4,8.1999999999999993]
["NE057","Dundy","Benkelman very fine sandy loam, 0 to 2 percent slopes","Well drained","B",0.25,61,8.8000000000000007]
["NE057","Dundy","Blackwood loam, 0 to 1 percent slopes","Well drained","B",1.5,33.299999999999997,8.1999999999999993]
["NE057","Dundy","Blackwood loam, 1 to 3 percent slopes","Well drained","B",1.5,33.299999999999997,8.1999999999999993]
["NE057","Dundy","Blanche loamy sand, 1 to 3 percent slopes","Well drained","B",0.375,62.5,7.6]
["NE057","Dundy","Blanche loamy sand, 3 to 6 percent slopes","Well drained","B",0.5,62.5,7.6]
["NE057","Dundy","Bolent-Almeria complex, channeled, frequently flooded","Poorly drained","B/D",0.25,84.5,7.6]
["NE057","Dundy","Calamus coarse sand, rarely flooded","Moderately well drained","A",0.25,94.6,7.6]
["NE057","Dundy","Colfer sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.25,82.2,7.3]
["NE057","Dundy","Craft very fine sandy loam, channeled, frequently flooded","Well drained","B",0.25,60.7,8.1999999999999993]
["NE057","Dundy","Craft very fine sandy loam, rarely flooded","Well drained","B",0.25,60.7,8.1999999999999993]
["NE057","Dundy","Dailey loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1,82.2,7]
["NE057","Dundy","Duroc loam, 0 to 1 percent slopes","Well drained","B",1.25,33.299999999999997,7.3]
["NE057","Dundy","Haigler very fine sandy loam, rarely flooded","Moderately well drained","B",0.25,71.199999999999989,8.8000000000000007]
["NE057","Dundy","Jayem loamy sand, 0 to 3 percent slopes","Well drained","A",1,62.5,7]
["NE057","Dundy","Kanorado silty clay loam, 6 to 9 percent slopes","Well drained","D",0.25,8,8.1999999999999993]
["NE057","Dundy","Keith silt loam, 1 to 3 percent slopes","Well drained","C",0.75,13.7,7]
["NE057","Dundy","Keith silt loam, 3 to 6 percent slopes, eroded","Well drained","C",0.75,13.7,7]
["NE057","Dundy","Laird fine sandy loam, 0 to 2 percent slopes","Well drained","B",0.25,62.5,8.1999999999999993]
["NE057","Dundy","Lodgepole silty clay loam, frequently ponded","Poorly drained","C/D",1.75,13.149999999999999,6.65]
["NE057","Dundy","Lodgepole silty clay loam, occasionally ponded","Somewhat poorly drained","C/D",1.5,7.6,7]
["NE057","Dundy","Otero fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.25,62.5,8.1999999999999993]
["NE057","Dundy","Overlake sand, 0 to 3 percent slopes","Well drained","B",0.25,81.150000000000006,8.5]
["NE057","Dundy","Sanborn loam, rarely flooded","Somewhat poorly drained","C",0.25,53.3,9.1]
["NE057","Dundy","Sarben loamy sand, 0 to 3 percent slopes","Well drained","A",0.25,62.5,7]
["NE057","Dundy","Sarben loamy sand, 3 to 6 percent slopes","Well drained","A",0.25,62.5,7]
["NE057","Dundy","Sarben loamy sand, 6 to 9 percent slopes","Well drained","A",0.25,62.5,7]
["NE057","Dundy","Sarben loamy sand, 9 to 30 percent slopes","Well drained","A",0.25,82.2,7.6]
["NE057","Dundy","Satanta fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,39.799999999999997,7.3]
["NE057","Dundy","Scoville loamy sand, calcareous, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,72.75,7.8999999999999995]
["NE057","Dundy","Sulco complex, 9 to 60 percent slopes","Well drained","B",0.25,43.6,8.1999999999999993]
["NE057","Dundy","Sulco fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.25,52.400000000000006,8.1999999999999993]
["NE057","Dundy","Sulco loam, 3 to 6 percent slopes","Well drained","B",0.25,43.6,8.8000000000000007]
["NE057","Dundy","Sulco loam, 6 to 9 percent slopes","Well drained","B",0.25,43.6,8.8000000000000007]
["NE057","Dundy","Sulco loam, 9 to 30 percent slopes","Well drained","B",0.25,43.6,8.1999999999999993]
["NE057","Dundy","Tassel-Ashollow-Rock outcrop complex, 9 to 60 percent slopes","Well drained","A",0.25,62.5,8.1999999999999993]
["NE057","Dundy","Ulysses loam, 1 to 3 percent slopes","Well drained","B",1,37.15,7.8999999999999995]
["NE057","Dundy","Ulysses loam, 3 to 6 percent slopes","Well drained","B",0.9,33.299999999999997,7.6]
["NE057","Dundy","Valent complex, rolling and hilly","Excessively drained","A",0.375,95,7]
["NE057","Dundy","Valent loamy sand, 3 to 9 percent slopes","Excessively drained","A",0.25,95,7]
["NE057","Dundy","Valent sand, 0 to 3 percent slopes","Excessively drained","A",0.25,95,7]
["NE057","Dundy","Valent sand, 3 to 9 percent slopes","Excessively drained","A",0.25,95,7]
["NE057","Dundy","Valent sand, rolling","Excessively drained","A",0.25,95,7]
["NE059","Fillmore",null,"",""]
["NE059","Fillmore","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE059","Fillmore","Butler silty clay loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.125,13.5,7.1]
["NE059","Fillmore","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE059","Fillmore","Crete silt loam, 1 to 3 percent slopes","Moderately well drained","C",1.625,19.2,6.25]
["NE059","Fillmore","Crete silt loam, 3 to 7 percent slopes","Moderately well drained","C",1.625,19.2,6.25]
["NE059","Fillmore","Crete silt loam, thick solum, 0 to 1 percent slopes","Moderately well drained","C",0.75,19.7,7.9]
["NE059","Fillmore","Crete silty clay loam, 0 to 1 percent slopes","Moderately well drained","C",1.25,17.600000000000001,6.7]
["NE059","Fillmore","Crete silty clay loam, 1 to 3 percent slopes","Moderately well drained","C",1.25,17.600000000000001,6.7]
["NE059","Fillmore","Crete silty clay loam, 3 to 7 percent slopes, eroded","Moderately well drained","C",1.5,18.7,6.7]
["NE059","Fillmore","Deroin silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,6.6,6.4]
["NE059","Fillmore","Fillmore silt loam, drained, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,12.649999999999999,7.1]
["NE059","Fillmore","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE059","Fillmore","Geary silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE059","Fillmore","Geary silty clay loam, 11 to 30 percent slopes","Well drained","C",1.25,6.9,6.7]
["NE059","Fillmore","Geary silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE059","Fillmore","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE059","Fillmore","Geary-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",1.75,10.4,7]
["NE059","Fillmore","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE059","Fillmore","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE059","Fillmore","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",1.625,22.5,6.55]
["NE059","Fillmore","Hastings silt loam, 7 to 11 percent slopes","Well drained","C",1.625,22.5,6.55]
["NE059","Fillmore","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.625,19.25,6.55]
["NE059","Fillmore","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.625,19.25,6.55]
["NE059","Fillmore","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE059","Fillmore","Hobbs silt loam, channeled, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE059","Fillmore","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE059","Fillmore","Holder silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.25,7.4,7]
["NE059","Fillmore","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE059","Fillmore","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE059","Fillmore","Kezan silt loam, channeled, frequently flooded","Poorly drained","C",1.875,8.1999999999999993,7.2]
["NE059","Fillmore","Massie silty clay loam, frequently ponded","Very poorly drained","D",1.25,6,6.4]
["NE059","Fillmore","Muir silt loam, 1 to 3 percent slopes","Well drained","B",2,7.3,6.7]
["NE059","Fillmore","Muir silt loam, 3 to 7 percent slopes","Well drained","B",2,7.3,6.7]
["NE059","Fillmore","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE059","Fillmore","Olbut-Butler silt loams, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.25,6,7.5]
["NE059","Fillmore","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE059","Fillmore","Scott silty clay loam, drained, frequently ponded","Poorly drained","D",1.5,18.7,6.7]
["NE059","Fillmore","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE059","Fillmore","Uly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,10.35,7]
["NE061","Franklin",null,"",""]
["NE061","Franklin","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE061","Franklin","Campus complex, 11 to 30 percent slopes","Well drained","C",0.25,37.9,7.6]
["NE061","Franklin","Canyon loam, 9 to 30 percent slopes","Well drained","D",0.75,43,7.9]
["NE061","Franklin","Canyon-Campus loams, 9 to 30 percent slopes","Well drained","C",0.5,39.75,7.75]
["NE061","Franklin","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE061","Franklin","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.8]
["NE061","Franklin","Coly-Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.6]
["NE061","Franklin","Coly-Uly silt loams, 3 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.6]
["NE061","Franklin","Coly-Uly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.8]
["NE061","Franklin","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE061","Franklin","Deroin soils, 6 to 11 percent slopes, severely eroded","Well drained","C",0.5,6.7,7]
["NE061","Franklin","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,23.5,7.2]
["NE061","Franklin","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE061","Franklin","Fluvaquents, frequently flooded","Very poorly drained","A/D",5,66.8,7.5]
["NE061","Franklin","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,44.85,3.75]
["NE061","Franklin","Gibbon silt loam, rarely flooded","Somewhat poorly drained","C",0.75,7.5,7.9]
["NE061","Franklin","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.125,10.4,7.1]
["NE061","Franklin","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE061","Franklin","Hersh-Valentine complex, 0 to 6 percent slopes","Well drained","A",0.25,87.3,6.7]
["NE061","Franklin","Hersh-Valentine complex, 6 to 11 percent slopes","Well drained","A",0.25,87.3,6.7]
["NE061","Franklin","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE061","Franklin","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE061","Franklin","Holdrege and Uly soils, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.4,7.2]
["NE061","Franklin","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.25,7.4]
["NE061","Franklin","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.4]
["NE061","Franklin","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.25,7.4]
["NE061","Franklin","Holdrege silt loam, 7 to 11 percent slopes","Well drained","C",0.75,9.25,7.4]
["NE061","Franklin","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE061","Franklin","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE061","Franklin","Inavale fine sandy loam, rarely flooded","Excessively drained","A",0.25,84.3,7.6]
["NE061","Franklin","Inavale loamy sand, rarely flooded","Excessively drained","A",0.25,84.9,7.6]
["NE061","Franklin","Kenesaw silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14,7.2]
["NE061","Franklin","Kenesaw silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14,7.2]
["NE061","Franklin","Kenesaw silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14,7.2]
["NE061","Franklin","Kipson complex, 7 to 30 percent slopes","Somewhat excessively drained","D",0.75,23.5,7.9]
["NE061","Franklin","McCook fine sandy loam, rarely flooded","Well drained","B",1,63.05,7.75]
["NE061","Franklin","McCook silt loam, rarely flooded","Well drained","B",1.75,36.6,7.75]
["NE061","Franklin","Munjor fine sandy loam, rarely flooded","Well drained","A",0.25,67.900000000000006,7.9]
["NE061","Franklin","Munjor loamy fine sand, rarely flooded","Well drained","A",0.25,87.6,7.9]
["NE061","Franklin","Nuckolls and Holdrege silt loams, 3 to 6 percent slopes","Well drained","C",0.75,9.1,7.2]
["NE061","Franklin","Nuckolls and Holdrege silt loams, 6 to 11 percent slopes","Well drained","C",0.75,9.1,7.2]
["NE061","Franklin","Nuckolls and Holdrege soils, 3 to 11 percent slopes, eroded","Well drained","C",0.75,9.1,7.2]
["NE061","Franklin","Nuckolls and Meadin soils, 11 to 30 percent slopes","Excessively drained","B",0.75,27.200000000000003,6.95]
["NE061","Franklin","Nuckolls-Hobbs complex, 11 to 30 percent slopes","Well drained","B",0.75,9.4499999999999993,7.2]
["NE061","Franklin","Rock Outcrop-Kipson complex, 7 to 45 percent slopes","Somewhat excessively drained","D",0.375,9.6,3.95]
["NE061","Franklin","Roxbury silt loam, rarely flooded","Well drained","B",1,9,7.9]
["NE061","Franklin","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE061","Franklin","Uly silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.5,7]
["NE061","Franklin","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE061","Franklin","Uly-Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.8]
["NE061","Franklin","Ustorthents, 3 to 30 percent slopes","Excessively drained","A",0.25,94.25,6.35]
["NE061","Franklin","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,7]
["NE061","Franklin","Valentine loamy fine sand, rolling","Excessively drained","A",0.25,87.3,7]
["NE061","Franklin","Valentine loamy sand, hilly","Excessively drained","A",0.25,87.3,6.5]
["NE061","Franklin","Valentine-Hersh complex, 11 to 30 percent slopes","Well drained","A",0.25,84.9,6.7]
["NE061","Franklin","Wann fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,66.2,8.1999999999999993]
["NE061","Franklin","Wann silt loam, rarely flooded","Somewhat poorly drained","C",0.75,66.2,8.1999999999999993]
["NE063","Frontier",null,"",""]
["NE063","Frontier","Barney soils, frequently flooded","Very poorly drained","B/D",1.625,67,7.35]
["NE063","Frontier","Blackwood silt loam, 0 to 1 percent slopes","Well drained","B",1.5,9.1,7.6]
["NE063","Frontier","Blackwood silt loam, 1 to 3 percent slopes","Well drained","B",1.5,9.5,7.6]
["NE063","Frontier","Blackwood silt loam, 3 to 6 percent slopes","Well drained","B",1.5,9.1,7.6]
["NE063","Frontier","Canyon-Sarben complex, 30 to 60 percent slopes","Well drained","D",0.75,62,7.2]
["NE063","Frontier","Canyon-Sulco-Rock outcrop complex, 17 to 60 percent slopes","Excessively drained","D",0.75,43.3,7.9]
["NE063","Frontier","Coly and Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE063","Frontier","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE063","Frontier","Coly silt loam, 6 to 11 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE063","Frontier","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE063","Frontier","Coly-Nuckolls silt loams, 11 to 30 percent slopes","Well drained","B",0.75,9.4,7.6]
["NE063","Frontier","Coly-Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE063","Frontier","Coly-Uly silt loams, 3 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE063","Frontier","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE063","Frontier","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",1.125,13,6.85]
["NE063","Frontier","Cozad silt loam, rarely flooded","Well drained","B",0.75,14.3,7.4]
["NE063","Frontier","Fillmore silt loam, occasionally ponded","Somewhat poorly drained","D",1.125,12.649999999999999,6.4]
["NE063","Frontier","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE063","Frontier","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.5,9.5,7]
["NE063","Frontier","Hall silt loam, 3 to 6 percent slopes","Well drained","C",1.5,9.5,7]
["NE063","Frontier","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7.5]
["NE063","Frontier","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE063","Frontier","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE063","Frontier","Holdrege and Keith silt loams, 1 to 3 percent slopes","Well drained","C",0.5,11.5,7.1]
["NE063","Frontier","Holdrege and Keith silt loams, 1 to 3 percent slopes, eroded","Well drained","C",0.5,11.5,7.1]
["NE063","Frontier","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE063","Frontier","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE063","Frontier","Holdrege silt loam, 1 to 3 percent slopes, eroded","Well drained","C",0.75,9.25,7.2]
["NE063","Frontier","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE063","Frontier","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.25,7.2]
["NE063","Frontier","Holdrege-Coly silt loams, 1 to 3 percent slopes, eroded","Well drained","B",1.375,9.4,7.75]
["NE063","Frontier","Holdrege-Coly silt loams, 3 to 7 percent slopes, eroded","Well drained","B",1.375,9.4,7.75]
["NE063","Frontier","Holdrege-Uly silt loams, 1 to 3 percent slopes","Well drained","C",0.75,9.4,7.2]
["NE063","Frontier","Holdrege-Uly silt loams, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.4,7.2]
["NE063","Frontier","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE063","Frontier","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE063","Frontier","Hord silt loam, 3 to 6 percent slopes","Well drained","B",1,9.3000000000000007,7]
["NE063","Frontier","Jayem loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.75,80,7.2]
["NE063","Frontier","Jayem loamy very fine sand, 1 to 3 percent slopes","Well drained","A",0.75,80,6.4]
["NE063","Frontier","Keith silt loam, 0 to 1 percent slopes","Well drained","C",0.75,13.7,7.3]
["NE063","Frontier","Keith silt loam, 1 to 3 percent slopes","Well drained","C",0.75,13.7,7.3]
["NE063","Frontier","Keith silt loam, 3 to 6 percent slopes","Well drained","C",0.75,13.7,7.3]
["NE063","Frontier","McCash loamy very fine sand, 0 to 3 percent slopes","Well drained","A",1.25,78.5,6.3]
["NE063","Frontier","McCash very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.25,60.3,7]
["NE063","Frontier","McCook silt loam, occasionally flooded","Well drained","B",1.75,12.75,7.5500000000000007]
["NE063","Frontier","McCook silt loam, rarely flooded","Well drained","B",1.875,12.95,7.5500000000000007]
["NE063","Frontier","McCook silt loam, wet, occasionally flooded","Somewhat poorly drained","B",1.75,12.95,7.5500000000000007]
["NE063","Frontier","Sarben loamy very fine sand, 20 to 60 percent slopes","Well drained","A",0.5,84,7.2]
["NE063","Frontier","Sarben loamy very fine sand, 3 to 6 percent slopes","Well drained","A",0.5,84,7.2]
["NE063","Frontier","Sarben loamy very fine sand, 3 to 9 percent slopes","Well drained","A",0.25,84,6.4]
["NE063","Frontier","Sarben loamy very fine sand, 6 to 9 percent slopes","Well drained","A",0.5,84,7.2]
["NE063","Frontier","Sulco silt loam, 30 to 60 percent slopes","Well drained","B",1,17.600000000000001,7.9]
["NE063","Frontier","Sulco silt loam, 9 to 30 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE063","Frontier","Sulco-Ulysses silt loams, 9 to 30 percent slopes, eroded","Well drained","B",1.25,13.6,7.9]
["NE063","Frontier","Uly and Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.6]
["NE063","Frontier","Uly and Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.6]
["NE063","Frontier","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE063","Frontier","Uly silt loam, 3 to 11 percent slopes","Well drained","B",0.75,9.5,7]
["NE063","Frontier","Uly silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE063","Frontier","Uly silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.5,7]
["NE063","Frontier","Uly-Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE063","Frontier","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE065","Furnas",null,"",""]
["NE065","Furnas","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE065","Furnas","Barney soils, frequently flooded","Very poorly drained","C/D",0.25,47.9,7.9]
["NE065","Furnas","Campus-Canyon loams, 11 to 30 percent slopes","Well drained","C",0.75,35.200000000000003,7.6]
["NE065","Furnas","Coly and Nuckolls silt loams, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.4,7.9]
["NE065","Furnas","Coly and Uly silt loams, 3 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE065","Furnas","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE065","Furnas","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE065","Furnas","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE065","Furnas","Coly-Nuckolls silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.4,7.6]
["NE065","Furnas","Coly-Nuckolls silt loams, 11 to 30 percent slopes","Well drained","B",0.75,9.4,7.6]
["NE065","Furnas","Coly-Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE065","Furnas","Coly-Uly silt loams, 3 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE065","Furnas","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE065","Furnas","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",1.125,35.700000000000003,7.3000000000000007]
["NE065","Furnas","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",1.125,35.700000000000003,7.3000000000000007]
["NE065","Furnas","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",1.125,35.700000000000003,7.3000000000000007]
["NE065","Furnas","Fillmore silty clay loam, occasionally ponded","Somewhat poorly drained","D",1.5,6.8,7.4]
["NE065","Furnas","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE065","Furnas","Gibbon silt loam, saline, occasionally flooded","Somewhat poorly drained","C",0.75,9.1,7.9]
["NE065","Furnas","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE065","Furnas","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE065","Furnas","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE065","Furnas","Hobbs-McCook silt loams, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE065","Furnas","Holdrege and Keith silt loams, 3 to 7 percent slopes, eroded","Well drained","C",0.5,11.5,7.1]
["NE065","Furnas","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,8.4,7.4]
["NE065","Furnas","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,8.4,7.4]
["NE065","Furnas","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,8.4,7.4]
["NE065","Furnas","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,8.4,7.4]
["NE065","Furnas","Holdrege-Coly silt loams, 1 to 3 percent slopes, eroded","Well drained","B",1.375,9.4,7.75]
["NE065","Furnas","Holdrege-Coly silt loams, 3 to 7 percent slopes, eroded","Well drained","B",1.375,9.4,7.75]
["NE065","Furnas","Holdrege-Uly silt loams, 1 to 3 percent slopes","Well drained","C",0.75,9.4,7.2]
["NE065","Furnas","Holdrege-Uly silt loams, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.4,7.2]
["NE065","Furnas","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,8.9,7]
["NE065","Furnas","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,8.9,7]
["NE065","Furnas","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,8.9,7]
["NE065","Furnas","Inavale soils, occasionally flooded","Excessively drained","A",0.25,92.2,7.9]
["NE065","Furnas","McCook silt loam, rarely flooded","Well drained","B",1.875,35.650000000000006,7.75]
["NE065","Furnas","Munjor fine sandy loam, rarely flooded","Well drained","A",0.25,82.6,7.9]
["NE065","Furnas","Nuckolls, Uly, and Canlon soils, 11 to 30 percent slopes","Well drained","D",0.75,9.4,7.5]
["NE065","Furnas","Uly silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.5,7]
["NE065","Furnas","Uly silt loam, 3 to 11 percent slopes","Well drained","B",0.75,9.5,7]
["NE065","Furnas","Uly silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.5,7]
["NE065","Furnas","Wann variant, fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,63.1,7.6]
["NE067","Gage",null,"",""]
["NE067","Gage","Burchard clay loam, 2 to 6 percent slopes","Well drained","C",0.75,34.799999999999997,7.3000000000000007]
["NE067","Gage","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE067","Gage","Burchard-Steinauer clay loams, 6 to 11 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE067","Gage","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","D",1.5,8,6.7]
["NE067","Gage","Chase silty clay loam, rarely flooded","Somewhat poorly drained","D",2.5,3,6.6]
["NE067","Gage","Cortland-Malmo complex, 6 to 11 percent slopes, eroded","Well drained","C",0.75,37.549999999999997,6.5]
["NE067","Gage","Deroin silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.5,6.6,6.4]
["NE067","Gage","Deroin silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,6.6,6.4]
["NE067","Gage","Edalgo silty clay loam, 11 to 20 percent slopes","Well drained","D",1.5,20,6.7]
["NE067","Gage","Filley fine sandy loam, 11 to 17 percent slopes","Well drained","A",0.75,67.599999999999994,5.8]
["NE067","Gage","Filley fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,67.599999999999994,5.8]
["NE067","Gage","Fluvaquents, silty, frequently flooded","Very poorly drained","B/D",2.5,3.9,3.75]
["NE067","Gage","Hedville cobbly loam, 7 to 30 percent slopes","Somewhat excessively drained","D",2.5,43.2,6.5]
["NE067","Gage","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE067","Gage","Kennebec silt loam, occasionally flooded","Moderately well drained","C",2,5,6.35]
["NE067","Gage","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,8,6.6]
["NE067","Gage","Kezan silt loam, channeled, frequently flooded","Poorly drained","B/D",2,7.05,7.2]
["NE067","Gage","Kezan silt loam, occasionally flooded","Poorly drained","B/D",2,7.3,7.2]
["NE067","Gage","Kipson-Sogn complex, 3 to 30 percent slopes","Somewhat excessively drained","D",1.375,8,7]
["NE067","Gage","Kipson-Sogn-Rock outcrop complex, 11 to 60 percent slopes","Somewhat excessively drained","D",0.75,8,7]
["NE067","Gage","Lancaster loam, 3 to 7 percent slopes","Well drained","C",1.5,42.1,6.1]
["NE067","Gage","Lancaster loam, 7 to 11 percent slopes","Well drained","C",1.5,42.1,6.1]
["NE067","Gage","Malmo clay loam, 2 to 6 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE067","Gage","Malmo, eroded-Pawnee complex, 6 to 11 percent slopes","Moderately well drained","D",0.75,29.9,7]
["NE067","Gage","Morrill loam, 11 to 17 percent slopes","Well drained","C",0.75,57,6.1]
["NE067","Gage","Muscotah silty clay loam, occasionally flooded","Somewhat poorly drained","C",2.25,4,6.8]
["NE067","Gage","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.5,6.7]
["NE067","Gage","Nodaway silt loam, channeled, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE067","Gage","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE067","Gage","Otoe silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE067","Gage","Padonia silty clay loam, 6 to 11 percent slopes","Well drained","D",2,7.7,7.2]
["NE067","Gage","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE067","Gage","Steinauer clay loam, 11 to 30 percent slopes","Well drained","C",0.75,33.5,8.1999999999999993]
["NE067","Gage","Steinauer clay loam, 30 to 50 percent slopes","Well drained","C",0.75,33.5,8.1999999999999993]
["NE067","Gage","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE067","Gage","Wymore silty clay loam, 2 to 6 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE067","Gage","Wymore silty clay loam, terrace, 0 to 2 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE069","Garden",null,"",""]
["NE069","Garden","Alliance loam, 0 to 1 percent slopes","Well drained","B",0.75,33.700000000000003,7.2]
["NE069","Garden","Alliance loam, 1 to 3 percent slopes","Well drained","B",0.75,37.4,7.2]
["NE069","Garden","Alliance-Rosebud loams, 1 to 3 percent slopes","Well drained","C",0.75,35.450000000000003,7.2]
["NE069","Garden","Almeria fine sandy loam, channeled, frequently flooded","Poorly drained","A/D",3.375,80.099999999999994,6.9]
["NE069","Garden","Ashollow-Tassel complex, 9 to 30 percent slopes","Well drained","A",0.75,63.3,7.9]
["NE069","Garden","Bankard loamy coarse sand, occasionally flooded","Somewhat excessively drained","A",0.75,80.900000000000006,7.5500000000000007]
["NE069","Garden","Bayard fine sandy loam, 0 to 1 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE069","Garden","Bayard fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE069","Garden","Bayard fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE069","Garden","Bayard loam, 0 to 1 percent slopes","Well drained","B",1.375,53.15,7.5500000000000007]
["NE069","Garden","Bayard very fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE069","Garden","Blanche loamy fine sand, 1 to 3 percent slopes","Well drained","B",0.75,66.5,7.2]
["NE069","Garden","Blueridge coarse sand, 6 to 30 percent slopes","Excessively drained","A",0.5,91.45,6.5]
["NE069","Garden","Broadwater loamy sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,84.3,7.2]
["NE069","Garden","Busher-Tassel complex, 3 to 9 percent slopes","Well drained","A",0.5,64.05,7.25]
["NE069","Garden","Busher-Tassel complex, 9 to 20 percent slopes","Well drained","A",0.5,64.05,7.25]
["NE069","Garden","Crowther loam, 0 to 1 percent slopes","Poorly drained","B/D",1.5,43.3,7.9]
["NE069","Garden","Crowther mucky peat","Very poorly drained","B/D",6.75,39.599999999999994,7.7]
["NE069","Garden","Dailey loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1.375,90.2,7.25]
["NE069","Garden","Dankworth loamy sand, 3 to 6 percent slopes","Excessively drained","A",0.5,90.7,6.7]
["NE069","Garden","Doughboy fine sandy loam, 0 to 3 percent slopes","Moderately well drained","A",2,50,7.9]
["NE069","Garden","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE069","Garden","Duroc loam, 0 to 1 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE069","Garden","Els fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,93.2,7.9]
["NE069","Garden","Elsmere loamy fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,79.400000000000006,7.9]
["NE069","Garden","Epping-Rock outcrop complex, 30 to 60 percent slopes","Well drained","D",0.375,30.65,3.75]
["NE069","Garden","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",5,95,7.5]
["NE069","Garden","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,91,7.2]
["NE069","Garden","Hoffland fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,78.2,7.5]
["NE069","Garden","Hoffland fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,78.2,7.5]
["NE069","Garden","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE069","Garden","Ipage fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",0.25,94.9,7.5]
["NE069","Garden","Jankosh loam, rarely flooded","Somewhat poorly drained","C",0.5,51.150000000000006,8.5]
["NE069","Garden","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE069","Garden","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE069","Garden","Jayem loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE069","Garden","Jayem loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE069","Garden","Keith loam, 1 to 3 percent slopes","Well drained","B",0.75,41.2,7]
["NE069","Garden","Keith loam, 3 to 6 percent slopes","Well drained","B",0.75,41.2,7]
["NE069","Garden","Kuma loam, 0 to 1 percent slopes","Well drained","C",2,36.9,7.5]
["NE069","Garden","Lemoyne sand, rarely flooded","Moderately well drained","C",0.75,90.6,8.5]
["NE069","Garden","Lewellen loam, rarely flooded","Somewhat poorly drained","C",0.75,63.2,8.5]
["NE069","Garden","Lewellen-McCuligan complex, rarely flooded","Somewhat poorly drained","C",0.75,67.3,8.1999999999999993]
["NE069","Garden","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",2,26.4,7]
["NE069","Garden","Lodgepole silt loam, occasionally ponded","Somewhat poorly drained","C/D",2,21,7]
["NE069","Garden","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7.5]
["NE069","Garden","Marlake mucky peat","Very poorly drained","A/D",14.625,42.25,6.6]
["NE069","Garden","Mitchell very fine sandy loam, 3 to 6 percent slopes","Well drained","B",1,60.5,7.9]
["NE069","Garden","Mitchell very fine sandy loam, 6 to 9 percent slopes","Well drained","B",1,60.5,7.9]
["NE069","Garden","Mitchell-Epping complex, 9 to 30 percent slopes","Well drained","D",0.75,60.5,7.9]
["NE069","Garden","Nenzel loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",1.25,86.8,6.7]
["NE069","Garden","Nenzel loamy fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",1.375,91.4,7.9]
["NE069","Garden","Rushcreek loam, rarely flooded","Moderately well drained","B",0.5,54.8,7.9]
["NE069","Garden","Sarben loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE069","Garden","Sarben loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE069","Garden","Sarben loamy fine sand, 6 to 9 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE069","Garden","Sarben loamy fine sand, 9 to 20 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE069","Garden","Scoville loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.25,78.599999999999994,7.2]
["NE069","Garden","Sidney loam, 3 to 6 percent slopes","Well drained","B",0.75,44.75,7.5500000000000007]
["NE069","Garden","Sidney-Canyon complex, 6 to 9 percent slopes","Well drained","D",0.75,44.3,7.9]
["NE069","Garden","Sulco loam, 30 to 60 percent slopes","Well drained","B",1,43.95,8.0500000000000007]
["NE069","Garden","Sulco-McConaughy complex, 3 to 6 percent slopes, eroded","Well drained","B",0.75,43.6,7.9]
["NE069","Garden","Sulco-McConaughy loams, 6 to 9 percent slopes, eroded","Well drained","B",0.75,43.6,7.9]
["NE069","Garden","Sulco-McConaughy loams, 9 to 30 percent slopes","Well drained","B",0.75,43.6,7.9]
["NE069","Garden","Tassel-Ashollow-Rock outcrop complex, 20 to 60 percent slopes","Well drained","A",0.75,63.3,7.9]
["NE069","Garden","Tassel-Busher-Rock outcrop complex, 9 to 60 percent slopes","Well drained","A",0.75,63.6,7]
["NE069","Garden","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,95,7.2]
["NE069","Garden","Valent fine sand, rolling","Excessively drained","A",0.5,95,7.2]
["NE069","Garden","Valent loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,94.4,7.2]
["NE069","Garden","Valent loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,94.4,7.2]
["NE069","Garden","Valent loamy fine sand, 6 to 9 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE069","Garden","Valentine complex, rolling and hilly","Excessively drained","A",0.5,94.9,7.2]
["NE069","Garden","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE069","Garden","Valentine fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE069","Garden","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,95.85,6.5]
["NE069","Garden","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE069","Garden","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,62,7]
["NE069","Garden","Wildhorse fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,94.550000000000011,9.1499999999999986]
["NE069","Garden","Wildhorse-Hoffland complex, 0 to 3 percent slopes","Poorly drained","A/D",1,93.2,8.6499999999999986]
["NE069","Garden","Wildhorse-Ipage, calcareous complex, 0 to 3 percent slopes","Moderately well drained","A",0.25,94.9,8.1999999999999993]
["NE071","Garfield",null,"",""]
["NE071","Garfield","Almeria fine sandy loam, channeled, frequently flooded","Very poorly drained","A/D",3.375,78.2,6.9]
["NE071","Garfield","Barney loam, channeled, frequently flooded","Very poorly drained","B/D",0.25,96,7.5]
["NE071","Garfield","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",1.5,11.3,7]
["NE071","Garfield","Coly-Hobbs silt loams, 3 to 60 percent slopes, moist","Well drained","B",2,17.5,7.35]
["NE071","Garfield","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,13.6,7]
["NE071","Garfield","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,13.6,7]
["NE071","Garfield","Els loamy sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,89.85,6.6]
["NE071","Garfield","Els-Ipage complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,95.15,6.35]
["NE071","Garfield","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE071","Garfield","Elsmere loamy fine sand, rarely flooded","Somewhat poorly drained","A",1.125,91.1,6.5]
["NE071","Garfield","Elsmere-Selia loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,86.35,8.1]
["NE071","Garfield","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",5,96,7.5]
["NE071","Garfield","Gates very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.5,58.6,7.5]
["NE071","Garfield","Gates very fine sandy loam, 11 to 30 percent slopes","Well drained","B",0.5,14.2,7.5]
["NE071","Garfield","Gates very fine sandy loam, 3 to 6 percent slopes, eroded","Well drained","B",0.5,58.6,7.5]
["NE071","Garfield","Gates very fine sandy loam, 6 to 11 percent slopes, eroded","Well drained","B",0.5,14.2,7.5]
["NE071","Garfield","Gibbon silt loam, rarely flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE071","Garfield","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE071","Garfield","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE071","Garfield","Hersh fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE071","Garfield","Hersh-Gates complex, 0 to 3 percent slopes","Well drained","B",0.625,62.349999999999994,7.35]
["NE071","Garfield","Hersh-Valentine complex, 11 to 24 percent slopes","Well drained","A",0.25,87.3,6.7]
["NE071","Garfield","Hersh-Valentine complex, 11 to 30 percent slopes","Well drained","A",0.75,66.900000000000006,6.7]
["NE071","Garfield","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,12.65,7]
["NE071","Garfield","Hord silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.1,7]
["NE071","Garfield","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,11.2,7]
["NE071","Garfield","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE071","Garfield","Ipage loamy fine sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,89.3,6.5]
["NE071","Garfield","Ipage loamy sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,89.6,6.2]
["NE071","Garfield","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,63.5,7.5]
["NE071","Garfield","Loup fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,79.2,6.6]
["NE071","Garfield","Loup fine sandy loam, occasionally flooded","Poorly drained","A/D",3.375,78.8,6.6]
["NE071","Garfield","Loup fine sandy loam, rarely flooded","Poorly drained","A/D",3.375,79.2,6.6]
["NE071","Garfield","Marlake loamy fine sand, frequently ponded","Very poorly drained","A/D",0.75,86.8,7.5]
["NE071","Garfield","Obert silt loam, occasionally flooded","Poorly drained","C/D",1.5,7.1,7.9]
["NE071","Garfield","Rusco variant silty clay loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",0.75,35.15,6.6]
["NE071","Garfield","Simeon loamy sand, 3 to 30 percent slopes","Excessively drained","A",0.5,87.3,7]
["NE071","Garfield","Tryon loamy fine sand, 0 to 3 percent slopes","Poorly drained","A/D",3.375,91.1,6.85]
["NE071","Garfield","Tryon loamy fine sand, frequently ponded","Very poorly drained","A/D",3.375,91.1,6.85]
["NE071","Garfield","Tryon-Ipage complex, 0 to 3 percent slopes","Moderately well drained","A",0.75,95.15,6.45]
["NE071","Garfield","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE071","Garfield","Uly silt loam, 11 to 17 percent slopes, eroded, moist","Well drained","B",0.69500000000000006,24.5,7.95]
["NE071","Garfield","Uly-Coly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",1.125,10.35,7.45]
["NE071","Garfield","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",1.125,10.35,7.45]
["NE071","Garfield","Uly-Coly silt loams, 17 to 30 percent slopes, eroded, moist","Well drained","B",1,24,7.5]
["NE071","Garfield","Uly-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",1.125,10.35,7.45]
["NE071","Garfield","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE071","Garfield","Valentine fine sand, rolling","Excessively drained","A",0.5,95.85,6.5]
["NE071","Garfield","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,95.85,6.5]
["NE071","Garfield","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,91.35,6.5]
["NE071","Garfield","Valentine loamy fine sand, rolling","Excessively drained","A",0.5,91.35,6.5]
["NE071","Garfield","Valentine-Els complex, 0 to 9 percent slopes","Somewhat poorly drained","A",0.5,95.4,6.5]
["NE071","Garfield","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE071","Garfield","Valentine-Ipage fine sands, 1 to 30 percent slopes","Moderately well drained","A",0.5,95.85,6.35]
["NE071","Garfield","Wann loam, rarely flooded","Somewhat poorly drained","C",0.75,63.1,8.1999999999999993]
["NE073","Gosper",null,"",""]
["NE073","Gosper","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE073","Gosper","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE073","Gosper","Anselmo fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE073","Gosper","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE073","Gosper","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE073","Gosper","Coly-Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE073","Gosper","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE073","Gosper","Cozad fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,14.3,7]
["NE073","Gosper","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",1.125,35.700000000000003,7.3000000000000007]
["NE073","Gosper","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.3,7.4]
["NE073","Gosper","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.3,7.4]
["NE073","Gosper","Cozad silt loam, rarely flooded","Well drained","B",0.75,14.3,7.4]
["NE073","Gosper","Fillmore silt loam, drained, frequently ponded","Somewhat poorly drained","D",1.125,12.649999999999999,7.1]
["NE073","Gosper","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE073","Gosper","Gosper loam, 0 to 1 percent slopes","Moderately well drained","B",0.75,61.55,7.7]
["NE073","Gosper","Gosper loam, saline-alkali, 0 to 1 percent slopes","Moderately well drained","C",0.75,43.2,7.9]
["NE073","Gosper","Gothenburg fine sandy loam, frequently flooded","Poorly drained","A/D",0.5,78.25,7.1]
["NE073","Gosper","Gothenburg soils, frequently flooded","Poorly drained","B/D",0.25,91.9,7.5]
["NE073","Gosper","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7.4]
["NE073","Gosper","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.5,9.5,7.4]
["NE073","Gosper","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7.5]
["NE073","Gosper","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7.5]
["NE073","Gosper","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,8.4,7.5500000000000007]
["NE073","Gosper","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,8.4,7.5500000000000007]
["NE073","Gosper","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,8.4,7.5500000000000007]
["NE073","Gosper","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,8.4,7.4]
["NE073","Gosper","Holdrege-Uly silt loams, 1 to 3 percent slopes","Well drained","C",0.75,9.4,7.2]
["NE073","Gosper","Holdrege-Uly silt loams, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.4,7.2]
["NE073","Gosper","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,8.9,7]
["NE073","Gosper","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,8.9,7]
["NE073","Gosper","Hord silt loam, wet substratum, 0 to 1 percent slopes","Somewhat poorly drained","C",0.75,9.1,7.9]
["NE073","Gosper","Lex loam, rarely flooded","Somewhat poorly drained","C",0.75,61,7.3]
["NE073","Gosper","Lex loam, saline-alkali, rarely flooded","Somewhat poorly drained","C",0.5,53.75,8.65]
["NE073","Gosper","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,67.3,7.5]
["NE073","Gosper","Scott silty clay loam, frequently ponded","Poorly drained","D",1.125,19.350000000000001,7.1]
["NE073","Gosper","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE073","Gosper","Uly silt loam, 3 to 11 percent slopes","Well drained","B",0.75,9.5,7]
["NE073","Gosper","Uly silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.5,7]
["NE073","Gosper","Uly-Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE073","Gosper","Ustorthents, 17 to 60 percent slopes","Well drained","B",0.75,6.8,7.9]
["NE075","Grant",null,"",""]
["NE075","Grant","Almeria loamy fine sand, channeled, frequently flooded","Very poorly drained","A/D",1.25,89.85,6.9]
["NE075","Grant","Crowther loam, 0 to 1 percent slopes","Poorly drained","B/D",1.125,37.200000000000003,7.7]
["NE075","Grant","Crowther mucky peat","Very poorly drained","B/D",6.75,38.5,7.7]
["NE075","Grant","Cullison loam, 0 to 1 percent slopes","Poorly drained","B/D",3,33.5,7.9]
["NE075","Grant","Cutcomb mucky peat","Very poorly drained","A/D",29,0,0]
["NE075","Grant","Dailey loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1.375,79.900000000000006,7.25]
["NE075","Grant","Dailey loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",1.375,79.900000000000006,7.25]
["NE075","Grant","Doger and Dunday loamy fine sands, 0 to 2 percent slopes","Well drained","A",1,87.05,6.85]
["NE075","Grant","Doger and Dunday loamy fine sands, 2 to 11 percent slopes","Well drained","A",1,87.05,6.85]
["NE075","Grant","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.75,86.8,6.7]
["NE075","Grant","Els calcareous-Hoffland complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.625,94.1,7.9]
["NE075","Grant","Els fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.7]
["NE075","Grant","Els fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,93.2,7.9]
["NE075","Grant","Els, calcareous-Hoffland complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,93.2,7.9]
["NE075","Grant","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE075","Grant","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.5]
["NE075","Grant","Elsmere loamy fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,7.9]
["NE075","Grant","Elsmere-Loup complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,91,6.7]
["NE075","Grant","Gannett mucky peat","Very poorly drained","B/D",0.5,42.55,6.5]
["NE075","Grant","Gannett-Loup fine sandy loams, 0 to 3 percent slopes","Very poorly drained","A/D",0.75,63.5,7.5]
["NE075","Grant","Gannett-Loup fine sandy loams, drained, 0 to 3 percent slopes","Poorly drained","A/D",0.75,63.5,7.5]
["NE075","Grant","Gus mucky peat","Very poorly drained","B/D",9.5,35.200000000000003,7]
["NE075","Grant","Hoffland fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,93.2,7.5]
["NE075","Grant","Hoffland fine sandy loam, frequently ponded","Very poorly drained","A/D",0.5,70.650000000000006,7.35]
["NE075","Grant","Ipage fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,7.5]
["NE075","Grant","Ipage-Els complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,96,6.5]
["NE075","Grant","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",3.375,79.2,6.6]
["NE075","Grant","Loup-Gannett loamy fine sands, drained, 0 to 3 percent slopes","Poorly drained","A/D",0.75,87,7.5]
["NE075","Grant","Loup-Gannett loamy fine sands, frequently ponded","Very poorly drained","A/D",0.75,87,7.5]
["NE075","Grant","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",0.5,72.150000000000006,6.85]
["NE075","Grant","Marlake mucky peat","Very poorly drained","A/D",14.625,42.25,6.6]
["NE075","Grant","Marlake, frequently ponded","Very poorly drained","A/D",0.5,70.849999999999994,7.5]
["NE075","Grant","Nenzel loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",1.25,86.8,6.7]
["NE075","Grant","Nenzel loamy fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",1.25,85.9,7.9]
["NE075","Grant","Ord loam, 0 to 3 percent slopes","Somewhat poorly drained","B",1.5,67,7.4]
["NE075","Grant","Tryon loamy fine sand, drained, 0 to 3 percent slopes","Poorly drained","A/D",3.375,91.1,6.85]
["NE075","Grant","Tryon loamy fine sand, frequently ponded","Very poorly drained","A/D",3.375,91.1,6.85]
["NE075","Grant","Valentine complex, rolling and hilly","Excessively drained","A",0.5,96.3,6.1]
["NE075","Grant","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,96.3,6.1]
["NE075","Grant","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.1]
["NE075","Grant","Valentine fine sand, hilly","Excessively drained","A",0.5,95.85,6.5]
["NE075","Grant","Valentine fine sand, rolling","Excessively drained","A",0.5,95.85,6.5]
["NE075","Grant","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,95.85,6.5]
["NE075","Grant","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.75,86.8,6.7]
["NE075","Grant","Valentine-Dunday complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.625,94,6.6]
["NE075","Grant","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.625,95.4,6.5]
["NE075","Grant","Valentine-Hoffland, complex, 0 to 24 percent slopes","Very poorly drained","A/D",0.625,94.1,7.15]
["NE075","Grant","Valentine-Tryon complex, 0 to 24 percent slopes","Very poorly drained","A/D",0.625,94.1,6.5]
["NE075","Grant","Wildhorse fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,92.95,9.1499999999999986]
["NE075","Grant","Wildhorse loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,90.1,9.1499999999999986]
["NE075","Grant","Wildhorse-Hoffland complex, 0 to 3 percent slopes","Poorly drained","A/D",2,94.9,9.1]
["NE075","Grant","Wildhorse-Ipage, calcareous complex, 0 to 3 percent slopes","Moderately well drained","A",0.25,94.9,8.1999999999999993]
["NE077","Greeley",null,"",""]
["NE077","Greeley","Almeria loamy fine sand, channeled, frequently flooded","Poorly drained","A/D",1.25,89.85,6.9]
["NE077","Greeley","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE077","Greeley","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE077","Greeley","Barney loam, channeled, frequently flooded","Poorly drained","B/D",0.25,47.9,7.5]
["NE077","Greeley","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.125,67,6.85]
["NE077","Greeley","Blendon loam, 0 to 2 percent slopes","Well drained","B",0.75,67.3,7]
["NE077","Greeley","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE077","Greeley","Cass fine sandy loam, rarely flooded","Well drained","A",1.125,65.55,6.9]
["NE077","Greeley","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE077","Greeley","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",1.125,11.3,7.45]
["NE077","Greeley","Coly-Hobbs silt loams, 3 to 60 percent slopes, moist","Well drained","B",2,17.5,7.35]
["NE077","Greeley","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE077","Greeley","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE077","Greeley","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE077","Greeley","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7.3]
["NE077","Greeley","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,82.9,6.85]
["NE077","Greeley","Dunday loamy fine sand, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,82.9,6.85]
["NE077","Greeley","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,40.85,3.75]
["NE077","Greeley","Gates silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.5,12.95,7.7]
["NE077","Greeley","Gates silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.5,12.95,7.7]
["NE077","Greeley","Gates silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.5,12.95,7.7]
["NE077","Greeley","Gates-Hersh complex, 0 to 3 percent slopes","Well drained","B",0.625,66.099999999999994,7.35]
["NE077","Greeley","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE077","Greeley","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.5,9.5,7]
["NE077","Greeley","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.5,66.5,6.95]
["NE077","Greeley","Hersh fine sandy loam, 11 to 17 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE077","Greeley","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE077","Greeley","Hersh fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE077","Greeley","Hersh-Gates complex, 17 to 30 percent slopes","Well drained","B",0.75,66.099999999999994,7.2]
["NE077","Greeley","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,11.3,7]
["NE077","Greeley","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE077","Greeley","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE077","Greeley","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE077","Greeley","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE077","Greeley","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.3500000000000014,7.2]
["NE077","Greeley","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.5,7.1,7.2]
["NE077","Greeley","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE077","Greeley","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE077","Greeley","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE077","Greeley","Hord-Uly complex, 0 to 6 percent slopes","Well drained","B",0.75,9,6.7]
["NE077","Greeley","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE077","Greeley","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE077","Greeley","Kenesaw very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,60.3,7.5]
["NE077","Greeley","Kenesaw very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,60.3,7.5]
["NE077","Greeley","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,11.6,7.5]
["NE077","Greeley","Loup loam, occasionally flooded","Poorly drained","B/D",3.375,70.150000000000006,6.6]
["NE077","Greeley","Saltine-Leshara silt loams, occasionally flooded","Somewhat poorly drained","C",1,11.3,8]
["NE077","Greeley","Scott silty clay loam, frequently ponded","Poorly drained","D",1.125,14.35,7.1]
["NE077","Greeley","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,87.3,7]
["NE077","Greeley","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE077","Greeley","Uly silt loam, 11 to 17 percent slopes, eroded, moist","Well drained","B",0.69500000000000006,24.5,7.95]
["NE077","Greeley","Uly silt loam, 11 to 30 percent slopes, eroded","Well drained","B",1,24,7.5]
["NE077","Greeley","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE077","Greeley","Uly-Coly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.73,24.5,7.9]
["NE077","Greeley","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE077","Greeley","Uly-Coly silt loams, 17 to 30 percent slopes, eroded, moist","Well drained","B",1,24,7.5]
["NE077","Greeley","Uly-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE077","Greeley","Uly-Holdrege silt loams, 7 to 11 percent slopes, eroded","Well drained","C",0.5,9.4,7.6]
["NE077","Greeley","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE077","Greeley","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE077","Greeley","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE077","Greeley","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,96.3,6.5]
["NE077","Greeley","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE077","Greeley","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE079","Hall",null,"",""]
["NE079","Hall","Alda loam, rarely flooded","Somewhat poorly drained","C",0.5,68.099999999999994,7.4]
["NE079","Hall","Alda sandy loam, rarely flooded","Somewhat poorly drained","B",0.5,65.75,7.35]
["NE079","Hall","Almeria loamy sand, frequently flooded","Poorly drained","A/D",0.25,96.5,6.5]
["NE079","Hall","Barney complex, channeled, frequently flooded","Poorly drained","C/D",0.75,44.3,7.3]
["NE079","Hall","Barney-Bolent complex, frequently flooded","Poorly drained","C/D",0.25,91.25,7.4]
["NE079","Hall","Blendon loam, 0 to 2 percent slopes","Well drained","B",1,67.900000000000006,6.8]
["NE079","Hall","Boelus, O'Neill, and Pivot complex, 0 to 3 percent slopes","Well drained","B",0.75,69.599999999999994,6.1]
["NE079","Hall","Bolent fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.25,73.2,7.3]
["NE079","Hall","Bolent loam, occasionally flooded","Somewhat poorly drained","C",0.25,62.8,7.9]
["NE079","Hall","Bolent loamy sand, occasionally flooded","Somewhat poorly drained","A",1,95.4,6.9]
["NE079","Hall","Bolent-Calamus complex, occasionally flooded","Somewhat poorly drained","C",0.25,95.4,7.1]
["NE079","Hall","Brocksburg loam, 0 to 2 percent slopes","Well drained","C",1.25,48.400000000000006,6.4499999999999993]
["NE079","Hall","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE079","Hall","Calamus loamy fine sand, rarely flooded","Moderately well drained","A",0.25,92.5,7]
["NE079","Hall","Caruso loam, rarely flooded","Somewhat poorly drained","C",0.5,51,7.3]
["NE079","Hall","Coly silt loam, 11 to 30 percent slopes","Well drained","B",0.875,21.3,7.9]
["NE079","Hall","Coly silt loam, 6 to 11 percent slopes","Well drained","B",1.125,8,7.9]
["NE079","Hall","Cozad loam, 0 to 1 percent slopes","Well drained","B",0.75,42.7,7]
["NE079","Hall","Cozad loam, sand substratum, 0 to 3 percent slopes","Well drained","B",1.375,47.45,6.35]
["NE079","Hall","Cozad, sand substratum-Hobbs, occasionally flooded, silt loams, 0 to 3 percent slopes","Well drained","B",2,10,7]
["NE079","Hall","Cullison fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,69.5,8.1999999999999993]
["NE079","Hall","Darr sandy loam, very rarely flooded","Somewhat excessively drained","A",1,66.550000000000011,6.3000000000000007]
["NE079","Hall","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,9.3000000000000007,7.2]
["NE079","Hall","Els-Tryon complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,81.8,6.2]
["NE079","Hall","Fillmore silty clay loam, occasionally ponded","Somewhat poorly drained","D",1.5,7.4,6.7]
["NE079","Hall","Fluvaquents, frequently flooded","Very poorly drained","A/D",5,23.5,7.5]
["NE079","Hall","Gates fine sandy loam, 0 to 3 percent slopes, hummocky","Well drained","B",0.5,52.95,6.3000000000000007]
["NE079","Hall","Gates silt loam, 0 to 1 percent slopes","Well drained","B",0.375,37.85,7.7]
["NE079","Hall","Gates silt loam, 1 to 3 percent slopes","Well drained","B",0.5,13.9,7.5]
["NE079","Hall","Gates silt loam, 3 to 6 percent slopes","Well drained","B",0.25,37.950000000000003,7.7]
["NE079","Hall","Gates silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.25,61.7,7.9]
["NE079","Hall","Gates silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.625,11.2,7.9]
["NE079","Hall","Gayville loam, rarely flooded","Somewhat poorly drained","C",0.25,14.3,8]
["NE079","Hall","Gibbon loam, saline, rarely flooded","Somewhat poorly drained","C",0.75,27,7.9]
["NE079","Hall","Gibbon silt loam, rarely flooded","Somewhat poorly drained","C",0.75,9.4,7.6]
["NE079","Hall","Gothenburg loam, frequently flooded","Poorly drained","B/D",0.5,81,7.2]
["NE079","Hall","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.75,16.5,7]
["NE079","Hall","Hall silt loam, 1 to 3 percent slopes, eroded","Well drained","C",1.25,17.2,7]
["NE079","Hall","Hall silt loam, sandy substratum, 0 to 1 percent slopes","Well drained","C",2,21.3,7]
["NE079","Hall","Hall silt loam. 3 to 6 percent slopes, eroded","Well drained","C",1.5,17.2,7]
["NE079","Hall","Hall, eroded-Hobbs, silt loams, 0 to 3 perent slopes","Well drained","C",2,11.3,7]
["NE079","Hall","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE079","Hall","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE079","Hall","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.5,6.95,7.0500000000000007]
["NE079","Hall","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.5,6.95,7.0500000000000007]
["NE079","Hall","Hersh fine sandy loam, silty substratum, 3 to 6 percent slopes","Well drained","A",0.25,69.599999999999994,7.2]
["NE079","Hall","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.75,11.4,7.5]
["NE079","Hall","Hobbs silt loam, occasionally flooded","Well drained","B",3,11.3,7]
["NE079","Hall","Holder loam, 0 to 3 percent slopes, overblown","Well drained","C",1.625,9.0500000000000007,7]
["NE079","Hall","Holder silt loam, 0 to 1 percent slopes","Well drained","C",0.75,10,6.6]
["NE079","Hall","Holder silt loam, 1 to 3 percent slopes","Well drained","C",0.75,10,6.6]
["NE079","Hall","Holder silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,6.9,7]
["NE079","Hall","Holder silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.25,6.7,7.5]
["NE079","Hall","Holdrege silt loam, 1 to 3 percent slopes, overblown","Well drained","C",2,7,7.2]
["NE079","Hall","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,7,7.2]
["NE079","Hall","Hord silt loam, 0 to 1 percent slopes","Well drained","B",2,7,7]
["NE079","Hall","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,7,7]
["NE079","Hall","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,7,7]
["NE079","Hall","Hord silt loam, sandy substratum, 0 to 1 percent slopes","Well drained","C",2.5,11.3,7]
["NE079","Hall","Inavale fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,82,6.7]
["NE079","Hall","Inavale loamy fine sand, very rarely flooded","Excessively drained","A",0.25,87.3,7]
["NE079","Hall","Inavale loamy sand, 3 to 11 percent slopes, very rarely flooded","Excessively drained","A",0.25,87.3,7.2]
["NE079","Hall","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,88,6]
["NE079","Hall","Ipage-Tryon, wet, complex, silty substratum, 0 to 3 percent slopes","Moderately well drained","A",0.25,95.4,5.85]
["NE079","Hall","Jansen fine sandy loam, overblown, leveled","Well drained","C",0.5,65.900000000000006,6.3]
["NE079","Hall","Janude loam, calcareous, rarely flooded","Moderately well drained","B",0.9,66.599999999999994,7.6]
["NE079","Hall","Janude sandy loam, very rarely flooded","Moderately well drained","B",0.75,66.599999999999994,7.3]
["NE079","Hall","Lamo silt loam, sand substratum, 0 to 1 percent slope","Poorly drained","C",1.5,9.4,7.6]
["NE079","Hall","Leshara and Gibbon silt loams","Somewhat poorly drained","C",0.75,11.350000000000001,7.7]
["NE079","Hall","Lex silt loam, rarely flooded","Somewhat poorly drained","C",1.375,41.6,8.1999999999999993]
["NE079","Hall","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","C/D",0.25,9.6999999999999993,5.9]
["NE079","Hall","Lockton loam","Moderately well drained","B",2,41.6,6.5]
["NE079","Hall","Loup fine sandy loam, loamy substratum, 0 to 2 percent slopes","Poorly drained","A/D",0.75,79.5,7.5]
["NE079","Hall","Loup loam, 0 to 3 percent slopes","Very poorly drained","B/D",0.75,79,6.5]
["NE079","Hall","Marlake loamy fine sand, frequently ponded","Very poorly drained","A/D",0.25,78.2,6.3]
["NE079","Hall","O'Neill and Pivot loams, 0 to 2 percent slopes","Well drained","B",0.75,70,6.8]
["NE079","Hall","O'Neill sandy loam, 2 to 6 percent slopes","Well drained","B",1.375,73.699999999999989,6.55]
["NE079","Hall","Ortello fine sandy loam, silty substratum, 0 to 3 percent slopes","Well drained","A",0.75,69.599999999999994,7.1]
["NE079","Hall","Ortello loam, 0 to 1 percent slopes","Well drained","B",0.75,69.599999999999994,6.8]
["NE079","Hall","Ortello, silty substratum-Holder, overblown complex, 0 to 3 percent slopes","Well drained","C",1,36.950000000000003,7.1]
["NE079","Hall","Ovina fine sandy loam","Somewhat poorly drained","B/D",0.875,55.8,8.1499999999999986]
["NE079","Hall","Platte-Alda loams, channeled, frequently flooded","Somewhat poorly drained","C",0.5,55.1,7.25]
["NE079","Hall","Platte-Bolent complex, occasionally flooded","Somewhat poorly drained","B",0.25,66.900000000000006,7.45]
["NE079","Hall","Platte-Inavale complex, 0 to 6 percent slopes, occasionally flooded","Excessively drained","A",0.25,87.3,7.2]
["NE079","Hall","Scott silty clay loam, frequently ponded","Poorly drained","D",1.5,8,6.7]
["NE079","Hall","Silver Creek complex, saline-alkali, rarely flooded","Somewhat poorly drained","D",1,26,8.3000000000000007]
["NE079","Hall","Silver Creek fine sandy loam, overblown, occasionally ponded","Poorly drained","C/D",0.5,39.200000000000003,9]
["NE079","Hall","Simeon sandy loam, 0 to 3 percent slopes","Excessively drained","A",0.25,83.2,6.2]
["NE079","Hall","Thurman fine sandy loam, 0 to 2 percent slopes","Somewhat excessively drained","A",0.875,63.3,6.7]
["NE079","Hall","Thurman loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE079","Hall","Thurman loamy fine sand, loamy substratum, 0 to 3 percent slopes","Somewhat excessively drained","A",1,80.2,6.5]
["NE079","Hall","Thurman loamy fine sand, loamy substratum, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,73.900000000000006,6.9]
["NE079","Hall","Thurman-Valentine loamy fine sands, terrace, 0 to 2 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE079","Hall","Uly and Holdrege silt loams, 6 to 11 percent slopes","Well drained","C",0.75,9.4,7.2]
["NE079","Hall","Uly silt loam, 1 to 3 percent slopes, eroded","Well drained","B",0.75,17,7]
["NE079","Hall","Uly silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.5,17.100000000000001,7.45]
["NE079","Hall","Uly, eroded-Coly silt loams, 11 to 17 percent slopes","Well drained","B",0.75,21.25,7.9]
["NE079","Hall","Uly, eroded-Coly silt loams, 6 to 11 percent slopes","Well drained","B",1.25,21.3,7.9]
["NE079","Hall","Uly, eroded-Hobbs silt loams, 2 to 40 percent slopes","Well drained","B",2,17.049999999999997,7]
["NE079","Hall","Uly, Holdrege, and Coly soils, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.4,7.2]
["NE079","Hall","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.2]
["NE079","Hall","Valentine fine sand, rolling","Excessively drained","A",0.25,96.3,5.9499999999999993]
["NE079","Hall","Valentine fine sand, rolling and hilly","Excessively drained","A",0.25,96.3,6.3]
["NE079","Hall","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.4]
["NE079","Hall","Valentine loamy fine sand, loamy substratum, 0 to 3 percent slopes","Excessively drained","A",0.5,80.3,6.1]
["NE079","Hall","Valentine loamy fine sand, rolling","Excessively drained","A",0.25,96.3,6.35]
["NE079","Hall","Valentine-Libory complex, 0 to 9 percent slopes","Moderately well drained","A",0.25,83.5,6.3]
["NE079","Hall","Valentine-Tryon, silty substratum, complex, 0 to 9 percent slopes","Very poorly drained","A/D",0.25,95.4,6.4]
["NE079","Hall","Wann loam, rarely flooded","Somewhat poorly drained","C",0.5,51.05,7.5500000000000007]
["NE079","Hall","Wann sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,68.900000000000006,7.2]
["NE079","Hall","Wood River silt loam, 0 to 1 percent slopes","Moderately well drained","C",0.75,22.4,7.4]
["NE079","Hall","Wood River-Silver Creek fine sandy loams, 0 to 1 percent slopes","Somewhat poorly drained","D",0.25,18.899999999999999,8.3000000000000007]
["NE079","Hall","Wood River-Silver Creek silt loams, 0 to 1 percent slopes","Somewhat poorly drained","D",0.625,18.5,7.4]
["NE081","Hamilton",null,"",""]
["NE081","Hamilton","Alda loam, occasionally flooded","Somewhat poorly drained","B/D",0.5,75.5,7.5]
["NE081","Hamilton","Alda sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,67.8,7.5]
["NE081","Hamilton","Barney loam, frequently flooded","Very poorly drained","B/D",0.25,47.9,7.5]
["NE081","Hamilton","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,7.4,6.7]
["NE081","Hamilton","Coly silt loam, 11 to 30 percent slopes","Somewhat excessively drained","B",1.125,11.3,7.9]
["NE081","Hamilton","Coly silt loam, 30 to 60 percent slopes","Excessively drained","B",1.125,11.3,7.9]
["NE081","Hamilton","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE081","Hamilton","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",1.125,11,6.85]
["NE081","Hamilton","Cozad silt loam, rarely flooded","Well drained","B",1.125,11,6.85]
["NE081","Hamilton","Cozad silt loam, wet substratum, rarely flooded","Moderately well drained","B",1.25,29,6.7]
["NE081","Hamilton","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE081","Hamilton","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,10,7.2]
["NE081","Hamilton","Detroit silt loam, terrace, 0 to 1 percent slopes","Moderately well drained","D",1.5,7.1,7.2]
["NE081","Hamilton","Detroit silt loam, terrace, 1 to 3 percent slopes","Moderately well drained","D",1.5,7.1,7.2]
["NE081","Hamilton","Fillmore silt loam, drained, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,12.649999999999999,7.1]
["NE081","Hamilton","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",0.5,6,7]
["NE081","Hamilton","Fonner variant loamy sand, occasionally flooded","Moderately well drained","A",0.25,85.5,6.7]
["NE081","Hamilton","Geary silt loam, 11 to 30 percent slopes","Somewhat excessively drained","C",2,9.1,6.1]
["NE081","Hamilton","Geary silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE081","Hamilton","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE081","Hamilton","Gothenburg loam, frequently flooded","Poorly drained","B/D",0.5,81,7.2]
["NE081","Hamilton","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,95,7.2]
["NE081","Hamilton","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.5,83.6,7.35]
["NE081","Hamilton","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",0.625,6.95,7.0500000000000007]
["NE081","Hamilton","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",0.625,6.95,7.0500000000000007]
["NE081","Hamilton","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.5,6.95,7.0500000000000007]
["NE081","Hamilton","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.5,6.95,7.0500000000000007]
["NE081","Hamilton","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,11.3,7]
["NE081","Hamilton","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE081","Hamilton","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE081","Hamilton","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE081","Hamilton","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE081","Hamilton","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE081","Hamilton","Hord silt loam, rarely flooded","Well drained","B",0.75,9.3000000000000007,7]
["NE081","Hamilton","Inavale loamy sand, rarely flooded","Somewhat excessively drained","A",0.25,84.9,6.7]
["NE081","Hamilton","Massie silt loam, frequently ponded","Very poorly drained","D",1,12.850000000000001,6.85]
["NE081","Hamilton","Ortello fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE081","Hamilton","Ortello fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE081","Hamilton","Ortello loam, loamy substratum, 0 to 1 percent slopes","Well drained","B",0.25,55.95,6.7]
["NE081","Hamilton","Ortello loam, loamy substratum, 1 to 3 percent slopes","Well drained","B",0.25,45,6.7]
["NE081","Hamilton","Ortello, silty substratum-Holder, overblown complex, 0 to 3 percent slopes","Well drained","C",1,36.950000000000003,7.1]
["NE081","Hamilton","Platte loam, occasionally flooded","Somewhat poorly drained","B/D",0.25,67.3,7.5]
["NE081","Hamilton","Rusco silt loam, 0 to 1 percent slopes","Moderately well drained","C/D",0.75,11.2,7]
["NE081","Hamilton","Scott silt loam, frequently ponded","Poorly drained","D",1.125,23.4,7.1]
["NE081","Hamilton","Scott silty clay loam, drained, frequently ponded","Poorly drained","D",1.5,20,6.7]
["NE081","Hamilton","Thurman fine sandy loam, 11 to 30 percent slopes","Somewhat excessively drained","A",0.875,75.900000000000006,6.5]
["NE081","Hamilton","Thurman fine sandy loam, 2 to 11 percent slopes","Somewhat excessively drained","A",0.875,75.900000000000006,6.5]
["NE081","Hamilton","Uly silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.5,7]
["NE081","Hamilton","Uly silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.5,7]
["NE081","Hamilton","Uly silt loam, 1 to 3 percent slopes, eroded","Well drained","B",0.75,17,7]
["NE081","Hamilton","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE081","Hamilton","Uly silt loam, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE081","Hamilton","Uly silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.5,7]
["NE081","Hamilton","Uly silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.5,17.100000000000001,7.45]
["NE083","Harlan",null,"",""]
["NE083","Harlan","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,15,7.3000000000000007]
["NE083","Harlan","Coly and Hobbs silt loams","Well drained","B",1.125,11.3,7.9]
["NE083","Harlan","Coly and Nuckolls silt loams, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.4,7.9]
["NE083","Harlan","Coly and Uly silt loams, 3 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE083","Harlan","Coly-Nuckolls silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.4,7.6]
["NE083","Harlan","Coly-Nuckolls silt loams, 11 to 30 percent slopes","Well drained","B",0.75,9.4,7.6]
["NE083","Harlan","Coly-Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE083","Harlan","Coly-Uly silt loams, 3 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE083","Harlan","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE083","Harlan","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE083","Harlan","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7]
["NE083","Harlan","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE083","Harlan","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,23.5,7.2]
["NE083","Harlan","Fluvaquents, frequently flooded","Very poorly drained","A/D",2.5,18.95,3.75]
["NE083","Harlan","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,44.85,3.75]
["NE083","Harlan","Hobbs and McCook silt loams, occasionally flooded","Well drained","B",1.875,11.3,7.75]
["NE083","Harlan","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE083","Harlan","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE083","Harlan","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE083","Harlan","Hobbs-McCook silt loams, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE083","Harlan","Holdrege and Uly soils, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.4,7.4]
["NE083","Harlan","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,8.4,7.4]
["NE083","Harlan","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.4]
["NE083","Harlan","Holdrege silt loam, 1 to 3 percent slopes, eroded","Well drained","C",0.75,8.4,7.4]
["NE083","Harlan","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,8.4,7.4]
["NE083","Harlan","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,8.4,7.6]
["NE083","Harlan","Holdrege-Coly silt loams, 3 to 7 percent slopes, eroded","Well drained","B",1.375,9.4,7.75]
["NE083","Harlan","Hord and Hall silt loams, 0 to 1 percent slopes","Well drained","C",0.75,9.3000000000000007,7.2]
["NE083","Harlan","Hord and Hall silt loams, 1 to 3 percent slopes","Well drained","C",0.75,9.3000000000000007,7.2]
["NE083","Harlan","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,8.9,7]
["NE083","Harlan","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,8.9,7]
["NE083","Harlan","Inavale fine sandy loam, 0 to 3 percent slopes","Excessively drained","A",0.25,84.3,7.8]
["NE083","Harlan","Inavale fine sandy loam, rarely flooded","Excessively drained","A",0.25,84.3,7.6]
["NE083","Harlan","Inavale soils, occasionally flooded","Excessively drained","A",0.25,92.2,7.9]
["NE083","Harlan","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.5,34.599999999999994,7.9]
["NE083","Harlan","Massie silty clay loam, frequently ponded","Very poorly drained","D",3.125,16.75,6.25]
["NE083","Harlan","McCook loam, occasionally flooded","Well drained","B",1.75,50.3,7.7]
["NE083","Harlan","McCook sand, occasionally flooded","Well drained","B",1,77.8,7.95]
["NE083","Harlan","McCook silt loam, rarely flooded","Well drained","B",1.875,35.650000000000006,7.75]
["NE083","Harlan","Munjor fine sandy loam, rarely flooded","Well drained","A",0.25,66.5,7.9]
["NE083","Harlan","Munjor loamy fine sand, rarely flooded","Moderately well drained","A",0.25,80.7,7.9]
["NE083","Harlan","Nuckolls and Uly silt loams, 11 to 17 percent slopes","Well drained","B",0.75,9.25,7.35]
["NE083","Harlan","Nuckolls and Uly silt loams, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.25,7.35]
["NE083","Harlan","Nuckolls, Uly, and Canlon soils, 11 to 30 percent slopes","Well drained","D",0.75,9.4,7.5]
["NE083","Harlan","Nuckolls-Hobbs complex, 11 to 30 percent slopes","Well drained","B",0.75,9.4499999999999993,7.2]
["NE083","Harlan","Platte and McCook soils","Well drained","B",0.5,59.6,7.9]
["NE083","Harlan","Scott silt loam, frequently ponded","Poorly drained","D",1.125,21.1,7.1]
["NE083","Harlan","Uly and Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE083","Harlan","Uly silt loam, 3 to 11 percent slopes","Well drained","B",0.75,9.5,7.5]
["NE083","Harlan","Uly silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.5,7]
["NE083","Harlan","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE085","Hayes",null,"",""]
["NE085","Hayes","Bankard loamy sand, occasionally flooded","Somewhat excessively drained","A",0.75,89.25,7.7]
["NE085","Hayes","Blackwood loam, 0 to 1 percent slopes","Well drained","B",1.5,33.299999999999997,8.1999999999999993]
["NE085","Hayes","Blackwood silt loam, 0 to 1 percent slopes","Well drained","B",1.5,9.1,7.6]
["NE085","Hayes","Blackwood silt loam, 1 to 3 percent slopes","Well drained","B",1.5,9.5,7.6]
["NE085","Hayes","Blackwood silt loam, 3 to 6 percent slopes","Well drained","B",1.5,9.1,7.6]
["NE085","Hayes","Bridget silt loam, 0 to 1 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE085","Hayes","Bridget silt loam, 1 to 3 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE085","Hayes","Bridget silt loam, 3 to 6 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE085","Hayes","Canyon-Sulco-Rock outcrop complex, 17 to 60 percent slopes","Excessively drained","D",0.75,43.3,7.9]
["NE085","Hayes","Coly silt loam, 17 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE085","Hayes","Duroc silt loam, 0 to 1 percent slopes","Well drained","B",2,9.5,7.2]
["NE085","Hayes","Duroc silt loam, 1 to 3 percent slopes","Well drained","B",2,9.5,7.2]
["NE085","Hayes","Fluvaquents, silty, frequently flooded","Very poorly drained","B/D",2.5,11.75,3.75]
["NE085","Hayes","Gannett silt loam, occasionally flooded","Very poorly drained","B/D",2.875,37.25,7.9]
["NE085","Hayes","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,14.3,7.9]
["NE085","Hayes","Glenberg fine sandy loam, rarely flooded","Well drained","A",0.75,73.8,7.9]
["NE085","Hayes","Haigler and Sanborn loams, rarely flooded","Moderately well drained","B",0.75,64.25,8.1999999999999993]
["NE085","Hayes","Jayem loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE085","Hayes","Jayem loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.75,80,7.2]
["NE085","Hayes","Jayem loamy very fine sand, 3 to 6 percent slopes","Well drained","A",1.1499999999999999,80.75,7.2]
["NE085","Hayes","Keith silt loam, 0 to 1 percent slopes","Well drained","C",0.75,13.7,7.3]
["NE085","Hayes","Keith silt loam, 1 to 3 percent slopes","Well drained","C",0.75,13.7,7.3]
["NE085","Hayes","Keith silt loam, 3 to 6 percent slopes","Well drained","C",0.75,13.7,7.3]
["NE085","Hayes","McCash very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.25,60.3,7]
["NE085","Hayes","McCash very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.25,60.3,7]
["NE085","Hayes","McCook silt loam, channeled, occasionally flooded","Well drained","B",1.75,36.6,7.9]
["NE085","Hayes","McCook silt loam, occasionally flooded","Well drained","B",0.5,36.900000000000006,7.9]
["NE085","Hayes","McCook silt loam, rarely flooded","Well drained","B",0.5,14.2,7.9]
["NE085","Hayes","Sarben loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.5,84,7.2]
["NE085","Hayes","Sarben loamy very fine sand, 20 to 60 percent slopes","Well drained","A",0.5,84,7.2]
["NE085","Hayes","Sarben loamy very fine sand, 3 to 6 percent slopes","Well drained","A",0.5,84,7.2]
["NE085","Hayes","Sarben loamy very fine sand, 6 to 9 percent slopes","Well drained","A",0.5,84,7.2]
["NE085","Hayes","Sarben loamy very fine sand, 9 to 20 percent slopes","Well drained","A",0.5,84,7.2]
["NE085","Hayes","Scott variant silty clay loam, frequently ponded","Poorly drained","C/D",2,7,7.2]
["NE085","Hayes","Sulco complex, 9 to 60 percent slopes","Well drained","B",0.25,43.6,8.1999999999999993]
["NE085","Hayes","Sulco silt loam, 30 to 60 percent slopes","Well drained","B",1,17.600000000000001,7.9]
["NE085","Hayes","Sulco silt loam, 6 to 9 percent slopes","Well drained","B",1,17.600000000000001,7.9]
["NE085","Hayes","Sulco silt loam, 9 to 30 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE085","Hayes","Sulco-Ulysses silt loams, 9 to 30 percent slopes, eroded","Well drained","B",1.25,13.6,7.9]
["NE085","Hayes","Ulysses silt loam, 3 to 6 percent slopes","Well drained","B",1.5,9.5,7.9]
["NE085","Hayes","Ulysses silt loam, 6 to 9 percent slopes, eroded","Well drained","B",1.5,9.5,7.9]
["NE085","Hayes","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE085","Hayes","Valent fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE085","Hayes","Valent fine sand, rolling and hilly","Excessively drained","A",0.5,94.9,7.2]
["NE085","Hayes","Valent sand, rolling","Excessively drained","A",0.5,95,7]
["NE087","Hitchcock",null,"",""]
["NE087","Hitchcock","Bankard loamy fine sand, rarely flooded","Somewhat excessively drained","A",0.75,93.6,7.9]
["NE087","Hitchcock","Barney loam, occasionally flooded","Poorly drained","B/D",0.25,91.6,7.5]
["NE087","Hitchcock","Bayard fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE087","Hitchcock","Bayard fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE087","Hitchcock","Bayard loam, 0 to 1 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE087","Hitchcock","Benkelman very fine sandy loam, 0 to 2 percent slopes","Well drained","B",0.25,61,8.8000000000000007]
["NE087","Hitchcock","Blackwood loam, 0 to 1 percent slopes","Well drained","B",1.5,33.299999999999997,8.1999999999999993]
["NE087","Hitchcock","Blackwood loam, 1 to 3 percent slopes","Well drained","B",1.5,33.299999999999997,8.1999999999999993]
["NE087","Hitchcock","Blackwood silt loam, 0 to 1 percent slopes","Well drained","B",1.25,11.6,7.6]
["NE087","Hitchcock","Blackwood silt loam, 1 to 3 percent slopes","Well drained","B",1.5,9.5,7.6]
["NE087","Hitchcock","Bolent-Almeria complex, channeled, frequently flooded","Poorly drained","B/D",0.25,84.5,7.6]
["NE087","Hitchcock","Bridget silt loam, 0 to 1 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE087","Hitchcock","Bridget silt loam, 1 to 3 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE087","Hitchcock","Bridget silt loam, 3 to 6 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE087","Hitchcock","Canyon soils, 30 to 50 percent slopes","Well drained","D",1.25,43,7.9]
["NE087","Hitchcock","Craft loam, channeled, frequently flooded","Well drained","B",0.25,42.7,7.9]
["NE087","Hitchcock","Craft very fine sandy loam, channeled, frequently flooded","Well drained","B",0.25,60.7,8.1999999999999993]
["NE087","Hitchcock","Craft very fine sandy loam, rarely flooded","Well drained","B",0.25,60.7,8.1999999999999993]
["NE087","Hitchcock","Duroc silt loam, terrace, 0 to 1 percent slopes","Well drained","B",2,9.5,7.2]
["NE087","Hitchcock","Duroc silt loam, terrace, 1 to 3 percent slopes","Well drained","B",2,9.5,7.2]
["NE087","Hitchcock","Dwyer-Valent loamy fine sands, 3 to 17 percent slopes","Excessively drained","A",0.75,86.8,7.5]
["NE087","Hitchcock","Glenberg fine sandy loam, rarely flooded","Well drained","A",0.75,73.8,7.9]
["NE087","Hitchcock","Haigler and Sanborn loams, rarely flooded","Moderately well drained","B",0.75,64.25,8.1999999999999993]
["NE087","Hitchcock","Haigler fine sandy loam, 0 to 1 percent slopes","Moderately well drained","A",0.25,80.3,8.5]
["NE087","Hitchcock","Haigler very fine sandy loam, rarely flooded","Moderately well drained","B",0.25,71.199999999999989,8.8000000000000007]
["NE087","Hitchcock","Haverson fine sandy loam, rarely flooded","Well drained","B",1,63.3,7.9]
["NE087","Hitchcock","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE087","Hitchcock","Inavale soils, frequently flooded","Excessively drained","A",0.5,88.550000000000011,7.1]
["NE087","Hitchcock","Jayem fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,63.5,7.2]
["NE087","Hitchcock","Jayem fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,63.5,7.2]
["NE087","Hitchcock","Jayem loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,78.2,7.2]
["NE087","Hitchcock","Keith and Blackwood silt loams, 0 to 1 percent slopes","Well drained","B",1,12.6,7.3]
["NE087","Hitchcock","Keith silt loam, 0 to 1 percent slopes","Well drained","C",0.75,13.7,7.3]
["NE087","Hitchcock","Keith silt loam, 1 to 3 percent slopes","Well drained","B",0.75,13.7,7]
["NE087","Hitchcock","Keith silt loam, 1 to 3 percent slopes, eroded","Well drained","B",0.75,13.7,7]
["NE087","Hitchcock","Keith silt loam, 3 to 6 percent slopes","Well drained","B",0.75,13.7,7]
["NE087","Hitchcock","Keith silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,13.7,7]
["NE087","Hitchcock","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",2,26.4,7]
["NE087","Hitchcock","McCook loam, frequently flooded","Well drained","B",1.75,27.6,7.9]
["NE087","Hitchcock","McCook loam, rarely flooded","Well drained","B",1.875,40.35,7.7]
["NE087","Hitchcock","McCook loam, sand substratum variant, occasionally flooded","Well drained","B",0.5,42.7,7.9]
["NE087","Hitchcock","McCook silt loam, channeled, occasionally flooded","Well drained","B",1.75,36.6,7.9]
["NE087","Hitchcock","McCook silt loam, occasionally flooded","Well drained","B",1.75,12.75,7.5500000000000007]
["NE087","Hitchcock","McCook silt loam, rarely flooded","Well drained","B",1.875,12.95,7.5500000000000007]
["NE087","Hitchcock","Otero fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.25,62.5,8.1999999999999993]
["NE087","Hitchcock","Sarben fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7.2]
["NE087","Hitchcock","Sarben fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,66.099999999999994,7.2]
["NE087","Hitchcock","Sarben loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.75,86.4,6.7]
["NE087","Hitchcock","Sarben loamy fine sand, hummocky","Well drained","A",0.75,75.699999999999989,7.3000000000000007]
["NE087","Hitchcock","Scott variant silty clay loam, frequently ponded","Poorly drained","C/D",2,7,7.2]
["NE087","Hitchcock","Sulco complex, 9 to 60 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE087","Hitchcock","Sulco loam, 6 to 9 percent slopes","Well drained","B",0.25,43.6,8.8000000000000007]
["NE087","Hitchcock","Sulco loam, 9 to 30 percent slopes","Well drained","B",0.25,43.6,8.1999999999999993]
["NE087","Hitchcock","Sulco silt loam, 30 to 60 percent slopes","Well drained","B",1,17.600000000000001,7.9]
["NE087","Hitchcock","Sulco silt loam, 6 to 9 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE087","Hitchcock","Sulco silt loam, 9 to 30 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE087","Hitchcock","Sulco-Ulysses silt loams, 9 to 30 percent slopes, eroded","Well drained","B",1.25,13.6,7.9]
["NE087","Hitchcock","Ulysses and Sulco silt loams, 6 to 9 percent slopes, eroded","Well drained","B",1.25,14.3,7.9]
["NE087","Hitchcock","Ulysses loam, 1 to 3 percent slopes","Well drained","B",1,37.15,7.8999999999999995]
["NE087","Hitchcock","Ulysses loam, 3 to 6 percent slopes","Well drained","B",0.9,33.299999999999997,7.6]
["NE087","Hitchcock","Ulysses silt loam, 3 to 6 percent slopes, eroded","Well drained","B",1.5,14.3,7.9]
["NE087","Hitchcock","Ulysses silt loam, 6 to 9 percent slopes, eroded","Well drained","B",1.5,14.3,7.9]
["NE087","Hitchcock","Valent fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE087","Hitchcock","Valent sand, rolling","Excessively drained","A",0.25,95,7]
["NE089","Holt",null,"",""]
["NE089","Holt","Almeria-Calamus complex, channeled, frequently flooded","Poorly drained","A/D",0.25,92.2,6.2]
["NE089","Holt","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE089","Holt","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE089","Holt","Anselmo loam, 0 to 1 percent slopes","Well drained","B",0.75,66.099999999999994,6.7]
["NE089","Holt","Anselmo-O'Neill sandy loams, 0 to 3 percent slopes","Well drained","A",0.75,67.849999999999994,6.7]
["NE089","Holt","Anselmo-O'Neill sandy loams, 3 to 6 percent slopes","Well drained","A",0.75,67.849999999999994,6.6]
["NE089","Holt","Aowa silt loam, channeled, frequently flooded","Well drained","B",1.625,9.0500000000000007,7.9]
["NE089","Holt","Barney loam, frequently flooded, wet","Very poorly drained","B/D",1.625,67.650000000000006,7.35]
["NE089","Holt","Barney silt loam, channeled, frequently flooded","Very poorly drained","B/D",0.25,91,7.5]
["NE089","Holt","Barney-Boel-Calamus complex, channeled","Poorly drained","B/D",0.25,92.1,7.2]
["NE089","Holt","Bazile loam, 0 to 2 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE089","Holt","Bazile loam, 2 to 6 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE089","Holt","Bazile silt loam, 0 to 2 percent slopes","Well drained","C",0.75,19.95,7]
["NE089","Holt","Bazile silt loam, 2 to 6 percent slopes","Well drained","C",0.75,21.9,6.85]
["NE089","Holt","Blackloup loam, occasionally flooded","Very poorly drained","B/D",0.5,72.55,7.4]
["NE089","Holt","Blackloup loam, rarely flooded","Poorly drained","B/D",0.75,65.900000000000006,7.4]
["NE089","Holt","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.25,96.3,7.5]
["NE089","Holt","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE089","Holt","Boel loamy fine sand, occasionally flooded, wet","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE089","Holt","Boel silty clay loam, overwash, occasionally flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE089","Holt","Boel-Inavale complex, channeled, frequently flooded","Somewhat poorly drained","A",0.25,96.3,7.5]
["NE089","Holt","Boelus loamy sand, 0 to 3 percent slopes","Well drained","B",0.5,51.849999999999994,7.15]
["NE089","Holt","Boelus loamy sand, 3 to 6 percent slopes","Well drained","B",0.5,53.9,7.15]
["NE089","Holt","Boelus loamy sand, 6 to 11 percent slopes","Well drained","B",0.5,53.9,7.15]
["NE089","Holt","Boelus loamy sand, gravelly substratum, 0 to 3 percent slopes","Well drained","B",0.5,87.25,6.5]
["NE089","Holt","Boelus-Meadin complex, 6 to 11 percent slopes","Well drained","B",0.5,75.599999999999994,6.6]
["NE089","Holt","Bristow silty clay, 20 to 40 percent slopes","Well drained","D",0.25,2.6,7.9]
["NE089","Holt","Bristow silty clay, 30 to 60 percent slopes","Well drained","D",0.25,2.6,7.9]
["NE089","Holt","Brunswick-Longpine fine sandy loams, 11 to 40 percent slopes","Well drained","B",0.25,64.599999999999994,6.5]
["NE089","Holt","Brunswick-Paka complex, 17 to 30 percent slopes","Well drained","B",0.5,32.1,6.6]
["NE089","Holt","Brunswick-Pivot complex, 11 to 30 percent slopes","Well drained","B",0.25,81.75,6.5]
["NE089","Holt","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE089","Holt","Dunday loamy fine sand, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE089","Holt","Dunday loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,89.6,6.85]
["NE089","Holt","Dunday loamy sand, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,89.6,6.85]
["NE089","Holt","Dunn loamy sand, 0 to 3 percent slopes","Moderately well drained","C/D",0.75,83,6.5]
["NE089","Holt","Els loamy sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,94.6,6.7]
["NE089","Holt","Els-Ipage complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.15,6.6]
["NE089","Holt","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE089","Holt","Els-Ipage-Tryon loamy sands, 0 to 6 percent slopes","Somewhat poorly drained","A",0.75,84.3,6.7]
["NE089","Holt","Elsmere fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.25,79.400000000000006,7]
["NE089","Holt","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,7]
["NE089","Holt","Elsmere loamy fine sand, clayey substratum, 0 to 3 percent slopes","Somewhat poorly drained","A/D",0.75,86.8,6.7]
["NE089","Holt","Elsmere loamy fine sand, rarely flooded","Somewhat poorly drained","A",1.125,91.1,6.5]
["NE089","Holt","Elsmere-Ipage loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,94.9,7]
["NE089","Holt","Elsmere-Selia loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,85.9,8.1]
["NE089","Holt","Fillmore silt loam, occasionally ponded","Somewhat poorly drained","D",1.125,16.100000000000001,7.1]
["NE089","Holt","Fluvaquents, frequently flooded, wet","Very poorly drained","B/D",5,19.2,7.5]
["NE089","Holt","Fluvaquents, sandy-Fluvaquents, loamy complex, frequently flooded","Very poorly drained","A/D",0.5,78.95,7.55]
["NE089","Holt","Gannett loam, 0 to 1 percent slopes","Poorly drained","B/D",0.75,45.3,7.9]
["NE089","Holt","Gannett mucky peat","Very poorly drained","B/D",0.5,42.55,7.9]
["NE089","Holt","Inavale fine sand, channeled, frequently flooded","Excessively drained","A",0.25,92.2,6.7]
["NE089","Holt","Inavale fine sand, channeled, frequently flooded, wet","Excessively drained","A",0.25,92.2,6.7]
["NE089","Holt","Inavale fine sand, rarely flooded","Excessively drained","A",0.25,92.2,7.5]
["NE089","Holt","Inavale loamy fine sand, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE089","Holt","Inavale loamy fine sand, occasionally flooded, wet","Excessively drained","A",0.25,87.3,6.7]
["NE089","Holt","Inavale loamy fine sand, rarely flooded","Excessively drained","A",0.25,92.2,7.5]
["NE089","Holt","Inavale loamy fine sand, rarely flooded, wet","Excessively drained","A",0.25,92.2,7.5]
["NE089","Holt","Inavale sand, channeled, frequently flooded","Excessively drained","A",0.5,93.55,7.25]
["NE089","Holt","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.199999999999989,6.2]
["NE089","Holt","Ipage loamy sand, 0 to 3 percent slopes","Moderately well drained","A",0.25,94.1,6.5]
["NE089","Holt","Ipage sand, 0 to 3 percent slopes","Moderately well drained","A",0.25,95.5,6.5]
["NE089","Holt","Ipage-Tryon fine sands, 0 to 3 percent slopes","Moderately well drained","A",0.75,95.5,6.5]
["NE089","Holt","Jansen loam, 0 to 2 percent slopes","Well drained","B",0.75,67.8,6.2]
["NE089","Holt","Jansen loam, 2 to 6 percent slopes","Well drained","B",0.75,60.949999999999996,6.2]
["NE089","Holt","Jansen-Meadin loams, 2 to 6 percent slopes","Well drained","B",1,61.15,6.2]
["NE089","Holt","Josburg fine sandy loam, 0 to 2 percent slopes","Moderately well drained","C",0.75,57.4,6.2]
["NE089","Holt","Josburg loam, 0 to 2 percent slopes","Moderately well drained","C",0.75,56.75,6]
["NE089","Holt","Labu silty clay, 2 to 6 percent slopes","Well drained","D",0.75,2.6,7.5]
["NE089","Holt","Labu silty clay, 6 to 11 percent slopes","Well drained","D",0.75,2.6,7.5]
["NE089","Holt","Labu-Sansarc silty clays, 11 to 30 percent slopes","Well drained","D",0.65,2.6,7.5]
["NE089","Holt","Labu-Sansarc silty clays, 11 to 40 percent slopes","Well drained","D",0.65,2.6,7.7]
["NE089","Holt","Lamo-Lute loams, 0 to 2 percent slopes","Somewhat poorly drained","C/D",0.5,53.1,7.9]
["NE089","Holt","Lawet loam, drained, rarely flooded","Somewhat poorly drained","B/D",0.75,38.5,7.9]
["NE089","Holt","Lawet-Lute complex, rarely flooded","Somewhat poorly drained","B/D",0.75,41.6,8.0500000000000007]
["NE089","Holt","Lex-Lute loams, rarely flooded","Somewhat poorly drained","C/D",0.625,42.3,7.7]
["NE089","Holt","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,86.4,6.5]
["NE089","Holt","Libory-Whitelake loamy fine sands, 0 to 3 percent slopes","Moderately well drained","A",1.25,63.5,6.7]
["NE089","Holt","Loretto loam, 0 to 2 percent slopes","Well drained","C",1.5,39.1,6.5]
["NE089","Holt","Loretto loam, 2 to 6 percent slopes","Well drained","C",1.5,36.5,6.5]
["NE089","Holt","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,63.5,7.5]
["NE089","Holt","Loup fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,79.2,7.5]
["NE089","Holt","Lynch silty clay, 2 to 6 percent slopes","Well drained","D",0.75,2.4500000000000002,7.9]
["NE089","Holt","Lynch silty clay, 6 to 11 percent slopes","Well drained","D",0.75,2.4500000000000002,7.9]
["NE089","Holt","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,78.2,7.5]
["NE089","Holt","Meadin loam, 0 to 2 percent slopes","Excessively drained","B",0.75,65.3,6.2]
["NE089","Holt","Meadin sandy loam, 0 to 2 percent slopes","Excessively drained","A",0.75,67.8,6.2]
["NE089","Holt","Meadin sandy loam, 2 to 30 percent slopes","Excessively drained","A",0.75,67.8,6.2]
["NE089","Holt","Meadin-O'Neill complex, 2 to 30 percent slopes","Excessively drained","B",0.75,68.150000000000006,6.35]
["NE089","Holt","Moody loam, 0 to 2 percent slopes","Well drained","C",3,9.4,6.5]
["NE089","Holt","Nimbro silt loam, 0 to 2 percent slopes","Well drained","B",1.75,33.35,7.9]
["NE089","Holt","Nora silt loam, 0 to 2 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE089","Holt","Nora silt loam, 2 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE089","Holt","Nora silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,8.9,7]
["NE089","Holt","Norway loamy fine sand, frequently flooded, wet","Very poorly drained","A/D",0.375,79.900000000000006,7.7]
["NE089","Holt","O'Neill fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,67.599999999999994,6.5]
["NE089","Holt","O'Neill fine sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,67.599999999999994,6.5]
["NE089","Holt","O'Neill loam, 0 to 2 percent slopes","Well drained","B",0.75,67.599999999999994,6.5]
["NE089","Holt","O'Neill loamy sand, 0 to 2 percent slopes","Well drained","A",0.75,84.3,6.5]
["NE089","Holt","O'Neill sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,68.5,6.5]
["NE089","Holt","O'Neill-Meadin fine sandy loams, 11 to 30 percent slopes","Excessively drained","A",0.75,66.449999999999989,6.35]
["NE089","Holt","O'Neill-Meadin fine sandy loams, 2 to 6 percent slopes","Excessively drained","A",0.75,66.449999999999989,6.35]
["NE089","Holt","O'Neill-Meadin fine sandy loams, 6 to 11 percent slopes","Excessively drained","A",0.75,66.449999999999989,6.35]
["NE089","Holt","Ord loam, rarely flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE089","Holt","Ord-Lute fine sandy loams, rarely flooded","Somewhat poorly drained","D",0.625,63,7.7]
["NE089","Holt","Ortello fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE089","Holt","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE089","Holt","Paka fine sandy loam, 0 to 2 percent slopes","Well drained","B",1.125,9.1,7.1]
["NE089","Holt","Paka fine sandy loam, 2 to 6 percent slopes","Well drained","B",1.125,9.1,7.45]
["NE089","Holt","Paka loam, 0 to 2 percent slopes","Well drained","B",1.125,9.3000000000000007,7.45]
["NE089","Holt","Paka loam, 2 to 6 percent slopes","Well drained","B",1.125,9.3000000000000007,7.45]
["NE089","Holt","Paka loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,9.3000000000000007,7.45]
["NE089","Holt","Pivot loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.5,88.2,6.5]
["NE089","Holt","Pivot loamy sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.5,88.2,6.5]
["NE089","Holt","Pivot-Valentine complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.75,92.1,6.5]
["NE089","Holt","Riverwash","Very poorly drained","A/D",0.15000000000000002,95.05,7.6]
["NE089","Holt","Sansarc silty clay, 20 to 40 percent slopes","Well drained","D",0.55000000000000004,5,7.5]
["NE089","Holt","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,87.3,6.9]
["NE089","Holt","Simeon sand, 0 to 3 percent slopes","Excessively drained","A",0.5,91.85,6.9]
["NE089","Holt","Simeon sand, 6 to 30 percent slopes, eroded","Excessively drained","A",0.5,91.85,7]
["NE089","Holt","Simeon-Valentine sands, 11 to 60 percent slopes, eroded","Excessively drained","A",0.5,93.8,6.75]
["NE089","Holt","Thurman fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.875,94.9,6.5]
["NE089","Holt","Thurman loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.875,89.9,6.5]
["NE089","Holt","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.875,89.9,6.5]
["NE089","Holt","Trent silt loam, 0 to 2 percent slopes","Moderately well drained","B",2.5,7,6.7]
["NE089","Holt","Tryon loamy fine sand, 0 to 3 percent slopes","Poorly drained","A/D",3.375,91.1,7]
["NE089","Holt","Tryon loamy fine sand, frequently ponded","Very poorly drained","A/D",3.375,91.1,6.85]
["NE089","Holt","Tryon-Els loamy sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,95.4,6.7]
["NE089","Holt","Uly silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.5,7]
["NE089","Holt","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE089","Holt","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE089","Holt","Valentine fine sand, 9 to 24 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE089","Holt","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE089","Holt","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,96.3,6.5]
["NE089","Holt","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE089","Holt","Valentine-Dunday loamy fine sands, 0 to 3 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE089","Holt","Valentine-Dunday loamy fine sands, 3 to 9 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE089","Holt","Valentine-Els complex, 0 to 9 percent slopes","Somewhat poorly drained","A",0.25,95.4,7]
["NE089","Holt","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE089","Holt","Valentine-Simeon sands, 3 to 9 percent slopes","Excessively drained","A",0.5,93.8,6.6]
["NE089","Holt","Valentine-Simeon sands, 9 to 30 percent slopes, eroded","Excessively drained","A",0.5,93.8,6.75]
["NE089","Holt","Valentine-Tryon fine sands, 0 to 17 percent slopes","Very poorly drained","A/D",0.75,95.9,6.75]
["NE089","Holt","Valentine-Wewela complex, 3 to 9 percent slopes","Excessively drained","A",0.625,70.650000000000006,6.7]
["NE089","Holt","Verdel silty clay loam, 0 to 2 percent slopes","Well drained","D",1.375,11.3,7.25]
["NE089","Holt","Wewela fine sandy loam, 0 to 2 percent slopes","Well drained","D",1.25,38.75,7]
["NE089","Holt","Wewela fine sandy loam, 2 to 6 percent slopes","Well drained","D",1.25,38.75,7]
["NE089","Holt","Wewela loam, 0 to 2 percent slopes","Well drained","D",1.25,31.6,7]
["NE091","Hooker",null,"",""]
["NE091","Hooker","Almeria-Fluvaquents, sandy complex, channeled, frequently flooded","Poorly drained","B/D",7.5,44.3,6.8]
["NE091","Hooker","Bolent-Almeria complex, channeled, frequently flooded","Very poorly drained","B/D",0.52500000000000002,89.5,7.4]
["NE091","Hooker","Calamus-Bolent loamy fine sands, channeled, occasionally flooded","Somewhat poorly drained","A",0.375,89.5,6.8]
["NE091","Hooker","Clawhammer-Ord complex, 0 to 3 percent slopes","Poorly drained","B/D",1.5,70,8]
["NE091","Hooker","Crowther loam, 0 to 1 percent slopes","Poorly drained","B/D",6.75,42.2,7.7]
["NE091","Hooker","Crowther mucky peat","Very poorly drained","B/D",6.75,38.5,7.7]
["NE091","Hooker","Cullison mucky peat","Very poorly drained","B/D",12,33.5,7.9]
["NE091","Hooker","Cutcomb mucky peat","Very poorly drained","A/D",55,0,5.8]
["NE091","Hooker","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,86.8,6.7]
["NE091","Hooker","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.75,86.8,6.7]
["NE091","Hooker","Els calcareous-Hoffland complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.625,94.1,7.9]
["NE091","Hooker","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.7]
["NE091","Hooker","Elsmere loamy fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,79.400000000000006,7.9]
["NE091","Hooker","Elsmere-Loup complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,91,6.7]
["NE091","Hooker","Gus mucky peat","Very poorly drained","B/D",9.5,35.200000000000003,7]
["NE091","Hooker","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.95]
["NE091","Hooker","Ipage-Els complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,96,6.5]
["NE091","Hooker","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,94.9,6.7]
["NE091","Hooker","Loup mucky peat","Very poorly drained","A/D",4,63.5,6.6]
["NE091","Hooker","Marlake mucky peat","Very poorly drained","A/D",3.375,76.449999999999989,6.5500000000000007]
["NE091","Hooker","Mullen loamy fine sand, 0 to 3 percent slopes","Well drained","B",1.125,79.050000000000011,6.95]
["NE091","Hooker","Natick sand, 0 to 3 percent slopes","Moderately well drained","A",0.57499999999999996,93.5,6.4]
["NE091","Hooker","Nenzel loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",1.25,86.8,6.7]
["NE091","Hooker","Nenzel loamy fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",1.375,91.4,7.9]
["NE091","Hooker","Thedford fine sand, 0 to 3 percent slopes","Moderately well drained","A",1.375,91.5,7.9]
["NE091","Hooker","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.75,93,6.5]
["NE091","Hooker","Valentine fine sand, hilly","Excessively drained","A",0.5,94.9,6.5]
["NE091","Hooker","Valentine fine sand, rolling","Excessively drained","A",0.5,94.9,6.5]
["NE091","Hooker","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,94.9,6.5]
["NE091","Hooker","Valentine-Birdwood complex, 9 to 80 percent slopes","Well drained","A",0.625,85.8,6.5]
["NE091","Hooker","Valentine-Dunday complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.625,94,6.6]
["NE091","Hooker","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.625,95.4,6.5]
["NE091","Hooker","Valentine-Hoffland, complex, 0 to 24 percent slopes","Very poorly drained","A/D",0.625,94.1,7.15]
["NE091","Hooker","Valentine-Libory complex, 0 to 9 percent slopes","Moderately well drained","B",0.625,90.05,6.55]
["NE091","Hooker","Valentine-Mullen complex, 0 to 9 percent slopes","Well drained","B",0.75,86,6.7]
["NE091","Hooker","Valentine-Tryon complex, 0 to 24 percent slopes","Very poorly drained","A/D",0.625,94.1,6.5]
["NE091","Hooker","Wildhorse-Hoffland complex, 0 to 3 percent slopes","Poorly drained","A/D",2,94.9,9.1]
["NE093","Howard",null,"",""]
["NE093","Howard","Almeria loam, occasionally flooded","Very poorly drained","B/D",3.375,68.199999999999989,6.9]
["NE093","Howard","Almeria soils, occasionally flooded","Poorly drained","B/D",3.375,68.949999999999989,6.9]
["NE093","Howard","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE093","Howard","Barney loam, frequently flooded","Very poorly drained","B/D",0.25,47.9,7.5]
["NE093","Howard","Boel fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.875,80.650000000000006,7.5]
["NE093","Howard","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE093","Howard","Boel loam, rarely flooded","Somewhat poorly drained","C",1.125,68.150000000000006,7.5]
["NE093","Howard","Boel loamy fine sand, rarely flooded","Somewhat poorly drained","A",0.875,88.15,7.5]
["NE093","Howard","Bolent loamy sand, occasionally flooded","Somewhat poorly drained","A",1,95.4,6.9]
["NE093","Howard","Coly silt loam, 11 to 30 percent slopes","Well drained","B",1.125,8,7.9]
["NE093","Howard","Coly silt loam, 11 to 30 percent slopes, moist","Well drained","B",1.23,24,7.8000000000000007]
["NE093","Howard","Coly silt loam, 3 to 6 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE093","Howard","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE093","Howard","Coly silt loam, 30 to 60 percent slopes, moist","Well drained","B",1.23,24,7.8000000000000007]
["NE093","Howard","Coly silt loam, 6 to 11 percent slopes","Well drained","B",1.125,8,7.9]
["NE093","Howard","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE093","Howard","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",1.125,11.3,7.45]
["NE093","Howard","Coly-Uly complex, 17 to 30 percent slopes","Well drained","B",0.75,9.1,7.9]
["NE093","Howard","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE093","Howard","Coly-Uly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE093","Howard","Cozad loam, sand substratum, 0 to 3 percent slopes","Well drained","B",1.375,47.45,6.35]
["NE093","Howard","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE093","Howard","Darr fine sandy loam, rarely flooded","Somewhat excessively drained","A",0.75,65,7]
["NE093","Howard","Darr silt loam, rarely flooded","Somewhat excessively drained","B",0.75,63,7.5]
["NE093","Howard","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,8,7.2]
["NE093","Howard","Els loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,80,6.7]
["NE093","Howard","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,81,6.5]
["NE093","Howard","Els-Tryon complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,81.8,6.2]
["NE093","Howard","Fluvaquents, frequently flooded","Very poorly drained","A/D",5,23.5,7.5]
["NE093","Howard","Gates fine sandy loam, 0 to 3 percent slopes, hummocky","Well drained","B",0.5,52.95,6.3000000000000007]
["NE093","Howard","Gayville loam, rarely flooded","Somewhat poorly drained","C",0.25,14.3,8]
["NE093","Howard","Gayville variant silt loam, rarely flooded","Somewhat poorly drained","C",1.5,14.3,9.1]
["NE093","Howard","Gibbon loam, occasionally flooded","Somewhat poorly drained","C",0.75,41.5,7.9]
["NE093","Howard","Gibbon silt loam, rarely flooded","Somewhat poorly drained","C",0.75,8,7.9]
["NE093","Howard","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,95.35,7.2]
["NE093","Howard","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.5,83.6,7.35]
["NE093","Howard","Grigston silt loam","Well drained","C",1.5,8,7.9]
["NE093","Howard","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8,7.1]
["NE093","Howard","Hall silt loam, sandy substratum, 0 to 1 percent slopes","Well drained","C",2,21.3,7]
["NE093","Howard","Harney silt loam, 0 to 1 percent slopes","Well drained","C",1.5,8,7.3]
["NE093","Howard","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,11.3,7]
["NE093","Howard","Hobbs silt loam, frequently flooded","Well drained","B",1.875,11.3,7]
["NE093","Howard","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,9.25,7.25]
["NE093","Howard","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",1.25,8,7.2]
["NE093","Howard","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",1.25,8,7.2]
["NE093","Howard","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.3500000000000014,7.2]
["NE093","Howard","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,8,7.2]
["NE093","Howard","Holdrege silt loam, 7 to 11 percent slopes","Well drained","C",1.25,8,7.2]
["NE093","Howard","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.5,7.1,7.2]
["NE093","Howard","Holdrege silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,8,7.2]
["NE093","Howard","Holdrege variant silty clay loam, 7 to 11 percent slopes, severely eroded","Well drained","C",0.75,8,7.2]
["NE093","Howard","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,8,7]
["NE093","Howard","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,8,7]
["NE093","Howard","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,8,7]
["NE093","Howard","Hord silt loam, rarely flooded","Well drained","B",0.75,8,7]
["NE093","Howard","Hord silt loam, sandy substratum, 0 to 1 percent slopes","Well drained","C",2.5,11.3,7]
["NE093","Howard","Inavale fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,82,6.7]
["NE093","Howard","Inavale fine sandy loam, 0 to 3 percent slopes","Excessively drained","A",0.25,80,6.7]
["NE093","Howard","Inavale loam, 0 to 3 percent slopes","Excessively drained","A",0.25,80,6.7]
["NE093","Howard","Inavale loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,80,6.7]
["NE093","Howard","Inavale loamy fine sand, very rarely flooded","Excessively drained","A",0.25,87.3,7]
["NE093","Howard","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE093","Howard","Ipage-Tryon, wet, complex, silty substratum, 0 to 3 percent slopes","Moderately well drained","A",0.25,95.4,5.85]
["NE093","Howard","Janude sandy loam, very rarely flooded","Moderately well drained","B",0.75,66.599999999999994,7.3]
["NE093","Howard","Kenesaw silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14,7.5]
["NE093","Howard","Kenesaw silt loam, 1 to 6 percent slopes","Well drained","B",0.75,14,7.5]
["NE093","Howard","Kenesaw silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14,7.5]
["NE093","Howard","Kenesaw silt loam, 6 to 11 percent slopes","Well drained","B",0.75,14,7.5]
["NE093","Howard","Kenesaw-Cozad complex","Moderately well drained","B",0.75,11.4,8.0500000000000007]
["NE093","Howard","Lamo silt loam, occasionally flooded","Somewhat poorly drained","C",1.375,8.8000000000000007,7.9]
["NE093","Howard","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","C/D",0.25,9.6999999999999993,5.9]
["NE093","Howard","Libory-Boelus fine sands","Well drained","B",0.75,83.8,6.7]
["NE093","Howard","Libory-Boelus loamy fine sands","Well drained","B",0.75,83.8,6.7]
["NE093","Howard","Loretto complex, 0 to 6 percent slopes","Well drained","A",1.5,24.2,6.5]
["NE093","Howard","Loretto fine sandy loam, 0 to 2 percent slopes","Well drained","C",1.5,19.899999999999999,6.5]
["NE093","Howard","Loretto-Valentine complex, 3 to 11 percent slopes","Well drained","C",0.75,77.099999999999994,6.5]
["NE093","Howard","Loup fine sandy loam, loamy substratum, 0 to 2 percent slopes","Poorly drained","A/D",0.75,79.5,7.5]
["NE093","Howard","Loup loam, occasionally flooded","Poorly drained","B/D",3.375,70.150000000000006,6.6]
["NE093","Howard","Novina sandy loam, rarely flooded","Moderately well drained","B",0.75,66.599999999999994,6.7]
["NE093","Howard","Nuckolls soils, 17 to 30 percent slopes, severely eroded","Well drained","C",0.75,9.1,7.2]
["NE093","Howard","Nuckolls variant soils, 11 to 17 percent slopes, severely eroded","Well drained","C",0.25,6,7.5]
["NE093","Howard","Nuckolls variant soils, 7 to 11 percent slopes, severely eroded","Well drained","C",0.25,6,7.5]
["NE093","Howard","O'Neill loam, 0 to 2 percent slopes","Well drained","B",0.75,67.599999999999994,6.5]
["NE093","Howard","Ord fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,65.3,7.5]
["NE093","Howard","Ord loam, rarely flooded","Somewhat poorly drained","C",0.75,65.3,7.5]
["NE093","Howard","Ortello fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE093","Howard","Ortello fine sandy loam, silty substratum, 0 to 3 percent slopes","Well drained","A",0.75,69.599999999999994,7.1]
["NE093","Howard","Ortello loam, 0 to 1 percent slopes","Well drained","B",0.75,63.5,6.7]
["NE093","Howard","Ortello loam, 1 to 5 percent slopes","Well drained","B",0.75,63.5,6.7]
["NE093","Howard","Ortello loamy fine sand, 1 to 6 percent slopes","Well drained","A",0.875,75.900000000000006,6.6]
["NE093","Howard","Ortello-Coly complex, 17 to 30 percent slopes","Well drained","B",1.125,37.400000000000006,7.3000000000000007]
["NE093","Howard","Ovina fine sandy loam","Somewhat poorly drained","B/D",0.875,55.8,8.1499999999999986]
["NE093","Howard","Ovina loam, rarely flooded","Somewhat poorly drained","C",1.125,54.55,7.7]
["NE093","Howard","Ovina loamy fine sand","Somewhat poorly drained","B",1.125,65.2,7.7]
["NE093","Howard","Rusco silt loam, occasionally flooded","Moderately well drained","C/D",0.75,11.2,7.5]
["NE093","Howard","Silver Creek complex, saline-alkali, rarely flooded","Somewhat poorly drained","D",1,26,8.3000000000000007]
["NE093","Howard","Silver Creek-Slickspots complex, rarely flooded","Somewhat poorly drained","D",1.375,20.9,8.0500000000000007]
["NE093","Howard","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,87.3,7]
["NE093","Howard","Thurman fine sand, 0 to 6 percent slopes","Somewhat excessively drained","A",0.25,94.9,6.5]
["NE093","Howard","Thurman loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE093","Howard","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE093","Howard","Thurman loamy fine sand, loamy substratum, 0 to 2 percent slopes","Somewhat excessively drained","A",1.375,89.5,6.85]
["NE093","Howard","Thurman-Valentine loamy fine sands, terrace, 0 to 2 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE093","Howard","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE093","Howard","Uly silt loam, 11 to 17 percent slopes, eroded, moist","Well drained","B",0.69500000000000006,24.5,7.95]
["NE093","Howard","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE093","Howard","Uly-Coly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.73,24.5,7.9]
["NE093","Howard","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE093","Howard","Uly-Coly silt loams, 17 to 30 percent slopes, eroded, moist","Well drained","B",1,24,7.5]
["NE093","Howard","Uly-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE093","Howard","Valentine and Thurman soils, 0 to 17 percent slopes","Somewhat excessively drained","A",0.25,91.1,6.5]
["NE093","Howard","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE093","Howard","Valentine fine sand, rolling","Excessively drained","A",0.25,96.3,6.5]
["NE093","Howard","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE093","Howard","Valentine-Libory complex, 0 to 9 percent slopes","Moderately well drained","A",0.25,83.5,6.3]
["NE093","Howard","Wann loam, occasionally flooded","Somewhat poorly drained","C",0.75,66.2,8.1999999999999993]
["NE093","Howard","Wann loam, rarely flooded","Somewhat poorly drained","C",0.5,51.05,7.5500000000000007]
["NE093","Howard","Wann sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,66.599999999999994,8.1999999999999993]
["NE093","Howard","Wood River-Silver Creek fine sandy loams, 0 to 1 percent slopes","Somewhat poorly drained","D",0.25,18.899999999999999,8.3000000000000007]
["NE095","Jefferson",null,"",""]
["NE095","Jefferson","Benfield silty clay loam, 11 to 30 percent slopes","Well drained","D",1.5,7.7,7.4]
["NE095","Jefferson","Benfield silty clay loam, 3 to 11 percent slopes, eroded","Well drained","D",1.5,7.25,7.4]
["NE095","Jefferson","Benfield silty clay loam, 6 to 11 percent slopes, eroded","Well drained","D",1.5,7.7,7.4]
["NE095","Jefferson","Burchard clay loam, 11 to 30 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE095","Jefferson","Burchard clay loam, 2 to 6 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE095","Jefferson","Burchard clay loam, 6 to 11 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE095","Jefferson","Burchard clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,36.5,6.7]
["NE095","Jefferson","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE095","Jefferson","Burchard-Steinauer clay loams, 11 to 30 percent slopes","Somewhat excessively drained","C",0.75,34.5,7.9]
["NE095","Jefferson","Burchard-Steinauer clay loams, 6 to 11 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE095","Jefferson","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,22.35,7.1]
["NE095","Jefferson","Cass loam, occasionally flooded","Well drained","A",0.75,63.5,7.3]
["NE095","Jefferson","Cass loam, rarely flooded","Well drained","A",0.75,63.5,7.3]
["NE095","Jefferson","Cortland-Malmo complex, 6 to 11 percent slopes, eroded","Well drained","C",0.75,37.549999999999997,6.5]
["NE095","Jefferson","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE095","Jefferson","Crete silt loam, 1 to 3 percent slopes","Moderately well drained","C",1.625,13.2,6.25]
["NE095","Jefferson","Crete silt loam, 7 to 11 percent slopes","Moderately well drained","C",1.625,13.2,6.25]
["NE095","Jefferson","Crete silty clay loam, 3 to 7 percent slopes, eroded","Moderately well drained","C",1.625,13.2,6.25]
["NE095","Jefferson","Deroin silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.5,6.6,6.4]
["NE095","Jefferson","Deroin silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,6.6,6.4]
["NE095","Jefferson","Edalgo silty clay loam, 3 to 7 percent slopes, eroded","Well drained","D",1.5,5.3,5.8]
["NE095","Jefferson","Edalgo silty clay loam, 7 to 11 percent slopes","Well drained","D",1.5,5.3,5.8]
["NE095","Jefferson","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,44.9,3.75]
["NE095","Jefferson","Geary and Jansen soils, 11 to 30 percent slopes","Well drained","C",1.25,25.35,6.2]
["NE095","Jefferson","Geary and Jansen soils, 7 to 11 percent slopes","Well drained","C",1.25,25.35,6.2]
["NE095","Jefferson","Geary and Jansen soils, 7 to 11 percent slopes, eroded","Well drained","C",1.25,25.35,6.2]
["NE095","Jefferson","Geary and Jansen soils, 7 to 11 percent slopes, severely eroded","Well drained","C",0.5,31.849999999999998,6.35]
["NE095","Jefferson","Geary silty clay loam, 11 to 30 percent slopes","Well drained","C",1.25,6.9,6.7]
["NE095","Jefferson","Geary silty clay loam, 11 to 30 percent slopes, severely eroded","Well drained","C",0.25,6.7,7]
["NE095","Jefferson","Geary silty clay loam, 3 to 11 percent slopes, severely eroded","Well drained","C",0.25,6.7,7]
["NE095","Jefferson","Geary silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,6.9,6.7]
["NE095","Jefferson","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.7]
["NE095","Jefferson","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",3,26.5,6.1]
["NE095","Jefferson","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",3,26.5,6.1]
["NE095","Jefferson","Hastings silt loam, 7 to 11 percent slopes","Well drained","C",3,26.5,6.1]
["NE095","Jefferson","Hastings silty clay loam, 3 to 11 percent slopes, severely eroded","Well drained","C",0.75,20,7.3]
["NE095","Jefferson","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",3,20,6.1]
["NE095","Jefferson","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE095","Jefferson","Hedville loam, 30 to 50 percent slopes","Somewhat excessively drained","D",1.25,22.15,3.25]
["NE095","Jefferson","Hedville loam, 7 to 30 percent slopes","Somewhat excessively drained","D",0.75,44.3,6.5]
["NE095","Jefferson","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE095","Jefferson","Hobbs silt loam, channeled, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE095","Jefferson","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,10.4,6.8]
["NE095","Jefferson","Hord silt loam, 1 to 3 percent slopes","Well drained","B",2.5,9.25,6.45]
["NE095","Jefferson","Jansen loam, 2 to 6 percent slopes","Well drained","B",1.25,57,6.2]
["NE095","Jefferson","Jansen loam, 3 to 7 percent slopes, eroded","Well drained","B",1.25,57,6.2]
["NE095","Jefferson","Jansen loam, 6 to 11 percent slopes","Well drained","B",1.25,57,6.2]
["NE095","Jefferson","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE095","Jefferson","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,8,6.6]
["NE095","Jefferson","Kipson silt loam, 7 to 30 percent slopes","Somewhat excessively drained","D",0.75,23.5,7.9]
["NE095","Jefferson","Kipson soils, 11 to 30 percent slopes","Somewhat excessively drained","D",0.75,23.5,7.9]
["NE095","Jefferson","Lancaster and Edalgo soils, 11 to 30 percent slopes","Well drained","D",1.5,6.9,6.1]
["NE095","Jefferson","Lancaster loam, 3 to 7 percent slopes, eroded","Well drained","C",1.5,35.200000000000003,6.1]
["NE095","Jefferson","Lancaster loam, 7 to 11 percent slopes","Well drained","C",1.5,35.200000000000003,6.1]
["NE095","Jefferson","Lancaster soils, 7 to 11 percent slopes, severely eroded","Well drained","C",1.5,35.200000000000003,6.1]
["NE095","Jefferson","Longford silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,19.899999999999999,6.5]
["NE095","Jefferson","Malcolm silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,11.4,6.1]
["NE095","Jefferson","Malmo clay loam, 2 to 6 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE095","Jefferson","Malmo clay, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE095","Jefferson","Malmo silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.75,28.95,7.45]
["NE095","Jefferson","Malmo silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.75,28.95,7.45]
["NE095","Jefferson","Malmo, eroded-Pawnee complex, 6 to 11 percent slopes","Moderately well drained","D",0.75,29.9,7]
["NE095","Jefferson","Mayberry silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.75,47.8,6.5]
["NE095","Jefferson","Mayberry silty clay loam, 6 to 11 percent slopes","Moderately well drained","D",0.75,26.1,6.5]
["NE095","Jefferson","Meadin loam, 6 to 30 percent slopes","Excessively drained","A",0.75,65.3,6.2]
["NE095","Jefferson","Morrill clay loam, 11 to 30 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE095","Jefferson","Morrill clay loam, 3 to 6 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE095","Jefferson","Morrill clay loam, 3 to 6 percent slopes, eroded","Well drained","C",0.6,35.200000000000003,6.1]
["NE095","Jefferson","Morrill clay loam, 6 to 11 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE095","Jefferson","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,35.4,6.1]
["NE095","Jefferson","Morrill soils, 6 to 11 percent slopes, severely eroded","Well drained","C",0.75,35.4,6.1]
["NE095","Jefferson","Muir silt loam, 1 to 3 percent slopes","Well drained","B",2,9,6.7]
["NE095","Jefferson","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE095","Jefferson","Nodaway silt loam, channeled, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE095","Jefferson","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE095","Jefferson","Obert soils, occasionally flooded","Very poorly drained","B/D",1.875,9.3000000000000007,7.9]
["NE095","Jefferson","Otoe silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE095","Jefferson","Steinauer clay loam, 11 to 30 percent slopes","Well drained","C",0.75,33.5,8.1999999999999993]
["NE095","Jefferson","Uly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,11.2,7]
["NE095","Jefferson","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE095","Jefferson","Wymore silty clay loam, 2 to 6 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE097","Johnson",null,"",""]
["NE097","Johnson","Aksarben silty clay loam, 2 to 6 percent slopes","Well drained","C",1.125,20,5.8]
["NE097","Johnson","Burchard clay loam, 2 to 6 percent slopes","Well drained","C",0.75,34.799999999999997,7.3000000000000007]
["NE097","Johnson","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.5,7.9]
["NE097","Johnson","Burchard-Steinauer clay loams, 6 to 11 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE097","Johnson","Cortland-Malmo complex, 6 to 11 percent slopes, eroded","Well drained","C",0.75,37.549999999999997,6.5]
["NE097","Johnson","Dickinson fine sandy loam, 11 to 20 percent slopes","Well drained","A",0.75,67.3,5.8]
["NE097","Johnson","Dickinson fine sandy loam, 6 to 11 percent slopes","Well drained","A",1,66.099999999999994,5.8]
["NE097","Johnson","Filley fine sandy loam, 11 to 17 percent slopes","Well drained","A",0.75,67.599999999999994,5.8]
["NE097","Johnson","Filley fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,67.599999999999994,5.8]
["NE097","Johnson","Judson silt loam, 2 to 6 percent slopes","Well drained","C",2.5,7.1,6.5]
["NE097","Johnson","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,8.3000000000000007,6.6]
["NE097","Johnson","Kennebec-Nodaway silt loams, rarely flooded","Moderately well drained","B",2,8.3000000000000007,6.7]
["NE097","Johnson","Kipson-Benfield complex, 11 to 25 percent slopes","Well drained","D",1.125,13.850000000000001,7.25]
["NE097","Johnson","Malcolm silt loam, 11 to 25 percent slopes","Well drained","C",1.25,11.4,6.1]
["NE097","Johnson","Malcolm silt loam, 6 to 11 percent slopes","Well drained","C",1.25,11.4,6.1]
["NE097","Johnson","Malmo clay loam, 2 to 6 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE097","Johnson","Malmo clay, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE097","Johnson","Malmo, eroded-Pawnee complex, 6 to 11 percent slopes","Moderately well drained","D",0.75,29.9,7]
["NE097","Johnson","Mayberry clay loam, 3 to 11 percent slopes","Moderately well drained","D",0.75,34.200000000000003,6.7]
["NE097","Johnson","Morrill clay loam, 6 to 11 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE097","Johnson","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,35.4,6.1]
["NE097","Johnson","Nishna silty clay, occasionally flooded","Poorly drained","D",3.25,7.8,7.9]
["NE097","Johnson","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.5,6.7]
["NE097","Johnson","Nodaway silt loam, channeled, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE097","Johnson","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,9.5,6.7]
["NE097","Johnson","Otoe silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE097","Johnson","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE097","Johnson","Pawnee clay loam, 6 to 11 percent slopes","Moderately well drained","D",2,26.1,7.3]
["NE097","Johnson","Pawnee clay, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,27.6,7.3]
["NE097","Johnson","Shelby clay loam, 11 to 17 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE097","Johnson","Shelby clay loam, 17 to 30 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE097","Johnson","Steinauer clay loam, 11 to 20 percent slopes","Well drained","C",0.75,33.6,7.9]
["NE097","Johnson","Steinauer clay loam, 11 to 30 percent slopes","Well drained","C",0.75,33.5,8.1999999999999993]
["NE097","Johnson","Wabash silty clay, occasionally flooded","Poorly drained","D",2.25,6.5,6.35]
["NE097","Johnson","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",0.75,17.3,6.5]
["NE097","Johnson","Wymore silty clay loam, 2 to 6 percent slopes","Moderately well drained","D",0.75,17.3,6.5]
["NE097","Johnson","Wymore silty clay, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.5,7.7,6.5]
["NE097","Johnson","Zoe-Zook silty clay loams, occasionally flooded","Poorly drained","C",2,7.6,7]
["NE097","Johnson","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.75,6.6]
["NE099","Kearney",null,"",""]
["NE099","Kearney","Alda loam, rarely flooded","Somewhat poorly drained","C",0.75,66,7.9]
["NE099","Kearney","Boel fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.25,84.3,7.8]
["NE099","Kearney","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE099","Kearney","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE099","Kearney","Coly silt loam, 11 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE099","Kearney","Coly silt loam, 3 to 6 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE099","Kearney","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE099","Kearney","Coly-Kenesaw silt loams, 0 to 3 percent slopes","Well drained","B",0.75,11.3,7.8]
["NE099","Kearney","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.8]
["NE099","Kearney","Coly-Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.6]
["NE099","Kearney","Coly-Uly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.8]
["NE099","Kearney","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,20,7.2]
["NE099","Kearney","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE099","Kearney","Gibbon loam, rarely flooded","Somewhat poorly drained","C",0.75,11.4,7.9]
["NE099","Kearney","Gibbon loam, saline, rarely flooded","Somewhat poorly drained","C",0.75,9.1,7.9]
["NE099","Kearney","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,91.9,7.3]
["NE099","Kearney","Gothenburg soils, frequently flooded","Poorly drained","B/D",0.25,91.9,7.5]
["NE099","Kearney","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.5]
["NE099","Kearney","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.5]
["NE099","Kearney","Hersh fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,6.5]
["NE099","Kearney","Hersh-Valentine complex, 6 to 11 percent slopes","Well drained","A",0.25,87.3,6.7]
["NE099","Kearney","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE099","Kearney","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE099","Kearney","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE099","Kearney","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE099","Kearney","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE099","Kearney","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE099","Kearney","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.25,7.2]
["NE099","Kearney","Holdrege silt loam, overblown, 0 to 1 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE099","Kearney","Holdrege silt loam, overblown, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE099","Kearney","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE099","Kearney","Inavale loamy fine sand, rarely flooded","Excessively drained","A",0.25,87.3,6.7]
["NE099","Kearney","Kenesaw silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14,7.3]
["NE099","Kearney","Kenesaw silt loam, 1 to 3 percent slopes","Well drained","B",0.75,6,7.5]
["NE099","Kearney","Kenesaw silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14,7.5]
["NE099","Kearney","Kenesaw-Coly silt loams, 1 to 3 percent slopes","Well drained","B",0.75,11.3,7.8]
["NE099","Kearney","Lex loam, rarely flooded","Somewhat poorly drained","C",0.75,41.6,7.4]
["NE099","Kearney","Lex loam, saline, rarely flooded","Somewhat poorly drained","C",0.75,42.1,8.5]
["NE099","Kearney","Lex silt loam, rarely flooded","Somewhat poorly drained","C",1.375,41.6,8.1999999999999993]
["NE099","Kearney","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,86.4,7.2]
["NE099","Kearney","Massie silty clay loam, frequently ponded","Very poorly drained","D",1.25,6,6.4]
["NE099","Kearney","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,45.7,7.5]
["NE099","Kearney","Rusco silt loam, 0 to 1 percent slopes","Moderately well drained","C/D",0.75,11.2,7.3]
["NE099","Kearney","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE099","Kearney","Simeon sandy loam, 0 to 3 percent slopes","Excessively drained","A",0.5,79.25,6.75]
["NE099","Kearney","Tryon loamy fine sand, rarely flooded","Poorly drained","A/D",3.375,91.1,7.4]
["NE099","Kearney","Uly-Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.8]
["NE099","Kearney","Ustorthents, steep","Well drained","B",0.75,6.8,7.9]
["NE099","Kearney","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,7]
["NE099","Kearney","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,7]
["NE099","Kearney","Valentine loamy fine sand, rolling","Excessively drained","A",0.25,87.3,7]
["NE099","Kearney","Valentine-Els loamy fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.25,91.35,7]
["NE099","Kearney","Wann fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,63.5,7.8]
["NE101","Keith",null,"",""]
["NE101","Keith","Alda fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,69.400000000000006,7.5]
["NE101","Keith","Altvan loam, 1 to 3 percent slopes","Well drained","B",0.75,43.849999999999994,7.85]
["NE101","Keith","Altvan loam, 3 to 6 percent slopes","Well drained","B",0.75,43.849999999999994,7.85]
["NE101","Keith","Altvan-Dix complex, 6 to 30 percent slopes","Well drained","B",0.75,45.5,7.5]
["NE101","Keith","Altvan-Eckley-Satanta complex, 3 to 9 percent slopes","Well drained","C",0.75,62,7.2]
["NE101","Keith","Bankard loamy sand, channeled, frequently flooded","Somewhat excessively drained","A",0.25,92.1,7.9]
["NE101","Keith","Bankard loamy sand, rarely flooded","Somewhat excessively drained","A",1.125,88.5,7.9]
["NE101","Keith","Bankard sand, rarely flooded","Somewhat excessively drained","A",0.75,70.849999999999994,7.9]
["NE101","Keith","Bayard fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE101","Keith","Bayard very fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,63.3,7.9]
["NE101","Keith","Blueridge-Altvan complex, 6 to 30 percent slopes","Well drained","C",0.75,83.5,7.2]
["NE101","Keith","Boel loamy fine sand, rarely flooded","Somewhat poorly drained","A",0.25,87.3,7.5]
["NE101","Keith","Bridget loam, 1 to 3 percent slopes","Well drained","B",1.375,43.150000000000006,7.5500000000000007]
["NE101","Keith","Bridget silt loam, 0 to 1 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE101","Keith","Broadwater loamy sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,84.3,7.2]
["NE101","Keith","Broadwater loamy sand, frequently flooded","Somewhat excessively drained","A",0.5,88.800000000000011,7.2]
["NE101","Keith","Chappell fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.3]
["NE101","Keith","Chappell-Alice-Broadwater complex, 0 to 3 percent slopes","Well drained","A",0.75,66.599999999999994,7.2]
["NE101","Keith","Cullison fine sandy loam, very rarely flooded","Poorly drained","B/D",5,38.5,7.9]
["NE101","Keith","Cullison mucky peat","Very poorly drained","B/D",8.5,38.5,7.9]
["NE101","Keith","Dix gravelly loam, 3 to 20 percent slopes","Excessively drained","B",1.125,68.800000000000011,7.25]
["NE101","Keith","Dix-Sulco-Sarben complex, 20 to 60 percent slopes","Excessively drained","B",0.75,62,7.35]
["NE101","Keith","Duroc loam, 0 to 1 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE101","Keith","Duroc loam, terrace, 0 to 1 percent slopes","Well drained","B",1.375,21.4,7.2]
["NE101","Keith","Duroc loam, terrace, 1 to 3 percent slopes","Well drained","B",1.375,21.4,7.2]
["NE101","Keith","Duroc silt loam, 0 to 1 percent slopes","Well drained","B",1.375,9.5,7.2]
["NE101","Keith","Duroc silt loam, 1 to 3 percent slopes","Well drained","B",1.375,9.5,7.2]
["NE101","Keith","Elsmere loamy fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,79.400000000000006,7.9]
["NE101","Keith","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",5,95.5,7.5]
["NE101","Keith","Gothenburg loamy sand, occasionally flooded","Poorly drained","A/D",0.25,91.9,7.5]
["NE101","Keith","Gothenburg soils, occasionally flooded","Poorly drained","A/D",0.25,91.9,7.5]
["NE101","Keith","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE101","Keith","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.95]
["NE101","Keith","Janise loam, drained, 0 to 3 percent slopes","Moderately well drained","C",0.75,43.8,9.1999999999999993]
["NE101","Keith","Janise loam, occasionally flooded","Somewhat poorly drained","C",0.75,42.2,9.4]
["NE101","Keith","Jankosh loam, rarely flooded","Somewhat poorly drained","C",0.5,48.400000000000006,8.5]
["NE101","Keith","Johnstown-Satanta-Richfield loams, 0 to 2 percent slopes","Well drained","C",1,42.1,7.25]
["NE101","Keith","Keith loam, 1 to 3 percent slopes","Well drained","B",0.75,21.2,7]
["NE101","Keith","Keith loam, 3 to 6 percent slopes","Well drained","B",0.75,21.2,7]
["NE101","Keith","Kuma loam, 0 to 1 percent slopes","Well drained","C",2,36.9,7.5]
["NE101","Keith","Kuma loam, 1 to 3 percent slopes","Well drained","C",2,36.9,7.5]
["NE101","Keith","Kuma silt loam, 1 to 3 percent slopes","Well drained","C",2,9,7.3]
["NE101","Keith","Lawet loam, rarely flooded","Poorly drained","C/D",2.875,48,8.0500000000000007]
["NE101","Keith","Lex loam, rarely flooded","Somewhat poorly drained","C",1,53.5,7.6]
["NE101","Keith","Lexsworth loam, very rarely flooded","Moderately well drained","C",0.25,91.9,8]
["NE101","Keith","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",2.5,16.599999999999998,7]
["NE101","Keith","Lodgepole silt loam, occasionally ponded","Somewhat poorly drained","C/D",2,21,7]
["NE101","Keith","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",3.125,80.150000000000006,7.5]
["NE101","Keith","Merrick loam, rarely flooded","Moderately well drained","C",1.25,39.1,7.6]
["NE101","Keith","Merrick sandy clay loam, very rarely flooded","Moderately well drained","C",0.75,41.1,7.9]
["NE101","Keith","Nenzel loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",1.25,86.8,6.7]
["NE101","Keith","Nenzel loamy fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",1.375,91.4,7.9]
["NE101","Keith","Norwest loam, 0 to 2 percent slopes","Somewhat poorly drained","C",0.75,39.799999999999997,7.9]
["NE101","Keith","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,67.3,7.5]
["NE101","Keith","Rosebud loam, 1 to 3 percent slopes","Well drained","C",0.75,38,7.35]
["NE101","Keith","Rosebud loam, 3 to 9 percent slopes","Well drained","C",0.75,38,7.35]
["NE101","Keith","Rosebud-Canyon loams, 3 to 6 percent slopes","Well drained","D",0.75,43.2,7.5]
["NE101","Keith","Sarben loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.5,73,6.95]
["NE101","Keith","Sarben loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.5,83,6.95]
["NE101","Keith","Sarben loamy fine sand, 6 to 9 percent slopes","Well drained","A",0.5,83,6.95]
["NE101","Keith","Sarben loamy fine sand, 9 to 20 percent slopes","Well drained","A",0.5,73,6.95]
["NE101","Keith","Satanta loam, 0 to 1 percent slopes","Well drained","B",1.25,43,7.5]
["NE101","Keith","Satanta loam, 1 to 3 percent slopes","Well drained","B",1.25,43,7.5]
["NE101","Keith","Satanta loam, 3 to 6 percent slopes","Well drained","B",1.25,43,7.5]
["NE101","Keith","Satanta very fine sandy loam, 1 to 3 percent slopes","Well drained","C",0.75,64.400000000000006,7.5]
["NE101","Keith","Satanta very fine sandy loam, 3 to 6 percent slopes","Well drained","C",0.75,64.400000000000006,8.4]
["NE101","Keith","Satanta-Dix complex, 3 to 9 percent slopes","Excessively drained","B",1.25,45.7,7.5]
["NE101","Keith","Satanta-Johnstown-Altvan loams, 1 to 3 percent slopes","Well drained","C",1,42.1,7.35]
["NE101","Keith","Sulco loam, 30 to 60 percent slopes","Well drained","B",1,43.95,8.0500000000000007]
["NE101","Keith","Sulco loam, 6 to 9 percent slopes","Well drained","B",1,43.95,8.0500000000000007]
["NE101","Keith","Sulco-Dix complex, 9 to 20 percent slopes","Excessively drained","B",1,45,7.7]
["NE101","Keith","Sulco-McConaughy loams, 6 to 9 percent slopes, eroded","Well drained","B",0.75,42.2,7.9]
["NE101","Keith","Sulco-McConaughy loams, 9 to 30 percent slopes","Well drained","B",0.75,43.6,7.9]
["NE101","Keith","Tassel-Ashollow-Rock outcrop complex, 20 to 60 percent slopes","Well drained","A",0.75,63.3,7.9]
["NE101","Keith","Tassel-Otero-Rock outcrop complex, 15 to 60 percent slopes","Well drained","A",0.625,64.400000000000006,7.9]
["NE101","Keith","Valent sand, rolling","Excessively drained","A",0.5,95,7]
["NE101","Keith","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE101","Keith","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE101","Keith","Valentine fine sand, gullied, 30 to 60 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE101","Keith","Valentine fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE101","Keith","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,94.9,7.2]
["NE101","Keith","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.75,86.8,6.7]
["NE101","Keith","Vetal loamy fine sand, 0 to 3 percent slopes","Well drained","A",2,85.9,7.2]
["NE101","Keith","Wann fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,63.5,8.1999999999999993]
["NE103","Keya Paha",null,"",""]
["NE103","Keya Paha","Albaton silty clay, occasionally flooded","Poorly drained","D",0.5,34.200000000000003,8.1999999999999993]
["NE103","Keya Paha","Almeria loamy fine sand, occasionally flooded","Poorly drained","A/D",1.25,89.4,6.9]
["NE103","Keya Paha","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE103","Keya Paha","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE103","Keya Paha","Anselmo loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,83.5,7]
["NE103","Keya Paha","Barney fine sandy loam, frequently flooded","Very poorly drained","A/D",0.25,91,7.5]
["NE103","Keya Paha","Barney-Boel complex, channeled","Very poorly drained","A/D",0.25,91,7.5]
["NE103","Keya Paha","Barney-Bolent complex, channeled, occasionally flooded","Poorly drained","A/D",0.5,89.9,7.25]
["NE103","Keya Paha","Blackloup loam, occasionally flooded","Very poorly drained","B/D",0.5,72.55,7.4]
["NE103","Keya Paha","Blackloup loam, rarely flooded","Poorly drained","B/D",0.75,65.900000000000006,7.4]
["NE103","Keya Paha","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.2,7.5]
["NE103","Keya Paha","Brocksburg loam, 0 to 2 percent slopes","Well drained","C",1.5,39.799999999999997,7.2]
["NE103","Keya Paha","Cass loam, channeled, frequently flooded","Well drained","B",0.75,66.900000000000006,7.3]
["NE103","Keya Paha","Cass loam, rarely flooded","Well drained","B",0.75,66.900000000000006,7.3]
["NE103","Keya Paha","Duda loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.5,86.8,6.7]
["NE103","Keya Paha","Duda loamy fine sand, 3 to 6 percent slopes","Somewhat excessively drained","A",0.5,86.8,6.7]
["NE103","Keya Paha","Duda-Fishberry loamy fine sands, 0 to 3 percent slopes","Somewhat excessively drained","A",0.5,80.099999999999994,6.85]
["NE103","Keya Paha","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE103","Keya Paha","Dunday-Duda loamy fine sands, 0 to 3 percent slopes","Somewhat excessively drained","A",0.5,86.8,6.7]
["NE103","Keya Paha","Els fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,94.4,6.7]
["NE103","Keya Paha","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.5]
["NE103","Keya Paha","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,44.85,3.75]
["NE103","Keya Paha","Fluvaquents, sandy-Fluvaquents, loamy complex, frequently flooded","Very poorly drained","A/D",0.5,78.95,7.55]
["NE103","Keya Paha","Hennings fine sandy loam, 0 to 3 percent slopes","Well drained","C",0.25,67.3,7.2]
["NE103","Keya Paha","Holt fine sandy loam, 0 to 2 percent slopes","Well drained","B",1,64.449999999999989,7.1]
["NE103","Keya Paha","Holt fine sandy loam, 2 to 6 percent slopes","Well drained","B",1,62.65,7.1]
["NE103","Keya Paha","Holt variant fine sandy loam, 3 to 6 percent slopes","Well drained","A",1,62.5,7]
["NE103","Keya Paha","Holt variant loamy fine sand, 0 to 3 percent slopes","Well drained","A",1,62.5,7]
["NE103","Keya Paha","Holt variant loamy fine sand, 3 to 6 percent slopes","Well drained","A",1,62.5,7]
["NE103","Keya Paha","Holt-Longpine fine sandy loams, 2 to 6 percent slopes","Well drained","B",0.75,64.599999999999994,7.2]
["NE103","Keya Paha","Holt-Longpine fine sandy loams, 6 to 11 percent slopes","Well drained","B",0.75,62.8,7.2]
["NE103","Keya Paha","Inavale fine sand, 3 to 11 percent slopes","Excessively drained","A",0.25,92.2,6.7]
["NE103","Keya Paha","Inavale fine sand, channeled, frequently flooded","Excessively drained","A",0.25,92.2,6.7]
["NE103","Keya Paha","Inavale loamy fine sand, occasionally flooded","Excessively drained","A",0.25,91.6,6.7]
["NE103","Keya Paha","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE103","Keya Paha","Jansen fine sandy loam, 0 to 2 percent slopes","Well drained","B",0.75,72.75,6.2]
["NE103","Keya Paha","Jansen loam, 0 to 2 percent slopes","Well drained","B",0.75,58.8,6.2]
["NE103","Keya Paha","Jansen loam, 2 to 6 percent slopes","Well drained","B",0.75,60.949999999999996,6.2]
["NE103","Keya Paha","Jansen-Meadin loams, 0 to 2 percent slopes","Well drained","B",0.75,65.3,6.2]
["NE103","Keya Paha","Labu silty clay, 6 to 11 percent slopes","Well drained","D",0.75,2.6,7.5]
["NE103","Keya Paha","Labu-Sansarc silty clays, 11 to 30 percent slopes","Well drained","D",0.65,2.6,7.7]
["NE103","Keya Paha","Longpine loamy fine sand, 3 to 30 percent slopes","Well drained","D",0.75,64.599999999999994,7.5]
["NE103","Keya Paha","Longpine-Duda complex, 3 to 15 percent slopes","Somewhat excessively drained","A",0.625,64.599999999999994,6.85]
["NE103","Keya Paha","Longpine-Ronson-Duda complex, 15 to 70 percent slopes","Somewhat excessively drained","A",0.75,66.099999999999994,7]
["NE103","Keya Paha","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",3.375,79.2,6.6]
["NE103","Keya Paha","Loup fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,79.2,6.6]
["NE103","Keya Paha","Mariaville-Keota silt loams, 11 to 60 percent slopes","Well drained","C",0.75,17.75,7.9]
["NE103","Keya Paha","Mariaville-Paka loams, 11 to 40 percent slopes","Well drained","D",0.75,19.899999999999999,7.2]
["NE103","Keya Paha","Marlake loamy fine sand, frequently ponded","Very poorly drained","A/D",0.75,93.2,7]
["NE103","Keya Paha","McKelvie loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,88,7]
["NE103","Keya Paha","McKelvie loamy fine sand, 9 to 30 percent slopes","Excessively drained","A",0.25,92.9,7]
["NE103","Keya Paha","McKelvie-Fishberry-Rock outcrop complex, 11 to 60 percent slopes","Excessively drained","D",0.375,83.55,7.25]
["NE103","Keya Paha","McKelvie-Rock outcrop complex, 30 to 60 percent slopes","Excessively drained","A",0.25,89.85,7]
["NE103","Keya Paha","Meadin gravelly sandy loam, 2 to 30 percent slopes","Excessively drained","A",0.25,84.3,6.2]
["NE103","Keya Paha","Munjor fine sandy loam, rarely flooded","Well drained","A",0.25,67.3,7.9]
["NE103","Keya Paha","O'Neill fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,67.400000000000006,6.5]
["NE103","Keya Paha","O'Neill fine sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,66.900000000000006,6.5]
["NE103","Keya Paha","O'Neill fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,67.400000000000006,6.5]
["NE103","Keya Paha","O'Neill loamy fine sand, 0 to 2 percent slopes","Well drained","A",0.75,86.8,6.5]
["NE103","Keya Paha","O'Neill-Meadin fine sandy loams, 0 to 2 percent slopes","Excessively drained","A",0.75,66.449999999999989,6.35]
["NE103","Keya Paha","O'Neill-Valentine complex, 2 to 11 percent slopes","Well drained","A",0.5,94.5,6.5]
["NE103","Keya Paha","Onita silt loam, 0 to 1 percent slopes","Well drained","C",1,19.7,6.7]
["NE103","Keya Paha","Ord fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE103","Keya Paha","Ord fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE103","Keya Paha","Ord-Loup fine sandy loams, 0 to 1 percent slopes","Poorly drained","A/D",0.75,66.900000000000006,7.5]
["NE103","Keya Paha","Paka fine sandy loam, 0 to 2 percent slopes","Well drained","C",1.5,7,7]
["NE103","Keya Paha","Paka fine sandy loam, 2 to 6 percent slopes","Well drained","C",1.125,18.05,7.1]
["NE103","Keya Paha","Paka loam, 0 to 2 percent slopes","Well drained","C",1.125,8.25,7.1]
["NE103","Keya Paha","Paka-Mariaville loams, 11 to 30 percent slopes","Well drained","D",0.75,9.5,7.2]
["NE103","Keya Paha","Paka-Mariaville loams, 2 to 6 percent slopes","Well drained","D",0.75,9.5,7.2]
["NE103","Keya Paha","Ree loam, 0 to 2 percent slopes","Well drained","C",1.25,39.1,7.5]
["NE103","Keya Paha","Ree loam, clayey substratum, 0 to 2 percent slopes","Well drained","C",0.25,38.5,7]
["NE103","Keya Paha","Reliance silt loam, 2 to 6 percent slopes","Well drained","C",0.875,23.9,7.1]
["NE103","Keya Paha","Ronson-Anselmo fine sandy loams, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE103","Keya Paha","Ronson-Anselmo fine sandy loams, 6 to 30 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE103","Keya Paha","Ronson-Longpine fine sandy loams, 0 to 2 percent slopes","Well drained","D",0.75,64.599999999999994,7.4]
["NE103","Keya Paha","Sansarc silty clay, 20 to 40 percent slopes","Well drained","D",0.55000000000000004,5,7.9]
["NE103","Keya Paha","Schamber gravelly sandy loam, 9 to 30 percent slopes","Excessively drained","A",0.875,79.3,7.6]
["NE103","Keya Paha","Simeon-Holt variant-Ronson complex, 6 to 17 percent slopes","Well drained","A",0.75,72.55,7]
["NE103","Keya Paha","Simeon-Valentine fine sands, 6 to 17 percent slopes, eroded","Excessively drained","A",0.5,94.25,6.75]
["NE103","Keya Paha","Simeon-Valentine loamy sands, 0 to 3 percent slopes","Excessively drained","A",0.5,88.5,6.75]
["NE103","Keya Paha","Simeon-Valentine loamy sands, 0 to 6 percent slopes","Excessively drained","A",0.25,92.1,6.5]
["NE103","Keya Paha","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.1]
["NE103","Keya Paha","Valentine fine sand, hilly","Excessively drained","A",0.5,96.3,6.5]
["NE103","Keya Paha","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE103","Keya Paha","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,94.5,6.5]
["NE103","Keya Paha","Valentine loamy fine sand, gently rolling","Excessively drained","A",0.5,91.8,6.5]
["NE103","Keya Paha","Valentine loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE103","Keya Paha","Valentine-Duda complex, 3 to 9 percent slopes","Somewhat excessively drained","A",0.5,86.8,6.4]
["NE103","Keya Paha","Valentine-Longpine complex, rolling","Well drained","D",0.75,64.599999999999994,6.5]
["NE103","Keya Paha","Valentine-Wewela loamy fine sands, 3 to 6 percent slopes","Excessively drained","A",0.625,60.150000000000006,6.6]
["NE103","Keya Paha","Valentine-Wewela loamy fine sands, 6 to 30 percent slopes","Excessively drained","A",0.625,70.650000000000006,6.6]
["NE103","Keya Paha","Verdel silty clay loam, 0 to 2 percent slopes","Well drained","D",1.375,11.3,7.4]
["NE103","Keya Paha","Verdel silty clay loam, 2 to 6 percent slopes","Well drained","D",1.375,11.3,7.4]
["NE103","Keya Paha","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE103","Keya Paha","Vetal loam, 0 to 1 percent slopes","Well drained","A",1.25,44.8,7]
["NE103","Keya Paha","Vetal loam, 1 to 3 percent slopes","Well drained","A",1.25,44.8,7]
["NE103","Keya Paha","Vetal loam, 3 to 6 percent slopes","Well drained","A",1.25,65.900000000000006,7]
["NE103","Keya Paha","Wewela fine sandy loam, 0 to 2 percent slopes","Well drained","D",1.25,38.75,6.7]
["NE103","Keya Paha","Wewela fine sandy loam, 2 to 6 percent slopes","Well drained","D",1.25,38.75,6.7]
["NE105","Kimball",null,"",""]
["NE105","Kimball","Albinas-Cheyenne loams, rarely flooded","Well drained","C",1.25,41.4,7.2]
["NE105","Kimball","Alliance loam, 0 to 1 percent slopes","Well drained","B",0.75,31.9,7.2]
["NE105","Kimball","Alliance loam, 1 to 3 percent slopes","Well drained","B",0.75,31.9,7.2]
["NE105","Kimball","Alliance loam, 3 to 6 percent slopes","Well drained","C",0.75,42.2,7.2]
["NE105","Kimball","Altvan fine sandy loam, 1 to 3 percent slopes","Well drained","C",0.75,54.5,7.5]
["NE105","Kimball","Altvan loam, 0 to 1 percent slopes","Well drained","C",1.25,38,7.2]
["NE105","Kimball","Altvan-Eckley complex, 3 to 9 percent slopes","Well drained","C",0.75,68,7.2]
["NE105","Kimball","Altvan-Eckley-Tassel complex, 3 to 9 percent slopes","Well drained","C",0.75,64.599999999999994,7.2]
["NE105","Kimball","Altvan-Satanta fine sandy loams, 1 to 3 percent slopes","Well drained","C",0.75,40.549999999999997,7.5]
["NE105","Kimball","Altvan-Satanta loams, 0 to 1 percent slopes","Well drained","C",0.75,40,7.5]
["NE105","Kimball","Bayard fine sandy loam, 0 to 1 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE105","Kimball","Bayard fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.125,65.400000000000006,6.85]
["NE105","Kimball","Bayard fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.125,65.400000000000006,6.85]
["NE105","Kimball","Bayard very fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE105","Kimball","Bridget very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE105","Kimball","Broadwater loamy sand, channeled, occasionally flooded","Excessively drained","A",0.25,91.9,7.2]
["NE105","Kimball","Brownson-Rosebud-Canyon loams, 0 to 3 percent slopes","Well drained","D",0.75,35.75,7.2]
["NE105","Kimball","Chappell-Bayard-Broadwater complex, 0 to 2 percent slopes","Well drained","A",0.75,68,7.2]
["NE105","Kimball","Duroc loam, 0 to 1 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE105","Kimball","Dwyer loamy fine sand, 9 to 17 percent slopes","Excessively drained","A",1.125,78.900000000000006,7.7]
["NE105","Kimball","Dwyer loamy sand, 0 to 3 percent slopes","Excessively drained","A",1,81,7]
["NE105","Kimball","Eckley and Altvan soils, 9 to 50 percent slopes","Well drained","C",1,69,7.2]
["NE105","Kimball","Glenberg fine sandy loam, rarely flooded","Well drained","A",0.75,80.75,7.45]
["NE105","Kimball","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,67.599999999999994,7.2]
["NE105","Kimball","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,67.599999999999994,7.2]
["NE105","Kimball","Keith loam, 0 to 1 percent slopes","Well drained","C",0.5,29.2,7.45]
["NE105","Kimball","Keith loam, 1 to 3 percent slopes","Well drained","C",0.5,29.2,7.45]
["NE105","Kimball","Kuma loam, 0 to 1 percent slopes","Well drained","C",2,36.9,7.5]
["NE105","Kimball","Las Animas loam, channeled, occasionally flooded","Poorly drained","B/D",1.125,53.5,7.9]
["NE105","Kimball","Lodgepole loam, occasionally ponded","Somewhat poorly drained","C/D",1.75,28,7.1]
["NE105","Kimball","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",1.375,26.55,7.25]
["NE105","Kimball","Rosebud loam, 0 to 1 percent slopes","Well drained","C",0.75,35.75,7.2]
["NE105","Kimball","Rosebud loam, 1 to 3 percent slopes","Well drained","C",0.75,38,7.35]
["NE105","Kimball","Rosebud-Blanche complex , 1 to 3 percent slopes","Well drained","B",0.5,38,7.6]
["NE105","Kimball","Rosebud-Canyon loams, 1 to 3 percent slopes","Well drained","D",0.75,37,7.2]
["NE105","Kimball","Rosebud-Hemingford loams, 0 to 1 percent slopes","Well drained","C",0.75,38,7.2]
["NE105","Kimball","Rosebud-Tassel sandy loams, 0 to 3 percent slopes","Well drained","C",0.5,53.3,7.5500000000000007]
["NE105","Kimball","Satanta fine sandy loam, 1 to 3 percent slopes","Well drained","C",1,65.400000000000006,7.7]
["NE105","Kimball","Sidney-Canyon loams, 6 to 9 percent slopes, eroded","Well drained","D",1,43.4,7.9]
["NE105","Kimball","Tassel and Dix and Altvan soils, 9 to 30 percent slopes","Well drained","C",0.75,68,7.2]
["NE105","Kimball","Tassel-Ashollow-Rock outcrop complex, 20 to 60 percent slopes","Well drained","B",0.75,63.3,7.9]
["NE105","Kimball","Tassel-Blanche complex, 9 to 30 percent slopes","Well drained","B",0.25,62.5,7.75]
["NE105","Kimball","Tassel-Blanche sandy loams, 3 to 9 percent slopes","Well drained","B",0.25,62.5,7.6]
["NE105","Kimball","Tripp loam, 0 to 1 percent slopes","Well drained","B",0.5,39.549999999999997,7.7]
["NE105","Kimball","Tripp loam, 1 to 3 percent slopes","Well drained","B",0.5,39.549999999999997,7.7]
["NE107","Knox",null,"",""]
["NE107","Knox","Albaton silty clay, frequently flooded","Very poorly drained","D",2.5,5.3,7.9]
["NE107","Knox","Albaton silty clay, frequently flooded, wet","Very poorly drained","D",1.5,3.9,7.9]
["NE107","Knox","Albaton silty clay, occasionally flooded","Poorly drained","D",1.5,3.9,7.9]
["NE107","Knox","Albaton silty clay, occasionally flooded, wet","Very poorly drained","D",1.5,3.9,7.9]
["NE107","Knox","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE107","Knox","Alcester silt loam, 6 to 11 percent slopes","Well drained","B",2.5,7.4,7]
["NE107","Knox","Aowa silt loam, channeled, frequently flooded","Well drained","B",1.625,9.0500000000000007,7.9]
["NE107","Knox","Aowa silt loam, channeled, frequently flooded, wet","Well drained","B",1.625,9.0500000000000007,7.9]
["NE107","Knox","Aowa silt loam, occasionally flooded","Well drained","B",1.625,9.0500000000000007,7.9]
["NE107","Knox","Aowa silt loam, occasionally flooded, wet","Well drained","B",1.625,9.0500000000000007,7.9]
["NE107","Knox","Barney loam, frequently flooded","Poorly drained","B/D",1.625,67.650000000000006,7.35]
["NE107","Knox","Barney loam, frequently flooded, wet","Very poorly drained","B/D",1.625,67.650000000000006,7.35]
["NE107","Knox","Bazile loam, 0 to 2 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE107","Knox","Bazile loam, 2 to 6 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE107","Knox","Bazile loam, 6 to 11 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE107","Knox","Bazile loamy fine sand, 0 to 2 percent slopes","Well drained","C",0.75,87.3,6.5]
["NE107","Knox","Bazile loamy fine sand, 2 to 6 percent slopes","Well drained","C",0.75,87.3,6.5]
["NE107","Knox","Bazile loamy fine sand, 6 to 11 percent slopes","Well drained","C",0.75,87.3,6.5]
["NE107","Knox","Betts clay loam, 11 to 15 percent slopes, eroded","Well drained","C",0.5,35.4,7.9]
["NE107","Knox","Betts clay loam, 15 to 30 percent slopes","Well drained","C",0.5,35.4,7.9]
["NE107","Knox","Betts clay loam, 30 to 60 percent slopes","Well drained","C",0.5,35.4,7.9]
["NE107","Knox","Betts clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,35.4,7.9]
["NE107","Knox","Betts clay loam, 6 to 15 percent slopes","Well drained","C",1.75,20.85,7.55]
["NE107","Knox","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,67.3,7.3]
["NE107","Knox","Blyburg silt loam, rarely flooded","Well drained","B",0.875,14,7.85]
["NE107","Knox","Blyburg silt loam, rarely flooded, wet","Well drained","B",0.875,14,7.85]
["NE107","Knox","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE107","Knox","Boel loamy fine sand, occasionally flooded, wet","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE107","Knox","Boelus loamy sand, 0 to 3 percent slopes","Well drained","B",0.5,53.9,7]
["NE107","Knox","Boelus loamy sand, 3 to 6 percent slopes","Well drained","B",0.5,53.9,7]
["NE107","Knox","Boelus loamy sand, 6 to 11 percent slopes","Well drained","B",0.5,53.9,7]
["NE107","Knox","Bristow silty clay, 30 to 60 percent slopes","Well drained","D",0.25,2.6,7.9]
["NE107","Knox","Brunswick fine sandy loam, 6 to 11 percent slopes","Well drained","B",0.25,66.900000000000006,6.5]
["NE107","Knox","Brunswick-Paka complex, 17 to 30 percent slopes","Well drained","B",0.5,32.1,6.6]
["NE107","Knox","Brunswick-Paka complex, 6 to 17 percent slopes","Well drained","B",0.5,23.55,6.6]
["NE107","Knox","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",2.25,23.450000000000003,6.25]
["NE107","Knox","Coleridge silt loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE107","Knox","Coleridge silt loam, occasionally flooded, wet","Somewhat poorly drained","C",2,6.9,6.5]
["NE107","Knox","Crofton silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE107","Knox","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE107","Knox","Crofton silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,10,7.9]
["NE107","Knox","Crofton silt loam, 30 to 60 percent slopes","Well drained","B",0.75,10,7.9]
["NE107","Knox","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10,7.9]
["NE107","Knox","Crofton silt loam, coarse, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE107","Knox","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE107","Knox","Crofton-Nora complex, 2 to 6 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE107","Knox","Crofton-Nora complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE107","Knox","Crofton-Nora silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE107","Knox","Crofton-Thurman complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,39.100000000000009,7.2]
["NE107","Knox","Crofton-Thurman complex, 17 to 30 percent slopes","Well drained","B",0.75,39.100000000000009,7.2]
["NE107","Knox","Crofton-Thurman complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,39.100000000000009,7.2]
["NE107","Knox","Elsmere fine sandy loam, rarely flooded","Somewhat poorly drained","B",1.125,80.150000000000006,6.6]
["NE107","Knox","Elsmere fine sandy loam, rarely flooded, wet","Somewhat poorly drained","B",1.125,80.150000000000006,6.6]
["NE107","Knox","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.5]
["NE107","Knox","Eltree silt loam, 0 to 3 percent slopes","Well drained","B",1,9.5,7.9]
["NE107","Knox","Eltree silt loam, 3 to 6 percent slopes","Well drained","B",1,9.5,7.9]
["NE107","Knox","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",2.25,15.05,6.25]
["NE107","Knox","Fluvaquents, frequently flooded","Very poorly drained","A/D",5,19.2,7.5]
["NE107","Knox","Fluvaquents, frequently flooded, wet","Very poorly drained","B/D",5,19.2,7.5]
["NE107","Knox","Gavins silt loam, 30 to 60 percent slopes","Well drained","D",0.5,24,7.5]
["NE107","Knox","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE107","Knox","Gibbon silt loam, occasionally flooded, wet","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE107","Knox","Hobbs silt loam, frequently flooded, wet","Well drained","B",1.875,11.3,7]
["NE107","Knox","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE107","Knox","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE107","Knox","Hord silt loam, rarely flooded, wet","Well drained","B",0.75,9.3000000000000007,7]
["NE107","Knox","Inavale fine sand, channeled, frequently flooded","Excessively drained","A",0.25,92.2,6.7]
["NE107","Knox","Inavale fine sand, channeled, frequently flooded, wet","Excessively drained","A",0.25,92.2,6.7]
["NE107","Knox","Inavale fine sand, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE107","Knox","Inavale fine sand, rarely flooded, wet","Excessively drained","A",0.25,92.2,7.5]
["NE107","Knox","Inavale fine sandy loam, occasionally flooded, wet","Excessively drained","A",0.25,92.2,6.7]
["NE107","Knox","Inavale fine sandy loam, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE107","Knox","Inavale loamy fine sand, occasionally flooded, wet","Excessively drained","A",0.25,87.3,6.7]
["NE107","Knox","Inavale loamy fine sand, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE107","Knox","Inavale loamy fine sand, rarely flooded, wet","Excessively drained","A",0.25,92.2,7.5]
["NE107","Knox","Inglewood loamy fine sand, rarely flooded","Moderately well drained","A",0.25,71.8,7]
["NE107","Knox","Kezan silt loam, channeled, frequently flooded","Poorly drained","C",1.875,7.95,7.7]
["NE107","Knox","Kezan silt loam, occasionally flooded","Poorly drained","C",1.875,7.85,7.35]
["NE107","Knox","Kezan silt loam, occasionally flooded, wet","Poorly drained","C",1.875,9.0500000000000007,7.35]
["NE107","Knox","Labu silty clay, 6 to 11 percent slopes","Well drained","D",0.75,2.6,7.5]
["NE107","Knox","Labu-Sansarc complex, 11 to 30 percent slopes","Well drained","D",0.65,1.3,7.7]
["NE107","Knox","Longford silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,19,6.5]
["NE107","Knox","Longford silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,19,6.5]
["NE107","Knox","Loretto fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE107","Knox","Loretto fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE107","Knox","Lynch-Bristow complex, 11 to 30 percent slopes","Well drained","D",0.5,2.5499999999999998,7.9]
["NE107","Knox","Lynch-Verdel complex, 6 to 11 percent slopes","Well drained","D",0.75,5.3,7.8]
["NE107","Knox","Mariaville very fine sandy loam, 2 to 30 percent slopes","Well drained","D",0.75,59,7.9]
["NE107","Knox","Meadin sandy loam, 0 to 2 percent slopes","Excessively drained","B",0.75,67.8,6.2]
["NE107","Knox","Meadin-O'Neill complex, 2 to 30 percent slopes","Excessively drained","B",0.75,68.150000000000006,6.35]
["NE107","Knox","Meckling loamy fine sand, occasionally flooded","Moderately well drained","A",0.5,87.2,7.9]
["NE107","Knox","Moody loam, 0 to 2 percent slopes","Well drained","C",3,9.4,6.5]
["NE107","Knox","Moody loam, 2 to 6 percent slopes","Well drained","C",3,9.4,6.5]
["NE107","Knox","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE107","Knox","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE107","Knox","Nora silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE107","Knox","Nora silty clay loam, 11 to 17 percent slopes","Well drained","C",0.75,8.9,7]
["NE107","Knox","Nora silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,8.9,7]
["NE107","Knox","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE107","Knox","Norway loamy fine sand, frequently flooded","Very poorly drained","A/D",0.375,79.900000000000006,7.7]
["NE107","Knox","Norway loamy fine sand, frequently flooded, wet","Very poorly drained","A/D",0.375,79.900000000000006,7.7]
["NE107","Knox","Obert silt loam, occasionally flooded","Very poorly drained","C/D",1.5,7.3,7.9]
["NE107","Knox","Obert silt loam, occasionally flooded, wet","Very poorly drained","B/D",1.5,7.3,7.9]
["NE107","Knox","Onawa silty clay, occasionally flooded, wet","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE107","Knox","Onawa silty clay, rarely flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE107","Knox","O'Neill sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,68.5,6.5]
["NE107","Knox","O'Neill sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,68.5,6.5]
["NE107","Knox","Ord fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE107","Knox","Ord fine sandy loam, occasionally flooded, wet","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE107","Knox","Ord loam, occasionally flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE107","Knox","Ortello fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE107","Knox","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE107","Knox","Orwet loam, rarely flooded","Poorly drained","B/D",0.75,84.9,7.5]
["NE107","Knox","Orwet loam, rarely flooded, wet","Poorly drained","B/D",0.75,84.9,7.5]
["NE107","Knox","Paka loam, 0 to 2 percent slopes","Well drained","B",1.125,8.25,7.1]
["NE107","Knox","Paka loam, 11 to 20 percent slopes","Well drained","B",1.125,8.25,7.1]
["NE107","Knox","Paka loam, 2 to 6 percent slopes","Well drained","B",1.125,8.25,7.1]
["NE107","Knox","Paka loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,8.25,7.1]
["NE107","Knox","Percival silty clay, rarely flooded","Somewhat poorly drained","D",1,5.3,7.9]
["NE107","Knox","Percival silty clay, rarely flooded, wet","Somewhat poorly drained","D",1,5.3,7.9]
["NE107","Knox","Redstoe silt loam, 6 to 11 percent slopes","Well drained","C",2,9,7.5]
["NE107","Knox","Redstoe-Gavins complex, 11 to 30 percent slopes","Well drained","D",1.25,10.1,7.5]
["NE107","Knox","Sansarc silty clay, 30 to 60 percent slopes","Well drained","D",0.55000000000000004,0,7.9]
["NE107","Knox","Sardak loamy fine sand, 2 to 11 percent slopes, very rare flooding","Excessively drained","A",0.5,87.9,7.5]
["NE107","Knox","Sardak loamy fine sand, 2 to 11 percent slopes, very rare flooding, wet","Excessively drained","A",0.5,87.9,7.5]
["NE107","Knox","Scott silt loam, frequently ponded","Poorly drained","D",1.5,18.7,6.7]
["NE107","Knox","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE107","Knox","Shell silt loam, occasionally flooded, wet","Well drained","B",0.75,9.1,6.5]
["NE107","Knox","Simeon loamy sand, 0 to 6 percent slopes","Excessively drained","A",0.5,87.3,7]
["NE107","Knox","Simeon sand, 6 to 30 percent slopes, eroded","Excessively drained","A",0.5,91.85,7]
["NE107","Knox","Simeon sandy loam, 0 to 6 percent slopes","Excessively drained","A",0.5,80.199999999999989,7]
["NE107","Knox","Simeon-Thurman complex, 6 to 30 percent slopes","Excessively drained","A",0.25,84.9,6.5]
["NE107","Knox","Solomon silty clay, occasionally flooded","Poorly drained","D",1.75,5.5,8.1999999999999993]
["NE107","Knox","Solomon silty clay, occasionally flooded, wet","Poorly drained","C/D",1.75,5.5,8.1999999999999993]
["NE107","Knox","Solomon silty clay, rarely flooded","Poorly drained","D",1.75,5.5,8.1999999999999993]
["NE107","Knox","Solomon silty clay, rarely flooded, wet","Poorly drained","C/D",1.75,5.5,8.1999999999999993]
["NE107","Knox","Thurman fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.875,94.9,6.5]
["NE107","Knox","Thurman fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.875,94.9,6.5]
["NE107","Knox","Thurman fine sandy loam, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE107","Knox","Thurman fine sandy loam, 11 to 30 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE107","Knox","Thurman fine sandy loam, 2 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE107","Knox","Thurman loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.875,89.9,6.5]
["NE107","Knox","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.875,89.9,6.5]
["NE107","Knox","Trent silt loam, 0 to 2 percent slopes","Well drained","B",2.5,8.8000000000000007,6.7]
["NE107","Knox","Trent silt loam, moderately wet, 0 to 2 percent slopes","Moderately well drained","B",1,8.6,7]
["NE107","Knox","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE107","Knox","Valentine fine sand, 9 to 24 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE107","Knox","Verdel silty clay, 0 to 2 percent slopes","Well drained","C",1.375,5.3,7.4]
["NE107","Knox","Verdel silty clay, 0 to 2 percent slopes, wet","Well drained","D",0.75,6.2,7.4499999999999993]
["NE107","Knox","Verdel silty clay, 2 to 6 percent slopes","Well drained","C",1.375,5.3,7.4]
["NE107","Knox","Verdel silty clay, 2 to 6 percent slopes, wet","Well drained","D",0.75,6.2,7.4499999999999993]
["NE107","Knox","Verdel silty clay, 6 to 11 percent slopes","Well drained","C",1.375,5.3,7.4]
["NE107","Knox","Verdigre fine sandy loam, 11 to 30 percent slopes","Well drained","C",0.75,18.2,6.5]
["NE107","Knox","Verdigre fine sandy loam, 2 to 6 percent slopes","Well drained","C",0.75,18.2,6.5]
["NE107","Knox","Verdigre fine sandy loam, 6 to 11 percent slopes","Well drained","C",0.75,18.2,6.5]
["NE107","Knox","Verdigre loam, 11 to 30 percent slopes","Well drained","C",0.75,18.2,6.5]
["NE107","Knox","Verdigre loam, 2 to 6 percent slopes","Well drained","C",0.75,18.2,6.5]
["NE107","Knox","Verdigre loam, 6 to 11 percent slopes","Well drained","C",0.75,18.2,6.5]
["NE107","Knox","Wann loam, occasionally flooded, wet","Somewhat poorly drained","C",0.75,66.2,8.1999999999999993]
["NE109","Lancaster",null,"",""]
["NE109","Lancaster","Aksarben silty clay loam, 0 to 2 percent slopes","Well drained","C",1.125,14,5.9499999999999993]
["NE109","Lancaster","Aksarben silty clay loam, 2 to 6 percent slopes","Well drained","C",1.5,20,6.1]
["NE109","Lancaster","Aksarben silty clay loam, 6 to 11 percent slopes","Well drained","C",1.5,20,6.1]
["NE109","Lancaster","Aksarben silty clay loam, terrace, 0 to 1 percent slopes","Well drained","C",1.5,20,6.1]
["NE109","Lancaster","Burchard clay loam, 11 to 17 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE109","Lancaster","Burchard clay loam, 6 to 11 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE109","Lancaster","Burchard-Nodaway complex, 2 to 30 percent slopes","Well drained","C",0.75,35.4,6.7]
["NE109","Lancaster","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.5,7.9]
["NE109","Lancaster","Burchard-Steinauer clay loams, 11 to 30 percent slopes","Somewhat excessively drained","C",0.75,34.5,7.9]
["NE109","Lancaster","Burchard-Steinauer clay loams, 6 to 11 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE109","Lancaster","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","D",1.5,22.1,6.3]
["NE109","Lancaster","Butler silt loam, terrace, 0 to 1 percent slopes","Somewhat poorly drained","D",1.5,22.1,6.3]
["NE109","Lancaster","Colo silty clay loam, occasionally flooded","Poorly drained","C/D",3.5,6.8,5.8]
["NE109","Lancaster","Colo-Nodaway complex, frequently flooded","Poorly drained","C/D",3,6.85,6.3]
["NE109","Lancaster","Colo-Nodaway silty clay loams, frequently flooded","Poorly drained","C/D",2.5,6.9,6.3]
["NE109","Lancaster","Cortland-Malmo complex, 6 to 11 percent slopes, eroded","Well drained","C",0.75,37.549999999999997,6.5]
["NE109","Lancaster","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE109","Lancaster","Crete silt loam, terrace, 0 to 1 percent slopes","Moderately well drained","C",1.625,19.850000000000001,6.25]
["NE109","Lancaster","Crete silty clay loam, terrace, 1 to 3 percent slopes","Moderately well drained","C",1.625,19.850000000000001,6.25]
["NE109","Lancaster","Crete silty clay loam, terrace, 3 to 7 percent slopes","Moderately well drained","C",1.25,19.7,6.7]
["NE109","Lancaster","Crete variant silty clay loam, 1 to 4 percent slopes","Moderately well drained","D",1.5,18.7,8.1999999999999993]
["NE109","Lancaster","Deroin silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,6.9,7]
["NE109","Lancaster","Dickinson fine sandy loam, 6 to 11 percent slopes","Somewhat excessively drained","A",0.75,67.3,5.8]
["NE109","Lancaster","Dickinson fine sandy loam, 6 to 11 percent slopes, eroded","Somewhat excessively drained","A",0.75,67.3,5.8]
["NE109","Lancaster","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1.5,6.8,6.9]
["NE109","Lancaster","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.3]
["NE109","Lancaster","Hedville sandy loam, 7 to 30 percent slopes","Somewhat excessively drained","D",2.5,43.2,6.3]
["NE109","Lancaster","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE109","Lancaster","Ida-Steinauer complex, 17 to 60 percent slopes","Well drained","B",0.5,22.35,7.9]
["NE109","Lancaster","Judson fine sandy loam, 2 to 6 percent slopes","Well drained","B",2.125,48.7,5.8]
["NE109","Lancaster","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3.5,7.9,5.8]
["NE109","Lancaster","Kennebec silt loam, occasionally flooded","Moderately well drained","B",2,5,6.35]
["NE109","Lancaster","Kenridge silty clay loam, occasionally flooded","Moderately well drained","C",2.75,6.8000000000000007,6.4]
["NE109","Lancaster","Kezan silt loam, channeled, frequently flooded","Poorly drained","B/D",2,7.05,7.2]
["NE109","Lancaster","Kezan silt loam, frequently flooded","Poorly drained","B/D",1.875,8.1999999999999993,7.2]
["NE109","Lancaster","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.6]
["NE109","Lancaster","Malcolm silt loam, 11 to 25 percent slopes","Well drained","C",1.25,11.4,5.8]
["NE109","Lancaster","Malcolm silt loam, 6 to 11 percent slopes","Well drained","C",1.25,11.4,5.8]
["NE109","Lancaster","Malcolm silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.25,7.1,6.1]
["NE109","Lancaster","Malmo clay loam, 2 to 6 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE109","Lancaster","Malmo clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE109","Lancaster","Malmo clay, 2 to 6 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE109","Lancaster","Malmo, eroded-Pawnee complex, 6 to 11 percent slopes","Moderately well drained","D",0.75,29.9,7]
["NE109","Lancaster","Mayberry clay loam, 3 to 11 percent slopes","Moderately well drained","D",0.75,34.200000000000003,6.5]
["NE109","Lancaster","Mayberry silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.75,26.1,6.5]
["NE109","Lancaster","Mayberry silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.75,26.1,6.5]
["NE109","Lancaster","Morrill clay loam, 11 to 17 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE109","Lancaster","Morrill clay loam, 6 to 11 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE109","Lancaster","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.6,35.200000000000003,6.1]
["NE109","Lancaster","Morrill-Malmo, eroded, complex, 3 to 11 percent slopes","Moderately well drained","D",0.75,35.4,6.8]
["NE109","Lancaster","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.4,6.3]
["NE109","Lancaster","Nodaway silt loam, channeled, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE109","Lancaster","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,9.5,6.3]
["NE109","Lancaster","Otoe silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE109","Lancaster","Otoe silty clay, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE109","Lancaster","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE109","Lancaster","Pawnee clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",2,33.5,7]
["NE109","Lancaster","Salmo silt loam, occasionally flooded","Somewhat poorly drained","C",2,7.7,7.5]
["NE109","Lancaster","Salmo silty clay loam, channeled, frequently flooded","Poorly drained","C/D",2,6.9,7.5]
["NE109","Lancaster","Salmo silty clay loam, occasionally flooded","Poorly drained","C/D",2,6.9,7.5]
["NE109","Lancaster","Saltillo silt loam, occasionally flooded","Poorly drained","B/D",0.25,4.6500000000000004,8.1999999999999993]
["NE109","Lancaster","Shelby and Burchard clay loams, 11 to 17 percent slopes","Well drained","C",0.625,35.4,6.6]
["NE109","Lancaster","Shelby clay loam, 6 to 11 percent slopes","Moderately well drained","C",0.5,34.700000000000003,5.8]
["NE109","Lancaster","Steinauer clay loam, 11 to 30 percent slopes","Well drained","C",0.75,33.6,8.1999999999999993]
["NE109","Lancaster","Steinauer clay loam, 20 to 40 percent slopes","Well drained","C",1,33.6,7.6]
["NE109","Lancaster","Steinauer clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1,33.6,7.6]
["NE109","Lancaster","Steinauer loam, 11 to 30 percent slopes","Well drained","C",0.75,36.200000000000003,7.6]
["NE109","Lancaster","Steinauer loam, 6 to 11 percent slopes","Well drained","C",0.75,36.200000000000003,7.6]
["NE109","Lancaster","Urban land-Crete-Aksarben complex, 0 to 2 percent slopes","Well drained","C",1.5,20,5.8]
["NE109","Lancaster","Urban land-Judson complex, 1 to 3 percent slopes","Moderately well drained","C",2.5,6.7,5.8]
["NE109","Lancaster","Urban land-Kennebec complex, 0 to 2 percent slopes","Moderately well drained","B",1.5,9.1,5.8]
["NE109","Lancaster","Urban land-Wymore-Aksarben complex, 2 to 6 percent slopes","Well drained","C",1.125,13.7,5.9499999999999993]
["NE109","Lancaster","Wabash silty clay, occasionally flooded","Poorly drained","D",2.25,6.5,6.4]
["NE109","Lancaster","Wymore silty clay loam, 0 to 1 percent slopes","Moderately well drained","D",1.5,17.3,7]
["NE109","Lancaster","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE109","Lancaster","Wymore silty clay loam, 1 to 3 percent slopes","Moderately well drained","D",1.5,17.3,7]
["NE109","Lancaster","Wymore silty clay loam, 2 to 6 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE109","Lancaster","Wymore silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",1.5,17.3,7]
["NE109","Lancaster","Wymore silty clay loam, 6 to 11 percent slopes","Moderately well drained","D",1.5,17.3,7]
["NE109","Lancaster","Wymore silty clay, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.5,7.7,6.5]
["NE109","Lancaster","Yutan silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.75,7.6,6.1]
["NE109","Lancaster","Yutan silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,7.6,6.1]
["NE109","Lancaster","Yutan, eroded-Aksarben silty clay loams, 2 to 6 percent slopes","Well drained","C",0.75,7.5,6.5]
["NE109","Lancaster","Yutan, eroded-Judson complex, 6 to 11 percent slopes","Well drained","C",0.875,7.2,6.6]
["NE109","Lancaster","Zoe silty clay loam, occasionally flooded","Poorly drained","D",0.75,7.2,7.6]
["NE109","Lancaster","Zook silt loam, occasionally flooded","Poorly drained","D",3,16.25,6.4]
["NE109","Lancaster","Zook silty clay loam, occasionally flooded","Poorly drained","D",4.5,7.75,6.4]
["NE111","Lincoln",null,"",""]
["NE111","Lincoln","Alda fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,69.400000000000006,7.5]
["NE111","Lincoln","Alda soils, occasionally flooded","Somewhat poorly drained","C",0.5,76.400000000000006,7.5]
["NE111","Lincoln","Almeria-Fluvaquents, sandy complex, channeled, frequently flooded","Poorly drained","B/D",7.5,44.3,6.8]
["NE111","Lincoln","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE111","Lincoln","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE111","Lincoln","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE111","Lincoln","Anselmo fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE111","Lincoln","Anselmo sandy loam, terrace, 0 to 3 percent slopes","Well drained","A",0.75,66.449999999999989,7.1]
["NE111","Lincoln","Anselmo sandy loam, terrace, 3 to 6 percent slopes","Well drained","A",0.75,66.449999999999989,7.1]
["NE111","Lincoln","Anselmo-Holdrege fine sandy loams, 3 to 7 percent slopes","Well drained","A",0.75,66.099999999999994,7.1]
["NE111","Lincoln","Bankard loamy fine sand, loamy subsoil variant","Well drained","C",0.25,64.150000000000006,8.1999999999999993]
["NE111","Lincoln","Barney soils, frequently flooded","Very poorly drained","B/D",1.625,67,7.35]
["NE111","Lincoln","Bayard very fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,63.3,7.9]
["NE111","Lincoln","Blackwood silt loam, 1 to 3 percent slopes","Well drained","B",1.5,9.5,7.6]
["NE111","Lincoln","Caruso loam","Moderately well drained","B",0.5,52.55,7.7]
["NE111","Lincoln","Cass fine sandy loam, calcareous variant, rarely flooded","Well drained","C",0.75,67.099999999999994,8.0500000000000007]
["NE111","Lincoln","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE111","Lincoln","Coly and Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE111","Lincoln","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE111","Lincoln","Coly silt loam, 17 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE111","Lincoln","Coly silt loam, 6 to 11 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE111","Lincoln","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE111","Lincoln","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE111","Lincoln","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE111","Lincoln","Cozad loam, sandy subsoil variant","Well drained","B",0.75,61.6,7.6]
["NE111","Lincoln","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7.6]
["NE111","Lincoln","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7.3]
["NE111","Lincoln","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7.6]
["NE111","Lincoln","Cozad silt loam, saline-alkali, 0 to 1 percent slopes","Moderately well drained","B",0.75,11.4,8.8000000000000007]
["NE111","Lincoln","Cozad silt loam, wet","Moderately well drained","C",1.5,60.3,7.6]
["NE111","Lincoln","Cozad silty clay loam, 0 to 1 percent slopes","Well drained","C",0.75,14.2,7.6]
["NE111","Lincoln","Cullison mucky peat","Very poorly drained","B/D",12,33.5,7.9]
["NE111","Lincoln","Cutcomb mucky peat","Very poorly drained","A/D",29,0,0]
["NE111","Lincoln","Dailey loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,80.400000000000006,7.2]
["NE111","Lincoln","Dix complex, 6 to 30 percent slopes","Excessively drained","A",0.25,67.900000000000006,7.5]
["NE111","Lincoln","Dix gravelly loam, 3 to 20 percent slopes","Excessively drained","B",1.125,68.800000000000011,7.25]
["NE111","Lincoln","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,82.9,6.85]
["NE111","Lincoln","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.75,86.8,6.7]
["NE111","Lincoln","Dunday-Valentine loamy fine sands, 0 to 6 percent slopes","Somewhat excessively drained","A",0.5,87.05,6.6]
["NE111","Lincoln","Duroc loam, terrace, 0 to 1 percent slopes","Well drained","B",1.375,21.4,7.2]
["NE111","Lincoln","Duroc silt loam, 1 to 3 percent slopes","Well drained","B",1.375,9.5,7.2]
["NE111","Lincoln","Elsmere complex, 0 to 6 percent slopes","Somewhat excessively drained","A",0.75,79,7]
["NE111","Lincoln","Elsmere loamy fine sand, loamy substratum, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,79.400000000000006,6.7]
["NE111","Lincoln","Elsmere loamy fine sand, very rarely flooded","Somewhat poorly drained","A",1.125,91.8,6.6]
["NE111","Lincoln","Fillmore complex, frequently ponded","Somewhat poorly drained","D",1.5,23.5,6.7]
["NE111","Lincoln","Fluvaquents, frequently flooded","Very poorly drained","A/D",5,12,7.5]
["NE111","Lincoln","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",0.15000000000000002,93.5,7.9]
["NE111","Lincoln","Fluvaquents, silty, frequently flooded","Very poorly drained","B/D",2.5,11.75,3.75]
["NE111","Lincoln","Gannett silt loam, occasionally flooded","Very poorly drained","B/D",2.875,37.25,7.9]
["NE111","Lincoln","Gothenburg loamy sand, occasionally flooded","Poorly drained","A/D",0.25,91.9,7.5]
["NE111","Lincoln","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.25,93.15,7.2]
["NE111","Lincoln","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.375,11.3,7.1]
["NE111","Lincoln","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.375,11.3,7.1]
["NE111","Lincoln","Hersh and Anselmo fine sandy loams, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE111","Lincoln","Hersh and Anselmo soils, 11 to 30 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE111","Lincoln","Hersh and Valentine soils, 11 to 30 percent slopes","Well drained","A",0.5,77.099999999999994,6.7]
["NE111","Lincoln","Hersh and Valentine soils, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE111","Lincoln","Hersh fine sandy loam, 11 to 17 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE111","Lincoln","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.5,66.5,6.95]
["NE111","Lincoln","Hersh fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE111","Lincoln","Hersh soils, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE111","Lincoln","Hersh soils, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE111","Lincoln","Hersh-Anselmo fine sandy loams, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE111","Lincoln","Hersh-Valentine complex, 15 to 30 percent slopes","Well drained","A",0.5,77.099999999999994,6.6]
["NE111","Lincoln","Hersh-Valentine loamy fine sands, 0 to 6 percent slopes","Well drained","A",0.75,87.3,6.7]
["NE111","Lincoln","Hobbs and McCook silt loams, occasionally flooded","Well drained","B",1.875,11.3,7.45]
["NE111","Lincoln","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE111","Lincoln","Holdrege and Uly silt loams, 7 to 11 percent slopes","Well drained","C",0.75,9.4,7]
["NE111","Lincoln","Holdrege fine sandy loam, 0 to 3 percent slopes","Well drained","C",0.5,11.3,6.85]
["NE111","Lincoln","Holdrege fine sandy loam, 1 to 3 percent slopes, overblown","Well drained","C",0.25,11.3,7.2]
["NE111","Lincoln","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.875,9.4,6.85]
["NE111","Lincoln","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.875,9.4,6.85]
["NE111","Lincoln","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.875,9.4,6.85]
["NE111","Lincoln","Holdrege silt loam, 7 to 11 percent slopes","Well drained","C",0.75,9.3500000000000014,7.2]
["NE111","Lincoln","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,6.8,7.2]
["NE111","Lincoln","Holdrege silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.75,6.8,7.2]
["NE111","Lincoln","Hord fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.25,59.7,7]
["NE111","Lincoln","Hord fine sandy loam, 3 to 6 percent slopes","Well drained","B",1.25,59.7,7]
["NE111","Lincoln","Hord silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE111","Lincoln","Hord silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE111","Lincoln","Hord silt loam, 3 to 6 percent slopes","Well drained","B",2,11.2,7.5]
["NE111","Lincoln","Hord silt loam, rarely flooded","Well drained","B",2,11.2,7.5]
["NE111","Lincoln","Humbarger loam, gravelly substratum","Moderately well drained","B",1,53,7.9]
["NE111","Lincoln","Inavale loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,7.4]
["NE111","Lincoln","Janise loam, occasionally flooded","Somewhat poorly drained","C",0.75,42.2,9.4]
["NE111","Lincoln","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE111","Lincoln","Jayem loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.75,80,7.2]
["NE111","Lincoln","Jayem loamy very fine sand, 3 to 6 percent slopes","Well drained","A",1.1499999999999999,80.75,7.2]
["NE111","Lincoln","Keith loam, 1 to 3 percent slopes","Well drained","B",0.75,21.2,7]
["NE111","Lincoln","Keith loam, 3 to 6 percent slopes","Well drained","B",0.75,21.2,7]
["NE111","Lincoln","Keith silt loam, 1 to 3 percent slopes","Well drained","C",0.75,13.7,7.3]
["NE111","Lincoln","Keith silt loam, 3 to 6 percent slopes","Well drained","C",0.75,13.7,7.3]
["NE111","Lincoln","Keith silt loam, 3 to 6 percent slopes, eroded","Well drained","C",0.75,13.7,7]
["NE111","Lincoln","Kuma loam, 0 to 1 percent slopes","Well drained","C",2,36.9,7.5]
["NE111","Lincoln","Kuma loam, 1 to 3 percent slopes","Well drained","C",2,36.9,7.5]
["NE111","Lincoln","Kuma silt loam, 0 to 1 percent slopes","Well drained","C",2,9,7.3]
["NE111","Lincoln","Kuma silt loam, 1 to 3 percent slopes","Well drained","C",2,9,7.3]
["NE111","Lincoln","Lawet fine sandy loam, drained, occasionally flooded","Somewhat poorly drained","C",0.75,67.05,7.85]
["NE111","Lincoln","Lawet loam, gravelly subsoil variant, occasionally flooded","Poorly drained","B/D",0.75,43.3,7.9]
["NE111","Lincoln","Lawet silt loam, drained, occasionally flooded","Somewhat poorly drained","C",1.25,39.1,7.9]
["NE111","Lincoln","Lawet silt loam, occasionally flooded","Poorly drained","B/D",1.25,54.4,7.9]
["NE111","Lincoln","Lawet silt loam, saline-alkali, occasionally flooded","Somewhat poorly drained","C",0.75,54.2,8.3500000000000014]
["NE111","Lincoln","Lawet silt loam, saline-alkali, rarely flooded","Somewhat poorly drained","B/D",0.75,41.55,8.3500000000000014]
["NE111","Lincoln","Lawet-Saltine complex, occasionally flooded","Somewhat poorly drained","C",0.75,19,8.5]
["NE111","Lincoln","Lex loam, occasionally flooded","Somewhat poorly drained","C",0.75,41.6,7.3]
["NE111","Lincoln","Lex loam, rarely flooded","Somewhat poorly drained","C",1,53.5,7.6]
["NE111","Lincoln","Lex loam, saline-alkali, occasionally flooded","Somewhat poorly drained","C",0.75,42.1,8.5]
["NE111","Lincoln","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",2.5,16.599999999999998,7]
["NE111","Lincoln","Loup complex, rarely flooded","Very poorly drained","B/D",3.375,69.75,7.1]
["NE111","Lincoln","Mace silt loam, 0 to 1 percent slopes","Well drained","C",1,11.25,7.1]
["NE111","Lincoln","Marlake loamy fine sand, frequently ponded","Very poorly drained","A/D",0.75,84.3,7.5]
["NE111","Lincoln","McCash very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.25,60.3,7]
["NE111","Lincoln","McCash very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.25,60.3,7]
["NE111","Lincoln","McCook loam, rarely flooded","Well drained","B",0.75,59.6,7.9]
["NE111","Lincoln","McCook loam, saline-alkali","Moderately well drained","B",0.25,59.6,8.1999999999999993]
["NE111","Lincoln","McCook silt loam, occasionally flooded","Well drained","B",0.5,36.900000000000006,7.9]
["NE111","Lincoln","Norwest loam, 0 to 2 percent slopes","Somewhat poorly drained","C",0.75,39.799999999999997,7.9]
["NE111","Lincoln","Platte-Alda complex, occasionally flooded","Somewhat poorly drained","C",0.5,66,7.5]
["NE111","Lincoln","Sarben loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.5,83,6.95]
["NE111","Lincoln","Sarben loamy fine sand, 6 to 9 percent slopes","Well drained","A",0.5,83,6.95]
["NE111","Lincoln","Sarben loamy fine sand, 9 to 20 percent slopes","Well drained","A",0.5,73,6.95]
["NE111","Lincoln","Sarben loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.5,84,7.2]
["NE111","Lincoln","Sarben loamy very fine sand, 3 to 6 percent slopes","Well drained","A",0.5,84,7.2]
["NE111","Lincoln","Sarben loamy very fine sand, 6 to 9 percent slopes","Well drained","A",0.5,84,7.2]
["NE111","Lincoln","Sarben loamy very fine sand, 9 to 20 percent slopes","Well drained","A",0.5,84,7.2]
["NE111","Lincoln","Satanta loam, 1 to 3 percent slopes","Well drained","B",1.25,43,7.5]
["NE111","Lincoln","Satanta loam, 3 to 6 percent slopes","Well drained","B",1.25,43,7.5]
["NE111","Lincoln","Satanta very fine sandy loam, 1 to 3 percent slopes","Well drained","C",0.75,64.400000000000006,7.5]
["NE111","Lincoln","Scott soils, frequently ponded","Poorly drained","D",1.5,18.7,6.7]
["NE111","Lincoln","Sidney complex, 6 to 20 percent slopes","Well drained","B",0.75,45,7.5500000000000007]
["NE111","Lincoln","Silver Creek silt loam, occasionally flooded","Somewhat poorly drained","D",0.5,32.1,7.9]
["NE111","Lincoln","Silver Creek-Saltine complex, rarely flooded","Somewhat poorly drained","C",0.5,9.6000000000000014,8.5]
["NE111","Lincoln","Sulco silt loam, 30 to 60 percent slopes","Well drained","B",1,17.600000000000001,7.9]
["NE111","Lincoln","Sulco silt loam, 6 to 9 percent slopes","Well drained","B",1,17.600000000000001,7.9]
["NE111","Lincoln","Sulco-Ulysses silt loams, 9 to 30 percent slopes, eroded","Well drained","B",1.25,13.6,7.9]
["NE111","Lincoln","Uly and Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE111","Lincoln","Uly and Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.6]
["NE111","Lincoln","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE111","Lincoln","Uly silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE111","Lincoln","Uly silt loam, 6 to 11 percent slopes","Well drained","B",1.25,9.5,7]
["NE111","Lincoln","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE111","Lincoln","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE111","Lincoln","Uly-Coly silt loams, 6 to 11 percent slopes","Well drained","B",1.25,11.2,7.9]
["NE111","Lincoln","Uly-Holdrege silt loams, 6 to 11 percent slopes","Well drained","C",0.75,13.6,7.2]
["NE111","Lincoln","Ulysses silt loam, 3 to 6 percent slopes","Well drained","B",1.5,9.5,7.9]
["NE111","Lincoln","Ulysses silt loam, 6 to 9 percent slopes, eroded","Well drained","B",1.5,9.5,7.9]
["NE111","Lincoln","Ulysses-Sulco silt loams, 6 to 9 percent slopes, eroded","Well drained","B",1,13.6,7.9]
["NE111","Lincoln","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE111","Lincoln","Valent fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE111","Lincoln","Valent fine sand, rolling and hilly","Excessively drained","A",0.5,94.9,7.2]
["NE111","Lincoln","Valent loamy sand, 3 to 9 percent slopes","Excessively drained","A",0.5,88.6,7]
["NE111","Lincoln","Valent sand, rolling","Excessively drained","A",0.5,95,7]
["NE111","Lincoln","Valentine complex, hilly","Excessively drained","A",0.5,95.85,6.5]
["NE111","Lincoln","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,95.85,6.5]
["NE111","Lincoln","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,6.5]
["NE111","Lincoln","Valentine fine sand, rolling","Excessively drained","A",0.5,95.85,6.5]
["NE111","Lincoln","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,94.9,6.5]
["NE111","Lincoln","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,91.35,6.5]
["NE111","Lincoln","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.75,86.8,6.7]
["NE111","Lincoln","Valentine loamy fine sand, rolling","Excessively drained","A",0.5,91.35,6.5]
["NE111","Lincoln","Valentine-Birdwood complex, 9 to 80 percent slopes","Well drained","A",0.625,85.8,6.5]
["NE111","Lincoln","Valentine-Mullen complex, 0 to 9 percent slopes","Well drained","B",0.75,86,6.7]
["NE111","Lincoln","Valentine-Ringgold complex, 0 to 9 percent slopes","Well drained","B",0.75,86.8,6.6]
["NE111","Lincoln","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE111","Lincoln","Vetal fine sandy loam, loamy substratum, 0 to 3 percent slopes","Well drained","A",1,65.75,7.15]
["NE111","Lincoln","Vetal loamy fine sand, 0 to 3 percent slopes","Well drained","A",2,85.9,7.2]
["NE111","Lincoln","Wann fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,63.5,8.1999999999999993]
["NE111","Lincoln","Wann fine sandy loam, saline-alkali, occasionally flooded","Somewhat poorly drained","B",0.75,66,8.8000000000000007]
["NE111","Lincoln","Wann fine sandy loam, saline-alkali, rarely flooded","Somewhat poorly drained","B",0.5,66.650000000000006,8.8000000000000007]
["NE111","Lincoln","Wann loam, rarely flooded","Somewhat poorly drained","C",0.75,63.1,8.1999999999999993]
["NE111","Lincoln","Woodly loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.5,65.400000000000006,7]
["NE113","Logan",null,"",""]
["NE113","Logan","Almeria fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,78.2,6.9]
["NE113","Logan","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE113","Logan","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE113","Logan","Anselmo fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE113","Logan","Anselmo fine sandy loam, terrace, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE113","Logan","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE113","Logan","Coly silt loam, 11 to 30 percent slopes","Well drained","B",1.125,8,7.9]
["NE113","Logan","Coly silt loam, 17 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE113","Logan","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE113","Logan","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,14.2,7.9]
["NE113","Logan","Doughboy fine sandy loam, 0 to 3 percent slopes","Moderately well drained","A",2,50,7.9]
["NE113","Logan","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE113","Logan","Dunday-Valentine loamy fine sands, 0 to 3 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE113","Logan","Dunday-Valentine loamy fine sands, 3 to 9 percent slopes","Somewhat excessively drained","A",0.5,91.1,6.6]
["NE113","Logan","Els and Elsmere fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.6]
["NE113","Logan","Els fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.7]
["NE113","Logan","Gannett fine sandy loam, occasionally flooded","Poorly drained","A/D",1,62.5,7.5]
["NE113","Logan","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,14,7]
["NE113","Logan","Hersh and Anselmo fine sandy loams, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE113","Logan","Hersh and Valentine soils, 11 to 30 percent slopes","Well drained","A",0.5,77.099999999999994,6.7]
["NE113","Logan","Hersh and Valentine soils, 6 to 11 percent slopes","Well drained","A",0.5,77.099999999999994,6.7]
["NE113","Logan","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE113","Logan","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.5,66.5,6.95]
["NE113","Logan","Hersh fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE113","Logan","Hersh-Valentine complex, 15 to 30 percent slopes","Well drained","A",0.5,77.099999999999994,6.6]
["NE113","Logan","Holdrege fine sandy loam, 1 to 3 percent slopes, overblown","Well drained","C",0.25,11.3,7.2]
["NE113","Logan","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",1.25,9.4,7.2]
["NE113","Logan","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.3500000000000014,7.2]
["NE113","Logan","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.3500000000000014,7.2]
["NE113","Logan","Holdrege silt loam, 7 to 11 percent slopes","Well drained","C",0.75,9.3500000000000014,7.2]
["NE113","Logan","Holdrege silt loam, 7 to 11 percent slopes, severely eroded","Well drained","C",0.75,9.3500000000000014,7.2]
["NE113","Logan","Holdrege-Hord silt loams, 0 to 3 percent slopes","Well drained","C",0.75,9.4,7.2]
["NE113","Logan","Hord fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE113","Logan","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,11.2,7]
["NE113","Logan","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,11.2,7]
["NE113","Logan","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,11.2,7]
["NE113","Logan","Hord silt loam, rarely flooded","Well drained","B",1.625,10.25,7.2]
["NE113","Logan","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE113","Logan","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",3.375,79.2,6.6]
["NE113","Logan","Marlake loamy fine sand, frequently ponded","Very poorly drained","A/D",0.75,78.2,7.5]
["NE113","Logan","Munjor fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.5,66.900000000000006,7.9]
["NE113","Logan","Ord fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE113","Logan","Ord very fine sandy loam, occasionally flooded","Somewhat poorly drained","C",0.75,63.3,7.5]
["NE113","Logan","Ovina loam, 0 to 1 percent slopes","Somewhat poorly drained","C",1.75,56.25,7.5]
["NE113","Logan","Ringgold-Valentine complex, 0 to 3 percent slopes","Well drained","B",0.75,86.8,6.7]
["NE113","Logan","Scott soils, frequently ponded","Poorly drained","D",1.5,26.3,6.7]
["NE113","Logan","Tryon loamy fine sand, 0 to 3 percent slopes","Poorly drained","A/D",3.375,79.45,6.85]
["NE113","Logan","Uly silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.3,7.9]
["NE113","Logan","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE113","Logan","Uly silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE113","Logan","Uly silt loam, 6 to 11 percent slopes","Well drained","B",1.25,9.5,7]
["NE113","Logan","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE113","Logan","Uly-Coly silt loams, 6 to 11 percent slopes","Well drained","B",1.25,11.2,7.9]
["NE113","Logan","Uly-Holdrege silt loams, 11 to 17 percent slopes","Well drained","C",0.75,13.6,7.2]
["NE113","Logan","Uly-Holdrege silt loams, 6 to 11 percent slopes","Well drained","C",0.75,13.6,7.2]
["NE113","Logan","Uly-Sully silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.5,40.75,7.9]
["NE113","Logan","Valentine complex, hilly","Excessively drained","A",0.5,95.85,6.5]
["NE113","Logan","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,95.85,6.5]
["NE113","Logan","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE113","Logan","Valentine fine sand, hilly","Excessively drained","A",0.5,95.85,6.5]
["NE113","Logan","Valentine fine sand, rolling","Excessively drained","A",0.5,95.85,6.5]
["NE113","Logan","Valentine fine sand, rolling and hilly","Excessively drained","A",0.25,96.3,6.5]
["NE113","Logan","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,91.35,6.5]
["NE113","Logan","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE113","Logan","Valentine loamy fine sand, rolling","Excessively drained","A",0.5,91.35,6.5]
["NE113","Logan","Valentine-Dunday complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.625,94,6.6]
["NE113","Logan","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.625,95.4,6.5]
["NE113","Logan","Valentine-Mullen complex, 0 to 9 percent slopes","Well drained","B",0.75,86,6.7]
["NE113","Logan","Valentine-Ringgold complex, 0 to 9 percent slopes","Well drained","B",0.75,86.8,6.6]
["NE113","Logan","Vetal fine sandy loam","Well drained","A",1.25,66.099999999999994,7]
["NE113","Logan","Wann variant fine sandy loam, alkali, rarely flooded","Somewhat poorly drained","B",0.75,67.3,8.8000000000000007]
["NE115","Loup",null,"",""]
["NE115","Loup","Almeria fine sandy loam, channeled, frequently flooded","Very poorly drained","A/D",3.375,78.2,6.9]
["NE115","Loup","Almeria loamy fine sand, occasionally flooded","Poorly drained","A/D",1.25,89.9,6.9]
["NE115","Loup","Almeria loamy fine sand, wet, occasionally flooded","Very poorly drained","A/D",1.25,89.9,6.9]
["NE115","Loup","Almeria-Histosols complex, channeled, frequently flooded","Very poorly drained","A/D",3.375,77.75,3.25]
["NE115","Loup","Boelus loamy fine sand, sandy substratum, 0 to 3 percent slopes","Well drained","B",0.25,79.400000000000006,7.2]
["NE115","Loup","Boelus sandy substratum-Simeon loamy sands, 0 to 3 percent slopes","Well drained","B",0.25,80,7]
["NE115","Loup","Bolent loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.5,89.9,7.7]
["NE115","Loup","Bolent loamy sand, occasionally flooded","Somewhat poorly drained","A",0.5,88.6,7.7]
["NE115","Loup","Calamus loamy fine sand, rarely flooded","Moderately well drained","A",0.5,92.6,7]
["NE115","Loup","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE115","Loup","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE115","Loup","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE115","Loup","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7.3]
["NE115","Loup","Els loamy sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.7]
["NE115","Loup","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE115","Loup","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1.125,91.8,6.6]
["NE115","Loup","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.75,87.35,7.5]
["NE115","Loup","Gates silt loam, 1 to 3 percent slopes","Well drained","B",0.5,13.9,7.5]
["NE115","Loup","Gates silt loam, 11 to 30 percent slopes","Well drained","B",0.5,13.9,7.5]
["NE115","Loup","Gates silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.5,13.9,7.5]
["NE115","Loup","Gates silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.5,13.9,7.5]
["NE115","Loup","Gates very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.5,58.6,7.5]
["NE115","Loup","Gates-Hersh complex, 20 to 60 percent slopes","Well drained","B",0.625,62.849999999999994,7.35]
["NE115","Loup","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE115","Loup","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.5,75.45,6.95]
["NE115","Loup","Hersh fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.5,75.45,6.95]
["NE115","Loup","Hersh loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.75,84,6.7]
["NE115","Loup","Hersh-Gates complex, 0 to 3 percent slopes","Well drained","B",0.5,66.099999999999994,7.2]
["NE115","Loup","Hersh-Gates complex, 30 to 60 percent slopes","Well drained","B",0.625,62.849999999999994,7.35]
["NE115","Loup","Hersh-Valentine complex, 11 to 24 percent slopes","Well drained","A",0.25,87.3,6.7]
["NE115","Loup","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11,7]
["NE115","Loup","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE115","Loup","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",1.25,9.4,7.2]
["NE115","Loup","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE115","Loup","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE115","Loup","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE115","Loup","Ipage fine sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,96.8,6.5]
["NE115","Loup","Ipage loamy fine sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,89.3,6.5]
["NE115","Loup","Kenesaw very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,60.3,7.5]
["NE115","Loup","Loup fine sandy loam, occasionally flooded","Poorly drained","A/D",3.375,78.8,6.6]
["NE115","Loup","Marlake loamy fine sand, frequently ponded","Very poorly drained","A/D",0.75,87.3,7.5]
["NE115","Loup","Ord very fine sandy loam, rarely flooded","Somewhat poorly drained","C",0.75,63.3,7.5]
["NE115","Loup","Simeon sand, 0 to 3 percent slopes","Excessively drained","A",0.5,91.85,7]
["NE115","Loup","Simeon sand, 3 to 30 percent slopes","Excessively drained","A",0.5,91.85,7]
["NE115","Loup","Tryon loamy fine sand, 0 to 3 percent slopes","Poorly drained","A/D",3.375,91.1,6.85]
["NE115","Loup","Tryon loamy fine sand, frequently ponded","Very poorly drained","A/D",3.375,91.1,6.85]
["NE115","Loup","Tryon-Els loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,95.4,6.7]
["NE115","Loup","Tryon-Ipage complex, 0 to 3 percent slopes","Moderately well drained","A",0.75,95.15,6.45]
["NE115","Loup","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE115","Loup","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE115","Loup","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE115","Loup","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE115","Loup","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,96.3,6.5]
["NE115","Loup","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE115","Loup","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE115","Loup","Valentine-Els complex, 0 to 9 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE115","Loup","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.5,94.7,6.5]
["NE115","Loup","Valentine-Simeon complex, 0 to 9 percent slopes","Excessively drained","A",0.5,93.25,6.75]
["NE115","Loup","Vetal very fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,62,7]
["NE115","Madison",null,"",""]
["NE115","Madison","Alcester silty clay loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE115","Madison","Bazile loam, 2 to 6 percent slopes","Well drained","C",0.75,36.5,6.5]
["NE115","Madison","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE115","Madison","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.125,65.75,7]
["NE115","Madison","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.599999999999994,7.5]
["NE115","Madison","Boel loamy fine sand, channeled, frequently flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE115","Madison","Boelus loamy fine sand, 2 to 6 percent slopes","Well drained","B",0.25,24,7]
["NE115","Madison","Cass fine sandy loam, occasionally flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE115","Madison","Cass loam, occasionally flooded","Well drained","B",0.75,63.5,7.3]
["NE115","Madison","Clarno loam, 2 to 6 percent slopes","Well drained","C",0.5,38.5,7.9]
["NE115","Madison","Coleridge silt loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE115","Madison","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE115","Madison","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE115","Madison","Crofton silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE115","Madison","Crofton silt loam, 30 to 60 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE115","Madison","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE115","Madison","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE115","Madison","Elsmere fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.25,79.400000000000006,6.5]
["NE115","Madison","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.5]
["NE115","Madison","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1.125,11.100000000000001,7.1]
["NE115","Madison","Fluvaquents, frequently flooded","Very poorly drained","A/D",2.5,23.5,3.75]
["NE115","Madison","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.4,7.9]
["NE115","Madison","Gibbon-Gayville silty clay loams, occasioanlly flooded","Somewhat poorly drained","D",1.125,14.7,7.9]
["NE115","Madison","Hadar loamy fine sand, 2 to 6 percent slopes","Well drained","C",0.75,85.3,6.1]
["NE115","Madison","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE115","Madison","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE115","Madison","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE115","Madison","Inavale loamy fine sand, occasionally flooded","Somewhat excessively drained","A",0.25,92.2,6.7]
["NE115","Madison","Inavale-Boel complex, 0 to 6 percent slopes, occasionally flooded","Somewhat poorly drained","C",0.25,92.2,7.5]
["NE115","Madison","Inglewood-Boel complex, channeled, occasionally flooded","Somewhat poorly drained","A",0.25,92.9,7.25]
["NE115","Madison","Lamo silt loam, occasionally flooded","Poorly drained","C",4.5,9.25,7.9]
["NE115","Madison","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE115","Madison","Lawet loam, rarely flooded","Poorly drained","B/D",1.25,54.4,7.9]
["NE115","Madison","Libory loamy fine sand, 3 to 6 percent slopes","Moderately well drained","A",0.75,86.4,6.5]
["NE115","Madison","Loretto fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE115","Madison","Loretto fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE115","Madison","Loretto loam, 0 to 2 percent slopes","Well drained","B",1.5,39.1,6.5]
["NE115","Madison","Loretto loam, 2 to 6 percent slopes","Well drained","B",1.5,39.1,6.5]
["NE115","Madison","Loup fine sandy loam, rarely flooded","Poorly drained","A/D",3.125,64.8,6.6]
["NE115","Madison","Loup loamy fine sand, frequently ponded","Very poorly drained","A/D",3.375,90.4,6.6]
["NE115","Madison","Marlake loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7]
["NE115","Madison","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE115","Madison","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE115","Madison","Moody silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE115","Madison","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE115","Madison","Muir silty clay loam, rarely flooded","Well drained","B",2,9,6.7]
["NE115","Madison","Nora silty clay loam, 11 to 17 percent slopes","Well drained","C",0.75,8.9,7]
["NE115","Madison","Nora silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,8.9,7]
["NE115","Madison","Nora silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE115","Madison","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE115","Madison","Nora-Crofton complex, 2 to 6 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE115","Madison","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE115","Madison","Obert silty clay loam, frequently ponded","Very poorly drained","C/D",2.25,7.1,7.9]
["NE115","Madison","Ord fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE115","Madison","Ord loam, occasionally flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE115","Madison","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE115","Madison","Ovina fine sandy loam, rarely flooded","Somewhat poorly drained","B",1.5,66.900000000000006,7.5]
["NE115","Madison","Ovina loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","C",0.75,63.5,7.9]
["NE115","Madison","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE115","Madison","Shell silty clay loam, 0 to 1 percent slopes","Well drained","C",0.75,9.1,6.5]
["NE115","Madison","Shell variant silty clay loam, 0 to 1 percent slopes","Moderately well drained","C",0.75,6.9,6.7]
["NE115","Madison","Thurman loamy fine sand, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE115","Madison","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE115","Madison","Thurman loamy fine sand, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE115","Madison","Thurman loamy fine sand, thick, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE115","Madison","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE115","Madison","Valentine fine sand, 9 to 24 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE115","Madison","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.75,6.6]
["NE117","McPherson",null,"",""]
["NE117","McPherson","Almeria-Fluvaquents, sandy complex, channeled, frequently flooded","Poorly drained","B/D",7.5,44.3,6.8]
["NE117","McPherson","Calamus-Bolent loamy fine sands, channeled, occasionally flooded","Somewhat poorly drained","A",0.375,89.5,6.8]
["NE117","McPherson","Crowther loam, 0 to 1 percent slopes","Poorly drained","B/D",6.75,42.2,7.7]
["NE117","McPherson","Crowther mucky peat","Very poorly drained","B/D",6.75,38.5,7.7]
["NE117","McPherson","Cullison loam, 0 to 1 percent slopes","Poorly drained","B/D",3,33.5,7.9]
["NE117","McPherson","Cullison mucky peat","Very poorly drained","B/D",12,33.5,7.9]
["NE117","McPherson","Doughboy fine sandy loam, 0 to 3 percent slopes","Moderately well drained","A",2,50,7.9]
["NE117","McPherson","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,86.8,6.7]
["NE117","McPherson","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.75,86.8,6.7]
["NE117","McPherson","Els calcareous-Hoffland complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.625,94.1,7.9]
["NE117","McPherson","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.7]
["NE117","McPherson","Elsmere loamy fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,79.400000000000006,7.9]
["NE117","McPherson","Ipage calcareous-Hoffland complex, 0 to 3 percent slopes","Very poorly drained","A/D",0.625,94.1,8]
["NE117","McPherson","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.95]
["NE117","McPherson","Ipage-Els complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,96,6.5]
["NE117","McPherson","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,94.9,6.7]
["NE117","McPherson","Loup mucky peat","Very poorly drained","A/D",4,63.5,6.6]
["NE117","McPherson","Marlake mucky peat","Very poorly drained","A/D",3.375,76.449999999999989,6.5500000000000007]
["NE117","McPherson","Mullen loamy fine sand, 0 to 3 percent slopes","Well drained","B",1.125,79.050000000000011,6.95]
["NE117","McPherson","Nenzel loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",1.25,86.8,6.7]
["NE117","McPherson","Nenzel loamy fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",1.375,91.4,7.9]
["NE117","McPherson","Ringgold-Valentine complex, 0 to 3 percent slopes","Well drained","B",0.75,86.8,6.7]
["NE117","McPherson","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,6.5]
["NE117","McPherson","Valentine fine sand, rolling","Excessively drained","A",0.5,94.9,6.5]
["NE117","McPherson","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,94.9,6.5]
["NE117","McPherson","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.75,86.8,6.7]
["NE117","McPherson","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.75,86.8,6.7]
["NE117","McPherson","Valentine-Birdwood complex, 9 to 80 percent slopes","Well drained","A",0.625,85.8,6.5]
["NE117","McPherson","Valentine-Dunday complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.625,94,6.6]
["NE117","McPherson","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.625,95.4,6.5]
["NE117","McPherson","Valentine-Hoffland, complex, 0 to 24 percent slopes","Very poorly drained","A/D",0.625,94.1,7.15]
["NE117","McPherson","Valentine-Mullen complex, 0 to 9 percent slopes","Well drained","B",0.75,86,6.7]
["NE117","McPherson","Valentine-Ringgold complex, 0 to 9 percent slopes","Well drained","B",0.75,86.8,6.6]
["NE117","McPherson","Valentine-Tryon complex, 0 to 24 percent slopes","Very poorly drained","A/D",0.625,94.1,6.5]
["NE121","Merrick",null,"",""]
["NE121","Merrick","Alda loam, occasionally flooded","Somewhat poorly drained","C",0.75,66,7.5]
["NE121","Merrick","Alda loam, rarely flooded","Somewhat poorly drained","C",0.5,68.099999999999994,7.4]
["NE121","Merrick","Alda sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,67.8,7.5]
["NE121","Merrick","Alda sandy loam, rarely flooded","Somewhat poorly drained","B",0.5,65.75,7.35]
["NE121","Merrick","Barney complex, channeled, frequently flooded","Poorly drained","C/D",0.75,44.3,7.3]
["NE121","Merrick","Barney loam, frequently flooded","Very poorly drained","B/D",0.25,47.9,7.5]
["NE121","Merrick","Barney-Bolent complex, frequently flooded","Poorly drained","C/D",0.25,91.25,7.4]
["NE121","Merrick","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.875,67,6.9]
["NE121","Merrick","Blendon fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.875,67,6.9]
["NE121","Merrick","Blendon loam, 0 to 2 percent slopes","Well drained","B",1,67.900000000000006,6.8]
["NE121","Merrick","Blendon variant fine sandy loam, 0 to 2 percent slopes","Well drained","B",0.75,67.599999999999994,6.7]
["NE121","Merrick","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE121","Merrick","Bolent fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.25,73.2,7.3]
["NE121","Merrick","Brocksburg loam, 0 to 2 percent slopes","Well drained","C",1.5,44.3,7.2]
["NE121","Merrick","Calamus loamy fine sand, rarely flooded","Moderately well drained","A",0.25,92.5,7]
["NE121","Merrick","Caruso loam, rarely flooded","Somewhat poorly drained","C",0.5,51,7.3]
["NE121","Merrick","Caruso-Gayville complex, 0 to 1 percent slopes","Somewhat poorly drained","C",0.75,37.9,7.9]
["NE121","Merrick","Coly silt loam, 6 to 11 percent slopes","Well drained","B",1.125,8,7.9]
["NE121","Merrick","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE121","Merrick","Cozad loam, sand substratum, 0 to 3 percent slopes","Well drained","B",1.375,47.45,6.35]
["NE121","Merrick","Cozad loam, wet substratum, 0 to 1 percent slopes","Moderately well drained","B",1.5,11.7,7.5]
["NE121","Merrick","Els loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,80,6.7]
["NE121","Merrick","Fonner loam, rarely flooded","Moderately well drained","B",0.75,84.3,6.2]
["NE121","Merrick","Fonner sandy loam, rarely flooded","Moderately well drained","A",0.75,84.3,6.2]
["NE121","Merrick","Fonner variant loamy sand, occasionally flooded","Moderately well drained","A",0.25,85.5,6.7]
["NE121","Merrick","Fonner variant loamy sand, rarely flooded","Well drained","A",0.25,79.599999999999994,6.7]
["NE121","Merrick","Gayville variant silt loam, rarely flooded","Somewhat poorly drained","C",1.5,14.3,9.1]
["NE121","Merrick","Gayville-Caruso complex, occasionally flooded","Somewhat poorly drained","C",0.75,37.9,7.9]
["NE121","Merrick","Gibbon loam, occasionally flooded","Somewhat poorly drained","C",0.75,41.5,7.9]
["NE121","Merrick","Gibbon silt loam, rarely flooded","Somewhat poorly drained","C",0.75,9.4,7.6]
["NE121","Merrick","Gibbon-Gayville silty clay loams, occasioanlly flooded","Somewhat poorly drained","C",0.75,22.25,8.0500000000000007]
["NE121","Merrick","Gothenburg fine sandy loam, frequently flooded","Poorly drained","A/D",0.5,85.550000000000011,7.35]
["NE121","Merrick","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,95.35,7.2]
["NE121","Merrick","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.5,83.6,7.35]
["NE121","Merrick","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.5,9.5,7]
["NE121","Merrick","Hall silt loam, sandy substratum, 0 to 1 percent slopes","Well drained","C",1.125,9.65,6.65]
["NE121","Merrick","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,9.25,7.25]
["NE121","Merrick","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE121","Merrick","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,9.25,7.25]
["NE121","Merrick","Holder silt loam, 0 to 1 percent slopes","Well drained","C",1.25,9.5,7]
["NE121","Merrick","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",1.25,8,7.2]
["NE121","Merrick","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",1.25,8,7.2]
["NE121","Merrick","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,8,7.2]
["NE121","Merrick","Hord silt loam, 0 to 1 percent slopes","Well drained","B",2,7,7]
["NE121","Merrick","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE121","Merrick","Hord silt loam, sandy substratum, 0 to 1 percent slopes","Well drained","B",0.75,9.5,7]
["NE121","Merrick","Hord very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.125,35.5,6.9]
["NE121","Merrick","Hord-Uly complex, 0 to 6 percent slopes","Well drained","B",0.75,9,6.7]
["NE121","Merrick","Inavale loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,84.3,6.7]
["NE121","Merrick","Inavale loamy fine sand, very rarely flooded","Excessively drained","A",0.25,87.3,7]
["NE121","Merrick","Inavale loamy sand, 3 to 11 percent slopes","Excessively drained","A",0.25,86.8,6.7]
["NE121","Merrick","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE121","Merrick","Ipage-Els loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,83.4,6.7]
["NE121","Merrick","Janude fine sandy loam, 0 to 1 percent slopes","Moderately well drained","B",1.25,63.5,7.5]
["NE121","Merrick","Janude loam, calcareous, rarely flooded","Moderately well drained","B",0.9,66.599999999999994,7.6]
["NE121","Merrick","Janude sandy loam, very rarely flooded","Moderately well drained","B",1.25,66.599999999999994,7.5]
["NE121","Merrick","Kenesaw silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14,7.5]
["NE121","Merrick","Kenesaw silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14,7.5]
["NE121","Merrick","Kenesaw-Cozad complex","Moderately well drained","B",0.75,11.4,8.0500000000000007]
["NE121","Merrick","Lamo clay loam, sandy substratum, 0 to 1 percent slopes","Somewhat poorly drained","C",0.5,40.1,7.9]
["NE121","Merrick","Lamo-Saltine complex, occasionally flooded","Somewhat poorly drained","C",0.5,7.15,8.5]
["NE121","Merrick","Lawet variant fine sandy loam, frequently flooded","Poorly drained","B/D",0.75,45.400000000000006,7.9]
["NE121","Merrick","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,11.6,7.5]
["NE121","Merrick","Lex clay loam, occasionally flooded","Somewhat poorly drained","C",0.75,61,7.3]
["NE121","Merrick","Lex loam, occasionally flooded","Somewhat poorly drained","C",0.75,61,7.3]
["NE121","Merrick","Lex variant loam, occasionally flooded","Somewhat poorly drained","C",0.75,42.1,7.9]
["NE121","Merrick","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,86.4,6.5]
["NE121","Merrick","Lockton loam","Moderately well drained","B",2,41.6,6.5]
["NE121","Merrick","Lockton loam, rarely flooded","Moderately well drained","B",2,41.6,6.5]
["NE121","Merrick","Loretto fine sandy loam, 0 to 2 percent slopes","Well drained","C",1.5,19.899999999999999,6.5]
["NE121","Merrick","Loretto-Valentine complex, 3 to 11 percent slopes","Well drained","C",0.75,77.099999999999994,6.5]
["NE121","Merrick","Loup fine sandy loam, occasionally flooded","Very poorly drained","A/D",3.375,79.2,6.6]
["NE121","Merrick","Marlake loamy sand, frequently ponded","Very poorly drained","A/D",3.125,90.15,7]
["NE121","Merrick","Meadin sandy loam, 2 to 11 percent slopes","Excessively drained","A",0.75,67.8,6.2]
["NE121","Merrick","Merrick loam, rarely flooded","Moderately well drained","B",2.125,39.700000000000003,6.7]
["NE121","Merrick","Novina fine sandy loam, rarely flooded","Moderately well drained","B",0.75,63.5,6.7]
["NE121","Merrick","Novina sandy loam, rarely flooded","Moderately well drained","B",0.75,66.599999999999994,6.7]
["NE121","Merrick","Nuckolls variant soils, 11 to 17 percent slopes, severely eroded","Well drained","C",0.25,6,7.5]
["NE121","Merrick","Obert silt loam, occasionally flooded","Poorly drained","C/D",1.5,11.3,7.9]
["NE121","Merrick","O'Neill and Pivot loams, 0 to 2 percent slopes","Well drained","B",0.75,70,6.8]
["NE121","Merrick","O'Neill loam, 0 to 2 percent slopes","Well drained","B",0.75,68.3,6.5]
["NE121","Merrick","O'Neill sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,68.5,6.5]
["NE121","Merrick","O'Neill sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,72.5,6.5]
["NE121","Merrick","Ortello fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE121","Merrick","Ovina loam, rarely flooded","Somewhat poorly drained","C",1.125,54.55,7.7]
["NE121","Merrick","Platte fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.25,73.900000000000006,7.5]
["NE121","Merrick","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,63.2,7.5]
["NE121","Merrick","Platte loam, wet, occasionally flooded","Poorly drained","B/D",0.25,63.5,7.5]
["NE121","Merrick","Platte-Alda complex, occasionally flooded","Somewhat poorly drained","B",0.25,73.2,7.5]
["NE121","Merrick","Platte-Alda loams, channeled, frequently flooded","Somewhat poorly drained","C",0.5,67.7,7.5]
["NE121","Merrick","Platte-Bolent complex, occasionally flooded","Somewhat poorly drained","B",0.25,66.900000000000006,7.45]
["NE121","Merrick","Platte-Gothenburg complex, channeled, frequently flooded","Poorly drained","A/D",0.25,79.2,7.5]
["NE121","Merrick","Rusco silt loam, occasionally flooded","Moderately well drained","C/D",0.75,11.2,7.5]
["NE121","Merrick","Silver Creek complex, saline-alkali, rarely flooded","Somewhat poorly drained","D",1,26,8.3000000000000007]
["NE121","Merrick","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,86.35,7]
["NE121","Merrick","Thurman loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE121","Merrick","Thurman loamy fine sand, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE121","Merrick","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE121","Merrick","Thurman-Ortello fine sandy loams, 0 to 2 percent slopes","Well drained","A",0.5,75.900000000000006,6.5]
["NE121","Merrick","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE121","Merrick","Uly-Coly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.73,24.5,7.9]
["NE121","Merrick","Uly-Coly silt loams, 17 to 30 percent slopes, eroded, moist","Well drained","B",1,24,7.5]
["NE121","Merrick","Uly-Holdrege silt loams, 7 to 11 percent slopes, eroded","Well drained","C",0.5,9.4,7.6]
["NE121","Merrick","Valentine and Thurman soils, 0 to 17 percent slopes","Somewhat excessively drained","A",0.25,91.1,6.5]
["NE121","Merrick","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE121","Merrick","Valentine fine sand, 9 to 24 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE121","Merrick","Valentine fine sand, rolling","Excessively drained","A",0.25,96.3,5.9499999999999993]
["NE121","Merrick","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE121","Merrick","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE121","Merrick","Valentine-Boelus loamy fine sands, 0 to 3 percent slopes","Well drained","A",0.5,86.85,6.5]
["NE121","Merrick","Valentine-Boelus loamy fine sands, 3 to 9 percent slopes","Well drained","A",0.5,86.85,6.5]
["NE121","Merrick","Valentine-Libory complex, 0 to 9 percent slopes","Moderately well drained","A",0.25,83.5,6.3]
["NE121","Merrick","Wann loam, occasionally flooded","Somewhat poorly drained","C",0.75,66.2,8.1999999999999993]
["NE121","Merrick","Wann sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,66.599999999999994,8.1999999999999993]
["NE121","Merrick","Wood River silt loam, 0 to 1 percent slopes","Moderately well drained","C",0.75,22.4,7.4]
["NE123","Morrill",null,"",""]
["NE123","Morrill","Alice fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,64.900000000000006,7.9]
["NE123","Morrill","Alice fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,64.900000000000006,7.9]
["NE123","Morrill","Alice fine sandy loam, 6 to 9 percent slopes, eroded","Well drained","A",0.75,64.900000000000006,7.9]
["NE123","Morrill","Alice loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,73.400000000000006,7.9]
["NE123","Morrill","Alice-Dix complex, 0 to 3 percent slopes","Well drained","A",0.75,67.900000000000006,7.5]
["NE123","Morrill","Alice-Dix complex, 3 to 6 percent slopes","Well drained","A",0.75,83.2,7.5]
["NE123","Morrill","Alice-Dix complex, 6 to 20 percent slopes","Well drained","B",0.75,67.900000000000006,7.5]
["NE123","Morrill","Altvan-Dix complex, 3 to 9 percent slopes","Well drained","B",0.75,67.900000000000006,7.5]
["NE123","Morrill","Angora very fine sandy loam, 1 to 6 percent slopes","Well drained","B",0.25,61.4,7.5]
["NE123","Morrill","Angora very fine sandy loam, 6 to 20 percent slopes","Well drained","B",0.25,61.4,7.5]
["NE123","Morrill","Ashollow-Tassel complex, 9 to 30 percent slopes","Well drained","A",0.75,63.3,7.9]
["NE123","Morrill","Bankard fine sand, channeled, frequently flooded","Somewhat excessively drained","A",1,87,7.5500000000000007]
["NE123","Morrill","Bankard loamy coarse sand, occasionally flooded","Somewhat excessively drained","A",0.75,80.900000000000006,7.5500000000000007]
["NE123","Morrill","Bankard loamy fine sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,78.599999999999994,7.9]
["NE123","Morrill","Bankard loamy fine sand, occasionally flooded","Somewhat excessively drained","A",0.75,82.949999999999989,7.5500000000000007]
["NE123","Morrill","Barney loam, frequently flooded","Very poorly drained","B/D",1.625,67.45,7.35]
["NE123","Morrill","Bayard fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.375,62.5,7.5500000000000007]
["NE123","Morrill","Bayard very fine sandy loam, 6 to 9 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE123","Morrill","Bayard-Dix complex, 9 to 20 percent slopes","Well drained","A",1.125,62.9,7.35]
["NE123","Morrill","Blueridge coarse sand, 6 to 30 percent slopes","Excessively drained","A",0.5,91.45,6.5]
["NE123","Morrill","Blueridge gravelly sandy loam, 20 to 30 percent slopes","Excessively drained","A",0.5,80.099999999999994,6.75]
["NE123","Morrill","Bridget very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.375,40.75,7.5500000000000007]
["NE123","Morrill","Bridget very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.375,40.75,7.5500000000000007]
["NE123","Morrill","Bridget very fine sandy loam, 3 to 6 percent slopes","Well drained","B",1.375,40.75,7.5500000000000007]
["NE123","Morrill","Bridget very fine sandy loam, 6 to 9 percent slopes","Well drained","B",1.375,40.75,7.5500000000000007]
["NE123","Morrill","Bridget very fine sandy loam, 9 to 20 percent slopes","Well drained","B",1.375,40.75,7.5500000000000007]
["NE123","Morrill","Broadwater loamy sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,84.3,7.2]
["NE123","Morrill","Broadwater loamy sand, channeled, occasionally flooded","Excessively drained","A",0.25,91.9,7.2]
["NE123","Morrill","Busher loamy very fine sand, 1 to 6 percent slopes","Well drained","A",0.75,79.5,7]
["NE123","Morrill","Busher loamy very fine sand, 9 to 20 percent slopes","Well drained","A",0.75,79.5,7]
["NE123","Morrill","Busher very fine sandy loam, 1 to 6 percent slopes","Well drained","A",0.75,63.6,7]
["NE123","Morrill","Busher very fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,63.6,7]
["NE123","Morrill","Busher very fine sandy loam, 9 to 20 percent slopes","Well drained","A",0.75,63.6,7]
["NE123","Morrill","Busher-Jayem loamy very fine sands, 3 to 6 percent slopes","Well drained","A",0.52500000000000002,80,7.2]
["NE123","Morrill","Busher-Tassel complex, 3 to 9 percent slopes","Well drained","A",0.5,64.05,7.25]
["NE123","Morrill","Busher-Tassel complex, 9 to 20 percent slopes","Well drained","A",0.5,64.05,7.25]
["NE123","Morrill","Busher-Tassel loamy very fine sand, 3 to 9 percent slopes","Well drained","A",1,79.5,7.25]
["NE123","Morrill","Busher-Tassel loamy very fine sands, 9 to 20 percent slopes","Well drained","A",1,79.5,7.25]
["NE123","Morrill","Craft loamy very fine sand, 0 to 2 percent slopes","Well drained","A",0.75,68.55,7.9]
["NE123","Morrill","Craft very fine sandy loam, alkali, 0 to 2 percent slopes","Well drained","B",0.875,64.05,9.1499999999999986]
["NE123","Morrill","Craft very fine sandy loam, rarely flooded","Well drained","A",0.75,62.150000000000006,7.9]
["NE123","Morrill","Creighton very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE123","Morrill","Dailey loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1.375,87.9,7.25]
["NE123","Morrill","Dailey loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",1.375,87.9,7.25]
["NE123","Morrill","Dix gravelly loam, 9 to 50 percent slopes","Excessively drained","B",1.125,68.800000000000011,7.25]
["NE123","Morrill","Dix loamy coarse sand, 6 to 50 percent slopes","Excessively drained","A",1.125,83.35,7.25]
["NE123","Morrill","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE123","Morrill","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE123","Morrill","Duroc loam, 0 to 1 percent slopes","Well drained","B",2,37.15,7.2]
["NE123","Morrill","Duroc loam, 1 to 3 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE123","Morrill","Duroc loam, 1 to 6 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE123","Morrill","Duroc loam, 3 to 6 percent slopes","Well drained","B",1.375,37.15,7.2]
["NE123","Morrill","Els fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,94.9,6.7]
["NE123","Morrill","Els fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,93.2,7.9]
["NE123","Morrill","Els loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,91.1,7]
["NE123","Morrill","Epping-Keota silt loams, 3 to 30 percent slopes","Well drained","D",0.5,17.55,7.9]
["NE123","Morrill","Gering loam, alkali, occasionally flooded","Somewhat poorly drained","C",0.75,41.1,8.5]
["NE123","Morrill","Glenberg fine sandy loam, 0 to 2 percent slopes","Well drained","A",1,55.699999999999996,7.9]
["NE123","Morrill","Glenberg loamy fine sand, 0 to 2 percent slopes","Well drained","A",1,88.75,7.9]
["NE123","Morrill","Glenberg very fine sandy loam, 0 to 2 percent slopes","Well drained","A",1,76.349999999999994,7.9]
["NE123","Morrill","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,96.3,7.2]
["NE123","Morrill","Hoffland fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,78.2,7.5]
["NE123","Morrill","Hoffland fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7.5]
["NE123","Morrill","Hoffland fine sandy loam, occasionally flooded","Poorly drained","A/D",0.75,93.2,7.5]
["NE123","Morrill","Janise loam, occasionally flooded","Somewhat poorly drained","C",1.75,41,9.1]
["NE123","Morrill","Jankosh loam, rarely flooded","Somewhat poorly drained","C",0.5,51.150000000000006,8.5]
["NE123","Morrill","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE123","Morrill","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE123","Morrill","Jayem fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE123","Morrill","Jayem fine sandy loam, 9 to 20 percent slopes","Well drained","A",0.52500000000000002,63,7.2]
["NE123","Morrill","Jayem loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE123","Morrill","Jayem loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.75,78.2,7.2]
["NE123","Morrill","Keith loam, 0 to 1 percent slopes","Well drained","B",0.75,25,7]
["NE123","Morrill","Keith loam, 1 to 3 percent slopes","Well drained","B",0.75,25,7]
["NE123","Morrill","Keith loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7]
["NE123","Morrill","Keith loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,14.2,7]
["NE123","Morrill","Keith loam, 6 to 9 percent slopes, eroded","Well drained","B",0.75,14.2,7]
["NE123","Morrill","Lewellen-McCuligan complex, rarely flooded","Somewhat poorly drained","C",0.75,67.3,8.1999999999999993]
["NE123","Morrill","Lisco very fine sandy loam, occasionally flooded","Somewhat poorly drained","C",0.25,64.849999999999994,8.9499999999999993]
["NE123","Morrill","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7.5]
["NE123","Morrill","Marlake mucky peat","Very poorly drained","A/D",14.625,42.25,6.6]
["NE123","Morrill","Marlake very fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7]
["NE123","Morrill","McCook very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.375,59.6,7.9]
["NE123","Morrill","Minatare-Janise complex, rarely flooded","Somewhat poorly drained","C",1,33.6,9.1]
["NE123","Morrill","Mitchell very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1,36.650000000000006,7.9]
["NE123","Morrill","Mitchell very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1,36.650000000000006,7.9]
["NE123","Morrill","Mitchell very fine sandy loam, 3 to 6 percent slopes","Well drained","B",1,36.650000000000006,7.9]
["NE123","Morrill","Mitchell very fine sandy loam, 6 to 9 percent slopes","Well drained","B",1,36.650000000000006,7.9]
["NE123","Morrill","Mitchell very fine sandy loam, 9 to 20 percent slopes","Well drained","B",1,36.650000000000006,7.9]
["NE123","Morrill","Mitchell-Epping very fine sandy loams, 3 to 9 percent slopes","Well drained","D",0.75,27.450000000000003,7.9]
["NE123","Morrill","Mitchell-Epping very fine sandy loams, 9 to 20 percent slopes","Well drained","D",0.75,30.1,7.9]
["NE123","Morrill","Oglala-Canyon very fine sandy loams, 3 to 9 percent slopes","Well drained","D",1,60.5,7.2]
["NE123","Morrill","Otero loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.625,73.25,7.9]
["NE123","Morrill","Otero loamy very fine sand, 0 to 6 percent slopes","Well drained","A",0.625,73.25,7.9]
["NE123","Morrill","Otero loamy very fine sand, 3 to 9 percent slopes","Well drained","A",0.75,80.3,7.9]
["NE123","Morrill","Otero loamy very fine sand, 9 to 20 percent slopes","Well drained","A",0.625,73.25,7.9]
["NE123","Morrill","Otero variant very fine sandy loam, 0 to 1 percent slopes","Somewhat poorly drained","B",0.625,64.400000000000006,7.9]
["NE123","Morrill","Otero very fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.625,64.75,7.9]
["NE123","Morrill","Otero very fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.625,64.75,7.9]
["NE123","Morrill","Otero very fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.625,64.75,7.9]
["NE123","Morrill","Otero-Epping complex, 9 to 60 percent slopes","Well drained","D",0.75,30.1,7.9]
["NE123","Morrill","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,70.900000000000006,7.5]
["NE123","Morrill","Rock outcrop-Epping complex, 20 to 60 percent slopes","Well drained","D",0.375,15.05,3.75]
["NE123","Morrill","Rushcreek loam, rarely flooded","Moderately well drained","B",0.5,54.8,7.9]
["NE123","Morrill","Sarben loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE123","Morrill","Sarben loamy fine sand, 6 to 9 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE123","Morrill","Sarben loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.25,84,7.2]
["NE123","Morrill","Sarben loamy very fine sand, 3 to 9 percent slopes","Well drained","A",0.75,81.5,7.2]
["NE123","Morrill","Sarben loamy very fine sand, 9 to 20 percent slopes","Well drained","A",0.75,81.5,7.2]
["NE123","Morrill","Sarben very fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,62,7.2]
["NE123","Morrill","Sarben very fine sandy loam, 3 to 9 percent slopes","Well drained","A",0.75,62,7.2]
["NE123","Morrill","Tassel loamy very fine sand, 20 to 50 percent slopes","Well drained","D",1.25,79.5,7.9]
["NE123","Morrill","Tassel-Ashollow-Rock outcrop complex, 20 to 60 percent slopes","Well drained","A",0.75,63.3,7.9]
["NE123","Morrill","Tassel-Busher complex, 3 to 30 percent slopes","Well drained","A",1,64.05,7.25]
["NE123","Morrill","Tassel-Busher loamy very fine sands, 3 to 30 percent slopes","Well drained","A",1,79.5,7.25]
["NE123","Morrill","Tassel-Busher-Rock outcrop complex, 20 to 60 percent slopes","Well drained","A",1,79.3,7.25]
["NE123","Morrill","Tassel-Busher-Rock outcrop complex, 9 to 60 percent slopes","Well drained","A",0.75,63.6,7]
["NE123","Morrill","Tripp very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE123","Morrill","Tripp very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE123","Morrill","Tripp very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE123","Morrill","Tripp very fine sandy loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,58.6,7.5]
["NE123","Morrill","Tripp very fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.75,58.6,7.5]
["NE123","Morrill","Tripp very fine sandy loam, 6 to 9 percent slopes, eroded","Well drained","B",0.75,58.6,7.5]
["NE123","Morrill","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,95,7.2]
["NE123","Morrill","Valent fine sand, rolling","Excessively drained","A",0.5,95,7.2]
["NE123","Morrill","Valent fine sand, rolling and hilly","Excessively drained","A",0.5,95,7.2]
["NE123","Morrill","Valent loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,94.4,7.2]
["NE123","Morrill","Valent loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,94.4,7.2]
["NE123","Morrill","Valent loamy fine sand, 6 to 9 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE123","Morrill","Valentine complex, rolling and hilly","Excessively drained","A",0.5,94.9,7.2]
["NE123","Morrill","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,95.85,6.5]
["NE123","Morrill","Valentine fine sand, hilly","Excessively drained","A",0.5,95.85,6.5]
["NE123","Morrill","Valentine fine sand, rolling","Excessively drained","A",0.5,95.85,6.5]
["NE123","Morrill","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,95.85,6.5]
["NE123","Morrill","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE123","Morrill","Wildhorse fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,94.550000000000011,9.1499999999999986]
["NE123","Morrill","Wildhorse loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,90.1,9.1499999999999986]
["NE123","Morrill","Wildhorse sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,92.5,9.1499999999999986]
["NE123","Morrill","Wildhorse-Ipage, calcareous complex, 0 to 3 percent slopes","Moderately well drained","A",0.25,94.9,8.1999999999999993]
["NE123","Morrill","Yockey loam, alkali, occasionally flooded","Somewhat poorly drained","C",0.625,49.5,8.75]
["NE123","Morrill","Yockey silt loam, alkali, occasionally flooded","Somewhat poorly drained","C",0.875,37.950000000000003,8.6499999999999986]
["NE123","Morrill","Yockey silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,37.5,7.9]
["NE123","Morrill","Yockey very fine sandy loam, channeled, occasionally flooded","Somewhat poorly drained","C",0.5,60.85,7.9]
["NE125","Nance",null,"",""]
["NE125","Nance","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE125","Nance","Belfore silt loam, 0 to 1 percent slopes","Well drained","C",0.75,10,6.5]
["NE125","Nance","Belfore silt loam, 1 to 3 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE125","Nance","Belfore silt loam, 1 to 3 percent slopes, eroded","Well drained","C",0.75,17.8,6.5]
["NE125","Nance","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE125","Nance","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.125,67,6.85]
["NE125","Nance","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.599999999999994,7.5]
["NE125","Nance","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE125","Nance","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE125","Nance","Boel-Inavale complex, channeled, frequently flooded","Somewhat poorly drained","C",0.25,92.2,7.5]
["NE125","Nance","Cass fine sandy loam, occasionally flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE125","Nance","Cass silt loam, occasionally flooded","Well drained","B",0.75,63.5,7.3]
["NE125","Nance","Coly silt loam, 3 to 6 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE125","Nance","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.625,8,7.9]
["NE125","Nance","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE125","Nance","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,9.25,7.9]
["NE125","Nance","Crofton silt loam, 17 to 30 percent slopes, severely eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE125","Nance","Crofton silt loam, 30 to 60 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE125","Nance","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE125","Nance","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE125","Nance","Crofton-Nora silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE125","Nance","Crofton-Nora silt loams, 17 to 30 percent slopes","Well drained","B",0.75,8.5,7.5]
["NE125","Nance","Crofton-Nora silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE125","Nance","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,20,7.2]
["NE125","Nance","Els loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,91.1,6.75]
["NE125","Nance","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.5]
["NE125","Nance","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1.5,6.8,6.7]
["NE125","Nance","Fillmore silt loam, occasionally ponded","Somewhat poorly drained","D",1.125,12.649999999999999,7.1]
["NE125","Nance","Gayville-Caruso complex, occasionally flooded","Somewhat poorly drained","C",0.75,37.9,7.9]
["NE125","Nance","Geary variant silty clay loam, 11 to 17 percent slopes, severely eroded","Well drained","C",0.25,6.7,7]
["NE125","Nance","Geary variant silty clay loam, 7 to 11 percent slopes, severely eroded","Well drained","C",0.25,6.7,7]
["NE125","Nance","Gibbon loam, occasionally flooded","Somewhat poorly drained","C",0.75,41.5,7.9]
["NE125","Nance","Gibbon silt loam, moderately saline, occasionally flooded","Somewhat poorly drained","C",0.75,9.1,7.9]
["NE125","Nance","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",1.125,37.799999999999997,8.0500000000000007]
["NE125","Nance","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,95.35,7.2]
["NE125","Nance","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.5,79.849999999999994,7.35]
["NE125","Nance","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE125","Nance","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.5,9.5,7]
["NE125","Nance","Hall silt loam, 3 to 6 percent slopes","Well drained","C",1.5,9.5,7]
["NE125","Nance","Hall silt loam, 3 to 6 percent slopes, eroded","Well drained","C",1.5,9.5,7]
["NE125","Nance","Hall-Gayville variant silt loams, 0 to 1 percent slopes","Somewhat poorly drained","C",1.5,11.3,7]
["NE125","Nance","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,11.3,7]
["NE125","Nance","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE125","Nance","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE125","Nance","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,8,7.2]
["NE125","Nance","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,8,7.2]
["NE125","Nance","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.625,7.1,7.6]
["NE125","Nance","Hord fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.125,38.649999999999991,6.9]
["NE125","Nance","Hord fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.125,38.649999999999991,6.9]
["NE125","Nance","Hord fine sandy loam, 3 to 6 percent slopes","Well drained","B",1.125,38.75,6.9]
["NE125","Nance","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE125","Nance","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE125","Nance","Hord silt loam, sandy substratum, 0 to 1 percent slopes","Well drained","B",0.75,9.5,7]
["NE125","Nance","Hord very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.125,35.5,6.9]
["NE125","Nance","Hord very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.125,57.7,6.9]
["NE125","Nance","Hord very fine sandy loam, 3 to 6 percent slopes","Well drained","B",1.125,57.7,6.9]
["NE125","Nance","Hord very fine sandy loam, imperfectly drained, 0 to 1 percent slopes","Somewhat poorly drained","C",0.75,9.3000000000000007,7.9]
["NE125","Nance","Hord-Uly complex, 0 to 6 percent slopes","Well drained","B",0.75,9,6.7]
["NE125","Nance","Inavale fine sand, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE125","Nance","Inavale fine sandy loam, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE125","Nance","Inavale loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,84.3,6.7]
["NE125","Nance","Inavale loamy fine sand, occasionally flooded","Excessively drained","A",0.25,92.2,6.7]
["NE125","Nance","Inavale soils, frequently flooded","Excessively drained","A",0.25,92.2,6.7]
["NE125","Nance","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE125","Nance","Ipage-Els loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,92.75,6.6]
["NE125","Nance","Janude fine sandy loam, 0 to 1 percent slopes","Moderately well drained","B",1.25,63.5,7.5]
["NE125","Nance","Janude loam, rarely flooded","Moderately well drained","B",1.25,45,7.5]
["NE125","Nance","Janude sandy loam, very rarely flooded","Moderately well drained","B",1.25,66.599999999999994,7.5]
["NE125","Nance","Lamo clay loam, sandy substratum, 0 to 1 percent slopes","Somewhat poorly drained","C",0.5,40.1,7.9]
["NE125","Nance","Lamo silt loam, moderately saline, occasionally flooded","Somewhat poorly drained","C",1.5,6.8,7.9]
["NE125","Nance","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE125","Nance","Lamo-Saltine complex, occasionally flooded","Somewhat poorly drained","C",0.5,7.15,8.5]
["NE125","Nance","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,11.6,7.5]
["NE125","Nance","Loretto-Rusco variant fine sandy loams, 0 to 2 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE125","Nance","Loretto-Thurman complex, 1 to 3 percent slopes","Well drained","A",1.125,63.5,6.6]
["NE125","Nance","Loretto-Thurman complex, 3 to 6 percent slopes","Well drained","A",1.125,63.5,6.6]
["NE125","Nance","Loup fine sandy loam, occasionally flooded","Very poorly drained","A/D",3.375,79.2,6.6]
["NE125","Nance","Loup silt loam, occasionally flooded","Very poorly drained","B/D",3.375,62.8,6.6]
["NE125","Nance","Meadin loamy fine sand, 0 to 2 percent slopes","Excessively drained","A",0.75,85.3,6.2]
["NE125","Nance","Moody silty clay loam, 1 to 3 percent slopes","Well drained","C",3,6.9,6.5]
["NE125","Nance","Moody silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE125","Nance","Moody-Nora silt loams, 3 to 6 percent slopes","Well drained","C",1.875,9.3500000000000014,6.85]
["NE125","Nance","Moody-Nora silt loams, 3 to 6 percent slopes, eroded","Well drained","C",1.875,9.3500000000000014,6.85]
["NE125","Nance","Moody-Nora silt loams, 3 to 6 percent slopes, severely eroded","Well drained","C",1.25,9.4,6.5]
["NE125","Nance","Muir silt loam, 1 to 3 percent slopes","Well drained","B",2,9,6.7]
["NE125","Nance","Muir silt loam, 3 to 7 percent slopes","Well drained","B",2,9,6.7]
["NE125","Nance","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE125","Nance","Nora silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE125","Nance","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7]
["NE125","Nance","Nora silt loam, 6 to 11 percent slopes, severely eroded","Well drained","C",1.25,9.1,6.5]
["NE125","Nance","Nora-Crofton complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE125","Nance","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE125","Nance","Nora-Crofton silt loams, 11 to 17 percent slopes","Well drained","B",0.75,9.4,7.5]
["NE125","Nance","Nora-Crofton silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE125","Nance","Nora-Hersh complex, 11 to 17 percent slopes, severely eroded","Well drained","A",1,37.75,6.7]
["NE125","Nance","Nora-Hersh complex, 6 to 11 percent slopes, severely eroded","Well drained","A",1,37.75,6.7]
["NE125","Nance","Nora-Ortello complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,36.450000000000003,6.85]
["NE125","Nance","Novina sandy loam, rarely flooded","Moderately well drained","B",0.75,66.599999999999994,6.7]
["NE125","Nance","Obert silt loam, occasionally flooded","Poorly drained","C/D",1.5,11.3,7.9]
["NE125","Nance","Obert soils, occasionally flooded","Very poorly drained","C/D",1.5,7.3,7.9]
["NE125","Nance","O'Neill fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,67.599999999999994,6.5]
["NE125","Nance","Ord variant fine sandy loam, 0 to 1 percent slopes","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE125","Nance","Ord variant very fine sandy loam, 0 to 1 percent slopes","Somewhat poorly drained","C",0.75,63.3,7.5]
["NE125","Nance","Ortello fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE125","Nance","Ortello fine sandy loam, 1 to 3 percent slopes, eroded","Well drained","A",0.75,63.5,6.7]
["NE125","Nance","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE125","Nance","Ortello fine sandy loam, 3 to 6 percent slopes, eroded","Well drained","A",0.75,63.5,6.7]
["NE125","Nance","Ortello very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,63.6,6.7]
["NE125","Nance","Ovina loam, rarely flooded","Somewhat poorly drained","C",1.125,54.55,7.7]
["NE125","Nance","Platte-Gothenburg complex, channeled, frequently flooded","Poorly drained","A/D",0.25,79.2,7.5]
["NE125","Nance","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,87.3,7]
["NE125","Nance","Thurman loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE125","Nance","Thurman loamy fine sand, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE125","Nance","Thurman loamy fine sand, 1 to 3 percent slopes, eroded","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE125","Nance","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE125","Nance","Thurman loamy fine sand, 2 to 6 percent slopes, eroded","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE125","Nance","Thurman loamy fine sand, 2 to 6 percent slopes, severely eroded","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE125","Nance","Thurman-Ortello fine sandy loams, 0 to 2 percent slopes","Well drained","A",0.5,75.900000000000006,6.5]
["NE125","Nance","Thurman-Ortello fine sandy loams, 2 to 6 percent slopes, eroded","Well drained","A",0.5,75.900000000000006,6.5]
["NE125","Nance","Thurman-Ortello fine sandy loams, 6 to 11 percent slopes, eroded","Well drained","A",0.5,75.900000000000006,6.5]
["NE125","Nance","Uly, eroded-Hersh complex, 11 to 60 percent slopes","Well drained","A",0.81499999999999995,50,6.8]
["NE125","Nance","Uly-Coly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.73,24.5,7.9]
["NE125","Nance","Uly-Coly silt loams, 17 to 30 percent slopes, eroded, moist","Well drained","B",1,24,7.5]
["NE125","Nance","Uly-Holdrege silt loams, 7 to 11 percent slopes, eroded","Well drained","C",0.5,9.4,7.6]
["NE125","Nance","Ustorthents, steep","Well drained","B",0.75,30.1,7.9]
["NE125","Nance","Valentine fine sand, 3 to 17 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE125","Nance","Valentine fine sand, 3 to 17 percent slopes, eroded","Excessively drained","A",0.5,96.3,6.5]
["NE125","Nance","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE125","Nance","Valentine fine sand, 9 to 24 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE125","Nance","Valentine loamy fine sand, 3 to 17 percent slopes","Excessively drained","A",0.5,91.8,6.5]
["NE125","Nance","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE125","Nance","Valentine-Boelus loamy fine sands, 3 to 9 percent slopes","Well drained","A",0.5,86.85,6.5]
["NE125","Nance","Wann fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,66.2,8.1999999999999993]
["NE125","Nance","Wann loam, occasionally flooded","Somewhat poorly drained","C",0.75,66.2,8.1999999999999993]
["NE125","Nance","Wann sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,66.599999999999994,8.1999999999999993]
["NE125","Nance","Wann silt loam, moderately saline, occasionally flooded","Somewhat poorly drained","C",0.75,64.2,8.8000000000000007]
["NE125","Nance","Wann silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,66.2,8.1999999999999993]
["NE127","Nemaha",null,"",""]
["NE127","Nemaha","Ackmore silt loam, occasionally flooded","Somewhat poorly drained","C",3.5,8.1,6.6]
["NE127","Nemaha","Aksarben silty clay loam, 0 to 2 percent slopes","Well drained","C",1.125,19.100000000000001,5.9499999999999993]
["NE127","Nemaha","Aksarben silty clay loam, 2 to 6 percent slopes","Well drained","C",1.125,19.100000000000001,5.9499999999999993]
["NE127","Nemaha","Albaton silty clay, occasionally flooded","Poorly drained","D",1.5,3.9,7.9]
["NE127","Nemaha","Benfield-Kipson silty clay loams, 11 to 30 percent slopes","Well drained","D",1.125,13.399999999999999,7.25]
["NE127","Nemaha","Benfield-Kipson silty clay loams, 6 to 11 percent slopes, eroded","Well drained","D",1.125,13.399999999999999,7.25]
["NE127","Nemaha","Blencoe silty clay, clayey substratum, rarely flooded","Somewhat poorly drained","D",0.75,5.5,7.2]
["NE127","Nemaha","Burchard clay loam, 11 to 17 percent slopes","Well drained","C",0.75,36.5,7.1]
["NE127","Nemaha","Colo silty clay loam, occasionally flooded","Poorly drained","C/D",3.5,6.8,5.8]
["NE127","Nemaha","Grable very fine sandy loam, occasionally flooded","Somewhat excessively drained","A",0.5,59.6,7.9]
["NE127","Nemaha","Gymer silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,20,6.1]
["NE127","Nemaha","Haynie silt loam, occasionally flooded","Moderately well drained","B",1.25,34.65,7.9]
["NE127","Nemaha","Haynie silty clay, overwash, occasionally flooded","Moderately well drained","D",0.75,11.4,8.1999999999999993]
["NE127","Nemaha","Judson silt loam, 0 to 2 percent slopes","Well drained","C",2.5,7.1,6.5]
["NE127","Nemaha","Judson silt loam, 2 to 6 percent slopes","Well drained","C",2.5,7.1,6.5]
["NE127","Nemaha","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,8.3000000000000007,6.6]
["NE127","Nemaha","Kennebec-Nodaway silt loams, occasionally flooded","Moderately well drained","B",2.5,9.1999999999999993,6.7]
["NE127","Nemaha","Malcolm silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,11.4,6.1]
["NE127","Nemaha","Malmo clay, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE127","Nemaha","Marshall silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,6.9,6.5]
["NE127","Nemaha","Monona-Ida silt loams, 30 to 60 percent slopes","Well drained","B",1,11.2,7.5]
["NE127","Nemaha","Monona-Kipson complex, 30 to 70 percent slopes","Somewhat excessively drained","D",0.875,10.350000000000001,7.1]
["NE127","Nemaha","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,35.4,6.1]
["NE127","Nemaha","Moville silt loam, occasionally flooded","Somewhat poorly drained","C",2.75,8.35,7.5500000000000007]
["NE127","Nemaha","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.4,6.7]
["NE127","Nemaha","Nodaway silt loam, occasionally flooded","Moderately well drained","B",2.5,9.5,6.7]
["NE127","Nemaha","Nodaway-Colo complex, occasionally flooded","Poorly drained","C",2,8.25,6.7]
["NE127","Nemaha","Nodaway-Colo silt loams, occasionally flooded","Poorly drained","C/D",2.5,6.9,6.3]
["NE127","Nemaha","Onawa silt loam, occasionally flooded","Somewhat poorly drained","D",0.5,27.1,7.9]
["NE127","Nemaha","Onawa silt loam, overwash, occasionally flooded","Somewhat poorly drained","D",0.5,27.1,7.9]
["NE127","Nemaha","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE127","Nemaha","Pawnee and Mayberry clay loams, 3 to 11 percent slopes, eroded","Moderately well drained","D",1.375,33.700000000000003,6.75]
["NE127","Nemaha","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE127","Nemaha","Percival-Albaton silty clays, occasionally flooded","Poorly drained","D",1,5.3,7.9]
["NE127","Nemaha","Pohocco silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.25,9.4,6.7]
["NE127","Nemaha","Pohocco silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.25,9.4,6.7]
["NE127","Nemaha","Pohocco silty clay loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,8.9,6.5]
["NE127","Nemaha","Pohocco silty clay loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,8.9,6.5]
["NE127","Nemaha","Pohocco, eroded-Ida silt loams, 11 to 17 percent slopes","Well drained","B",0.25,9.4,7.5]
["NE127","Nemaha","Pohocco, eroded-Ida silt loams, 17 to 30 percent slopes","Well drained","B",0.25,9.4,7.5]
["NE127","Nemaha","Pohocco, eroded-Ida silt loams, 6 to 11 percent slopes","Well drained","B",0.25,9.4,7.5]
["NE127","Nemaha","Sarpy loamy fine sand, occasionally flooded","Excessively drained","A",0.75,87.9,7.5]
["NE127","Nemaha","Sarpy-Haynie complex, frequently flooded","Well drained","B",0.75,47.100000000000009,7.5]
["NE127","Nemaha","Sarpy-Haynie complex, occasionally flooded","Moderately well drained","B",0.75,78.45,7.5]
["NE127","Nemaha","Shelby clay loam, 17 to 30 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE127","Nemaha","Shelby clay loam, 6 to 11 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE127","Nemaha","Sogn-Kipson complex, 7 to 30 percent slopes","Somewhat excessively drained","D",1,10,3.6]
["NE127","Nemaha","Udorthents silty clay loam","Well drained","B",0.375,10,3.9]
["NE127","Nemaha","Wabash silty clay, frequently flooded, depressional","Very poorly drained","D",2.25,5.5,6.35]
["NE127","Nemaha","Wabash silty clay, occasionally flooded","Poorly drained","D",2.25,6.5,6.35]
["NE127","Nemaha","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",0.75,17.3,6.5]
["NE127","Nemaha","Wymore silty clay loam, 2 to 6 percent slopes","Moderately well drained","D",0.75,17.3,6.5]
["NE127","Nemaha","Wymore silty clay loam, 3 to 11 percent slopes, eroded","Moderately well drained","D",1.5,17.3,6.5]
["NE127","Nemaha","Wymore silty clay, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.5,7.7,6.5]
["NE127","Nemaha","Yutan silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.625,7.6,6.6]
["NE127","Nemaha","Yutan silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.625,7.6,6.6]
["NE127","Nemaha","Zoe-Zook silty clay loams, occasionally flooded","Poorly drained","D",2,7.6,7]
["NE127","Nemaha","Zook silt loam, occasionally flooded","Poorly drained","D",3,15.85,6.6]
["NE127","Nemaha","Zook silty clay loam, occasionally flooded","Poorly drained","D",4.5,7.35,6.6]
["NE129","Nuckolls",null,"",""]
["NE129","Nuckolls","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,15,7.1]
["NE129","Nuckolls","Cass fine sandy loam, occasionally flooded","Well drained","A",0.5,70,7.15]
["NE129","Nuckolls","Cass loam, occasionally flooded","Well drained","B",0.75,63.5,7.3]
["NE129","Nuckolls","Coly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",1.125,11.3,7.7]
["NE129","Nuckolls","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE129","Nuckolls","Cozad silt loam, 0 to 1 percent slopes","Well drained","C",0.75,14.2,7]
["NE129","Nuckolls","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE129","Nuckolls","Deroin soils, 3 to 6 percent slopes, severely eroded","Well drained","C",0.5,6.7,7]
["NE129","Nuckolls","Deroin soils, 6 to 11 percent slopes, severely eroded","Well drained","C",0.5,6.7,7]
["NE129","Nuckolls","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1.125,7.65,7.1]
["NE129","Nuckolls","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,44.9,3.75]
["NE129","Nuckolls","Geary and Hobbs soils","Well drained","B",2,7.3,7]
["NE129","Nuckolls","Geary and Jansen silt loams, 3 to 7 percent slopes","Well drained","C",1.25,20.3,6.2]
["NE129","Nuckolls","Geary and Jansen soils, 11 to 30 percent slopes","Well drained","C",1.25,20.3,6.2]
["NE129","Nuckolls","Geary and Jansen soils, 7 to 11 percent slopes, eroded","Well drained","C",1.25,19.200000000000003,6.2]
["NE129","Nuckolls","Geary silt loam, 3 to 7 percent slopes","Well drained","C",1.25,9.1,6.7]
["NE129","Nuckolls","Geary silt loam, 7 to 11 percent slopes","Well drained","C",1.25,9.1,6.7]
["NE129","Nuckolls","Geary silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,6.9,6.7]
["NE129","Nuckolls","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.7]
["NE129","Nuckolls","Geary variant-Uly complex, 11 to 30 percent slopes, severely eroded","Well drained","C",0.5,7.9,7]
["NE129","Nuckolls","Geary-Hobbs silt loams, 0 to 30 percent slopes","Well drained","C",0.75,9.5,7]
["NE129","Nuckolls","Geary-Uly complex, 11 to 30 percent slopes","Well drained","C",1,9.3000000000000007,7]
["NE129","Nuckolls","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE129","Nuckolls","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.5,8.9,7.9]
["NE129","Nuckolls","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.5,88,7.35]
["NE129","Nuckolls","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE129","Nuckolls","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",3,26.5,6.1]
["NE129","Nuckolls","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",3,26.5,6.1]
["NE129","Nuckolls","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",3,26.5,6.1]
["NE129","Nuckolls","Hastings silt loam, 7 to 11 percent slopes","Well drained","C",1.75,13.100000000000001,6.3]
["NE129","Nuckolls","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,20,7.3]
["NE129","Nuckolls","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE129","Nuckolls","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE129","Nuckolls","Holder silt loam, 1 to 3 percent slopes","Well drained","C",1.25,9.4,7]
["NE129","Nuckolls","Holder silt loam, 3 to 7 percent slopes","Well drained","C",1.25,9.4,7]
["NE129","Nuckolls","Holder silt loam, 7 to 11 percent slopes","Well drained","C",1.25,9.4,7]
["NE129","Nuckolls","Holder silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,6.8,7]
["NE129","Nuckolls","Holder silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,6.8,7]
["NE129","Nuckolls","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",1.25,7,7.2]
["NE129","Nuckolls","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",1.25,7,7.2]
["NE129","Nuckolls","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,7,7.2]
["NE129","Nuckolls","Holdrege silt loam, 7 to 11 percent slopes","Well drained","C",1.25,7,7.2]
["NE129","Nuckolls","Holdrege soils, 3 to 7 percent slopes, severely eroded","Well drained","C",0.75,6.3,7.2]
["NE129","Nuckolls","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE129","Nuckolls","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE129","Nuckolls","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE129","Nuckolls","Inavale fine sandy loam, rarely flooded","Excessively drained","A",0.5,73.55,6.7]
["NE129","Nuckolls","Inavale loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,85.8,7.1]
["NE129","Nuckolls","Kipson silt loam, 7 to 30 percent slopes","Somewhat excessively drained","D",0.75,23.5,7.9]
["NE129","Nuckolls","Massie silty clay loam, frequently ponded","Very poorly drained","D",3.125,4.8499999999999996,6.25]
["NE129","Nuckolls","McCook fine sandy loam, rarely flooded","Well drained","B",1.375,61.05,7.7]
["NE129","Nuckolls","McCook silt loam, rarely flooded","Well drained","B",1.875,35.650000000000006,7.9]
["NE129","Nuckolls","Meadin loam, 6 to 30 percent slopes","Excessively drained","B",0.75,65.3,6.2]
["NE129","Nuckolls","Muir silt loam, very rarely flooded","Well drained","B",1.5,16.5,6.9]
["NE129","Nuckolls","Munjor soils, occasionally flooded","Well drained","B",0.625,62.650000000000006,7.9]
["NE129","Nuckolls","Saltine loam, occasionally flooded","Somewhat poorly drained","C",0.4,8,8.5]
["NE129","Nuckolls","Scott silt loam, frequently ponded","Poorly drained","D",1.125,21.1,7.1]
["NE129","Nuckolls","Uly silt loam, 11 to 17 percent slopes, eroded","Somewhat excessively drained","B",0.75,9.5,7]
["NE129","Nuckolls","Uly silt loam, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE129","Nuckolls","Uly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,10.35,7]
["NE129","Nuckolls","Wann fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,66.2,8.1999999999999993]
["NE129","Nuckolls","Wann loam, rarely flooded","Somewhat poorly drained","C",0.75,66.2,8.1999999999999993]
["NE131","Otoe",null,"",""]
["NE131","Otoe","Aksarben silty clay loam, 0 to 2 percent slopes","Well drained","C",1.5,20,5.8]
["NE131","Otoe","Aksarben silty clay loam, 2 to 6 percent slopes","Well drained","C",1.5,20,5.8]
["NE131","Otoe","Albaton silty clay, occasionally flooded","Poorly drained","D",1.5,3.9,7.9]
["NE131","Otoe","Burchard-Morrill clay loams, 6 to 11 percent slopes","Well drained","C",0.75,36.5,6.55]
["NE131","Otoe","Colo silty clay loam, occasionally flooded","Poorly drained","C/D",3.5,6.8,5.8]
["NE131","Otoe","Colo-Nodaway complex, frequently flooded","Poorly drained","C/D",3,6.85,6.3]
["NE131","Otoe","Dickinson fine sandy loam, 11 to 20 percent slopes","Well drained","A",0.75,67.3,5.8]
["NE131","Otoe","Dickinson fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,67.3,5.8]
["NE131","Otoe","Haynie silt loam, occasionally flooded","Moderately well drained","B",1.25,12.600000000000001,7.7]
["NE131","Otoe","Judson silt loam, 0 to 2 percent slopes","Well drained","C",3.5,7.9,6.5]
["NE131","Otoe","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3.5,7.9,6.5]
["NE131","Otoe","Kennebec silt loam, occasionally flooded","Moderately well drained","B",2,5,6.35]
["NE131","Otoe","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE131","Otoe","Kennebec-Nodaway silt loams, occasionally flooded","Moderately well drained","B",2,9.35,6.7]
["NE131","Otoe","Kennebec-Nodaway silt loams, rarely flooded","Moderately well drained","B",2,8.3000000000000007,6.7]
["NE131","Otoe","Kipson-Benfield complex, 7 to 20 percent slopes","Well drained","D",1.125,13.850000000000001,7.25]
["NE131","Otoe","Malcolm silt loam, 11 to 25 percent slopes","Well drained","C",1.25,11.4,6.1]
["NE131","Otoe","Malcolm silt loam, 6 to 11 percent slopes","Well drained","C",1.25,11.4,6.1]
["NE131","Otoe","Malcolm silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,11.4,6.1]
["NE131","Otoe","Malmo clay, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE131","Otoe","Malmo, eroded-Pawnee complex, 6 to 11 percent slopes","Moderately well drained","D",0.75,29.9,7]
["NE131","Otoe","Marshall silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,6.9,6.5]
["NE131","Otoe","Marshall-Ponca silt loams, 11 to 17 percent slopes","Well drained","C",1.125,9.0500000000000007,6.85]
["NE131","Otoe","Mayberry clay loam, 3 to 11 percent slopes","Moderately well drained","D",0.75,34.200000000000003,6.5]
["NE131","Otoe","Mayberry silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.75,26.1,6.5]
["NE131","Otoe","Monona silt loam, 17 to 30 percent slopes","Well drained","B",1,9.4,6.7]
["NE131","Otoe","Monona silt loam, 2 to 6 percent slopes","Well drained","B",1,9.4,6.7]
["NE131","Otoe","Monona-Kipson complex, 30 to 70 percent slopes","Somewhat excessively drained","D",0.875,10.350000000000001,7.1]
["NE131","Otoe","Monona-Shelby-Kipson complex, 30 to 70 percent slopes","Somewhat excessively drained","D",0.75,23.5,6.7]
["NE131","Otoe","Morrill clay loam, 6 to 11 percent slopes","Well drained","C",0.6,42.4,6.1]
["NE131","Otoe","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,35.4,6.1]
["NE131","Otoe","Morrill-Malmo, eroded, complex, 3 to 11 percent slopes","Moderately well drained","D",0.75,35.4,6.8]
["NE131","Otoe","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.5,6.7]
["NE131","Otoe","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,9.5,6.7]
["NE131","Otoe","Nodaway-Colo complex, occasionally flooded","Poorly drained","C",2,8.25,6.7]
["NE131","Otoe","Nodaway-Colo silt loams, occasionally flooded","Poorly drained","C/D",2.5,6.9,6.3]
["NE131","Otoe","Onawa silt loam, overwash, occasionally flooded","Somewhat poorly drained","D",0.5,27.1,7.9]
["NE131","Otoe","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE131","Otoe","Otoe silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE131","Otoe","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE131","Otoe","Pawnee clay loam, 6 to 11 percent slopes","Moderately well drained","D",2,33.9,7]
["NE131","Otoe","Pawnee clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",2,33.5,7]
["NE131","Otoe","Pawnee clay, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,27.6,6.5]
["NE131","Otoe","Pohocco silty clay loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,8.9,7.2]
["NE131","Otoe","Pohocco, eroded-Ida silt loams, 6 to 11 percent slopes","Well drained","B",0.25,9.4,7.5]
["NE131","Otoe","Ponca-Dow silt loams, 11 to 17 percent slopes, eroded","Well drained","B",1.5,11.2,7.5]
["NE131","Otoe","Ponca-Dow silt loams, 6 to 11 percent slopes, eroded","Well drained","B",1.5,11.2,7.5]
["NE131","Otoe","Sarpy-Haynie complex, occasionally flooded","Moderately well drained","B",0.75,78.45,7.5]
["NE131","Otoe","Shelby and Burchard clay loams, 11 to 17 percent slopes","Well drained","C",0.625,35.4,6.6]
["NE131","Otoe","Shelby clay loam, 11 to 17 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE131","Otoe","Shelby clay loam, 17 to 30 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE131","Otoe","Shelby clay loam, 6 to 11 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE131","Otoe","Steinauer clay loam, 11 to 20 percent slopes","Well drained","C",0.75,33.6,7.9]
["NE131","Otoe","Wabash silty clay, occasionally flooded","Poorly drained","D",2.25,6.5,6.65]
["NE131","Otoe","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",0.75,17.3,6.5]
["NE131","Otoe","Wymore silty clay loam, 2 to 6 percent slopes","Moderately well drained","D",0.75,17.3,6.5]
["NE131","Otoe","Wymore silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",1.5,17.3,6.5]
["NE131","Otoe","Wymore silty clay, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.5,7.7,6.5]
["NE131","Otoe","Yutan silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.75,7.6,6.5]
["NE131","Otoe","Yutan silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,7.6,6.5]
["NE131","Otoe","Zoe silty clay loam, occasionally flooded","Poorly drained","D",0.75,7.2,7]
["NE131","Otoe","Zoe-Zook silty clay loams, occasionally flooded","Poorly drained","C",2,7.6,7]
["NE131","Otoe","Zook silty clay loam, occasionally flooded","Poorly drained","D",4.5,7.75,6.6]
["NE133","Pawnee",null,"",""]
["NE133","Pawnee","Benfield silty clay loam, 3 to 11 percent slopes, eroded","Well drained","D",1.5,7.7,7.25]
["NE133","Pawnee","Benfield soils, 3 to 11 percent slopes, severely eroded","Well drained","D",1.5,7.25,7.25]
["NE133","Pawnee","Burchard clay loam, 11 to 17 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE133","Pawnee","Burchard clay loam, 6 to 11 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE133","Pawnee","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE133","Pawnee","Burchard-Steinauer clay loams, 6 to 11 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE133","Pawnee","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,13.649999999999999,7.1]
["NE133","Pawnee","Colo and Kennebec soils, occasionally flooded","Poorly drained","C/D",3.5,6.9,6.3]
["NE133","Pawnee","Cortland-Malmo complex, 6 to 11 percent slopes, eroded","Well drained","C",0.75,37.549999999999997,6.5]
["NE133","Pawnee","Crete silt loam, terrace, 0 to 1 percent slopes","Moderately well drained","C",1,14.149999999999999,7.3000000000000007]
["NE133","Pawnee","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3.5,7.9,6.5]
["NE133","Pawnee","Kennebec silt loam, occasionally flooded","Moderately well drained","C",2,5,6.35]
["NE133","Pawnee","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE133","Pawnee","Kennebec-Nodaway silt loams, rarely flooded","Moderately well drained","B",2,8.3000000000000007,6.7]
["NE133","Pawnee","Kezan silt loam, frequently flooded","Poorly drained","C/D",1.875,9.0500000000000007,7.2]
["NE133","Pawnee","Kipson-Benfield complex, 11 to 25 percent slopes","Well drained","D",1.125,13.850000000000001,7.25]
["NE133","Pawnee","Kipson-Benfield silty clay loams, 7 to 17 percent slopes","Well drained","D",1.5,7.7,7.5]
["NE133","Pawnee","Kipson-Sogn complex, 3 to 30 percent slopes","Somewhat excessively drained","D",0.75,10,7.9]
["NE133","Pawnee","Malcolm complex, 11 to 25 percent slopes","Well drained","C",1.25,11.4,6.1]
["NE133","Pawnee","Malcolm complex, 6 to 11 percent slopes","Well drained","C",1.25,11.4,6.1]
["NE133","Pawnee","Malcolm silt loam, 6 to 11 percent slopes","Well drained","C",1.25,11.4,6.1]
["NE133","Pawnee","Malmo clay loam, 2 to 6 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE133","Pawnee","Malmo clay loam, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE133","Pawnee","Malmo clay, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE133","Pawnee","Malmo soils, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE133","Pawnee","Malmo, eroded-Pawnee complex, 6 to 11 percent slopes","Moderately well drained","D",0.75,29.9,7]
["NE133","Pawnee","Mayberry clay loam, 3 to 11 percent slopes","Moderately well drained","D",0.75,34.200000000000003,6.7]
["NE133","Pawnee","Mayberry loam, 3 to 11 percent slopes","Moderately well drained","D",0.75,38.799999999999997,6.5]
["NE133","Pawnee","Morrill clay loam, 6 to 11 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE133","Pawnee","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,35.4,6.1]
["NE133","Pawnee","Morrill loam, 11 to 17 percent slopes","Well drained","C",0.6,41.6,6.1]
["NE133","Pawnee","Morrill loam, 3 to 6 percent slopes","Well drained","C",0.6,41.6,6.1]
["NE133","Pawnee","Morrill loam, 6 to 11 percent slopes","Well drained","C",0.6,41.6,6.1]
["NE133","Pawnee","Morrill soils, 11 to 17 percent slopes, severely eroded","Well drained","C",0.75,35.4,6.1]
["NE133","Pawnee","Morrill soils, 6 to 11 percent slopes, severely eroded","Well drained","C",0.75,35.4,6.1]
["NE133","Pawnee","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.5,6.7]
["NE133","Pawnee","Nodaway silt loam, channeled, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE133","Pawnee","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.875,9.4,6.7]
["NE133","Pawnee","Otoe soils, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE133","Pawnee","Pawnee and Malmo soils, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.75,29.9,7]
["NE133","Pawnee","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE133","Pawnee","Pawnee clay, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,27.6,7.3]
["NE133","Pawnee","Pawnee loam, 0 to 3 percent slopes","Moderately well drained","D",2,33.5,7]
["NE133","Pawnee","Shelby and Burchard clay loams, 11 to 17 percent slopes","Well drained","C",0.75,35.4,6.6]
["NE133","Pawnee","Shelby clay loam, 11 to 17 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE133","Pawnee","Shelby clay loam, 17 to 30 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE133","Pawnee","Shelby clay loam, 6 to 11 percent slopes","Moderately well drained","C",0.5,34.700000000000003,6.2]
["NE133","Pawnee","Steinauer clay loam, 11 to 20 percent slopes","Well drained","C",0.75,33.6,7.9]
["NE133","Pawnee","Steinauer clay loam, 30 to 50 percent slopes","Well drained","C",0.75,33.6,8.1999999999999993]
["NE133","Pawnee","Steinauer clay loam, 6 to 11 percent slopes","Well drained","C",0.75,33.6,7.9]
["NE133","Pawnee","Wabash silty clay loam, occasionally flooded","Poorly drained","D",2.25,12.649999999999999,6.35]
["NE133","Pawnee","Wabash silty clay, occasionally flooded","Poorly drained","D",2.25,6.5,6.35]
["NE133","Pawnee","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE133","Pawnee","Wymore silty clay loam, 1 to 3 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE133","Pawnee","Wymore silty clay loam, 2 to 6 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE133","Pawnee","Wymore silty clay loam, 3 to 11 percent slopes, eroded","Moderately well drained","D",1.5,17.3,6.5]
["NE133","Pawnee","Wymore silty clay loam, 3 to 6 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE133","Pawnee","Wymore silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",1,6,6.4]
["NE133","Pawnee","Wymore silty clay loam, terrace, 0 to 2 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE133","Pawnee","Wymore silty clay, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.5,7.7,6.5]
["NE135","Perkins",null,"",""]
["NE135","Perkins","Alliance silt loam, 0 to 1 percent slopes","Well drained","B",0.75,10.25,7.2]
["NE135","Perkins","Alliance silt loam, 1 to 3 percent slopes","Well drained","B",0.75,10.25,7.2]
["NE135","Perkins","Altvan loam, 1 to 3 percent slopes","Well drained","B",0.75,43.849999999999994,7.85]
["NE135","Perkins","Altvan loam, 3 to 6 percent slopes","Well drained","B",0.75,43.849999999999994,7.85]
["NE135","Perkins","Altvan-Dix complex, 6 to 30 percent slopes","Well drained","B",0.75,56.55,7.5]
["NE135","Perkins","Altvan-Eckley-Satanta complex, 3 to 9 percent slopes","Well drained","C",0.75,62,7.2]
["NE135","Perkins","Ascalon fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,64.599999999999994,7.9]
["NE135","Perkins","Ascalon fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,64.599999999999994,7.9]
["NE135","Perkins","Bankard loamy sand, channeled, frequently flooded","Somewhat excessively drained","A",0.25,92.1,7.9]
["NE135","Perkins","Blanche fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,62.8,7.2]
["NE135","Perkins","Creighton very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE135","Perkins","Creighton very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,63.3,7.2]
["NE135","Perkins","Dailey loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,80.400000000000006,7.2]
["NE135","Perkins","Duda-Tassel complex, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,63.3,6.85]
["NE135","Perkins","Gannett variant silt loam, occasionally flooded","Very poorly drained","B/D",2.875,39.299999999999997,6.6]
["NE135","Perkins","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",1.875,36.9,8.0500000000000007]
["NE135","Perkins","Haxtun fine sandy loam, 0 to 3 percent slopes","Well drained","B",1.75,59.6,7]
["NE135","Perkins","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE135","Perkins","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE135","Perkins","Jayem loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,62.5,7.2]
["NE135","Perkins","Keith loam, 1 to 3 percent slopes","Well drained","B",0.75,21.2,7]
["NE135","Perkins","Keith loam, 3 to 6 percent slopes","Well drained","B",0.75,21.2,7]
["NE135","Perkins","Keith silt loam, 1 to 3 percent slopes","Well drained","C",0.75,11.8,7]
["NE135","Perkins","Keith silt loam, 3 to 6 percent slopes, eroded","Well drained","C",0.75,13.7,7]
["NE135","Perkins","Kuma loam, 0 to 1 percent slopes","Well drained","C",2,36.9,7.5]
["NE135","Perkins","Kuma loam, 1 to 3 percent slopes","Well drained","C",2,36.9,7.5]
["NE135","Perkins","Kuma silt loam, 0 to 1 percent slopes","Well drained","C",2,9,7.3]
["NE135","Perkins","Kuma silt loam, 1 to 3 percent slopes","Well drained","C",2,9,7.3]
["NE135","Perkins","Lodgepole silt loam, frequently ponded","Somewhat poorly drained","C/D",2,26.4,7]
["NE135","Perkins","Mace silt loam, 0 to 1 percent slopes","Well drained","C",1,11.25,7.1]
["NE135","Perkins","Mace silt loam, 1 to 3 percent slopes","Well drained","C",1,11.25,7.1]
["NE135","Perkins","McCash very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.25,60.3,7]
["NE135","Perkins","McCash very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.25,60.3,7]
["NE135","Perkins","McCook silt loam, occasionally flooded","Well drained","B",1.75,35.450000000000003,7.9]
["NE135","Perkins","Rosebud loam, 0 to 1 percent slopes","Well drained","C",0.75,39.4,7.35]
["NE135","Perkins","Rosebud loam, 1 to 3 percent slopes","Well drained","C",0.75,39.4,7.35]
["NE135","Perkins","Rosebud-Canyon loams, 1 to 3 percent slopes","Well drained","D",0.75,43.2,7.5]
["NE135","Perkins","Rosebud-Canyon loams, 3 to 6 percent slopes","Well drained","D",0.75,43.2,7.5]
["NE135","Perkins","Rosebud-Canyon loams, 6 to 12 percent slopes, eroded","Well drained","D",0.75,43,7.5]
["NE135","Perkins","Sarben loamy fine sand, 3 to 6 percent slopes","Well drained","A",0.5,83,6.95]
["NE135","Perkins","Sarben loamy fine sand, 6 to 9 percent slopes","Well drained","A",0.5,83,6.95]
["NE135","Perkins","Sarben loamy very fine sand, 3 to 6 percent slopes","Well drained","A",1,81,7.3000000000000007]
["NE135","Perkins","Sarben loamy very fine sand, 6 to 9 percent slopes","Well drained","A",1,81,7.3000000000000007]
["NE135","Perkins","Satanta loam, 0 to 1 percent slopes","Well drained","C",0.75,42.7,7.5]
["NE135","Perkins","Satanta loam, 1 to 3 percent slopes","Well drained","C",0.75,43,7.5]
["NE135","Perkins","Satanta loam, 3 to 6 percent slopes","Well drained","C",0.75,43,7.5]
["NE135","Perkins","Satanta very fine sandy loam, 1 to 3 percent slopes","Well drained","C",0.75,64.400000000000006,7.5]
["NE135","Perkins","Satanta very fine sandy loam, 3 to 6 percent slopes","Well drained","C",0.75,64.400000000000006,8.4]
["NE135","Perkins","Satanta-Altvan complex, 3 to 6 percent slopes","Well drained","C",0.75,62,7.7]
["NE135","Perkins","Sulco-Ulysses silt loams, 9 to 30 percent slopes, eroded","Well drained","B",1.25,13.6,7.9]
["NE135","Perkins","Tassel-Duda loamy sands, 6 to 30 percent slopes","Somewhat excessively drained","A",0.875,71.900000000000006,6.85]
["NE135","Perkins","Ulysses-Sulco silt loams, 3 to 6 percent slopes, eroded","Well drained","B",1,13.6,7.9]
["NE135","Perkins","Ulysses-Sulco silt loams, 6 to 9 percent slopes, eroded","Well drained","B",1,13.6,7.9]
["NE135","Perkins","Valent loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,88.6,7]
["NE135","Perkins","Valent loamy sand, 3 to 9 percent slopes","Excessively drained","A",0.5,88.6,7]
["NE135","Perkins","Valent sand, rolling","Excessively drained","A",0.5,95,7]
["NE135","Perkins","Valent sand, rolling and hilly","Excessively drained","A",0.375,95,7]
["NE135","Perkins","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE135","Perkins","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE135","Perkins","Vetal loamy fine sand, 0 to 3 percent slopes","Well drained","A",2,85.9,7.2]
["NE135","Perkins","Woodly fine sandy loam, 0 to 3 percent slopes","Well drained","B",0.5,65.400000000000006,7]
["NE135","Perkins","Woodly loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.5,65.400000000000006,7]
["NE137","Phelps",null,"",""]
["NE137","Phelps","Alda loam, rarely flooded","Somewhat poorly drained","C",0.75,66,7.9]
["NE137","Phelps","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE137","Phelps","Anselmo fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE137","Phelps","Anselmo fine sandy loam, hummocky, eroded","Well drained","A",0.75,66.099999999999994,7]
["NE137","Phelps","Anselmo fine sandy loam, terrace, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE137","Phelps","Anselmo very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,66.099999999999994,7]
["NE137","Phelps","Anselmo very fine sandy loam, terrace, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE137","Phelps","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE137","Phelps","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.8]
["NE137","Phelps","Coly and Kenesaw silt loams, 6 to 11 percent slopes","Well drained","B",0.75,11.3,7.9]
["NE137","Phelps","Coly and Nuckolls silt loams, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.4,7.9]
["NE137","Phelps","Coly and Uly silt loams, 3 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE137","Phelps","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE137","Phelps","Coly silt loam, 11 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE137","Phelps","Coly silt loam, 3 to 6 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE137","Phelps","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE137","Phelps","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE137","Phelps","Coly-Kenesaw silt loams, 0 to 3 percent slopes","Well drained","B",0.75,11.3,7.8]
["NE137","Phelps","Coly-Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.6]
["NE137","Phelps","Coly-Uly silt loams, 3 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.6]
["NE137","Phelps","Coly-Uly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.8]
["NE137","Phelps","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE137","Phelps","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7.8]
["NE137","Phelps","Cozad silt loam, rarely flooded","Well drained","B",0.75,14.3,7.4]
["NE137","Phelps","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE137","Phelps","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,20,7.4]
["NE137","Phelps","Dunday loamy fine sand, terrace, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,82.9,6.85]
["NE137","Phelps","Fillmore silt loam, drained, frequently ponded","Somewhat poorly drained","D",1.125,12.649999999999999,7.1]
["NE137","Phelps","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE137","Phelps","Gibbon loam, saline, rarely flooded","Somewhat poorly drained","C",0.75,9.1,7.9]
["NE137","Phelps","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,91.9,7.3]
["NE137","Phelps","Gothenburg soils, frequently flooded","Poorly drained","B/D",0.25,91.9,7.5]
["NE137","Phelps","Grigston silt loam","Well drained","B",1.5,9.1,7]
["NE137","Phelps","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7.4]
["NE137","Phelps","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.5]
["NE137","Phelps","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,10.4,7.45]
["NE137","Phelps","Hobbs silt loam, overwash, occasionally flooded","Well drained","B",1.875,10.4,7.45]
["NE137","Phelps","Holdrege and Uly soils, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.4,7.4]
["NE137","Phelps","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.25,7.6]
["NE137","Phelps","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.6]
["NE137","Phelps","Holdrege silt loam, 1 to 3 percent slopes, eroded","Well drained","C",0.75,8.4,7.6]
["NE137","Phelps","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,8.4,7.6]
["NE137","Phelps","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,8.4,7.6]
["NE137","Phelps","Holdrege silt loam, 7 to 11 percent slopes","Well drained","C",0.75,8.4,7.6]
["NE137","Phelps","Holdrege soils, 3 to 7 percent slopes, severely eroded","Well drained","C",0.75,7.1,7.6]
["NE137","Phelps","Holdrege-Coly complex, 7 to 11 percent slopes, eroded","Well drained","B",1,9.4,7.65]
["NE137","Phelps","Holdrege-Uly silt loams, 1 to 3 percent slopes","Well drained","C",0.75,9.4,7.2]
["NE137","Phelps","Holdrege-Uly silt loams, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.4,7.2]
["NE137","Phelps","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7.3]
["NE137","Phelps","Kenesaw and Coly silt loams, 1 to 3 percent slopes","Well drained","B",0.75,11.3,7.9]
["NE137","Phelps","Kenesaw and Coly silt loams, hummocky","Well drained","B",0.75,11.3,7.9]
["NE137","Phelps","Kenesaw and Coly silt loams, hummocky, eroded","Well drained","B",0.75,11.3,7.9]
["NE137","Phelps","Kenesaw silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14,7]
["NE137","Phelps","Kenesaw silt loam, terrace, 1 to 3 percent slopes","Well drained","B",0.75,14,7.5]
["NE137","Phelps","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.5,11.45,8.1999999999999993]
["NE137","Phelps","Leshara-Saltine silt loams, occasionally flooded","Somewhat poorly drained","C",0.25,11.3,8.1999999999999993]
["NE137","Phelps","Lex loam, rarely flooded","Somewhat poorly drained","C",0.75,41.6,7.4]
["NE137","Phelps","Massie silty clay loam, frequently ponded","Very poorly drained","D",1.25,6,6.4]
["NE137","Phelps","Meadin loamy sand, terrace, 0 to 2 percent slopes","Excessively drained","A",0.75,83,6.7]
["NE137","Phelps","Meadin silt loam, terrace, 0 to 2 percent slopes","Excessively drained","B",0.75,65.3,6.7]
["NE137","Phelps","Nuckolls and Uly silt loams, 11 to 17 percent slopes","Well drained","B",0.75,9.25,7.35]
["NE137","Phelps","O'Neill fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,68.3,7]
["NE137","Phelps","Platte soils, occasionally flooded","Somewhat poorly drained","C",0.25,67.3,8.1]
["NE137","Phelps","Platte-Alda complex, occasionally flooded","Somewhat poorly drained","B",0.5,66.3,7.5]
["NE137","Phelps","Platte-Wann complex, channeled, occasionally flooded","Somewhat poorly drained","C",0.5,64.7,8.1]
["NE137","Phelps","Rusco silt loam, 0 to 1 percent slopes","Moderately well drained","C/D",0.75,11.2,7.5]
["NE137","Phelps","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE137","Phelps","Scott silty clay loam, frequently ponded","Poorly drained","D",1.125,19.350000000000001,7.1]
["NE137","Phelps","Simeon sandy loam, 0 to 3 percent slopes","Excessively drained","A",0.5,79.25,6.75]
["NE137","Phelps","Uly and Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE137","Phelps","Uly silt loam, 3 to 11 percent slopes","Well drained","B",0.75,9.5,7.5]
["NE137","Phelps","Uly-Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.8]
["NE137","Phelps","Ustorthents, 17 to 60 percent slopes","Well drained","B",0.75,6.8,7.9]
["NE137","Phelps","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,7]
["NE137","Phelps","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,7]
["NE137","Phelps","Valentine loamy fine sand, rolling","Excessively drained","A",0.25,87.3,7]
["NE137","Phelps","Valentine loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.25,84.9,7.6]
["NE137","Phelps","Valentine-Els loamy fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.25,91.35,7]
["NE137","Phelps","Wann fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,66.2,7.6]
["NE137","Phelps","Wann loam, rarely flooded","Somewhat poorly drained","C",0.75,66.2,7.6]
["NE137","Phelps","Wann loam, saline, occasionally flooded","Somewhat poorly drained","C",0.75,64.2,8.8000000000000007]
["NE139","Pierce",null,"",""]
["NE139","Pierce","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE139","Pierce","Alcester silty clay loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE139","Pierce","Aowa silt loam, channeled, frequently flooded","Well drained","B",1.625,9.0500000000000007,7.9]
["NE139","Pierce","Bazile complex, 0 to 3 percent slopes","Well drained","C",0.75,58,6.75]
["NE139","Pierce","Bazile complex, 3 to 6 percent slopes","Well drained","C",0.75,58,6.75]
["NE139","Pierce","Bazile loam, 0 to 2 percent slopes","Well drained","C",0.75,32.6,6.75]
["NE139","Pierce","Bazile loam, 2 to 6 percent slopes","Well drained","C",0.75,36.5,6.5]
["NE139","Pierce","Bazile loam, terrace, 0 to 1 percent slopes","Well drained","C",0.75,36.5,6.5]
["NE139","Pierce","Bazile loamy fine sand, 2 to 6 percent slopes","Well drained","C",0.75,87.3,6.5]
["NE139","Pierce","Bazile silt loam, 0 to 2 percent slopes","Well drained","C",0.75,11.2,6.5]
["NE139","Pierce","Bazile silt loam, 1 to 6 percent slopes","Well drained","C",0.75,11.2,6.5]
["NE139","Pierce","Bazile soils, 0 to 1 percent slopes","Well drained","C",0.75,87.3,6.5]
["NE139","Pierce","Bazile soils, 1 to 6 percent slopes","Well drained","C",0.75,87.3,6.5]
["NE139","Pierce","Bazile soils, terrace, 0 to 1 percent slopes","Well drained","C",0.75,87.3,6.5]
["NE139","Pierce","Betts clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,35.4,7.9]
["NE139","Pierce","Betts loam, 3 to 11 percent slopes, eroded","Well drained","C",0.5,37.200000000000003,7.9]
["NE139","Pierce","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.125,65.75,7]
["NE139","Pierce","Boelus loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.5,55.2,6.65]
["NE139","Pierce","Boelus loamy fine sand, 2 to 6 percent slopes","Well drained","B",0.25,24,7]
["NE139","Pierce","Boelus loamy sand, 3 to 6 percent slopes","Well drained","B",0.5,53.9,7]
["NE139","Pierce","Boelus loamy sand, 6 to 11 percent slopes","Well drained","B",0.5,53.9,7]
["NE139","Pierce","Boelus-Loretto complex, 0 to 2 percent slopes","Well drained","B",0.75,39.1,7]
["NE139","Pierce","Boelus-Loretto complex, 2 to 6 percent slopes","Well drained","B",0.75,39.1,7]
["NE139","Pierce","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",2.25,23.450000000000003,6.25]
["NE139","Pierce","Butler silty clay loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.125,21.05,7.1]
["NE139","Pierce","Cass fine sandy loam, occasionally flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE139","Pierce","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE139","Pierce","Cass loam, rarely flooded","Well drained","B",0.75,63.5,7.3]
["NE139","Pierce","Clamo silty clay, occasionally flooded","Somewhat poorly drained","C/D",3,7,7.3000000000000007]
["NE139","Pierce","Clamo-Saltine complex, occasionally flooded","Somewhat poorly drained","C/D",1.125,6.85,8.1999999999999993]
["NE139","Pierce","Clarno loam, 2 to 6 percent slopes","Well drained","B",2,38.5,7]
["NE139","Pierce","Clarno loam, 6 to 11 percent slopes","Well drained","B",2,38.5,7]
["NE139","Pierce","Coleridge silt loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE139","Pierce","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE139","Pierce","Colo fine sandy loam, overblown, occasionally flooded","Somewhat poorly drained","B/D",1.375,37.199999999999996,7.4]
["NE139","Pierce","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE139","Pierce","Crofton silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE139","Pierce","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE139","Pierce","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE139","Pierce","Crofton silt loam, coarse, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE139","Pierce","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE139","Pierce","Crofton-Nora complex, 2 to 6 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE139","Pierce","Crofton-Nora complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE139","Pierce","Crofton-Nora silt loams, 1 to 6 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE139","Pierce","Crofton-Nora silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE139","Pierce","Crofton-Nora silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE139","Pierce","Elsmere fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.25,79.400000000000006,6.5]
["NE139","Pierce","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A/D",0.25,86.8,6.5]
["NE139","Pierce","Fillmore complex, frequently ponded","Somewhat poorly drained","D",1.125,12.649999999999999,7.1]
["NE139","Pierce","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1.125,11.100000000000001,7.1]
["NE139","Pierce","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE139","Pierce","Hadar loamy fine sand, 2 to 6 percent slopes","Well drained","C",0.75,85.3,6.1]
["NE139","Pierce","Hadar-Thurman complex, 6 to 11 percent slopes","Well drained","C",0.5,85.1,6.5]
["NE139","Pierce","Hadar-Thurman complex, 6 to 17 percent slopes","Well drained","C",0.5,82.1,6.5]
["NE139","Pierce","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE139","Pierce","Hobbs silt loam, frequently flooded","Well drained","B",1.875,11.3,7]
["NE139","Pierce","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,9.25,7.25]
["NE139","Pierce","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE139","Pierce","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE139","Pierce","Hord silt loam, rarely flooded","Well drained","B",0.75,9.3000000000000007,7]
["NE139","Pierce","Hord-Hobbs silt loams, 0 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE139","Pierce","Inavale loamy fine sand, frequently flooded","Excessively drained","A",0.5,89.75,6.7]
["NE139","Pierce","Judson silt loam, 2 to 6 percent slopes","Well drained","C",2.5,7,6.5]
["NE139","Pierce","Kezan silt loam, occasionally flooded","Poorly drained","C",1.875,7.85,7.35]
["NE139","Pierce","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE139","Pierce","Lawet loam, occasionally flooded","Poorly drained","B/D",1.25,54.4,7.9]
["NE139","Pierce","Lawet silt loam, occasionally flooded","Poorly drained","C/D",2.875,40.35,8.0500000000000007]
["NE139","Pierce","Lawet soils, wet, occasionally flooded","Very poorly drained","C/D",2.875,40.35,8.0500000000000007]
["NE139","Pierce","Lawet-Saltine complex, occasionally flooded","Poorly drained","B/D",0.25,11.3,8.5]
["NE139","Pierce","Leisy fine sandy loam, 6 to 11 percent slopes","Well drained","C",0.75,39.200000000000003,6.5]
["NE139","Pierce","Leisy loam, 0 to 6 percent slopes","Well drained","B",0.75,39.200000000000003,6.5]
["NE139","Pierce","Leshara silt loam, occasionally flooded","Somewhat poorly drained","B/D",0.75,11.6,7.5]
["NE139","Pierce","Longford loam, 1 to 7 percent slopes","Well drained","B",2,24,6.5]
["NE139","Pierce","Longford silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,19,6.5]
["NE139","Pierce","Longford soils, 3 to 7 percent slopes, eroded","Well drained","C",2,20,6.5]
["NE139","Pierce","Loretto fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE139","Pierce","Loretto fine sandy loam, terrace, 0 to 2 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE139","Pierce","Loretto loam, 0 to 2 percent slopes","Well drained","B",1.5,39.1,6.5]
["NE139","Pierce","Loretto loam, 2 to 6 percent slopes","Well drained","B",1.5,39.1,6.5]
["NE139","Pierce","Loretto sandy loam, 0 to 3 percent slopes","Well drained","B",1.5,39.1,6.5]
["NE139","Pierce","Loup fine sandy loam, rarely flooded","Poorly drained","A/D",3.125,64.8,6.6]
["NE139","Pierce","Loup soils, rarely flooded","Very poorly drained","B/D",3.125,55.75,6.6]
["NE139","Pierce","Marlake loam, frequently ponded","Very poorly drained","A/D",3.125,69.900000000000006,7]
["NE139","Pierce","Moody loam, 2 to 6 percent slopes","Well drained","C",3,9.4,6.5]
["NE139","Pierce","Moody silty clay loam, 0 to 1 percent slopes","Well drained","C",3,6.9,6.5]
["NE139","Pierce","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE139","Pierce","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE139","Pierce","Moody silty clay loam, 6 to 11 percent slopes","Well drained","C",3,7,6.5]
["NE139","Pierce","Muir silt loam, calcareous, rarely flooded","Well drained","B",2.5,9.25,6.6]
["NE139","Pierce","Muir silt loam, rarely flooded","Well drained","B",2.5,9.25,6.6]
["NE139","Pierce","Muir silty clay loam, rarely flooded","Well drained","B",2,9,6.7]
["NE139","Pierce","Nora silt loam, 1 to 6 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE139","Pierce","Nora silt loam, 11 to 17 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE139","Pierce","Nora silt loam, 2 to 6 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE139","Pierce","Nora silt loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,9.1,6.5]
["NE139","Pierce","Nora silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE139","Pierce","Nora silty clay loam, 11 to 17 percent slopes","Well drained","C",0.75,8.9,7]
["NE139","Pierce","Nora silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,8.9,7]
["NE139","Pierce","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE139","Pierce","Nora-Crofton complex, 2 to 6 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE139","Pierce","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE139","Pierce","Nora-Thurman complex, 11 to 17 percent slopes","Well drained","B",0.625,38.150000000000006,6.6]
["NE139","Pierce","Nora-Thurman complex, 6 to 11 percent slopes","Well drained","B",0.625,38.150000000000006,6.6]
["NE139","Pierce","Obert silt loam, frequently ponded","Very poorly drained","B/D",1.875,9.3000000000000007,7.9]
["NE139","Pierce","Ord fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE139","Pierce","Ord loam, occasionally flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE139","Pierce","Ortello fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE139","Pierce","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE139","Pierce","Ortello fine sandy loam, terrace, 0 to 2 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE139","Pierce","Ortello loam, terrace, 0 to 1 percent slopes","Well drained","B",0.75,63.5,6.7]
["NE139","Pierce","Orwet loam, rarely flooded","Poorly drained","B/D",1.875,68.199999999999989,7.45]
["NE139","Pierce","Ovina fine sandy loam, rarely flooded","Somewhat poorly drained","B",1.5,66.900000000000006,7.5]
["NE139","Pierce","Ovina loam, rarely flooded","Somewhat poorly drained","C",1.5,63.5,7.5]
["NE139","Pierce","Ovina loamy fine sand, rarely flooded","Somewhat poorly drained","B",1.125,75.2,7.7]
["NE139","Pierce","Ovina-Lute complex, rarely flooded","Somewhat poorly drained","D",1.125,63.65,7.7]
["NE139","Pierce","Paka complex, 2 to 6 percent slopes","Well drained","C",0.75,27.1,6.5]
["NE139","Pierce","Paka sandy clay loam, 2 to 11 percent slopes","Well drained","C",1.125,8.25,7.1]
["NE139","Pierce","Paka sandy loam, 2 to 11 percent slopes","Well drained","B",1.125,8.25,7.1]
["NE139","Pierce","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE139","Pierce","Simeon sandy loam, 3 to 11 percent slopes","Excessively drained","A",0.5,80.199999999999989,7]
["NE139","Pierce","Thurman fine sandy loam, 2 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE139","Pierce","Thurman fine sandy loam, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE139","Pierce","Thurman loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE139","Pierce","Thurman loamy fine sand, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE139","Pierce","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE139","Pierce","Thurman loamy fine sand, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE139","Pierce","Thurman loamy fine sand, terrace, 0 to 3 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE139","Pierce","Thurman loamy fine sand, thick, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE139","Pierce","Thurman-Valentine complex, undulating","Somewhat excessively drained","A",0.25,94,6.5]
["NE139","Pierce","Trent silt loam, 0 to 2 percent slopes","Well drained","B",2.5,8.8000000000000007,6.7]
["NE139","Pierce","Trent silty clay loam","Moderately well drained","B",2.5,6.9,6.7]
["NE139","Pierce","Valentine fine sand, 0 to 6 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE139","Pierce","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE139","Pierce","Valentine fine sand, 9 to 24 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE139","Pierce","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE141","Platte",null,"",""]
["NE141","Platte","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE141","Platte","Alcester silty clay loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE141","Platte","Alda loam, occasionally flooded","Somewhat poorly drained","C",0.75,66,7.5]
["NE141","Platte","Barney loam, frequently flooded","Poorly drained","B/D",0.25,80,7.5]
["NE141","Platte","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE141","Platte","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1,65.75,7]
["NE141","Platte","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.599999999999994,7.5]
["NE141","Platte","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE141","Platte","Boel-Inavale complex, channeled, frequently flooded","Somewhat poorly drained","C",0.25,92.2,7.5]
["NE141","Platte","Boelus loamy fine sand, 2 to 6 percent slopes","Well drained","B",0.25,24,7]
["NE141","Platte","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.125,22.35,7.1]
["NE141","Platte","Coleridge silt loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE141","Platte","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE141","Platte","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE141","Platte","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE141","Platte","Crofton-Nora complex, 2 to 6 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE141","Platte","Els loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,91.1,6.75]
["NE141","Platte","Fillmore silt loam, frequently ponded","Very poorly drained","D",1.625,15.75,6.1]
["NE141","Platte","Fillmore silt loam, occasionally ponded","Somewhat poorly drained","D",1.125,12.649999999999999,7.1]
["NE141","Platte","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",5,89.7,7.5]
["NE141","Platte","Fluvaquents, silty, frequently flooded","Very poorly drained","B/D",2.5,11.75,3.75]
["NE141","Platte","Geary silty clay loam, 11 to 17 percent slopes, eroded","Well drained","B",2,7.4,6.1]
["NE141","Platte","Geary silty clay loam, 11 to 30 percent slopes","Well drained","B",2,7.4,6.1]
["NE141","Platte","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","B",2,7.4,6.1]
["NE141","Platte","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE141","Platte","Gibbon-Gayville silty clay loams, occasioanlly flooded","Somewhat poorly drained","C",0.75,22.25,8.0500000000000007]
["NE141","Platte","Gothenburg fine sandy loam, frequently flooded","Poorly drained","A/D",0.5,85.550000000000011,7.35]
["NE141","Platte","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.5,79.849999999999994,7.35]
["NE141","Platte","Grigston silt loam, rarely flooded","Well drained","B",1.5,9.1,7.9]
["NE141","Platte","Grigston silt loam, wet substratum, rarely flooded","Well drained","B",1.5,9.1,7.9]
["NE141","Platte","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE141","Platte","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,11.3,7]
["NE141","Platte","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE141","Platte","Inavale fine sandy loam, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE141","Platte","Inavale loamy fine sand, 3 to 11 percent slopes, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE141","Platte","Inavale loamy fine sand, rarely flooded","Excessively drained","A",0.25,92.2,6.7]
["NE141","Platte","Inavale loamy sand, 3 to 6 percent slopes, rarely flooded","Excessively drained","A",0.25,84.9,6.7]
["NE141","Platte","Inavale-Boel complex, 0 to 6 percent slopes, occasionally flooded","Somewhat poorly drained","C",0.25,92.2,7.5]
["NE141","Platte","Ipage-Els loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,92.75,6.6]
["NE141","Platte","Janude fine sandy loam, 0 to 1 percent slopes","Moderately well drained","B",1.25,63.5,7.5]
["NE141","Platte","Janude loam, rarely flooded","Moderately well drained","B",1.25,45,7.5]
["NE141","Platte","Kezan silt loam, frequently flooded","Poorly drained","C",1.875,9.0500000000000007,7.35]
["NE141","Platte","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE141","Platte","Lawet silt loam, occasionally flooded","Somewhat poorly drained","B/D",1.25,54.4,7.9]
["NE141","Platte","Loup loam, frequently ponded","Very poorly drained","A/D",3.375,79.2,6.6]
["NE141","Platte","Merrick loam, rarely flooded","Moderately well drained","B",2.125,39.700000000000003,6.7]
["NE141","Platte","Moody silty clay loam, 0 to 1 percent slopes","Well drained","C",3,6.9,6.5]
["NE141","Platte","Moody silty clay loam, 1 to 3 percent slopes","Well drained","C",3,6.9,6.5]
["NE141","Platte","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE141","Platte","Moody silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE141","Platte","Moody silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",3,6.9,6.5]
["NE141","Platte","Moody silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE141","Platte","Moody-Thurman complex, 2 to 6 percent slopes, eroded","Well drained","C",1,47.15,6.5]
["NE141","Platte","Moody-Thurman complex, 6 to 11 percent slopes, eroded","Well drained","C",1,38.150000000000006,6.5]
["NE141","Platte","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE141","Platte","Muir silt loam, sandy substratum, 0 to 1 percent slopes","Well drained","B",2,9.5,7]
["NE141","Platte","Muir silty clay loam, rarely flooded","Well drained","B",2,9,6.7]
["NE141","Platte","Nora silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE141","Platte","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE141","Platte","Nora-Crofton complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE141","Platte","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE141","Platte","Novina fine sandy loam, rarely flooded","Moderately well drained","B",0.75,63.5,6.7]
["NE141","Platte","Obert silty clay loam, frequently ponded","Very poorly drained","C/D",1.5,7.3,7.9]
["NE141","Platte","O'Neill fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,67.599999999999994,6.5]
["NE141","Platte","Platte loam, occasionally flooded","Somewhat poorly drained","C",1.125,68.099999999999994,7.5]
["NE141","Platte","Platte-Inavale complex, channeled, frequently flooded","Excessively drained","A",0.25,89.6,7.5]
["NE141","Platte","Shell silt loam, clayey substratum, occasionally flooded","Moderately well drained","C",0.75,11.2,7]
["NE141","Platte","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE141","Platte","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,87.3,7]
["NE141","Platte","Thurman loamy fine sand, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE141","Platte","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE141","Platte","Thurman loamy fine sand, loamy substratum, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,86.8,7]
["NE141","Platte","Ustorthents, level","Excessively drained","A",0.25,96.3,5.6]
["NE141","Platte","Ustorthents, steep","Well drained","B",0.75,30.1,7.9]
["NE141","Platte","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE141","Platte","Valentine fine sand, rolling","Excessively drained","A",0.25,96.3,6.5]
["NE141","Platte","Valentine-Thurman complex, 3 to 9 percent slopes","Somewhat excessively drained","A",0.25,91.1,6.5]
["NE141","Platte","Wann loam, occasionally flooded","Somewhat poorly drained","C",0.75,66.2,8.1999999999999993]
["NE141","Platte","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.75,6.6]
["NE141","Platte","Zook silty clay, occasionally flooded","Poorly drained","C/D",4.5,7.85,6.6]
["NE143","Polk",null,"",""]
["NE143","Polk","Alda fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.5,73.2,7.5]
["NE143","Polk","Alda loam, occasionally flooded","Somewhat poorly drained","C",0.5,73.2,7.5]
["NE143","Polk","Alda sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,67.8,7.5]
["NE143","Polk","Barney loam, frequently flooded","Very poorly drained","B/D",0.25,47.9,7.5]
["NE143","Polk","Barney-Alda complex, frequently flooded","Somewhat poorly drained","B",0.25,66,7.5]
["NE143","Polk","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,67.599999999999994,6.7]
["NE143","Polk","Blendon fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,67.599999999999994,6.7]
["NE143","Polk","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE143","Polk","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE143","Polk","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE143","Polk","Coly silt loam, 11 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE143","Polk","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE143","Polk","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE143","Polk","Coly soils, 3 to 6 percent slopes, severely eroded","Well drained","B",1.125,11.3,7.9]
["NE143","Polk","Coly soils, 6 to 11 percent slopes, severely eroded","Well drained","B",1.125,11.3,7.9]
["NE143","Polk","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE143","Polk","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE143","Polk","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7]
["NE143","Polk","Cozad-variant complex","Well drained","B",0.75,11.600000000000001,8.0500000000000007]
["NE143","Polk","Darr fine sandy loam, rarely flooded","Somewhat excessively drained","A",0.5,77.349999999999994,7.5]
["NE143","Polk","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE143","Polk","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.4,7.9]
["NE143","Polk","Gothenburg fine sandy loam, frequently flooded","Poorly drained","A/D",0.5,85.550000000000011,7.35]
["NE143","Polk","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,95,7.2]
["NE143","Polk","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.5,83.6,7.35]
["NE143","Polk","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE143","Polk","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE143","Polk","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE143","Polk","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",0.375,23.25,6.75]
["NE143","Polk","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE143","Polk","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE143","Polk","Hastings soils, 3 to 7 percent slopes, severely eroded","Well drained","C",0.75,15.4,6.5]
["NE143","Polk","Hastings soils, 7 to 11 percent slopes, severely eroded","Well drained","C",0.75,15.4,6.5]
["NE143","Polk","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,9.25,7.25]
["NE143","Polk","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE143","Polk","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,10.4,7.25]
["NE143","Polk","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE143","Polk","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE143","Polk","Hord silt loam, rarely flooded","Well drained","B",0.75,9.3000000000000007,7]
["NE143","Polk","Inavale loamy fine sand, rarely flooded","Excessively drained","A",0.25,86.8,6.7]
["NE143","Polk","Inavale loamy sand, 3 to 11 percent slopes","Excessively drained","A",0.25,86.8,6.7]
["NE143","Polk","Inavale loamy sand, 3 to 6 percent slopes, rarely flooded","Excessively drained","A",0.25,84.9,6.7]
["NE143","Polk","Inavale loamy sand, rarely flooded","Somewhat excessively drained","A",0.25,84.9,6.7]
["NE143","Polk","Inavale-Boel complex, 0 to 6 percent slopes, occasionally flooded","Somewhat poorly drained","B",0.25,92.2,7.5]
["NE143","Polk","Inavale-Platte complex, rarely flooded","Excessively drained","A",0.25,84.3,7.5]
["NE143","Polk","Janude sandy loam, very rarely flooded","Moderately well drained","B",1.25,66.599999999999994,7.5]
["NE143","Polk","Lamo silty clay loam, sandy substratum","Somewhat poorly drained","C",0.5,42.1,7.9]
["NE143","Polk","Leshara silt loam, drained, rarely flooded","Well drained","B",0.75,11.6,7.5]
["NE143","Polk","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,11.6,7.5]
["NE143","Polk","Meadin loamy sand, 0 to 6 percent slopes","Excessively drained","A",0.75,84.3,6.2]
["NE143","Polk","Muir silt loam, 0 to 1 percent slopes","Well drained","B",2,9,6.7]
["NE143","Polk","Muir silt loam, 1 to 3 percent slopes","Well drained","B",2,9,6.7]
["NE143","Polk","Muir silt loam, 3 to 7 percent slopes","Well drained","B",2,9,6.7]
["NE143","Polk","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE143","Polk","O'Neill fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,83.7,6.5]
["NE143","Polk","Ortello complex, 6 to 11 percent slopes","Well drained","A",1.125,63.5,6.6]
["NE143","Polk","Ortello complex, 6 to 11 percent slopes, eroded","Well drained","A",1.125,63.5,6.6]
["NE143","Polk","Ortello-Coly complex, 11 to 30 percent slopes","Well drained","B",1.125,37.400000000000006,7.3000000000000007]
["NE143","Polk","Platte fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.25,73.900000000000006,7.5]
["NE143","Polk","Platte loam, occasionally flooded","Somewhat poorly drained","C",0.25,63.2,7.5]
["NE143","Polk","Platte-Alda complex, occasionally flooded","Somewhat poorly drained","B",0.25,73.2,7.5]
["NE143","Polk","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,86.35,7]
["NE143","Polk","Thurman fine sandy loam, 2 to 11 percent slopes","Somewhat excessively drained","A",0.875,75.900000000000006,6.5]
["NE143","Polk","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE143","Polk","Thurman loamy sand, 0 to 6 percent slopes","Somewhat excessively drained","A",0.25,82.5,6.5]
["NE143","Polk","Thurman loamy sand, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,82.5,6.5]
["NE143","Polk","Uly silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.5,7]
["NE143","Polk","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE143","Polk","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE143","Polk","Wann fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,66.2,8.1999999999999993]
["NE145","Red Willow",null,"",""]
["NE145","Red Willow","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",1.125,66.099999999999994,6.85]
["NE145","Red Willow","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.125,66.099999999999994,6.85]
["NE145","Red Willow","Barney loam, occasionally flooded","Poorly drained","B/D",0.25,91.6,7.5]
["NE145","Red Willow","Barney silty clay loam, frequently flooded","Very poorly drained","C/D",0.25,96.8,7.2]
["NE145","Red Willow","Barney soils, frequently flooded","Very poorly drained","B/D",1.625,67,7.35]
["NE145","Red Willow","Bridget silt loam, 0 to 1 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE145","Red Willow","Bridget silt loam, 3 to 6 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE145","Red Willow","Canyon-Rock outcrop complex, 12 to 60 percent slopes","Well drained","D",0.625,22.15,3.95]
["NE145","Red Willow","Canyon-Sarben complex, 30 to 60 percent slopes","Well drained","D",0.75,62,7.2]
["NE145","Red Willow","Coly and Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE145","Red Willow","Coly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE145","Red Willow","Coly silt loam, 11 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE145","Red Willow","Coly silt loam, 3 to 11 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE145","Red Willow","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE145","Red Willow","Coly-Nuckolls silt loams, 11 to 30 percent slopes","Well drained","B",0.75,9.4,7.6]
["NE145","Red Willow","Coly-Uly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.9]
["NE145","Red Willow","Coly-Uly silt loams, 3 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE145","Red Willow","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE145","Red Willow","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,59.6,7]
["NE145","Red Willow","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,59.6,7]
["NE145","Red Willow","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,59.6,7]
["NE145","Red Willow","Duroc silt loam, terrace, 0 to 1 percent slopes","Well drained","B",2,9.5,7.2]
["NE145","Red Willow","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE145","Red Willow","Haigler and Sanborn loams, rarely flooded","Moderately well drained","B",0.75,64.25,8.1999999999999993]
["NE145","Red Willow","Haigler fine sandy loam, 0 to 1 percent slopes","Moderately well drained","A",0.25,80.3,8.5]
["NE145","Red Willow","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE145","Red Willow","Hobbs-McCook silt loams, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE145","Red Willow","Holdrege and Keith silt loams, 0 to 1 percent slopes","Well drained","C",0.5,10.600000000000001,7.1]
["NE145","Red Willow","Holdrege and Keith silt loams, 1 to 3 percent slopes","Well drained","C",0.5,11.5,7.1]
["NE145","Red Willow","Holdrege and Keith silt loams, 1 to 3 percent slopes, eroded","Well drained","C",0.5,11.5,7.1]
["NE145","Red Willow","Holdrege and Keith silt loams, 3 to 7 percent slopes","Well drained","C",0.5,10.600000000000001,7.1]
["NE145","Red Willow","Holdrege and Keith silt loams, 3 to 7 percent slopes, eroded","Well drained","C",0.5,11.5,7.1]
["NE145","Red Willow","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE145","Red Willow","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE145","Red Willow","Holdrege silt loam, 1 to 3 percent slopes, eroded","Well drained","C",0.75,9.25,7.2]
["NE145","Red Willow","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE145","Red Willow","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.25,7.2]
["NE145","Red Willow","Holdrege-Coly silt loams, 1 to 3 percent slopes, eroded","Well drained","B",1.375,9.4,7.75]
["NE145","Red Willow","Holdrege-Coly silt loams, 3 to 7 percent slopes, eroded","Well drained","B",1.375,9.4,7.75]
["NE145","Red Willow","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE145","Red Willow","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE145","Red Willow","Hord-Saltine complex","Well drained","B",0.5,9.1000000000000014,8.1999999999999993]
["NE145","Red Willow","Inavale fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,92.2,6.7]
["NE145","Red Willow","Inavale loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,92.2,6.7]
["NE145","Red Willow","Inavale soils, frequently flooded","Excessively drained","A",0.25,92.2,6.7]
["NE145","Red Willow","Inavale soils, occasionally flooded","Excessively drained","A",0.25,92.2,7.9]
["NE145","Red Willow","Keith and Blackwood silt loams, 0 to 1 percent slopes","Well drained","B",1,12.6,7.3]
["NE145","Red Willow","Keith silt loam, 1 to 3 percent slopes","Well drained","B",0.75,13.7,7]
["NE145","Red Willow","Keith silt loam, 1 to 3 percent slopes, eroded","Well drained","B",0.75,13.7,7]
["NE145","Red Willow","Keith silt loam, 3 to 6 percent slopes","Well drained","B",0.75,13.7,7]
["NE145","Red Willow","Keith silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,13.7,7]
["NE145","Red Willow","Las Animas loam, occasionally flooded","Somewhat poorly drained","C",0.25,63.5,7.9]
["NE145","Red Willow","Las Animas sand, occasionally flooded","Somewhat poorly drained","B",1,86.4,7.9]
["NE145","Red Willow","Las-Wann variant complex, occasionally flooded","Somewhat poorly drained","C",0.75,45.3,8.8000000000000007]
["NE145","Red Willow","McCook and Bigbend loams","Well drained","B",1.375,48.8,7.7]
["NE145","Red Willow","McCook loam, occasionally flooded","Well drained","B",1.75,50.3,7.9]
["NE145","Red Willow","McCook loam, rarely flooded","Well drained","B",1.875,40.35,7.7]
["NE145","Red Willow","McCook silt loam, occasionally flooded","Well drained","B",1.75,12.75,7.5500000000000007]
["NE145","Red Willow","McCook silt loam, rarely flooded","Well drained","B",1.875,12.95,7.5500000000000007]
["NE145","Red Willow","Munjor fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.5,56.1,7.9]
["NE145","Red Willow","Munjor fine sandy loam, rarely flooded","Well drained","A",0.5,67.2,7.9]
["NE145","Red Willow","Munjor loam, 0 to 1 percent slopes","Well drained","B",0.5,44.35,7.9]
["NE145","Red Willow","Sulco complex, 9 to 60 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE145","Red Willow","Sulco silt loam, 9 to 30 percent slopes","Well drained","B",1,17.600000000000001,8.0500000000000007]
["NE145","Red Willow","Sulco-Ulysses silt loams, 9 to 30 percent slopes, eroded","Well drained","B",1.25,13.6,7.9]
["NE145","Red Willow","Uly and Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.6]
["NE145","Red Willow","Uly silt loam, 3 to 11 percent slopes","Well drained","B",0.75,9.5,7]
["NE145","Red Willow","Uly silt loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE145","Red Willow","Uly silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.5,7]
["NE145","Red Willow","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE145","Red Willow","Ulysses and Sulco silt loams, 6 to 9 percent slopes, eroded","Well drained","B",1.25,14.3,7.9]
["NE145","Red Willow","Ulysses silt loam, 6 to 9 percent slopes, eroded","Well drained","B",1.5,14.3,7.9]
["NE145","Red Willow","Wann fine sandy loam, occasionally flooded","Somewhat poorly drained","B",1.375,64.849999999999994,7.85]
["NE145","Red Willow","Wann loam, occasionally flooded","Somewhat poorly drained","C",1.375,54.6,7.85]
["NE147","Richardson",null,"",""]
["NE147","Richardson","Aksarben silty clay loam, 0 to 2 percent slopes","Well drained","C",1.125,19.100000000000001,5.9499999999999993]
["NE147","Richardson","Aksarben silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.125,19.100000000000001,5.9499999999999993]
["NE147","Richardson","Aksarben silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.125,19.100000000000001,5.9499999999999993]
["NE147","Richardson","Albaton silty clay, occasionally flooded","Poorly drained","D",1.5,4.1500000000000004,7.9]
["NE147","Richardson","Benfield silty clay loam, 3 to 11 percent slopes, eroded","Well drained","D",1.5,7.7,7]
["NE147","Richardson","Benfield-Kipson silty clay loams, 3 to 9 percent slopes, severely eroded","Well drained","D",1.5,7.7,7]
["NE147","Richardson","Deroin silty clay loam, 6 to 11 percent slopes, severely eroded","Well drained","C",0.5,6.9,7]
["NE147","Richardson","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.7]
["NE147","Richardson","Haynie and Albaton soils, occasionally flooded","Poorly drained","D",1.25,8.35,7.9]
["NE147","Richardson","Haynie and Sarpy soils, occasionally flooded","Moderately well drained","B",0.75,46.850000000000009,7.5]
["NE147","Richardson","Haynie silt loam, occasionally flooded","Moderately well drained","B",1.25,12.600000000000001,7.7]
["NE147","Richardson","Ida silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.875,11.2,7.7]
["NE147","Richardson","Ida silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.875,11.2,7.7]
["NE147","Richardson","Ida soils, 30 to 60 percent slopes","Well drained","B",0.5,9.5,7.7]
["NE147","Richardson","Judson silt loam, 2 to 6 percent slopes","Well drained","C",2.5,7.1,6.5]
["NE147","Richardson","Kennebec silt loam, occasionally flooded","Moderately well drained","C",2,5,6.35]
["NE147","Richardson","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,8.3000000000000007,6.6]
["NE147","Richardson","Kezan silt loam, frequently flooded","Poorly drained","C/D",1.875,9.0500000000000007,7.2]
["NE147","Richardson","Kipson-Benfield silty clay loams, 7 to 17 percent slopes","Well drained","D",1.5,7.7,7.5]
["NE147","Richardson","Kipson-Sogn complex, 3 to 30 percent slopes","Somewhat excessively drained","C",0.75,20,7.9]
["NE147","Richardson","Malmo clay loam, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE147","Richardson","Malmo clay, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE147","Richardson","Malmo soils, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE147","Richardson","Marshall silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,6.9,6.5]
["NE147","Richardson","Marshall silty clay loam, 2 to 6 percent slopes","Well drained","C",0.75,6.9,6.5]
["NE147","Richardson","Marshall silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,6.9,6.5]
["NE147","Richardson","Monona silt loam, 1 to 6 percent slopes","Well drained","B",1,9.4,6.7]
["NE147","Richardson","Monona silt loam, 11 to 17 percent slopes","Well drained","B",1,9.4,6.7]
["NE147","Richardson","Monona silt loam, 17 to 30 percent slopes","Well drained","B",1,9.4,6.7]
["NE147","Richardson","Monona silt loam, 6 to 11 percent slopes","Well drained","B",1,9.4,6.7]
["NE147","Richardson","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,35.4,6.1]
["NE147","Richardson","Morrill loam, 6 to 11 percent slopes","Well drained","C",0.6,41.6,6.1]
["NE147","Richardson","Morrill soils, 11 to 17 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE147","Richardson","Morrill soils, 6 to 11 percent slopes, eroded","Well drained","C",0.6,35.200000000000003,6.1]
["NE147","Richardson","Morrill soils, 6 to 11 percent slopes, severely eroded","Well drained","C",0.75,35.4,6.1]
["NE147","Richardson","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.4,6.7]
["NE147","Richardson","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,8.5,6.7]
["NE147","Richardson","Nodaway-Colo silt loams, occasionally flooded","Poorly drained","C/D",2.5,6.9,6.3]
["NE147","Richardson","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.9]
["NE147","Richardson","Otoe silty clay loam, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE147","Richardson","Otoe silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE147","Richardson","Pawnee and Malmo clay loams, 3 to 11 percent slopes, eroded","Moderately well drained","D",0.75,29.9,7]
["NE147","Richardson","Pawnee and Mayberry clay loams, 3 to 11 percent slopes, eroded","Moderately well drained","D",1.375,33.700000000000003,6.75]
["NE147","Richardson","Pawnee and Mayberry clay loams, 6 to 11 percent slopes, eroded","Moderately well drained","D",1.375,33.700000000000003,6.75]
["NE147","Richardson","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE147","Richardson","Pohocco silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.25,9.4,7.2]
["NE147","Richardson","Pohocco silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.25,9.4,6.7]
["NE147","Richardson","Pohocco silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.25,9.4,7.2]
["NE147","Richardson","Pohocco silty clay loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,8.9,7.2]
["NE147","Richardson","Pohocco, eroded-Ida silt loams, 11 to 17 percent slopes","Well drained","B",0.25,9.4,7.5]
["NE147","Richardson","Pohocco, eroded-Ida silt loams, 17 to 30 percent slopes","Well drained","B",0.25,9.4,7.5]
["NE147","Richardson","Sarpy loamy fine sand, occasionally flooded","Excessively drained","A",0.75,79.900000000000006,7.5]
["NE147","Richardson","Shelby clay loam, 17 to 30 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE147","Richardson","Slickspots-Wabash complex","Poorly drained","D",1.5,7.2,7]
["NE147","Richardson","Wabash silty clay loam, occasionally flooded","Poorly drained","D",2.25,12.649999999999999,6.35]
["NE147","Richardson","Wabash silty clay, occasionally flooded","Poorly drained","D",2.25,6.5,6.35]
["NE147","Richardson","Wymore silty clay loam, 0 to 1 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE147","Richardson","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",0.75,17.3,6.5]
["NE147","Richardson","Wymore silty clay loam, 1 to 3 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE147","Richardson","Wymore silty clay loam, 3 to 11 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE147","Richardson","Wymore silty clay loam, 3 to 11 percent slopes, eroded","Moderately well drained","D",1.5,17.3,6.5]
["NE147","Richardson","Yutan silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.625,7.6,6.6]
["NE147","Richardson","Yutan silty clay loam, 3 to 11 percent slopes, eroded","Well drained","C",0.625,7.6,6.6]
["NE147","Richardson","Yutan silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.625,7.6,6.6]
["NE147","Richardson","Zook silty clay loam, occasionally flooded","Poorly drained","D",3,16.25,6.4]
["NE149","Rock",null,"",""]
["NE149","Rock","Almeria fine sandy loam, channeled, frequently flooded","Very poorly drained","A/D",3.375,78.2,6.9]
["NE149","Rock","Almeria loamy fine sand, occasionally flooded","Poorly drained","A/D",1.25,89.4,6.9]
["NE149","Rock","Barney-Boel complex, channeled","Very poorly drained","A/D",0.25,91,7.5]
["NE149","Rock","Blackloup loam, occasionally flooded","Very poorly drained","B/D",0.5,72.55,7.4]
["NE149","Rock","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE149","Rock","Boelus loamy sand, 0 to 3 percent slopes","Well drained","B",0.5,69.900000000000006,7]
["NE149","Rock","Brunswick-Longpine fine sandy loams, 11 to 40 percent slopes","Well drained","B",0.25,64.599999999999994,6.5]
["NE149","Rock","Brunswick-Longpine loamy sands, 3 to 11 percent slopes","Well drained","B",0.25,66.900000000000006,6.5]
["NE149","Rock","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE149","Rock","Els loamy sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.7]
["NE149","Rock","Els-Ipage complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE149","Rock","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,95.15,6.35]
["NE149","Rock","Els-Ipage-Tryon loamy sands, 0 to 6 percent slopes","Somewhat poorly drained","A",0.75,84.3,6.7]
["NE149","Rock","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,96,6.5]
["NE149","Rock","Elsmere-Selia loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,84.45,7.4]
["NE149","Rock","Inavale-Barney complex, channeled, occasionally flooded","Very poorly drained","A/D",0.25,91,7.2]
["NE149","Rock","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE149","Rock","Ipage fine sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,96.8,6.5]
["NE149","Rock","Ipage loamy fine sand, terrace, 0 to 3 percent slopes","Moderately well drained","A",0.25,89.3,6.5]
["NE149","Rock","Ipage loamy sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,89.6,6.2]
["NE149","Rock","Jansen loamy sand, 0 to 2 percent slopes","Well drained","C",1.25,79.2,6.2]
["NE149","Rock","Labu-Sansarc silty clays, 11 to 40 percent slopes","Well drained","D",0.65,2.6,7.7]
["NE149","Rock","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,86.4,6.5]
["NE149","Rock","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",3.375,79.2,6.6]
["NE149","Rock","Loup fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,66.099999999999994,6.5]
["NE149","Rock","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,72.150000000000006,7.15]
["NE149","Rock","Marlake loamy fine sand, frequently ponded","Very poorly drained","A/D",0.75,86.8,7]
["NE149","Rock","McKelvie-Longpine-Ronson complex, 17 to 70 percent slopes","Well drained","D",0.75,64.599999999999994,7.5]
["NE149","Rock","Meadin sandy loam, 0 to 2 percent slopes","Excessively drained","A",0.75,90.1,6.2]
["NE149","Rock","O'Neill fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,67.3,6.5]
["NE149","Rock","O'Neill sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,68.5,6.5]
["NE149","Rock","O'Neill sandy loam, 2 to 6 percent slopes","Well drained","A",0.75,68.5,6.5]
["NE149","Rock","O'Neill-Meadin sandy loams, 2 to 6 percent slopes","Excessively drained","A",0.75,75.949999999999989,6.35]
["NE149","Rock","O'Neill-Meadin sandy loams, 6 to 11 percent slopes","Excessively drained","A",0.75,68.5,6.5]
["NE149","Rock","Ord loam, rarely flooded","Somewhat poorly drained","C",0.75,65.3,7.5]
["NE149","Rock","Pivot loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,91.5,6.5]
["NE149","Rock","Pivot-Valentine complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.75,92.1,6.5]
["NE149","Rock","Sandose loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.75,72.949999999999989,6.95]
["NE149","Rock","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,87.3,7]
["NE149","Rock","Simeon loamy sand, 3 to 11 percent slopes","Excessively drained","A",0.5,86.35,7]
["NE149","Rock","Simeon-Meadin complex, 0 to 9 percent slopes","Excessively drained","A",0.5,86.3,6.85]
["NE149","Rock","Simeon-Valentine sands, 11 to 60 percent slopes, eroded","Excessively drained","A",0.5,93.8,6.75]
["NE149","Rock","Tryon loamy fine sand, 0 to 3 percent slopes","Poorly drained","A/D",3.375,91.1,6.85]
["NE149","Rock","Tryon loamy fine sand, frequently ponded","Very poorly drained","A/D",3.375,91.1,6.85]
["NE149","Rock","Tryon-Els loamy sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,95.4,6.7]
["NE149","Rock","Tryon-Ipage complex, 0 to 3 percent slopes","Moderately well drained","A",0.75,95.15,6.45]
["NE149","Rock","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE149","Rock","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE149","Rock","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE149","Rock","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,96.3,6.5]
["NE149","Rock","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,92.7,6.5]
["NE149","Rock","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE149","Rock","Valentine-Boelus fine sands, 0 to 9 percent slopes","Well drained","B",0.5,92.1,6.5]
["NE149","Rock","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE149","Rock","Valentine-Pivot complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.75,91.5,6.5]
["NE149","Rock","Valentine-Simeon complex, 9 to 40 percent slopes, eroded","Excessively drained","A",0.5,92.6,6.75]
["NE149","Rock","Vetal loam, 1 to 3 percent slopes","Well drained","B",1.25,65.900000000000006,7]
["NE149","Rock","Wewela fine sandy loam, 2 to 6 percent slopes","Well drained","D",1.25,38.75,6.7]
["NE151","Saline",null,"",""]
["NE151","Saline","Burchard clay loam, 11 to 17 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE151","Saline","Burchard clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.75,36.5,6.7]
["NE151","Saline","Burchard clay loam, 6 to 11 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE151","Saline","Burchard clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,36.5,6.7]
["NE151","Saline","Burchard-Steinauer clay loams, 11 to 30 percent slopes","Somewhat excessively drained","C",0.75,34.5,7.9]
["NE151","Saline","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE151","Saline","Butler silt loam, terrace, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,13.649999999999999,7.1]
["NE151","Saline","Butler-Gayville silt loams, 0 to 1 percent slopes","Somewhat poorly drained","D",1.5,19.899999999999999,7.5]
["NE151","Saline","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE151","Saline","Crete silt loam, 1 to 3 percent slopes","Moderately well drained","C",1.625,19.850000000000001,6.25]
["NE151","Saline","Crete silt loam, terrace, 0 to 1 percent slopes","Moderately well drained","C",1.625,19.850000000000001,6.25]
["NE151","Saline","Crete silt loam, terrace, 1 to 3 percent slopes","Moderately well drained","C",1.625,19.850000000000001,6.25]
["NE151","Saline","Crete silty clay loam, 3 to 7 percent slopes, eroded","Moderately well drained","C",1,18.7,7.1]
["NE151","Saline","Deroin silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,6.9,7]
["NE151","Saline","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE151","Saline","Geary silty clay loam, 11 to 30 percent slopes","Well drained","C",1.25,6.9,6.7]
["NE151","Saline","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.7]
["NE151","Saline","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE151","Saline","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE151","Saline","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",0.75,18.5,6.5]
["NE151","Saline","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE151","Saline","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE151","Saline","Hastings silty clay loam, 7 to 11 percent slopes, severely eroded","Well drained","C",0.75,20,7.3]
["NE151","Saline","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE151","Saline","Hobbs silt loam, channeled, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE151","Saline","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE151","Saline","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE151","Saline","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE151","Saline","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,8,6.6]
["NE151","Saline","Kezan silt loam, frequently flooded","Poorly drained","B/D",1.875,8.1999999999999993,7.2]
["NE151","Saline","Longford silty clay loam, 3 to 7 percent slopes","Well drained","C",1.25,19.899999999999999,6.5]
["NE151","Saline","Longford silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,19.899999999999999,6.5]
["NE151","Saline","Longford silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,19.899999999999999,6.5]
["NE151","Saline","Malmo silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",0.75,28.95,7.45]
["NE151","Saline","Malmo silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.75,28.95,7.45]
["NE151","Saline","Malmo, eroded-Pawnee complex, 6 to 11 percent slopes","Moderately well drained","D",0.75,29.9,7]
["NE151","Saline","Mayberry silty clay loam, 3 to 6 percent slopes","Moderately well drained","D",0.75,26,6.5]
["NE151","Saline","Morrill clay loam, 11 to 30 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE151","Saline","Morrill clay loam, 6 to 11 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE151","Saline","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,35.4,6.1]
["NE151","Saline","Muir silt loam, 1 to 3 percent slopes","Well drained","B",2,9,6.7]
["NE151","Saline","Muir silt loam, 3 to 7 percent slopes","Well drained","B",2,9,6.7]
["NE151","Saline","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE151","Saline","Nodaway silt loam, channeled, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE151","Saline","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE151","Saline","Otoe silty clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,5,6.9]
["NE151","Saline","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE151","Saline","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE151","Saline","Uly silt loam, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE151","Saline","Wymore silty clay loam, 0 to 2 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE151","Saline","Wymore silty clay loam, 2 to 6 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE151","Saline","Wymore silty clay loam, 3 to 6 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE151","Saline","Wymore silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",1.5,17.3,6.5]
["NE151","Saline","Wymore silty clay loam, terrace, 0 to 2 percent slopes","Moderately well drained","D",1.5,6,6.3]
["NE151","Saline","Zook silt loam, occasionally flooded","Poorly drained","D",3,16.25,6.6]
["NE153","Sarpy",null,"",""]
["NE153","Sarpy","Alda-Platte complex, occasionally flooded","Somewhat poorly drained","C",0.75,65.7,7.9]
["NE153","Sarpy","Alda-Platte-Lex complex, occasionally flooded","Somewhat poorly drained","C",0.75,60.7,7.9]
["NE153","Sarpy","Burchard-Contrary-Steinauer complex, 7 to 16 percent slopes","Well drained","C",0.75,33.5,7.45]
["NE153","Sarpy","Carr-Ticonic-Scroll complex, occasionally flooded","Well drained","B",0.25,45,7.9]
["NE153","Sarpy","Cass-Novina complex, occasionally flooded","Well drained","B",0.75,64.599999999999994,6.8]
["NE153","Sarpy","Cass-Wann fine sandy loams, occasionally flooded","Well drained","A",0.75,65.7,8.1999999999999993]
["NE153","Sarpy","Clamo-Zook-Kezan silty clay loams, occasionally flooded","Poorly drained","D",3.5,7.6,6.7]
["NE153","Sarpy","Contrary-Marshall silty clay loams, 6 to 11 percent slopes","Well drained","C",1,3.5,6.3]
["NE153","Sarpy","Contrary-Monona silty clay loams, 6 to 11 percent slopes","Well drained","C",1,3.5,6.3]
["NE153","Sarpy","Contrary-Monona-Ida complex, 6 to 17 percent slopes","Well drained","C",1,3.5,7]
["NE153","Sarpy","Dickinson-Monona complex, 6 to 20 percent slopes","Somewhat excessively drained","B",0.875,36.549999999999997,6.4]
["NE153","Sarpy","Fluvaquents, silty, frequently flooded and Tieville soils, rarely flooded","Very poorly drained","B/D",1.25,6.9499999999999993,7.75]
["NE153","Sarpy","Gibbon loamy fine sand, overwash, occasionally flooded","Somewhat poorly drained","A",0.75,27.6,7.9]
["NE153","Sarpy","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,16.899999999999999,7.9]
["NE153","Sarpy","Gibbon-Wann complex, occasionally flooded","Somewhat poorly drained","C",1.375,39.75,8.1999999999999993]
["NE153","Sarpy","Gilliam-Onawa complex, occasionally flooded","Somewhat poorly drained","C",1.25,7.85,7.6]
["NE153","Sarpy","Haynie silt loam, occasionally flooded","Well drained","B",1.25,12.600000000000001,7.5]
["NE153","Sarpy","Hedville, Sogn, and Contrary soils, 12 to 75 percent slopes","Well drained","C",1,3.5,6.3]
["NE153","Sarpy","Ida-Pohocco-Monona silt loams, 11 to 30 percent slopes","Well drained","B",0.75,3.5,7.5]
["NE153","Sarpy","Inglewood-Novina complex, occasionally flooded","Moderately well drained","B",0.25,66.599999999999994,7]
["NE153","Sarpy","Judson silty clay loam, 2 to 6 percent slopes","Well drained","C",1.75,3.5,6.3]
["NE153","Sarpy","Judson-Nodaway channeled-Contrary complex, 3 to 10 percent slopes","Well drained","C",1,3.5,6.3]
["NE153","Sarpy","Kennebec silt loam, occasionally flooded","Moderately well drained","B",2,9.1999999999999993,6.3]
["NE153","Sarpy","Lex-Platte complex, occasionally flooded","Somewhat poorly drained","C",2,60,7.9]
["NE153","Sarpy","Marshall-Contrary silty clay loams, 2 to 7 percent slopes","Well drained","C",1,3.5,6.3]
["NE153","Sarpy","Melia silt loam, 0 to 2 percent slopes","Well drained","B",1.25,3.5,6.65]
["NE153","Sarpy","Melia silty clay loam, 0 to 2 percent slopes","Well drained","C",1.25,3.5,6.65]
["NE153","Sarpy","Monona-Pohocco-Ida silt loams, 17 to 33 percent slopes","Well drained","B",0.75,3.5,7.5]
["NE153","Sarpy","Muscotah silty clay loam, occasionally flooded","Somewhat poorly drained","C",2.25,4,6.8]
["NE153","Sarpy","Nishna silty clay loam, occasionally flooded","Poorly drained","C/D",2.25,7.65,7.9]
["NE153","Sarpy","Novina-Gibbon complex, occasionally flooded","Somewhat poorly drained","C",0.75,16,7.9]
["NE153","Sarpy","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,8.1999999999999993,7.6]
["NE153","Sarpy","Onawa-Lossing silty clays, occasionally flooded","Somewhat poorly drained","D",0.5,6.2,7.9]
["NE153","Sarpy","Platte and Alda soils, frequently flooded","Somewhat poorly drained","C",0.75,65.7,7.9]
["NE153","Sarpy","Platte, Inglewood, and Barney soils, frequently flooded","Poorly drained","C/D",0.25,74.5,7.5]
["NE153","Sarpy","Pohocco-Ida-Monona complex, 6 to 17 percent slopes","Well drained","B",0.75,3.5,7.5]
["NE153","Sarpy","Pohocco-Judson silt loams, 11 to 40 percent slopes","Well drained","C",0.75,4.75,6.65]
["NE153","Sarpy","Pohocco-Monona silt loams, 11 to 54 percent slopes","Well drained","B",0.75,4.75,7]
["NE153","Sarpy","Scroll-Percival complex, occasionally flooded","Somewhat poorly drained","D",0.75,13.65,7.75]
["NE153","Sarpy","Smithland-Kenridge silty clay loams, occasionally flooded","Moderately well drained","C",2.5,6.7,6.5]
["NE153","Sarpy","Ticonic-Sarpy-Carr complex, occasionally flooded","Well drained","B",0.25,73.400000000000006,7.9]
["NE153","Sarpy","Udorthents-Urban land-Pohocco complex, 0 to 39 percent slopes","Well drained","B",0.5,6,7]
["NE153","Sarpy","Urban land-Udorthents-Judson complex, 0 to 11 percent slopes","Well drained","C",0.75,3.5,6.05]
["NE153","Sarpy","Urban land-Udorthents-Marshall complex, 0 to 9 percent slopes","Well drained","C",0.47500000000000003,3.5,5.8]
["NE153","Sarpy","Urban land-Udorthents-Pohocco complex, 0 to 16 percent slopes","Well drained","B",0.5,6,7]
["NE153","Sarpy","Wann-Caruso-Ingelwood complex, occasionally flooded","Somewhat poorly drained","C",0.75,63.15,7.2]
["NE155","Saunders",null,"",""]
["NE155","Saunders","Aksarben silty clay loam, 0 to 2 percent slopes","Well drained","C",1.125,14,5.9499999999999993]
["NE155","Saunders","Alda fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,65.7,7.5]
["NE155","Saunders","Barney silty clay loam, frequently flooded","Poorly drained","B/D",1.625,67.449999999999989,7.35]
["NE155","Saunders","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.25,78.599999999999994,7.5]
["NE155","Saunders","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE155","Saunders","Burchard-Steinauer clay loams, 6 to 11 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE155","Saunders","Deroin silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,6.6,6.4]
["NE155","Saunders","Filbert silt loam, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,8.75,6.4]
["NE155","Saunders","Fillmore silt loam, terrace, occasionally ponded","Somewhat poorly drained","D",1.5,10,5.8]
["NE155","Saunders","Fluvaquents, silty, frequently flooded","Very poorly drained","B/D",2.5,3.9,3.75]
["NE155","Saunders","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",1.375,16,7.9]
["NE155","Saunders","Gibbon-Saltine loams, occasionally flooded","Somewhat poorly drained","C",0.5,11.850000000000001,8.5]
["NE155","Saunders","Hedville cobbly loam, 7 to 30 percent slopes","Somewhat excessively drained","D",2.5,43.2,6.5]
["NE155","Saunders","Ida-Steinauer complex, 17 to 60 percent slopes","Well drained","B",0.5,22.35,7.9]
["NE155","Saunders","Inglewood loamy fine sand, rarely flooded","Moderately well drained","A",0.25,87.55,7]
["NE155","Saunders","Janude loam, clayey substratum, rarely flooded","Moderately well drained","B",0.75,44.3,7.5]
["NE155","Saunders","Judson silt loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE155","Saunders","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE155","Saunders","Kenridge silty clay loam, occasionally flooded","Moderately well drained","C",2.75,6.8000000000000007,6.4]
["NE155","Saunders","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,10,7.9]
["NE155","Saunders","Lex loam, occasionally flooded","Somewhat poorly drained","C",2,39.1,7.9]
["NE155","Saunders","Malcolm silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.25,7.1,6.1]
["NE155","Saunders","Malmo clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.75,31.9,7.45]
["NE155","Saunders","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,57,6.1]
["NE155","Saunders","Muscotah silty clay loam, occasionally flooded","Somewhat poorly drained","C",2.25,4,6.8]
["NE155","Saunders","Nodaway silt loam, channeled, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE155","Saunders","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,7,6.7]
["NE155","Saunders","Obert silty clay loam, frequently flooded","Very poorly drained","C/D",1.5,6.8,7.9]
["NE155","Saunders","Obert silty clay loam, occasionally flooded","Poorly drained","C/D",1.5,6.9,7.9]
["NE155","Saunders","Olmitz loam, 2 to 6 percent slopes","Well drained","B",2,34.15,6.7]
["NE155","Saunders","Pawnee clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",1.5,29.9,7]
["NE155","Saunders","Platte and Alda soils, frequently flooded","Somewhat poorly drained","C",0.75,65.7,7.9]
["NE155","Saunders","Platte fine sandy loam, occasionally flooded","Somewhat poorly drained","B",2,64.400000000000006,7.2]
["NE155","Saunders","Platte-Barney complex, channeled, frequently flooded","Poorly drained","C/D",2,64.400000000000006,7.2]
["NE155","Saunders","Pohocco silty clay loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.1,7.35]
["NE155","Saunders","Pohocco silty clay loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.1,7.35]
["NE155","Saunders","Pohocco-Pahuk complex, 11 to 17 percent slopes, eroded","Excessively drained","A",0.75,9.3000000000000007,7.2]
["NE155","Saunders","Pohocco-Pahuk complex, 6 to 11 percent slopes, eroded","Excessively drained","A",0.75,9.3000000000000007,7.2]
["NE155","Saunders","Saltillo silt loam, occasionally flooded","Poorly drained","B/D",0.25,4.6500000000000004,8.1999999999999993]
["NE155","Saunders","Sarpy loamy fine sand, frequently flooded","Excessively drained","A",0.5,87.9,7.25]
["NE155","Saunders","Sarpy-Haynie complex, occasionally flooded","Well drained","B",0.75,69.599999999999994,7.5]
["NE155","Saunders","Scott silt loam, terrace, frequently ponded","Poorly drained","D",1.5,8,5.8]
["NE155","Saunders","Steinauer clay loam, 11 to 30 percent slopes","Well drained","C",0.75,33.5,8.1999999999999993]
["NE155","Saunders","Steinauer clay loam, 20 to 40 percent slopes","Well drained","C",1,33.6,7.6]
["NE155","Saunders","Tomek silt loam, 0 to 2 percent slopes","Well drained","C",2.5,18.850000000000001,6.95]
["NE155","Saunders","Wann fine sandy loam, occasionally flooded","Somewhat poorly drained","B",1.375,65.349999999999994,7.85]
["NE155","Saunders","Yutan silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.5,7.5,6.7]
["NE155","Saunders","Yutan silty clay loam, terrace, 2 to 6 percent slopes, eroded","Well drained","C",0.5,7.5,6.7]
["NE155","Saunders","Yutan, eroded-Aksarben silty clay loams, 2 to 6 percent slopes","Well drained","C",0.75,7.5,6.5]
["NE155","Saunders","Yutan, eroded-Judson complex, 6 to 11 percent slopes","Well drained","C",0.875,7.2,6.6]
["NE157","Scotts Bluff",null,"",""]
["NE157","Scotts Bluff","Alice fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,64.599999999999994,7.9]
["NE157","Scotts Bluff","Alice fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,67.5,7.9]
["NE157","Scotts Bluff","Alice fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,67.5,7.9]
["NE157","Scotts Bluff","Alice loamy fine sand, 0 to 3 percent slopes","Well drained","A",0.75,67.5,7.9]
["NE157","Scotts Bluff","Alice-Dix complex, 3 to 6 percent slopes","Well drained","A",0.75,83.2,7.5]
["NE157","Scotts Bluff","Altvan-Dix complex, 3 to 9 percent slopes","Well drained","B",0.75,67.900000000000006,7.5]
["NE157","Scotts Bluff","Angora very fine sandy loam, 1 to 6 percent slopes","Well drained","B",0.25,61.4,7.5]
["NE157","Scotts Bluff","Arvada clay loam, 0 to 1 percent slopes","Well drained","D",0.5,32.4,8.8000000000000007]
["NE157","Scotts Bluff","Ashollow loamy very fine sand, 3 to 9 percent slopes","Well drained","A",1.125,81.8,7.9]
["NE157","Scotts Bluff","Ashollow loamy very fine sand, 9 to 20 percent slopes","Well drained","A",1.125,81.8,7.9]
["NE157","Scotts Bluff","Bankard fine sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,93.6,7.9]
["NE157","Scotts Bluff","Bankard loamy fine sand, 0 to 2 percent slopes","Somewhat excessively drained","A",0.5,85.9,8.1999999999999993]
["NE157","Scotts Bluff","Bankard loamy fine sand, occasionally flooded","Somewhat excessively drained","A",0.75,90.449999999999989,8.0500000000000007]
["NE157","Scotts Bluff","Bankard loamy fine sand, wet variant","Somewhat poorly drained","A",0.625,88.3,7.9]
["NE157","Scotts Bluff","Barney loam, frequently flooded","Very poorly drained","B/D",0.25,91.9,7.2]
["NE157","Scotts Bluff","Bayard fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.375,76.400000000000006,7.5500000000000007]
["NE157","Scotts Bluff","Bayard fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,62.5,7.9]
["NE157","Scotts Bluff","Bayard fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.375,76.400000000000006,7.5500000000000007]
["NE157","Scotts Bluff","Bayard fine sandy loam, 6 to 9 percent slopes","Well drained","A",1.375,76.400000000000006,7.5500000000000007]
["NE157","Scotts Bluff","Bayard fine sandy loam, 9 to 20 percent slopes","Well drained","A",1.375,76.400000000000006,7.5500000000000007]
["NE157","Scotts Bluff","Bayard very fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE157","Scotts Bluff","Bayard very fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE157","Scotts Bluff","Bayard very fine sandy loam, 6 to 9 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE157","Scotts Bluff","Bayard very fine sandy loam, 9 to 20 percent slopes","Well drained","A",1.375,63.3,7.5500000000000007]
["NE157","Scotts Bluff","Bayard-Dix complex, 3 to 9 percent slopes","Well drained","A",1.125,62.9,7.35]
["NE157","Scotts Bluff","Blueridge gravelly loamy sand, 20 to 50 percent slopes","Excessively drained","A",0.5,86.5,6.75]
["NE157","Scotts Bluff","Blueridge gravelly sandy loam, 20 to 30 percent slopes","Excessively drained","A",0.5,80.099999999999994,6.75]
["NE157","Scotts Bluff","Blueridge-Bayard complex, 6 to 20 percent slopes","Well drained","A",0.75,84.3,7.2]
["NE157","Scotts Bluff","Bridget very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,20.8,7.9]
["NE157","Scotts Bluff","Bridget very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,62.7,7.9]
["NE157","Scotts Bluff","Bridget very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,62.7,7.9]
["NE157","Scotts Bluff","Bridget very fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.75,62.7,7.9]
["NE157","Scotts Bluff","Bridget very fine sandy loam, 9 to 20 percent slopes","Well drained","B",0.75,62.7,7.9]
["NE157","Scotts Bluff","Bridget-Otero complex, 3 to 6 percent slopes, eroded","Well drained","B",0.75,54,7.9]
["NE157","Scotts Bluff","Bridget-Otero complex, 6 to 9 percent slopes","Well drained","B",0.75,54,7.9]
["NE157","Scotts Bluff","Buffington silty clay loam, 0 to 1 percent slopes","Well drained","C",0.25,17.8,7.9]
["NE157","Scotts Bluff","Buffington silty clay loam, 1 to 3 percent slopes","Well drained","C",0.25,17.8,7.9]
["NE157","Scotts Bluff","Buffington silty clay loam, alkali, 0 to 1 percent slopes","Well drained","C",0.25,17.8,8.1999999999999993]
["NE157","Scotts Bluff","Busher loamy very fine sand, 1 to 6 percent slopes","Well drained","A",0.75,79.5,7]
["NE157","Scotts Bluff","Busher-Jayem loamy very fine sands, 0 to 3 percent slopes","Well drained","A",0.52500000000000002,79.75,7.2]
["NE157","Scotts Bluff","Busher-Jayem loamy very fine sands, 3 to 6 percent slopes","Well drained","A",0.52500000000000002,80,7.2]
["NE157","Scotts Bluff","Busher-Tassel complex, 0 to 6 percent slopes","Well drained","A",1,72.05,7.25]
["NE157","Scotts Bluff","Busher-Tassel complex, 6 to 30 percent slopes","Well drained","A",1,72.05,7.25]
["NE157","Scotts Bluff","Busher-Tassel loamy very fine sands, 6 to 30 percent slopes","Well drained","A",1,79.5,7.25]
["NE157","Scotts Bluff","Busher-Tassel loamy very fine sands, 9 to 20 percent slopes","Well drained","A",1,79.3,7.25]
["NE157","Scotts Bluff","Chappell-Dix complex, 1 to 3 percent slopes","Well drained","A",0.75,67.449999999999989,7.4]
["NE157","Scotts Bluff","Chappell-Dix complex, 3 to 6 percent slopes","Well drained","A",0.75,68.3,7.5]
["NE157","Scotts Bluff","Creighton very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,62.7,7.2]
["NE157","Scotts Bluff","Creighton very fine sandy loam, 6 to 11 percent slopes","Well drained","B",0.75,62.7,7.2]
["NE157","Scotts Bluff","Dailey and Valent loamy fine sands, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,79.900000000000006,7.2]
["NE157","Scotts Bluff","Dailey and Valent loamy fine sands, 3 to 6 percent slopes","Somewhat excessively drained","A",0.75,79.900000000000006,7.2]
["NE157","Scotts Bluff","Dailey loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1.375,87.9,7.25]
["NE157","Scotts Bluff","Dix complex, 6 to 30 percent slopes","Excessively drained","A",0.75,83.2,7.5]
["NE157","Scotts Bluff","Dix loamy coarse sand, 6 to 50 percent slopes","Excessively drained","A",1.125,83.35,7.25]
["NE157","Scotts Bluff","Dix-Bayard complex, 6 to 20 percent slopes","Well drained","A",0.75,81.5,7.5]
["NE157","Scotts Bluff","Duroc loam, 1 to 6 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE157","Scotts Bluff","Epping silt loam, 1 to 3 percent slopes","Well drained","D",0.75,34.75,7.7]
["NE157","Scotts Bluff","Epping silt loam, 3 to 30 percent slopes","Well drained","D",0.75,34.75,7.7]
["NE157","Scotts Bluff","Epping-Keota silt loams, 3 to 30 percent slopes","Well drained","D",0.5,17.55,7.9]
["NE157","Scotts Bluff","Gering loam, alkali, occasionally flooded","Somewhat poorly drained","B",0.75,41.1,8.5]
["NE157","Scotts Bluff","Gering loam, rarely flooded","Somewhat poorly drained","B",0.25,45.6,8.1999999999999993]
["NE157","Scotts Bluff","Glenberg fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,77.099999999999994,8.0500000000000007]
["NE157","Scotts Bluff","Glenberg fine sandy loam, frequently flooded","Well drained","A",1,54.8,7.9]
["NE157","Scotts Bluff","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.25,96.3,7.2]
["NE157","Scotts Bluff","Gothenburg soils, frequently flooded","Poorly drained","A/D",0.25,91.9,7.3]
["NE157","Scotts Bluff","Haverson fine sandy loam, rarely flooded","Well drained","B",1,48.8,7.9]
["NE157","Scotts Bluff","Janise loam, occasionally flooded","Somewhat poorly drained","C",0.75,42.2,9.4]
["NE157","Scotts Bluff","Janise soils, rarely flooded","Somewhat poorly drained","C",1.75,28.2,9.1]
["NE157","Scotts Bluff","Jayem fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,67.5,7.2]
["NE157","Scotts Bluff","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,67.5,7.2]
["NE157","Scotts Bluff","Jayem fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,67.5,7.2]
["NE157","Scotts Bluff","Jayem fine sandy loam, 9 to 20 percent slopes","Well drained","A",0.75,67.5,7.2]
["NE157","Scotts Bluff","Jayem loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.5,62.5,7.2]
["NE157","Scotts Bluff","Jayem loamy very fine sand, 3 to 6 percent slopes","Well drained","A",0.5,62.5,7.2]
["NE157","Scotts Bluff","Jayem loamy very fine sand, 6 to 9 percent slopes","Well drained","A",1.1499999999999999,71.25,7.2]
["NE157","Scotts Bluff","Keith loam, alkali substratum variant, 0 to 3 percent slopes","Moderately well drained","B",0.75,31.1,7.9]
["NE157","Scotts Bluff","Keota silt loam, 1 to 3 percent slopes","Well drained","C",0.25,11.4,7.9]
["NE157","Scotts Bluff","Keota silt loam, 3 to 6 percent slopes","Well drained","C",0.25,11.4,7.9]
["NE157","Scotts Bluff","Keota-Epping silt loams, 6 to 9 percent slopes","Well drained","D",0.75,20.8,7.9]
["NE157","Scotts Bluff","Laird fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,69.599999999999994,8.5]
["NE157","Scotts Bluff","Las Animas fine sandy loam, channeled, frequently flooded","Somewhat poorly drained","B",1,63,7.9]
["NE157","Scotts Bluff","Las Animas fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.25,83,7.9]
["NE157","Scotts Bluff","Las Animas loam, occasionally flooded","Somewhat poorly drained","C",0.25,63.5,7.9]
["NE157","Scotts Bluff","Marlake, frequently ponded","Very poorly drained","A/D",0.75,78.2,7]
["NE157","Scotts Bluff","McCook loam, rarely flooded","Well drained","B",1.75,27.6,7.9]
["NE157","Scotts Bluff","McCook silty clay loam, gravel substratum variant","Well drained","C",0.5,42.7,7.9]
["NE157","Scotts Bluff","McGrew fine sandy loam","Somewhat poorly drained","B",0.25,71.3,7.9]
["NE157","Scotts Bluff","McGrew loam","Somewhat poorly drained","C",0.25,70.099999999999994,7.9]
["NE157","Scotts Bluff","McGrew loam, alkali, occasionally flooded","Somewhat poorly drained","B",0.75,62.7,8.8000000000000007]
["NE157","Scotts Bluff","Minatare-Janise complex, rarely flooded","Somewhat poorly drained","C",1,33.6,9.1]
["NE157","Scotts Bluff","Minatare-Janise soils, rarely flooded","Somewhat poorly drained","C",0.625,35.049999999999997,9.25]
["NE157","Scotts Bluff","Mitchell and Buffington soils, alkali, 0 to 3 percent slopes","Somewhat poorly drained","C",0.75,16.899999999999999,7.9]
["NE157","Scotts Bluff","Mitchell fine sandy loam, 0 to 3 percent slopes","Well drained","B",1,41.400000000000006,7.9]
["NE157","Scotts Bluff","Mitchell fine sandy loam, 3 to 6 percent slopes","Well drained","B",1,41.400000000000006,7.9]
["NE157","Scotts Bluff","Mitchell fine sandy loam, 6 to 9 percent slopes","Well drained","B",1,41.400000000000006,7.9]
["NE157","Scotts Bluff","Mitchell silt loam, 0 to 1 percent slopes","Well drained","B",1,14,7.9]
["NE157","Scotts Bluff","Mitchell silt loam, 1 to 3 percent slopes","Well drained","B",1,28.450000000000003,7.9]
["NE157","Scotts Bluff","Mitchell silt loam, 3 to 6 percent slopes","Well drained","B",1,14,7.9]
["NE157","Scotts Bluff","Mitchell silt loam, 6 to 9 percent slopes","Well drained","B",1,14,7.9]
["NE157","Scotts Bluff","Mitchell silt loam, 9 to 20 percent slopes","Well drained","B",1,27.25,7.9]
["NE157","Scotts Bluff","Mitchell silt loam, thin, 1 to 6 percent slopes","Well drained","B",1,12.8,7.9]
["NE157","Scotts Bluff","Mitchell silt loam, thin, 6 to 9 percent slopes","Well drained","B",1,12.8,7.9]
["NE157","Scotts Bluff","Mitchell silt loam, thin, 9 to 20 percent slopes","Well drained","B",1,12.8,7.9]
["NE157","Scotts Bluff","Mitchell silt loam, wet variant, 0 to 1 percent slopes","Somewhat poorly drained","B/D",1,12.850000000000001,7.9]
["NE157","Scotts Bluff","Mitchell very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1,60.5,7.9]
["NE157","Scotts Bluff","Mitchell very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1,60.5,7.9]
["NE157","Scotts Bluff","Mitchell very fine sandy loam, 3 to 6 percent slopes","Well drained","B",1,60.5,7.9]
["NE157","Scotts Bluff","Mitchell very fine sandy loam, 6 to 9 percent slopes","Well drained","B",1,60.5,7.9]
["NE157","Scotts Bluff","Mitchell-Epping complex, 3 to 9 percent slopes","Well drained","D",0.75,30.1,7.9]
["NE157","Scotts Bluff","Mitchell-Epping complex, 9 to 30 percent slopes","Well drained","D",0.75,30.1,7.9]
["NE157","Scotts Bluff","Orella clay, 0 to 3 percent slopes","Well drained","D",0.75,21.6,7.9]
["NE157","Scotts Bluff","Otero fine sandy loam, 1 to 6 percent slopes","Well drained","A",0.75,71.3,7.9]
["NE157","Scotts Bluff","Otero fine sandy loam, 6 to 12 percent slopes","Well drained","A",0.75,71.3,7.9]
["NE157","Scotts Bluff","Otero loamy fine sand, 0 to 6 percent slopes","Well drained","A",0.75,71.3,7.9]
["NE157","Scotts Bluff","Otero loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.75,80.3,7.9]
["NE157","Scotts Bluff","Otero variant very fine sandy loam, 0 to 1 percent slopes","Somewhat poorly drained","B",0.625,64.400000000000006,7.9]
["NE157","Scotts Bluff","Otero very fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.625,64.75,7.9]
["NE157","Scotts Bluff","Otero very fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.625,64.75,7.9]
["NE157","Scotts Bluff","Otero very fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.625,64.75,7.9]
["NE157","Scotts Bluff","Otero-Bayard fine sandy loams, 0 to 3 percent slopes","Well drained","A",0.75,71.3,7.9]
["NE157","Scotts Bluff","Otero-Bayard fine sandy loams, 3 to 6 percent slopes","Well drained","A",0.75,71.3,7.9]
["NE157","Scotts Bluff","Otero-Bayard fine sandy loams, 6 to 9 percent slopes","Well drained","A",0.75,71.3,7.9]
["NE157","Scotts Bluff","Otero-Bayard very fine sandy loams, 0 to 1 percent slopes","Well drained","A",0.75,71.3,7.9]
["NE157","Scotts Bluff","Otero-Epping complex, 9 to 60 percent slopes","Well drained","D",0.75,30.1,7.9]
["NE157","Scotts Bluff","Pathfinder loamy fine sand, rarely flooded","Somewhat excessively drained","A",0.75,88.1,8.5]
["NE157","Scotts Bluff","Platte soils, occasionally flooded","Somewhat poorly drained","C",0.25,77.400000000000006,7.5]
["NE157","Scotts Bluff","Rock outcrop-Epping complex","Well drained","D",0.75,26.5,7.5]
["NE157","Scotts Bluff","Rock outcrop-Epping complex, 20 to 60 percent slopes","Well drained","D",0.375,15.05,3.95]
["NE157","Scotts Bluff","Rosebud loam, 6 to 9 percent slopes","Well drained","C",0.75,36.5,7.2]
["NE157","Scotts Bluff","Sarben loamy very fine sand, 3 to 9 percent slopes","Well drained","A",0.25,84,7.2]
["NE157","Scotts Bluff","Satanta fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,42.7,7.5]
["NE157","Scotts Bluff","Scoville fine sand, 0 to 1 percent slopes","Somewhat excessively drained","A",0.25,94.4,7.2]
["NE157","Scotts Bluff","Scoville fine sand, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,94.4,7.2]
["NE157","Scotts Bluff","Scoville loamy fine sand, 0 to 1 percent slopes","Somewhat excessively drained","B",0.25,78.599999999999994,7.2]
["NE157","Scotts Bluff","Scoville loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","B",0.25,78.599999999999994,7.2]
["NE157","Scotts Bluff","Shingle complex, 3 to 9 percent slopes","Well drained","D",0.75,18,8.1999999999999993]
["NE157","Scotts Bluff","Slickspots-Keith complex","Moderately well drained","B",0.75,14,7.9]
["NE157","Scotts Bluff","Sulco complex, 9 to 60 percent slopes","Well drained","B",1,53.35,7.9]
["NE157","Scotts Bluff","Tassel loamy very fine sand, 20 to 50 percent slopes","Well drained","D",1.25,79.5,7.9]
["NE157","Scotts Bluff","Tassel soils, 20 to 50 percent slopes","Well drained","D",1.25,68.5,7.9]
["NE157","Scotts Bluff","Tassel-Ashollow-Rock outcrop complex, 9 to 60 percent slopes","Well drained","A",1,73.199999999999989,7.9]
["NE157","Scotts Bluff","Tassel-Busher complex, 3 to 30 percent slopes","Well drained","A",1,69.099999999999994,7.25]
["NE157","Scotts Bluff","Tassel-Busher loamy very fine sands, 3 to 30 percent slopes","Well drained","A",1,79.5,7.25]
["NE157","Scotts Bluff","Tassel-Busher-Rock outcrop complex, 20 to 60 percent slopes","Well drained","A",1,79.3,7.25]
["NE157","Scotts Bluff","Tripp fine sandy loam, 0 to 3 percent slopes","Well drained","B",0.75,61.7,7.5]
["NE157","Scotts Bluff","Tripp very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,61.7,7.5]
["NE157","Scotts Bluff","Tripp very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,61.7,7.5]
["NE157","Scotts Bluff","Tripp very fine sandy loam, 3 to 6 percent slopes, eroded","Well drained","B",0.75,61.7,7.5]
["NE157","Scotts Bluff","Tripp very fine sandy loam, 6 to 9 percent slopes, eroded","Well drained","B",0.75,61.7,7.5]
["NE157","Scotts Bluff","Valent and Dwyer fine sands, rolling","Excessively drained","A",0.75,95.15,7.35]
["NE157","Scotts Bluff","Valent and Dwyer loamy fine sands, rolling","Excessively drained","A",0.75,88.1,7.35]
["NE157","Scotts Bluff","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE157","Scotts Bluff","Valent fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE157","Scotts Bluff","Valent loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,89.45,7.2]
["NE157","Scotts Bluff","Valent loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,89.45,7.2]
["NE157","Scotts Bluff","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7.3]
["NE157","Scotts Bluff","Wildhorse loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,87.5,9.1499999999999986]
["NE157","Scotts Bluff","Yockey fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.625,67.55,8.6499999999999986]
["NE157","Scotts Bluff","Yockey loam, occasionally flooded","Somewhat poorly drained","B",0.625,50.15,8.6499999999999986]
["NE157","Scotts Bluff","Yockey silt loam, alkali, occasionally flooded","Somewhat poorly drained","C",0.875,37.950000000000003,8.6499999999999986]
["NE157","Scotts Bluff","Yockey silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,37.5,7.9]
["NE159","Seward",null,"",""]
["NE159","Seward","Aksarben silty clay loam, 2 to 6 percent slopes","Well drained","C",1.5,20,6.1]
["NE159","Seward","Aksarben silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.125,14,5.9499999999999993]
["NE159","Seward","Aksarben silty clay loam, 6 to 11 percent slopes","Well drained","C",1.5,20,6.1]
["NE159","Seward","Aksarben silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.125,14,5.9499999999999993]
["NE159","Seward","Burchard clay loam, 11 to 17 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE159","Seward","Burchard clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.75,36.5,6.7]
["NE159","Seward","Burchard clay loam, 6 to 11 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE159","Seward","Burchard clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,36.5,6.7]
["NE159","Seward","Burchard loam, 11 to 17 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE159","Seward","Burchard loam, 6 to 11 percent slopes","Well drained","C",0.75,36.5,6.7]
["NE159","Seward","Burchard-Steinauer clay loams, 11 to 17 percent slopes","Well drained","C",0.75,34.5,7.9]
["NE159","Seward","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.5,7.9]
["NE159","Seward","Burchard-Steinauer clay loams, 11 to 30 percent slopes","Somewhat excessively drained","C",0.75,34.5,7.9]
["NE159","Seward","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE159","Seward","Butler silt loam, terrace, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.125,15,7.1]
["NE159","Seward","Butler-Olbut complex, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.125,20.200000000000003,7.4]
["NE159","Seward","Coly silt loam, 30 to 60 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE159","Seward","Coly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,11.3,7.5]
["NE159","Seward","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE159","Seward","Crete silt loam, 1 to 3 percent slopes","Moderately well drained","C",1,12.650000000000002,7.3000000000000007]
["NE159","Seward","Crete silt loam, terrace, 0 to 1 percent slopes","Moderately well drained","C",1.625,19.850000000000001,6.25]
["NE159","Seward","Crete silt loam, terrace, 1 to 3 percent slopes","Moderately well drained","C",1,13.100000000000001,7.3000000000000007]
["NE159","Seward","Deroin silty clay loam, 11 to 30 percent slopes, severely eroded","Well drained","B",0.5,6.9,7]
["NE159","Seward","Deroin silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,6.9,7]
["NE159","Seward","Deroin silty clay loam, 6 to 11 percent slopes, severely eroded","Well drained","B",0.5,6.9,7]
["NE159","Seward","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE159","Seward","Geary silty clay loam, 11 to 30 percent slopes","Well drained","C",1.25,6.9,6.7]
["NE159","Seward","Geary silty clay loam, 3 to 7 percent slopes, eroded","Well drained","B",1.5,7.1,7]
["NE159","Seward","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","B",1.5,7.1,7]
["NE159","Seward","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE159","Seward","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.5,9.5,7]
["NE159","Seward","Hall-Olbut complex, 1 to 3 percent slopes","Well drained","C",1.5,9.5,7.2]
["NE159","Seward","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE159","Seward","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE159","Seward","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",0.75,18.5,6.5]
["NE159","Seward","Hastings silty clay loam, 1 to 3 percent slopes, eroded","Well drained","C",3,15.4,6.1]
["NE159","Seward","Hastings silty clay loam, 11 to 17 percent slopes, severely eroded","Well drained","C",0.75,20,7.3]
["NE159","Seward","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",3,15.4,6.1]
["NE159","Seward","Hastings silty clay loam, 3 to 7 percent slopes, severely eroded","Well drained","C",0.75,20,7.3]
["NE159","Seward","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",3,15.4,6.1]
["NE159","Seward","Hastings silty clay loam, 7 to 11 percent slopes, severely eroded","Well drained","C",0.75,20,7.3]
["NE159","Seward","Hastings silty clay loam, terrace, 3 to 7 percent slopes, eroded","Well drained","C",0.75,15.4,6.5]
["NE159","Seward","Hastings soils, 1 to 3 percent slopes, severely eroded","Well drained","C",0.75,15.4,6.5]
["NE159","Seward","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE159","Seward","Hobbs silt loam, frequently flooded","Well drained","B",1.875,11.3,7]
["NE159","Seward","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE159","Seward","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE159","Seward","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE159","Seward","Hord-Hastings complex, 3 to 6 percent slopes","Well drained","C",0.625,10.25,6.75]
["NE159","Seward","Judson silt loam, 2 to 6 percent slopes","Well drained","C",3.5,7.9,5.8]
["NE159","Seward","Kennebec silt loam, occasionally flooded","Moderately well drained","C",2,5,6.35]
["NE159","Seward","Kezan silt loam, occasionally flooded","Poorly drained","C",0.75,8.6999999999999993,7.2]
["NE159","Seward","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C/D",1.5,6.9,7.9]
["NE159","Seward","Longford silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.625,19.95,6.6]
["NE159","Seward","Massie silty clay loam, frequently ponded","Very poorly drained","D",1.25,6,6.4]
["NE159","Seward","Meadin soils, 7 to 30 percent slopes, eroded","Excessively drained","B",0.75,65.3,6.2]
["NE159","Seward","Morrill clay loam, 6 to 11 percent slopes","Well drained","C",0.6,35.200000000000003,6.1]
["NE159","Seward","Morrill clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.6,35.200000000000003,6.1]
["NE159","Seward","Muir silt loam, 0 to 1 percent slopes","Well drained","B",2,9,6.7]
["NE159","Seward","Muir silt loam, 1 to 3 percent slopes","Well drained","B",2,9,6.7]
["NE159","Seward","Muir silt loam, 3 to 7 percent slopes","Well drained","B",2,9,6.7]
["NE159","Seward","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE159","Seward","Muir silty clay loam, rarely flooded","Well drained","B",2,9,6.7]
["NE159","Seward","Nodaway silt loam, channeled, frequently flooded","Moderately well drained","B",1.875,9.4,6.3]
["NE159","Seward","Nodaway silt loam, occasionally flooded","Moderately well drained","B",1.375,9.5,6.3]
["NE159","Seward","Obert silty clay loam, frequently ponded","Very poorly drained","C/D",1.5,7.3,7.9]
["NE159","Seward","Pawnee clay loam, 4 to 8 percent slopes, eroded","Moderately well drained","D",1.4500000000000002,24.5,6.4]
["NE159","Seward","Pawnee clay loam, 6 to 11 percent slopes","Moderately well drained","D",2,33.5,7]
["NE159","Seward","Pawnee clay loam, 6 to 11 percent slopes, eroded","Moderately well drained","D",2,33.5,7]
["NE159","Seward","Pawnee soils, 6 to 11 percent slopes, severely eroded","Moderately well drained","D",0.5,27.6,6.5]
["NE159","Seward","Pohocco silty clay loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,8.9,7.2]
["NE159","Seward","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE159","Seward","Shelby clay loam, 6 to 11 percent slopes","Well drained","C",0.5,34.700000000000003,6.2]
["NE159","Seward","Shelby clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,34.700000000000003,6.2]
["NE159","Seward","Steinauer clay loam, 11 to 30 percent slopes","Well drained","C",0.75,33.6,8.1999999999999993]
["NE159","Seward","Steinauer clay loam, 11 to 30 percent slopes, eroded","Well drained","C",0.75,33.6,8.1999999999999993]
["NE159","Seward","Steinauer clay loam, 20 to 40 percent slopes","Well drained","C",1,33.6,7.6]
["NE159","Seward","Steinauer clay loam, 30 to 50 percent slopes","Well drained","C",1,33.6,8.0500000000000007]
["NE159","Seward","Steinauer clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,33.6,8.1999999999999993]
["NE159","Seward","Steinauer loam, 11 to 30 percent slopes","Well drained","C",0.75,36.200000000000003,7.6]
["NE159","Seward","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE159","Seward","Uly-Hobbs silt loams, 0 to 30 percent slopes, eroded","Well drained","B",0.75,10.35,7]
["NE159","Seward","Uly-Hobbs silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7]
["NE159","Seward","Wymore silty clay loam, 0 to 1 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE159","Seward","Wymore silty clay loam, 1 to 3 percent slopes","Moderately well drained","D",1.5,17.3,6.5]
["NE159","Seward","Wymore silty clay loam, 3 to 6 percent slopes, eroded","Moderately well drained","D",1.5,17.3,6.5]
["NE159","Seward","Wymore soils, 6 to 11 percent slopes, eroded","Moderately well drained","D",0.5,7.7,6.5]
["NE159","Seward","Yutan silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.5,7.5,6.7]
["NE159","Seward","Yutan silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",0.75,7.6,6.5]
["NE159","Seward","Yutan silty clay loam, 3 to 6 percent slopes, eroded","Well drained","C",0.5,7.5,6.7]
["NE159","Seward","Yutan silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.5,7.5,6.7]
["NE161","Sheridan",null,"",""]
["NE161","Sheridan","Alliance loam, 0 to 1 percent slopes","Well drained","B",0.75,23.900000000000002,7.2]
["NE161","Sheridan","Alliance loam, 1 to 3 percent slopes","Well drained","B",0.75,23.900000000000002,7.2]
["NE161","Sheridan","Alliance loam, 3 to 6 percent slopes","Well drained","B",0.75,23.900000000000002,7.2]
["NE161","Sheridan","Almeria loamy fine sand, channeled, frequently flooded","Very poorly drained","A/D",1.25,89.85,6.9]
["NE161","Sheridan","Bankard loamy fine sand, channeled, frequently flooded","Somewhat excessively drained","A",1,43.65,7.9]
["NE161","Sheridan","Beckton silt loam, 0 to 2 percent slopes","Moderately well drained","C",0.5,23.8,8]
["NE161","Sheridan","Bolent loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.5,75.349999999999994,7.7]
["NE161","Sheridan","Bridget loam, 0 to 1 percent slopes","Well drained","B",1.375,52.45,7.5500000000000007]
["NE161","Sheridan","Bridget very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1.375,61.7,7.5500000000000007]
["NE161","Sheridan","Bridget very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.375,61.7,7.5500000000000007]
["NE161","Sheridan","Bufton silty clay loam, 1 to 3 percent slopes","Well drained","C",0.75,17.3,8.1999999999999993]
["NE161","Sheridan","Bufton silty clay loam, 9 to 20 percent slopes","Well drained","C",0.75,17.3,8.1999999999999993]
["NE161","Sheridan","Bufton-Orella complex, 3 to 9 percent slopes","Well drained","C",0.75,18,8.0500000000000007]
["NE161","Sheridan","Busher fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,63.5,7]
["NE161","Sheridan","Busher fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,7]
["NE161","Sheridan","Busher fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,63.5,7]
["NE161","Sheridan","Busher-Tassel complex, 0 to 6 percent slopes","Well drained","A",1,64.05,7.25]
["NE161","Sheridan","Busher-Tassel complex, 6 to 30 percent slopes","Well drained","A",1,64.05,7.25]
["NE161","Sheridan","Busher-Tassel fine sandy loams, 9 to 30 percent slopes","Well drained","A",0.75,64.5,7.25]
["NE161","Sheridan","Calamus loamy fine sand, rarely flooded","Moderately well drained","A",0.75,78.2,7]
["NE161","Sheridan","Crowther loam, 0 to 1 percent slopes","Poorly drained","C/D",1.5,38.5,7.9]
["NE161","Sheridan","Crowther mucky peat","Very poorly drained","B/D",6.75,36,7.7]
["NE161","Sheridan","Dailey loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",1.375,79.800000000000011,7.25]
["NE161","Sheridan","Dailey loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",1.375,79.800000000000011,7.25]
["NE161","Sheridan","Doger and Dunday loamy fine sands, 0 to 2 percent slopes","Well drained","A",1,87.05,6.85]
["NE161","Sheridan","Duroc loam, 0 to 1 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE161","Sheridan","Duroc loam, 1 to 3 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE161","Sheridan","Duroc very fine sandy loam, 1 to 3 percent slopes","Well drained","B",2,33.299999999999997,7.2]
["NE161","Sheridan","Els fine sand, calcareous, 0 to 3 percent slopes","Somewhat poorly drained","A",1,94.050000000000011,7.9]
["NE161","Sheridan","Els, calcareous-Hoffland complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,93.2,7.9]
["NE161","Sheridan","Els, calcareous-Ipage complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,94.9,7.0500000000000007]
["NE161","Sheridan","Els, calcareous-Selia fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,93.2,8.1]
["NE161","Sheridan","Els, calcareous-Tryon complex, 0 to 3 percent slopes","Somewhat poorly drained","A",1.25,94.050000000000011,7.45]
["NE161","Sheridan","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE161","Sheridan","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1.125,91.8,6.6]
["NE161","Sheridan","Enning-Minnequa complex, 6 to 20 percent slopes","Well drained","D",0.375,6.8,7.7]
["NE161","Sheridan","Enning-Rock outcrop complex, 11 to 40 percent slopes","Well drained","D",0.25,9.6,3.75]
["NE161","Sheridan","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,40.85,3.75]
["NE161","Sheridan","Gannett loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,67.5,7.5]
["NE161","Sheridan","Haverson loam, frequently flooded","Well drained","B",1,51.5,7.9]
["NE161","Sheridan","Hoffland fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,93.2,7.5]
["NE161","Sheridan","Hoffland fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7.5]
["NE161","Sheridan","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.6,6.2]
["NE161","Sheridan","Ipage fine sand, calcareous, 0 to 3 percent slopes","Moderately well drained","A",0.25,94.9,7.5]
["NE161","Sheridan","Ipage loamy fine sand, alkali substratum, 0 to 3 percent slopes","Moderately well drained","A",0.5,79,8]
["NE161","Sheridan","Jayem fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,67.5,7.2]
["NE161","Sheridan","Jayem fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,67.5,7.2]
["NE161","Sheridan","Jayem fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,67.5,7.2]
["NE161","Sheridan","Johnstown loam, 0 to 2 percent slopes","Well drained","B",0.75,34.150000000000006,7.1]
["NE161","Sheridan","Kadoka silt loam, 0 to 2 percent slopes","Well drained","C",1,6.9,7.2]
["NE161","Sheridan","Kadoka silt loam, 2 to 6 percent slopes","Well drained","C",1,6.9,7.2]
["NE161","Sheridan","Kadoka silt loam, 6 to 11 percent slopes","Well drained","C",1,6.9,7.2]
["NE161","Sheridan","Keith loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE161","Sheridan","Keith loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE161","Sheridan","Keith loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7]
["NE161","Sheridan","Keith loam, gravelly substratum, 0 to 1 percent slopes","Well drained","C",0.75,38.200000000000003,7.9]
["NE161","Sheridan","Keith loam, gravelly substratum, 1 to 3 percent slopes","Well drained","C",0.75,38.200000000000003,7.9]
["NE161","Sheridan","Keith loam, gravelly substratum, 3 to 6 percent slopes","Well drained","C",0.75,38.200000000000003,7.9]
["NE161","Sheridan","Keya loam, 0 to 2 percent slopes","Well drained","B",1.25,39.5,7.2]
["NE161","Sheridan","Las Animas loam, occasionally flooded","Somewhat poorly drained","C",0.75,52.8,7.9]
["NE161","Sheridan","Lodgepole silt loam, occasionally ponded","Somewhat poorly drained","C/D",1.375,27.75,7.25]
["NE161","Sheridan","Lute loam, 0 to 2 percent slopes","Somewhat poorly drained","D",0.5,59.9,8.6]
["NE161","Sheridan","Manvel silty clay loam, 3 to 6 percent slopes","Well drained","C",0.875,6.8,8.1999999999999993]
["NE161","Sheridan","Marlake fine sandy loam, frequently ponded","Very poorly drained","A/D",0.75,93.2,7.5]
["NE161","Sheridan","McCook loam, channeled, frequently flooded","Well drained","B",1.75,51.85,7.9]
["NE161","Sheridan","McCook loam, rarely flooded","Well drained","B",1.875,50.35,7.7]
["NE161","Sheridan","Minnequa silty clay loam, 6 to 12 percent slopes","Well drained","C",0.25,6.8,7.9]
["NE161","Sheridan","Mitchell-Epping complex, 9 to 30 percent slopes","Well drained","D",0.75,44.3,7.9]
["NE161","Sheridan","Munjor fine sandy loam, channeled, frequently flooded","Well drained","A",0.5,56.1,7.9]
["NE161","Sheridan","Munjor fine sandy loam, rarely flooded","Well drained","A",0.5,56.1,7.9]
["NE161","Sheridan","Oglala-Canyon complex, 3 to 6 percent slopes","Well drained","D",1,43.400000000000006,7.1]
["NE161","Sheridan","Oglala-Canyon complex, 6 to 9 percent slopes","Well drained","D",1,43.400000000000006,7.1]
["NE161","Sheridan","Oglala-Canyon complex, 9 to 30 percent slopes","Well drained","D",1,43.400000000000006,7.1]
["NE161","Sheridan","Onita silty clay loam, 0 to 1 percent slopes","Moderately well drained","C",1.75,17.399999999999999,6.7]
["NE161","Sheridan","Orella silty clay loam, 3 to 30 percent slopes","Well drained","D",0.75,18.7,7.9]
["NE161","Sheridan","Orpha loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,86.4,7.2]
["NE161","Sheridan","Orpha-Niobrara complex, 9 to 30 percent slopes","Excessively drained","D",0.375,83.15,7.35]
["NE161","Sheridan","Orpha-Niobrara loamy fine sands, 9 to 30 percent slopes","Excessively drained","D",0.375,83.15,7.35]
["NE161","Sheridan","Orpha-Rock outcrop complex, 30 to 60 percent slopes","Excessively drained","A",0.25,86.4,7.2]
["NE161","Sheridan","Ponderosa very fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,62.7,7.2]
["NE161","Sheridan","Ponderosa very fine sandy loam, 6 to 9 percent slopes","Well drained","A",0.75,62.7,7.2]
["NE161","Sheridan","Ponderosa-Tassel-Vetal complex, 6 to 30 percent slopes","Well drained","A",1.25,62.7,7.2]
["NE161","Sheridan","Rosebud loam, 1 to 3 percent slopes","Well drained","C",0.75,39.4,7.35]
["NE161","Sheridan","Satanta fine sandy loam, 1 to 3 percent slopes","Well drained","B",1.25,63.5,7.5]
["NE161","Sheridan","Satanta fine sandy loam, 3 to 6 percent slopes","Well drained","B",1.25,63.5,7.5]
["NE161","Sheridan","Satanta fine sandy loam, 6 to 9 percent slopes","Well drained","B",1.25,63.5,7.5]
["NE161","Sheridan","Satanta-Canyon complex, 12 to 20 percent slopes","Well drained","D",1.25,58.6,7.9]
["NE161","Sheridan","Satanta-Canyon complex, 6 to 12 percent slopes","Well drained","D",1.25,51.45,7.7]
["NE161","Sheridan","Tassel-Ponderosa-Rock outcrop association, 9 to 70 percent slopes","Well drained","A",0.75,62.7,7.2]
["NE161","Sheridan","Thirtynine loam, 1 to 3 percent slopes","Well drained","B",0.25,20.7,8.5]
["NE161","Sheridan","Thirtynine loam, 3 to 6 percent slopes","Well drained","B",0.25,20.7,8.5]
["NE161","Sheridan","Thirtynine loam, 6 to 9 percent slopes","Well drained","B",0.25,20.7,8.5]
["NE161","Sheridan","Tryon fine sandy loam, 0 to 3 percent slopes","Poorly drained","A/D",3.375,79.45,6.85]
["NE161","Sheridan","Tryon fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,79.45,6.85]
["NE161","Sheridan","Tuthill fine sandy loam, 0 to 3 percent slopes","Well drained","B",1,65.400000000000006,7]
["NE161","Sheridan","Tuthill fine sandy loam, 3 to 6 percent slopes","Well drained","B",1,65.400000000000006,7]
["NE161","Sheridan","Tuthill fine sandy loam, 6 to 9 percent slopes","Well drained","B",1,65.400000000000006,7]
["NE161","Sheridan","Tuthill loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.75,86.8,7.2]
["NE161","Sheridan","Tuthill loamy fine sand, 3 to 9 percent slopes","Well drained","B",0.75,86.8,7.2]
["NE161","Sheridan","Valent complex, rolling and hilly","Excessively drained","A",0.5,94.9,7.2]
["NE161","Sheridan","Valent fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE161","Sheridan","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE161","Sheridan","Valent fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE161","Sheridan","Valent loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE161","Sheridan","Valent loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE161","Sheridan","Valent loamy fine sand, 9 to 20 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE161","Sheridan","Valentine complex, rolling and hilly","Excessively drained","A",0.5,95.85,6.5]
["NE161","Sheridan","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,96.3,6.1]
["NE161","Sheridan","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,95.85,6.5]
["NE161","Sheridan","Valentine fine sand, 9 to 17 percent slopes","Excessively drained","A",0.5,95.85,6.5]
["NE161","Sheridan","Valentine fine sand, hilly","Excessively drained","A",0.5,95.85,6.5]
["NE161","Sheridan","Valentine fine sand, rolling","Excessively drained","A",0.5,95.85,6.5]
["NE161","Sheridan","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,95.85,6.5]
["NE161","Sheridan","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,83.35,6.5]
["NE161","Sheridan","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,91.35,6.5]
["NE161","Sheridan","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7]
["NE161","Sheridan","Vetal loamy fine sand, 0 to 3 percent slopes","Well drained","A",2,83.1,7.2]
["NE161","Sheridan","Wildhorse fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",1,92.95,9.1499999999999986]
["NE161","Sheridan","Wildhorse-Hoffland complex, 0 to 3 percent slopes","Poorly drained","A/D",1.25,92.95,8.6499999999999986]
["NE161","Sheridan","Wildhorse-Ipage, calcareous complex, 0 to 3 percent slopes","Moderately well drained","A",0.5,94.050000000000011,8.3000000000000007]
["NE163","Sherman",null,"",""]
["NE163","Sherman","Almeria loam, occasionally flooded","Very poorly drained","B/D",3.375,68.199999999999989,6.9]
["NE163","Sherman","Almeria soils, occasionally flooded","Poorly drained","B/D",3.375,68.949999999999989,6.9]
["NE163","Sherman","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE163","Sherman","Barney loam, channeled, frequently flooded","Very poorly drained","B/D",1.625,69.5,7.35]
["NE163","Sherman","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.599999999999994,7.5]
["NE163","Sherman","Boelus loamy fine sand, 0 to 3 percent slopes","Well drained","B",0.75,86.4,7]
["NE163","Sherman","Bolent loamy sand, occasionally flooded","Somewhat poorly drained","A",0.5,74.3,7.7]
["NE163","Sherman","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",1.125,11.3,7.45]
["NE163","Sherman","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE163","Sherman","Coly-Uly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE163","Sherman","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7]
["NE163","Sherman","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7]
["NE163","Sherman","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,33.4,3.75]
["NE163","Sherman","Gibbon silt loam, rarely flooded","Somewhat poorly drained","C",1.875,9.4499999999999993,7.9]
["NE163","Sherman","Gibbon-Saltine silt loams, rarely flooded","Somewhat poorly drained","C",0.75,11.3,8.5]
["NE163","Sherman","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE163","Sherman","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE163","Sherman","Hersh-Valentine complex, 11 to 24 percent slopes","Well drained","A",0.5,77.099999999999994,6.6]
["NE163","Sherman","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,11.3,7]
["NE163","Sherman","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE163","Sherman","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",1.25,9.4,7.2]
["NE163","Sherman","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",1.25,9.4,7.2]
["NE163","Sherman","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",1.25,9.4,7.2]
["NE163","Sherman","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.25,7.5,7.2]
["NE163","Sherman","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE163","Sherman","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE163","Sherman","Hord silt loam, 3 to 6 percent slopes","Well drained","B",0.75,8,7]
["NE163","Sherman","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE163","Sherman","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,86.4,6.5]
["NE163","Sherman","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",3.375,79.2,6.6]
["NE163","Sherman","Loup loam, frequently ponded","Very poorly drained","B/D",3.375,70.150000000000006,6.6]
["NE163","Sherman","Loup loam, occasionally flooded","Poorly drained","B/D",3.375,69.75,6.6]
["NE163","Sherman","Ronson fine sandy loam, 0 to 2 percent slopes","Well drained","B",0.75,66.099999999999994,7.3]
["NE163","Sherman","Scott silty clay loam, frequently ponded","Poorly drained","D",1.5,19.2,6.7]
["NE163","Sherman","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE163","Sherman","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE163","Sherman","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE163","Sherman","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE163","Sherman","Uly-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE163","Sherman","Ustorthents, steep","Well drained","B",0.75,10,7.9]
["NE163","Sherman","Valentine fine sand, rolling","Excessively drained","A",0.25,96.3,6.5]
["NE163","Sherman","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE163","Sherman","Valentine-Bolent complex, 0 to 6 percent slopes","Somewhat poorly drained","A",0.5,90.3,7]
["NE163","Sherman","Wann fine sandy loam, rarely flooded","Somewhat poorly drained","B",0.75,68.099999999999994,8.1999999999999993]
["NE165","Sioux",null,"",""]
["NE165","Sioux","Alice fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,64.599999999999994,7.9]
["NE165","Sioux","Alice fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,64.599999999999994,7.9]
["NE165","Sioux","Alice fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,64.599999999999994,7.9]
["NE165","Sioux","Alliance loam, 1 to 3 percent slopes","Well drained","B",0.75,11.4,7.2]
["NE165","Sioux","Alliance loam, 3 to 6 percent slopes","Well drained","B",0.75,11.4,7.2]
["NE165","Sioux","Arvada loam, 0 to 3 percent slopes","Well drained","D",0.5,30.7,8.8000000000000007]
["NE165","Sioux","Ashollow loamy very fine sand, 3 to 9 percent slopes","Well drained","A",1.125,81.8,7.9]
["NE165","Sioux","Ashollow loamy very fine sand, 9 to 20 percent slopes","Well drained","A",1.125,81.8,7.9]
["NE165","Sioux","Bahl clay, 0 to 6 percent slopes","Well drained","D",0.75,26.1,8.5]
["NE165","Sioux","Bankard loamy fine sand, channeled, frequently flooded","Somewhat excessively drained","A",0.75,78.599999999999994,7.9]
["NE165","Sioux","Bankard loamy fine sand, occasionally flooded","Somewhat excessively drained","A",0.75,78.599999999999994,7.9]
["NE165","Sioux","Bayard fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,62.5,7.9]
["NE165","Sioux","Bayard fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,62.5,7.9]
["NE165","Sioux","Bayard fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,62.5,7.9]
["NE165","Sioux","Bigwinder fine sandy loam, frequently flooded","Poorly drained","C",2,66.8,7.9]
["NE165","Sioux","Blueridge gravelly loamy sand, 20 to 50 percent slopes","Excessively drained","A",0.5,86.5,6.75]
["NE165","Sioux","Blueridge-Bayard complex, 6 to 20 percent slopes","Well drained","A",0.75,84.3,7.2]
["NE165","Sioux","Bridget very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE165","Sioux","Bridget very fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE165","Sioux","Bridget very fine sandy loam, 9 to 20 percent slopes","Well drained","B",0.75,60.7,7.9]
["NE165","Sioux","Bufton clay loam, 0 to 1 percent slopes","Well drained","C",0.75,29,8.1999999999999993]
["NE165","Sioux","Bufton clay loam, 1 to 3 percent slopes","Well drained","C",0.75,29,8.1999999999999993]
["NE165","Sioux","Bufton clay loam, 3 to 9 percent slopes","Well drained","C",0.75,29,8.1999999999999993]
["NE165","Sioux","Bufton clay loam, 9 to 20 percent slopes","Well drained","C",0.75,17.3,8.1999999999999993]
["NE165","Sioux","Busher loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.75,79.5,7]
["NE165","Sioux","Busher loamy very fine sand, 3 to 6 percent slopes","Well drained","A",0.75,79.5,7]
["NE165","Sioux","Busher loamy very fine sand, 6 to 9 percent slopes","Well drained","A",0.75,79.5,7]
["NE165","Sioux","Busher-Phiferson complex, 0 to 6 percent slopes","Well drained","A",0.5,71.150000000000006,7.1]
["NE165","Sioux","Busher-Tassel complex, 0 to 6 percent slopes","Well drained","A",1,72.05,7.25]
["NE165","Sioux","Busher-Tassel complex, 6 to 30 percent slopes","Well drained","A",1,72.05,7.25]
["NE165","Sioux","Craft loam, 0 to 2 percent slopes","Well drained","B",0.25,42.7,7.9]
["NE165","Sioux","Craft loam, channeled, frequently flooded","Well drained","B",0.75,66.849999999999994,7.9]
["NE165","Sioux","Craft loam, occasionally flooded","Well drained","B",0.25,42.7,7.9]
["NE165","Sioux","Draknab loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.875,87.5,7.75]
["NE165","Sioux","Epping silt loam, 3 to 30 percent slopes","Well drained","D",0.75,34.950000000000003,7.75]
["NE165","Sioux","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",5,81.7,7.5]
["NE165","Sioux","Glenberg fine sandy loam, 0 to 2 percent slopes","Well drained","A",1,68.05,7.9]
["NE165","Sioux","Glenberg fine sandy loam, channeled, frequently flooded","Well drained","A",1,68.05,7.9]
["NE165","Sioux","Hisle-Slickspots complex, 0 to 6 percent slopes","Well drained","D",0.875,17.100000000000001,7.6]
["NE165","Sioux","Interior silty clay, channeled, frequently flooded","Well drained","D",0.5,29.7,8.35]
["NE165","Sioux","Jayem loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.5,62.5,7.2]
["NE165","Sioux","Jayem loamy very fine sand, 3 to 6 percent slopes","Well drained","A",0.5,62.5,7.2]
["NE165","Sioux","Jayem loamy very fine sand, 6 to 9 percent slopes","Well drained","A",1.1499999999999999,71.25,7.2]
["NE165","Sioux","Keith loam, 1 to 3 percent slopes","Well drained","C",0.5,14.2,7.45]
["NE165","Sioux","Keith loam, 3 to 6 percent slopes","Well drained","C",0.5,14.2,7.45]
["NE165","Sioux","Kyle silty clay, 0 to 1 percent slopes","Well drained","D",0.75,11.4,7.9]
["NE165","Sioux","Kyle silty clay, 1 to 6 percent slopes","Well drained","D",0.75,11.4,7.9]
["NE165","Sioux","Las Animas fine sandy loam, channeled, frequently flooded","Somewhat poorly drained","B",1,63,7.9]
["NE165","Sioux","Las Animas fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,74.95,7.9]
["NE165","Sioux","Las Animas-Lisco complex, occasionally flooded","Somewhat poorly drained","B",0.25,63.5,8.5]
["NE165","Sioux","Lisco very fine sandy loam, occasionally flooded","Somewhat poorly drained","C",0.25,64.400000000000006,9.1]
["NE165","Sioux","Lohmiller silty clay loam, channeled, frequently flooded","Well drained","C",1,17.149999999999999,7.7]
["NE165","Sioux","Lohmiller silty clay loam, rarely flooded","Well drained","C",1.25,7.1999999999999993,7.5]
["NE165","Sioux","Lohmiller silty clay, occasionally flooded","Well drained","D",1,7.45,7.7]
["NE165","Sioux","Mitchell silt loam, 0 to 1 percent slopes","Well drained","B",1,27.25,7.9]
["NE165","Sioux","Mitchell silt loam, 1 to 3 percent slopes","Well drained","B",1,27.25,7.9]
["NE165","Sioux","Mitchell silt loam, 3 to 6 percent slopes","Well drained","B",1,27.25,7.9]
["NE165","Sioux","Mitchell silt loam, 6 to 9 percent slopes","Well drained","B",1,27.25,7.9]
["NE165","Sioux","Mitchell silt loam, 9 to 20 percent slopes","Well drained","B",1,27.25,7.9]
["NE165","Sioux","Mitchell very fine sandy loam, 0 to 1 percent slopes","Well drained","B",1,51.1,7.9]
["NE165","Sioux","Mitchell very fine sandy loam, 1 to 3 percent slopes","Well drained","B",1,51.1,7.9]
["NE165","Sioux","Mitchell very fine sandy loam, 3 to 6 percent slopes","Well drained","B",1,51.1,7.9]
["NE165","Sioux","Mitchell-Epping complex, 3 to 9 percent slopes","Well drained","D",0.75,43.2,7.9]
["NE165","Sioux","Mitchell-Epping complex, 9 to 30 percent slopes","Well drained","D",0.75,30.1,7.9]
["NE165","Sioux","Norrest clay loam, 1 to 3 percent slopes","Well drained","C",0.75,7.1,7.9]
["NE165","Sioux","Norrest clay loam, 3 to 9 percent slopes","Well drained","C",0.75,7.1,7.9]
["NE165","Sioux","Norrest silty clay loam, 9 to 20 percent slopes","Well drained","C",0.5,7.1,7.9]
["NE165","Sioux","Oglala very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,44.1,7]
["NE165","Sioux","Oglala very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.75,44.1,7]
["NE165","Sioux","Oglala very fine sandy loam, 6 to 9 percent slopes","Well drained","B",0.75,44.1,7]
["NE165","Sioux","Oglala-Canyon complex, 3 to 9 percent slopes","Well drained","D",1,52.2,7.1]
["NE165","Sioux","Oglala-Canyon complex, 9 to 30 percent slopes","Well drained","D",1,52.2,7.1]
["NE165","Sioux","Olney loam, 3 to 9 percent slopes","Well drained","B",0.75,55.8,7.2]
["NE165","Sioux","Orella clay, 1 to 30 percent slopes","Well drained","D",0.75,21.6,7.9]
["NE165","Sioux","Otero loamy very fine sand, 0 to 3 percent slopes","Well drained","A",0.625,73.25,7.9]
["NE165","Sioux","Pathfinder loamy fine sand, rarely flooded","Somewhat excessively drained","A",0.75,88.1,8.5]
["NE165","Sioux","Phiferson-Tassel-Rock outcrop complex, 6 to 30 percent slopes","Well drained","B",0.25,62.8,7.2]
["NE165","Sioux","Pierre clay, 1 to 6 percent slopes","Well drained","D",0.5,17.100000000000001,7]
["NE165","Sioux","Pierre clay, 6 to 20 percent slopes","Well drained","D",0.5,17.100000000000001,7]
["NE165","Sioux","Ponderosa loamy very fine sand, 6 to 9 percent slopes","Well drained","A",0.75,63.3,7.2]
["NE165","Sioux","Ponderosa loamy very fine sand, 9 to 20 percent slopes","Well drained","A",0.75,63.3,7.2]
["NE165","Sioux","Ponderosa-Tassel-Vetal complex, 6 to 30 percent slopes","Well drained","A",1.25,63.949999999999996,7.1]
["NE165","Sioux","Samsil-Pierre complex, 3 to 30 percent slopes","Well drained","D",0.5,16.649999999999999,7.25]
["NE165","Sioux","Sarben loamy very fine sand, 3 to 9 percent slopes","Well drained","A",1,82.75,6.95]
["NE165","Sioux","Sarben loamy very fine sand, 9 to 30 percent slopes","Well drained","A",1,82.75,6.95]
["NE165","Sioux","Sarben-Busher complex, 0 to 3 percent slopes","Well drained","A",0.75,79.75,7.1]
["NE165","Sioux","Sarben-Busher complex, 3 to 9 percent slopes","Well drained","A",0.75,79.75,7.1]
["NE165","Sioux","Satanta very fine sandy loam, 1 to 3 percent slopes","Well drained","C",1.25,63.5,7.5]
["NE165","Sioux","Satanta very fine sandy loam, 3 to 6 percent slopes","Well drained","C",1.25,63.5,7.5]
["NE165","Sioux","Savo silty clay loam, 0 to 3 percent slopes","Well drained","C",1.25,18.850000000000001,7.45]
["NE165","Sioux","Savo silty clay loam, 3 to 6 percent slopes","Well drained","C",2,17.8,7]
["NE165","Sioux","Schamber gravelly sandy loam, 3 to 30 percent slopes","Excessively drained","A",0.875,78.05,7.6]
["NE165","Sioux","Scoville fine sand, 0 to 1 percent slopes","Somewhat excessively drained","A",0.25,94.4,7.2]
["NE165","Sioux","Scoville fine sand, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,94.4,7.2]
["NE165","Sioux","Scoville loamy fine sand, 0 to 1 percent slopes","Somewhat excessively drained","B",0.25,78.599999999999994,7.2]
["NE165","Sioux","Scoville loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","B",0.25,78.599999999999994,7.2]
["NE165","Sioux","Skilak silty clay loam, 6 to 20 percent slopes","Well drained","C",0.875,7.1,8.1999999999999993]
["NE165","Sioux","Tassel-Ashollow-Rock outcrop complex, 9 to 60 percent slopes","Well drained","A",1,73.199999999999989,7.9]
["NE165","Sioux","Tassel-Busher-Rock outcrop complex, 6 to 30 percent slopes","Well drained","A",0.75,64.599999999999994,7]
["NE165","Sioux","Tassel-Ponderosa-Rock outcrop association, 9 to 70 percent slopes","Well drained","A",0.75,63.3,7.2]
["NE165","Sioux","Thirtynine loam, 1 to 3 percent slopes","Well drained","B",0.5,9.5,7.9]
["NE165","Sioux","Thirtynine loam, 3 to 6 percent slopes","Well drained","B",0.5,9.5,7.9]
["NE165","Sioux","Thirtynine loam, 6 to 9 percent slopes","Well drained","B",0.5,9.5,7.9]
["NE165","Sioux","Tripp very fine sandy loam, 0 to 1 percent slopes","Well drained","B",0.75,13.9,7.5]
["NE165","Sioux","Tripp very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.75,13.9,7.5]
["NE165","Sioux","Valent complex, rolling and hilly","Excessively drained","A",0.5,94.9,7.2]
["NE165","Sioux","Valent fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE165","Sioux","Valent fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,94.9,7.2]
["NE165","Sioux","Valent fine sand, rolling","Excessively drained","A",0.5,94.9,7.2]
["NE165","Sioux","Valent loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,90.6,7.2]
["NE165","Sioux","Valent loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,89.45,7.2]
["NE165","Sioux","Vetal fine sandy loam, 0 to 3 percent slopes","Well drained","A",1.25,66.099999999999994,7.3]
["NE165","Sioux","Vetal very fine sandy loam, 1 to 3 percent slopes","Well drained","A",1.25,65.900000000000006,7.3]
["NE165","Sioux","Vetal very fine sandy loam, 3 to 6 percent slopes","Well drained","A",1.25,65.900000000000006,7.3]
["NE165","Sioux","Wildhorse loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,88.85,9.1499999999999986]
["NE167","Stanton",null,"",""]
["NE167","Stanton","Alcester silty clay loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE167","Stanton","Barney loam, frequently flooded","Poorly drained","B/D",0.25,80,7.5]
["NE167","Stanton","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE167","Stanton","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",0.75,66.099999999999994,7.3]
["NE167","Stanton","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.599999999999994,7.5]
["NE167","Stanton","Boel loam, occasionally flooded","Somewhat poorly drained","C",1.125,69.2,7.5]
["NE167","Stanton","Boelus loamy fine sand, 2 to 6 percent slopes","Well drained","B",0.25,24,7]
["NE167","Stanton","Cass fine sandy loam, occasionally flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE167","Stanton","Cass fine sandy loam, rarely flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE167","Stanton","Clarno loam, 2 to 6 percent slopes","Well drained","C",0.5,38.5,7.9]
["NE167","Stanton","Clarno loam, 6 to 11 percent slopes","Well drained","C",0.5,38.5,7.9]
["NE167","Stanton","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE167","Stanton","Crofton silt loam, 17 to 30 percent slopes","Somewhat excessively drained","B",0.75,10.350000000000001,7.9]
["NE167","Stanton","Crofton silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE167","Stanton","Crofton silt loam, 30 to 60 percent slopes","Excessively drained","B",0.75,10.350000000000001,7.9]
["NE167","Stanton","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE167","Stanton","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE167","Stanton","Crofton silt loam, coarse, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE167","Stanton","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE167","Stanton","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A/D",0.25,86.8,6.5]
["NE167","Stanton","Fluvaquents, frequently flooded","Very poorly drained","A/D",2.5,23.5,3.75]
["NE167","Stanton","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.4,7.9]
["NE167","Stanton","Hadar loamy fine sand, 2 to 6 percent slopes","Well drained","C",0.75,85.3,6.1]
["NE167","Stanton","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE167","Stanton","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE167","Stanton","Inavale loamy fine sand, occasionally flooded","Somewhat excessively drained","A",0.25,92.2,6.7]
["NE167","Stanton","Inavale-Boel complex, 0 to 6 percent slopes, occasionally flooded","Somewhat poorly drained","C",0.25,92.2,7.5]
["NE167","Stanton","Inavale-Boel complex, channeled, occasionally flooded","Somewhat poorly drained","C",0.25,92.2,7.5]
["NE167","Stanton","Kezan silt loam, frequently flooded","Poorly drained","C",1.875,7.85,7.35]
["NE167","Stanton","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE167","Stanton","Lawet silty clay loam, rarely flooded","Poorly drained","B/D",1.25,54.4,7.9]
["NE167","Stanton","Loretto fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE167","Stanton","Loretto fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.5,39.1,6.5]
["NE167","Stanton","Loretto loam, 2 to 6 percent slopes","Well drained","B",1.5,39.1,6.5]
["NE167","Stanton","Loup fine sandy loam, occasionally flooded","Poorly drained","A/D",3.375,79.2,6.6]
["NE167","Stanton","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,6.5]
["NE167","Stanton","Moody silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE167","Stanton","Muir silty clay loam, rarely flooded","Well drained","B",2,9,6.7]
["NE167","Stanton","Nora silty clay loam, 11 to 17 percent slopes","Well drained","B",0.75,8.9,7]
["NE167","Stanton","Nora silty clay loam, 6 to 11 percent slopes","Well drained","B",0.75,8.9,7]
["NE167","Stanton","Nora-Crofton complex, 2 to 6 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE167","Stanton","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE167","Stanton","Obert silty clay loam, frequently ponded","Very poorly drained","C/D",2.25,7.1,7.9]
["NE167","Stanton","Ord fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.75,62.5,7.5]
["NE167","Stanton","Ord loam, occasionally flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE167","Stanton","Ord silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE167","Stanton","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,6.7]
["NE167","Stanton","Ovina loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","C",0.75,63.5,7.9]
["NE167","Stanton","Riverwash","Very poorly drained","A/D",0.15000000000000002,95.45,7.9]
["NE167","Stanton","Shell loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE167","Stanton","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE167","Stanton","Shell silty clay loam, 0 to 1 percent slopes","Well drained","C",0.75,9.1,6.5]
["NE167","Stanton","Shell variant silty clay loam, 0 to 1 percent slopes","Moderately well drained","C",0.75,6.9,6.7]
["NE167","Stanton","Thurman loamy fine sand, 1 to 3 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE167","Stanton","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE167","Stanton","Thurman loamy fine sand, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE167","Stanton","Thurman loamy fine sand, thick, 0 to 2 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE167","Stanton","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE167","Stanton","Valentine fine sand, 9 to 24 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE167","Stanton","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.75,6.6]
["NE169","Thayer",null,"",""]
["NE169","Thayer","Benfield silty clay loam, 6 to 11 percent slopes, eroded","Well drained","D",1.5,7.7,7.4]
["NE169","Thayer","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","D",1.125,15,7.1]
["NE169","Thayer","Cass fine sandy loam, occasionally flooded","Well drained","A",0.75,67.599999999999994,7.3]
["NE169","Thayer","Cass loam, occasionally flooded","Well drained","B",0.75,63.5,7.3]
["NE169","Thayer","Cass very fine sandy loam, rarely flooded","Well drained","A",0.75,63.5,7.3]
["NE169","Thayer","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE169","Thayer","Crete silt loam, 1 to 3 percent slopes","Moderately well drained","C",1.625,18.149999999999999,6.25]
["NE169","Thayer","Crete silty clay loam, 1 to 3 percent slopes","Moderately well drained","C",1.25,17.600000000000001,6.7]
["NE169","Thayer","Crete silty clay loam, 3 to 7 percent slopes, eroded","Moderately well drained","C",1.625,18.149999999999999,6.25]
["NE169","Thayer","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,23.5,7.2]
["NE169","Thayer","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1.125,12.649999999999999,7.1]
["NE169","Thayer","Geary and Jansen soils, 11 to 30 percent slopes","Well drained","C",1.25,20.3,6.2]
["NE169","Thayer","Geary and Jansen soils, 7 to 11 percent slopes","Well drained","C",1.25,25.35,6.2]
["NE169","Thayer","Geary and Jansen soils, 7 to 11 percent slopes, eroded","Well drained","C",1.25,19.200000000000003,6.2]
["NE169","Thayer","Geary and Jansen soils, 7 to 11 percent slopes, severely eroded","Well drained","C",0.5,31.849999999999998,6.35]
["NE169","Thayer","Geary silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.25,6.7,7]
["NE169","Thayer","Geary silty clay loam, 11 to 30 percent slopes","Well drained","C",1.25,6.9,6.7]
["NE169","Thayer","Geary silty clay loam, 11 to 30 percent slopes, severely eroded","Well drained","C",0.25,6.7,7]
["NE169","Thayer","Geary silty clay loam, 3 to 11 percent slopes, severely eroded","Well drained","C",0.25,6.7,7]
["NE169","Thayer","Geary silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,6.9,6.7]
["NE169","Thayer","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.7]
["NE169","Thayer","Geary silty clay loam, 7 to 11 percent slopes, severely eroded","Well drained","C",0.25,6.7,7]
["NE169","Thayer","Geary-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",1.75,10.4,7]
["NE169","Thayer","Geary-Uly complex, 11 to 30 percent slopes","Well drained","C",1,9.3000000000000007,7]
["NE169","Thayer","Gothenburg loamy sand, frequently flooded","Poorly drained","A/D",0.5,88,7.35]
["NE169","Thayer","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE169","Thayer","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.75,13.100000000000001,6.3]
["NE169","Thayer","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.75,13.100000000000001,6.3]
["NE169","Thayer","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",1.75,13.100000000000001,6.3]
["NE169","Thayer","Hastings silt loam, 7 to 11 percent slopes","Well drained","C",1.75,13.100000000000001,6.3]
["NE169","Thayer","Hastings silty clay loam, 0 to 1 percent slopes","Well drained","C",0.5,18.5,6.5]
["NE169","Thayer","Hastings silty clay loam, 3 to 11 percent slopes, severely eroded","Well drained","C",0.75,20,7.3]
["NE169","Thayer","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.5,18.5,6.5]
["NE169","Thayer","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.5,18.5,6.5]
["NE169","Thayer","Hastings soils, eroded","Well drained","C",0.75,18.100000000000001,6.5]
["NE169","Thayer","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE169","Thayer","Hobbs silt loam, channeled, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE169","Thayer","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE169","Thayer","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE169","Thayer","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE169","Thayer","Jansen loam, 6 to 11 percent slopes","Well drained","B",1.25,57,6.2]
["NE169","Thayer","Jansen sandy clay loam, 6 to 11 percent slopes, eroded","Well drained","B",1.25,63.8,6.2]
["NE169","Thayer","Jansen-Meadin complex, 11 to 30 percent slopes, eroded","Well drained","B",0.75,65.3,6.2]
["NE169","Thayer","Jansen-Meadin complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,65.3,6.2]
["NE169","Thayer","Kipson silt loam, 7 to 30 percent slopes","Somewhat excessively drained","D",0.75,23.5,7.9]
["NE169","Thayer","Kipson soils, 11 to 30 percent slopes","Somewhat excessively drained","D",0.75,23.5,7.9]
["NE169","Thayer","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,7.9]
["NE169","Thayer","Lancaster loam, 7 to 16 percent slopes, severely eroded","Well drained","C",1.125,39.5,6.3]
["NE169","Thayer","Lancaster soils, 7 to 11 percent slopes, severely eroded","Well drained","C",1.5,35.200000000000003,6.1]
["NE169","Thayer","Meadin loam, 2 to 30 percent slopes","Excessively drained","A",0.75,65.3,6.2]
["NE169","Thayer","Meadin loam, 6 to 30 percent slopes","Excessively drained","B",0.75,65.3,6.2]
["NE169","Thayer","Muir silt loam, 1 to 3 percent slopes","Well drained","B",2,9,6.7]
["NE169","Thayer","Muir silt loam, 3 to 7 percent slopes, eroded","Well drained","B",2,9,6.7]
["NE169","Thayer","Muir silt loam, rarely flooded","Well drained","B",2,9,6.7]
["NE169","Thayer","Muir-Meadin complex, 0 to 3 percent slopes","Excessively drained","A",1.125,27.25,6.6]
["NE169","Thayer","Roxbury silty clay loam, rarely flooded","Moderately well drained","C",2,7.3,7.9]
["NE169","Thayer","Scott soils, frequently ponded","Poorly drained","D",1.125,23.4,7.1]
["NE169","Thayer","Uly silt loam, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE169","Thayer","Uly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,11.2,7]
["NE169","Thayer","Wakeen and Kipson silty clay loams, 6 to 11 percent slopes","Somewhat excessively drained","D",0.75,7.1,7.9]
["NE169","Thayer","Wakeen and Kipson variant silty clay loams, 6 to 11 percent slopes, severely eroded","Somewhat excessively drained","D",0.75,7.1,7.9]
["NE169","Thayer","Wakeen silty clay loam, 12 to 30 percent slopes","Well drained","C",0.75,6.9,7.9]
["NE171","Thomas",null,"",""]
["NE171","Thomas","Almeria fine sandy loam, occasionally flooded","Poorly drained","A/D",3.375,78.5,6.9]
["NE171","Thomas","Bolent-Almeria complex, channeled, frequently flooded","Very poorly drained","B/D",0.52500000000000002,89.5,7.4]
["NE171","Thomas","Bolent-Calamus loamy sands, rarely flooded","Somewhat poorly drained","B",0.27500000000000002,91,7.25]
["NE171","Thomas","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,86.8,6.7]
["NE171","Thomas","Dunday loamy fine sand, 3 to 9 percent slopes","Somewhat excessively drained","A",0.75,86.8,6.7]
["NE171","Thomas","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",37.5,45,6.65]
["NE171","Thomas","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.95]
["NE171","Thomas","Jansen fine sandy loam, 0 to 2 percent slopes","Well drained","B",0.75,67,6.2]
["NE171","Thomas","Josburg-Dunn complex, 9 to 20 percent slopes","Moderately well drained","A",0.47499999999999998,68.5,6.5]
["NE171","Thomas","Josburg-Dunn loamy fine sands, 0 to 2 percent slopes","Moderately well drained","A",0.47499999999999998,68.5,6.5]
["NE171","Thomas","Meadin loamy sand, 0 to 2 percent slopes","Excessively drained","A",1,84,6.2]
["NE171","Thomas","Meadin loamy sand, 2 to 30 percent slopes","Excessively drained","A",1,84,6.2]
["NE171","Thomas","Mullen loamy fine sand, 0 to 3 percent slopes","Well drained","B",1.125,79.050000000000011,6.95]
["NE171","Thomas","Natick sand, 0 to 3 percent slopes","Moderately well drained","A",0.57499999999999996,93.5,6.4]
["NE171","Thomas","Pivot loamy sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.75,85,6.5]
["NE171","Thomas","Simeon sand, 0 to 3 percent slopes","Excessively drained","A",0.5,92,7]
["NE171","Thomas","Simeon-Valentine complex, 0 to 9 percent slopes","Excessively drained","A",0.5,93,6.5]
["NE171","Thomas","Simeon-Valentine complex, 11 to 30 percent slopes","Excessively drained","A",0.5,93,6.5]
["NE171","Thomas","Thedford fine sand, 0 to 3 percent slopes","Moderately well drained","A",1.375,91.5,7.9]
["NE171","Thomas","Valentine fine sand, hilly","Excessively drained","A",0.5,94.9,6.5]
["NE171","Thomas","Valentine fine sand, rolling","Excessively drained","A",0.5,94.9,6.5]
["NE171","Thomas","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,94.9,6.5]
["NE171","Thomas","Valentine-Birdwood complex, 9 to 80 percent slopes","Well drained","A",0.625,85.8,6.5]
["NE171","Thomas","Valentine-Dunday complex, 0 to 9 percent slopes","Somewhat excessively drained","A",0.625,94,6.6]
["NE171","Thomas","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.625,95.4,6.5]
["NE171","Thomas","Valentine-Libory complex, 0 to 9 percent slopes","Moderately well drained","B",0.625,90.05,6.55]
["NE171","Thomas","Valentine-Mullen complex, 0 to 9 percent slopes","Well drained","B",0.75,86,6.7]
["NE173","Thurston",null,"",""]
["NE173","Thurston","Albaton silty clay loam, occasionally flooded","Poorly drained","D",1.5,10.6,7.6]
["NE173","Thurston","Albaton silty clay, frequently flooded","Very poorly drained","D",2.5,2.2999999999999998,7.9]
["NE173","Thurston","Albaton silty clay, occasionally flooded","Poorly drained","D",1.5,3.9,7.6]
["NE173","Thurston","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE173","Thurston","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,17.8,6.5]
["NE173","Thurston","Belfore-Moody silty clay loams, 0 to 1 percent slopes","Well drained","C",1.875,8.8000000000000007,6.75]
["NE173","Thurston","Belfore-Moody silty clay loams, 1 to 3 percent slopes","Well drained","C",1.875,10.1,6.5]
["NE173","Thurston","Burchard clay loam, 11 to 17 percent slopes, eroded","Well drained","C",0.75,35.4,6.7]
["NE173","Thurston","Burchard clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,36.5,6.7]
["NE173","Thurston","Burchard silt loam, 11 to 17 percent slopes","Well drained","C",0.75,35.4,6.7]
["NE173","Thurston","Burchard silt loam, 6 to 11 percent slopes","Well drained","C",0.75,35.4,7.9]
["NE173","Thurston","Calco silt loam, overwash, occasionally flooded","Poorly drained","C/D",4,7.1,7.9]
["NE173","Thurston","Calco silty clay loam, occasionally flooded","Poorly drained","C/D",4,6.9,7.9]
["NE173","Thurston","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE173","Thurston","Colo and Lamo silty clay loams, occasionally flooded","Somewhat poorly drained","C",2,6.8,7.5]
["NE173","Thurston","Colo silty clay loam, occasionally flooded","Poorly drained","C/D",3.5,6.9,6.5]
["NE173","Thurston","Crofton silt loam, 1 to 6 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,8.5]
["NE173","Thurston","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,8.5]
["NE173","Thurston","Crofton silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,7.9]
["NE173","Thurston","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,10.350000000000001,8.5]
["NE173","Thurston","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE173","Thurston","Fluvaquents, frequently flooded","Very poorly drained","A/D",2.5,44.85,3.75]
["NE173","Thurston","Gullied land-Ida complex, 30 to 60 percent slopes","Well drained","B",0.5,10.35,7.7]
["NE173","Thurston","Haynie silt loam, occasionally flooded","Well drained","B",1.25,12.600000000000001,7.9]
["NE173","Thurston","Haynie silt loam, rarely flooded","Well drained","B",1.25,12.600000000000001,8.1999999999999993]
["NE173","Thurston","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,10.4,7.25]
["NE173","Thurston","Hobbs silt loam, frequently flooded","Well drained","B",1.875,11.3,7]
["NE173","Thurston","Ida silt loam, 11 to 17 percent slopes","Well drained","B",1.375,11.2,8.1999999999999993]
["NE173","Thurston","Ida silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.375,11.2,8.1999999999999993]
["NE173","Thurston","Ida silt loam, 17 to 30 percent slopes","Well drained","B",1.375,11.2,8.1999999999999993]
["NE173","Thurston","Ida silt loam, 17 to 30 percent slopes, eroded","Well drained","B",1.375,11.2,8.1999999999999993]
["NE173","Thurston","Ida silt loam, 30 to 60 percent slopes","Well drained","B",0.5,9.5,8.1999999999999993]
["NE173","Thurston","Ida silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.375,11.2,8.1999999999999993]
["NE173","Thurston","Ida soils, 30 to 60 percent slopes","Well drained","B",0.5,9.5,8.1999999999999993]
["NE173","Thurston","Judson silt loam, 0 to 2 percent slopes","Well drained","C",2.5,7.1,6.3]
["NE173","Thurston","Judson silt loam, 2 to 6 percent slopes","Well drained","C",2.5,7.1,6.3]
["NE173","Thurston","Judson silty clay loam, 2 to 6 percent slopes","Well drained","C",2.5,7,7]
["NE173","Thurston","Kennebec silt loam, occasionally flooded","Moderately well drained","B",3.5,9.1499999999999986,6.6]
["NE173","Thurston","Kennebec silt loam, overwash, occasionally flooded","Moderately well drained","B",3.5,9.1499999999999986,7.4]
["NE173","Thurston","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,9.1499999999999986,6.65]
["NE173","Thurston","Lamo silt loam, overwash, occasionally flooded","Somewhat poorly drained","C",1.375,7.95,8.1999999999999993]
["NE173","Thurston","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,7.1,8.1999999999999993]
["NE173","Thurston","Leisy fine sandy loam, 6 to 11 percent slopes","Well drained","C",1.625,43.65,6.5]
["NE173","Thurston","Luton silty clay loam, rarely flooded","Poorly drained","D",0.5,5.3,8.1999999999999993]
["NE173","Thurston","Luton silty clay, rarely flooded","Poorly drained","D",0.5,5.3,8.1999999999999993]
["NE173","Thurston","McPaul silt loam, occasionally flooded","Well drained","B",1.5,14.2,8.1999999999999993]
["NE173","Thurston","Monona silt loam, 1 to 6 percent slopes","Well drained","B",1.25,9.4,7]
["NE173","Thurston","Monona silt loam, 1 to 6 percent slopes, eroded","Well drained","B",1.25,9.4,7]
["NE173","Thurston","Monona silt loam, 11 to 17 percent slopes","Well drained","B",1.25,9.4,7]
["NE173","Thurston","Monona silt loam, 11 to 17 percent slopes, eroded","Well drained","B",1.25,9.4,7]
["NE173","Thurston","Monona silt loam, 17 to 30 percent slopes","Well drained","B",1.25,9.4,7]
["NE173","Thurston","Monona silt loam, 6 to 11 percent slopes","Well drained","B",1.25,9.4,7]
["NE173","Thurston","Monona silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.4,7]
["NE173","Thurston","Moody silty clay loam, 0 to 1 percent slopes","Well drained","C",3,6.9,7]
["NE173","Thurston","Moody silty clay loam, 0 to 2 percent slopes","Well drained","C",3,6.9,6.5]
["NE173","Thurston","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,6.9,7]
["NE173","Thurston","Moody silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",3,6.9,7]
["NE173","Thurston","Moody silty clay loam, 6 to 11 percent slopes","Well drained","C",3,6.9,7]
["NE173","Thurston","Moody silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",3,6.9,7]
["NE173","Thurston","Nora silt loam, 1 to 6 percent slopes, eroded","Well drained","C",0.75,9.3000000000000007,7.8]
["NE173","Thurston","Nora silt loam, 11 to 17 percent slopes","Well drained","C",0.75,9.3000000000000007,7.8]
["NE173","Thurston","Nora silt loam, 11 to 17 percent slopes, eroded","Well drained","C",1.25,9.1,7.8]
["NE173","Thurston","Nora silt loam, 17 to 30 percent slopes","Well drained","C",0.75,9.3000000000000007,7]
["NE173","Thurston","Nora silt loam, 17 to 30 percent slopes, eroded","Well drained","C",0.75,9.3000000000000007,7.8]
["NE173","Thurston","Nora silt loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,9.1,6.6]
["NE173","Thurston","Nora silt loam, 6 to 11 percent slopes","Well drained","C",0.75,9.3000000000000007,7.8]
["NE173","Thurston","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,9.1,8]
["NE173","Thurston","Nora silty clay loam, 11 to 17 percent slopes","Well drained","C",0.75,8.9,7]
["NE173","Thurston","Nora silty clay loam, 11 to 17 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE173","Thurston","Nora silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE173","Thurston","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE173","Thurston","Nora silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE173","Thurston","Nora variant silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE173","Thurston","Nora-Moody silty clay loams, 6 to 11 percent slopes","Well drained","C",1.875,7,6.85]
["NE173","Thurston","Omadi silt loam, rarely flooded","Moderately well drained","B",1.125,10.45,7.6]
["NE173","Thurston","Onawa and Haynie soils, occasionally flooded","Well drained","B",0.5,13.8,8.1999999999999993]
["NE173","Thurston","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.6]
["NE173","Thurston","Onawet silty clay loam, frequently flooded","Very poorly drained","D",0.75,29.3,7.9]
["NE173","Thurston","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,63.5,7]
["NE173","Thurston","Ortello fine sandy loam, 6 to 11 percent slopes, eroded","Well drained","A",0.75,63.5,7]
["NE173","Thurston","Pohocco silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.4,7.2]
["NE173","Thurston","Riverwash","Very poorly drained","A/D",0.15000000000000002,47.05,7.9]
["NE173","Thurston","Sarpy fine sand, 3 to 11 percent slopes","Excessively drained","A",0.5,95.9,8]
["NE173","Thurston","Sarpy loamy fine sand, occasionally flooded","Excessively drained","A",0.5,87.9,8]
["NE173","Thurston","Sarpy soils, occasionally flooded","Excessively drained","A",0.75,80.550000000000011,7.85]
["NE173","Thurston","Steinauer clay loam, 11 to 30 percent slopes, eroded","Well drained","C",0.75,33.6,7.9]
["NE173","Thurston","Steinauer soils, 11 to 30 percent slopes","Well drained","C",0.75,33.6,8.1999999999999993]
["NE173","Thurston","Thurman loamy sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.3]
["NE173","Thurston","Thurman soils, 6 to 17 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.3]
["NE173","Thurston","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",3,7.9,6.7]
["NE173","Thurston","Zook silty clay, occasionally flooded","Poorly drained","D",3,7.9,6.7]
["NE175","Valley",null,"",""]
["NE175","Valley","Barney loam, channeled, frequently flooded","Poorly drained","B/D",1.625,46.099999999999994,7.5]
["NE175","Valley","Blendon fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,66.099999999999994,6.7]
["NE175","Valley","Boel fine sandy loam, occasionally flooded","Somewhat poorly drained","B",0.875,81.599999999999994,7.5]
["NE175","Valley","Boel loamy fine sand, occasionally flooded","Somewhat poorly drained","A",0.875,91.8,7.5]
["NE175","Valley","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.125,15,7.1]
["NE175","Valley","Coly-Hobbs silt loams, 3 to 17 percent slopes, eroded","Well drained","B",1.125,11.3,7.45]
["NE175","Valley","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",1.125,11.3,7.45]
["NE175","Valley","Coly-Hobbs silt loams, 3 to 60 percent slopes, moist","Well drained","B",2,17.5,7.35]
["NE175","Valley","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE175","Valley","Cozad silt loam, 0 to 1 percent slopes","Well drained","B",0.75,14.2,7.3]
["NE175","Valley","Cozad silt loam, 1 to 3 percent slopes","Well drained","B",0.75,14.2,7.3]
["NE175","Valley","Cozad silt loam, 3 to 6 percent slopes","Well drained","B",0.75,14.2,7.3]
["NE175","Valley","Detroit silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,23.5,7.2]
["NE175","Valley","Fillmore variant silt loam, frequently ponded","Somewhat poorly drained","B/D",1.375,9.1999999999999993,7]
["NE175","Valley","Gates very fine sandy loam, 3 to 6 percent slopes, eroded","Well drained","B",0.5,58.6,7.5]
["NE175","Valley","Gates very fine sandy loam, 6 to 11 percent slopes, eroded","Well drained","B",0.5,58.6,7.5]
["NE175","Valley","Gibbon silt loam, rarely flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE175","Valley","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE175","Valley","Hersh fine sandy loam, 11 to 17 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE175","Valley","Hersh fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE175","Valley","Hersh fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE175","Valley","Histosols, wet","Very poorly drained","A/D",29.875,48.4,0]
["NE175","Valley","Hobbs silt loam, channeled, frequently flooded","Well drained","B",1.875,11.3,7]
["NE175","Valley","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE175","Valley","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE175","Valley","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE175","Valley","Holdrege silt loam, 3 to 7 percent slopes","Well drained","C",0.75,9.25,7.2]
["NE175","Valley","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.25,7.2]
["NE175","Valley","Holdrege silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.25,7.5,7.2]
["NE175","Valley","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE175","Valley","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE175","Valley","Ipage loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,90.85,6.2]
["NE175","Valley","Ipage loamy sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,89.6,6.2]
["NE175","Valley","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",1.375,11.45,7.4]
["NE175","Valley","Loup fine sandy loam, rarely flooded","Poorly drained","A/D",3.375,79.2,6.6]
["NE175","Valley","Loup loam, occasionally flooded","Poorly drained","B/D",3.375,69.75,6.6]
["NE175","Valley","Saltine-Leshara silt loams, occasionally flooded","Somewhat poorly drained","C",1,11.3,8]
["NE175","Valley","Scott silt loam, frequently ponded","Poorly drained","D",1.125,19.350000000000001,7.1]
["NE175","Valley","Simeon loamy sand, 0 to 3 percent slopes","Excessively drained","A",0.5,86.35,7]
["NE175","Valley","Simeon loamy sand, 3 to 30 percent slopes","Excessively drained","A",0.5,86.35,7]
["NE175","Valley","Uly silt loam, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE175","Valley","Uly silt loam, 11 to 17 percent slopes, eroded, moist","Well drained","B",0.69500000000000006,24.5,7.95]
["NE175","Valley","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE175","Valley","Uly-Coly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",1.125,10.35,7.45]
["NE175","Valley","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE175","Valley","Uly-Coly silt loams, 17 to 30 percent slopes, eroded, moist","Well drained","B",1,24,7.5]
["NE175","Valley","Uly-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE175","Valley","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE175","Valley","Valentine fine sand, rolling and hilly","Excessively drained","A",0.25,96.3,6.5]
["NE175","Valley","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE175","Valley","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE177","Washington",null,"",""]
["NE177","Washington","Albaton silty clay, frequently flooded","Very poorly drained","C/D",1.5,11.2,7.75]
["NE177","Washington","Albaton silty clay, occasionally flooded","Poorly drained","C/D",0.5,9.85,7.9]
["NE177","Washington","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",1.5,6,7]
["NE177","Washington","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,4.5,6.05]
["NE177","Washington","Belfore silty clay loam, terrace, 0 to 2 percent slopes","Well drained","C",0.75,4.5,6.05]
["NE177","Washington","Blyburg silty clay loam, rarely flooded","Well drained","C",1.5,14,8]
["NE177","Washington","Burchard clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,34.599999999999994,7.3000000000000007]
["NE177","Washington","Burchard-Contrary-Steinauer complex, 7 to 16 percent slopes","Well drained","C",0.75,33.5,7.45]
["NE177","Washington","Burchard-Steinauer clay loams, 11 to 17 percent slopes, eroded","Well drained","C",0.75,34.4,7.9]
["NE177","Washington","Cass fine sandy loam, occasionally flooded","Well drained","A",0.75,66.900000000000006,6.8]
["NE177","Washington","Cass loam, occasionally flooded","Well drained","B",0.75,63.5,6.8]
["NE177","Washington","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE177","Washington","Contrary-Marshall silty clay loams, 6 to 11 percent slopes","Well drained","C",1,3.5,6.3]
["NE177","Washington","Contrary-Monona silty clay loams, 6 to 11 percent slopes","Well drained","C",1,3.5,6.3]
["NE177","Washington","Contrary-Monona-Ida complex, 6 to 17 percent slopes","Well drained","C",1,3.5,7]
["NE177","Washington","Cooper silty clay loam, rarely flooded","Somewhat poorly drained","C",2,6.1,7.6]
["NE177","Washington","Crofton silt loam, 17 to 30 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE177","Washington","Crofton silt loam, 17 to 30 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE177","Washington","Crofton silt loam, 30 to 60 percent slopes","Well drained","B",0.75,10.350000000000001,7.9]
["NE177","Washington","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE177","Washington","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",1,85.7,7.2]
["NE177","Washington","Fluvaquents, silty, frequently flooded","Very poorly drained","B/D",1,11.8,7.2]
["NE177","Washington","Fontanelle silty clay loam, frequently flooded","Very poorly drained","C/D",0.75,15,7.6]
["NE177","Washington","Forney silt loam, overwash, rarely flooded","Poorly drained","C/D",1.5,3.9,7.15]
["NE177","Washington","Gilliam-Eudora silt loams, occasionally flooded","Well drained","A",1.1499999999999999,29,7.65]
["NE177","Washington","Grable silt loam, occasionally flooded","Well drained","B",0.5,14.2,7.6]
["NE177","Washington","Gullied land-Napier complex, 5 to 60 percent slopes","Well drained","B",1,3.5,7.3]
["NE177","Washington","Haynie silt loam, occasionally flooded","Well drained","B",1.25,12.600000000000001,7.65]
["NE177","Washington","Ida silt loam, 17 to 30 percent slopes, eroded","Well drained","B",1,3.5,7.9]
["NE177","Washington","Ida silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1,3.5,7.9]
["NE177","Washington","Ida-Pohocco-Monona silt loams, 11 to 30 percent slopes","Well drained","B",0.75,3.5,7.5]
["NE177","Washington","Inglewood loamy fine sand, occasionally flooded","Moderately well drained","A",0.25,87.55,7]
["NE177","Washington","Judson silty clay loam, 2 to 6 percent slopes","Well drained","C",1.25,3.5,6.3]
["NE177","Washington","Judson-Nodaway channeled-Contrary complex, 3 to 10 percent slopes","Well drained","C",1,3.5,6.3]
["NE177","Washington","Kennebec silt loam, occasionally flooded","Moderately well drained","B",2,9.1999999999999993,6.3]
["NE177","Washington","Kezan silt loam, occasionally flooded","Poorly drained","B/D",2,9.1,7.2]
["NE177","Washington","Kezan-Kennebec silt loams, drained, occasionally flooded","Moderately well drained","B",2,9.1,7.2]
["NE177","Washington","Luton silty clay, occasionally flooded","Poorly drained","D",2.25,5.3,7.35]
["NE177","Washington","Luton silty clay, rarely flooded","Poorly drained","C/D",0.875,5.3,7.6]
["NE177","Washington","Marshall silty clay loam, 0 to 2 percent slopes","Well drained","C",1.375,3.5,6.05]
["NE177","Washington","Marshall silty clay loam, 2 to 6 percent slopes","Well drained","C",1.375,3.5,6.05]
["NE177","Washington","Marshall-Contrary silty clay loams, 2 to 7 percent slopes","Well drained","C",1,3.5,6.3]
["NE177","Washington","Marshall-Pohocco silty clay loams, 6 to 11 percent slopes, eroded","Well drained","C",0.75,4.75,7]
["NE177","Washington","Monona silt loam, 2 to 6 percent slopes, eroded","Well drained","B",1.125,3.5,6.65]
["NE177","Washington","Monona silt loam, bench, 0 to 2 percent slopes","Well drained","B",1.125,3.5,6.65]
["NE177","Washington","Monona silt loam, bench, 2 to 6 percent slopes","Well drained","B",1.125,3.5,6.65]
["NE177","Washington","Monona-Ida silt loams, 17 to 30 percent slopes, eroded","Well drained","B",1,3.5,7.5]
["NE177","Washington","Monona-Pohocco complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,4.75,7]
["NE177","Washington","Monona-Pohocco-Ida silt loams, 17 to 33 percent slopes","Well drained","B",0.75,3.5,7.5]
["NE177","Washington","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",0.625,6,7.6]
["NE177","Washington","Moville silt loam, rarely flooded","Moderately well drained","C",1.75,8.35,7.6]
["NE177","Washington","Napier-Nodaway-Gullied land complex, 0 to 60 percent slopes","Well drained","B",1,3.5,7.3]
["NE177","Washington","Nora silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.625,6,7.25]
["NE177","Washington","Nora-Crofton complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.5]
["NE177","Washington","Omadi silt loam, rarely flooded","Moderately well drained","B",0.75,11.6,8.1999999999999993]
["NE177","Washington","Onawa silty clay loam, occasionally flooded","Somewhat poorly drained","D",0.5,8.1999999999999993,7.6]
["NE177","Washington","Onawa silty clay, occasionally flooded","Somewhat poorly drained","D",0.5,5.5,7.6]
["NE177","Washington","Onawa-Haynie complex, occasionally flooded","Well drained","B",0.5,11.4,7.6]
["NE177","Washington","Onawet silty clay, depressional, frequently flooded","Very poorly drained","C/D",0.75,29.3,7.6]
["NE177","Washington","Percival silty clay, occasionally flooded","Somewhat poorly drained","D",1,5.3,7.6]
["NE177","Washington","Platte loam, occasionally flooded","Somewhat poorly drained","C",1.125,60,8.1999999999999993]
["NE177","Washington","Platte, Inglewood, and Barney soils, frequently flooded","Poorly drained","C/D",0.25,74.5,7.5]
["NE177","Washington","Pohocco-Ida complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.6]
["NE177","Washington","Pohocco-Ida-Monona complex, 6 to 17 percent slopes","Well drained","B",0.75,3.5,7.5]
["NE177","Washington","Pohocco-Monona complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,4.75,7]
["NE177","Washington","Salix silty clay loam, rarely flooded","Moderately well drained","C",1.5,6.9,7]
["NE177","Washington","Sarpy fine sand, occasionally flooded","Excessively drained","A",0.5,95.9,7.25]
["NE177","Washington","Sarpy loamy fine sand, occasionally flooded","Excessively drained","A",0.5,87.9,7.25]
["NE177","Washington","Shell silt loam, occasionally flooded","Well drained","B",0.75,6.9,7]
["NE177","Washington","Wathena fine sandy loam, occasionally flooded","Moderately well drained","B",0.25,75.349999999999994,7.3000000000000007]
["NE177","Washington","Wathena fine sandy loam, rarely flooded","Moderately well drained","B",0.25,75.349999999999994,7.3000000000000007]
["NE177","Washington","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",2,7.9,6.3]
["NE179","Wayne",null,"",""]
["NE179","Wayne","Alcester silt loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE179","Wayne","Alcester silty clay loam, 2 to 6 percent slopes","Well drained","B",2.5,7.4,7]
["NE179","Wayne","Aowa silt loam, occasionally flooded","Well drained","B",1.625,21.15,7.9]
["NE179","Wayne","Belfore silty clay loam, 0 to 2 percent slopes","Well drained","C",0.75,12,6.5]
["NE179","Wayne","Belfore-Moody silty clay loams, 1 to 3 percent slopes","Well drained","C",1.875,10.1,6.5]
["NE179","Wayne","Blendon fine sandy loam, 2 to 6 percent slopes","Well drained","A",1.125,66.699999999999989,6.85]
["NE179","Wayne","Blendon fine sandy loam, clayey substratum, 1 to 6 percent slopes","Well drained","A",0.75,65,6.7]
["NE179","Wayne","Boelus loamy fine sand, 2 to 6 percent slopes","Well drained","B",0.25,24,7]
["NE179","Wayne","Coleridge silt loam, occasionally flooded","Somewhat poorly drained","C",2,6.8,6.5]
["NE179","Wayne","Coleridge silty clay loam, occasionally flooded","Somewhat poorly drained","C",2,6.9,6.5]
["NE179","Wayne","Colo and Lamo silty clay loams, occasionally flooded","Somewhat poorly drained","C",2,6.8,7.5]
["NE179","Wayne","Crofton silt loam, 2 to 6 percent slopes, eroded","Well drained","B",0.75,11.15,7.9]
["NE179","Wayne","Crofton silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,11.15,7.9]
["NE179","Wayne","Crofton silt loam, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE179","Wayne","Crofton silt loam, coarse, 8 to 17 percent slopes, eroded","Well drained","B",0.75,6,7.9]
["NE179","Wayne","Crofton-Nora complex, 11 to 17 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE179","Wayne","Crofton-Nora complex, 2 to 6 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE179","Wayne","Crofton-Nora complex, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.3000000000000007,7.5]
["NE179","Wayne","Crofton-Nora silt loams, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.4,7.5]
["NE179","Wayne","Fillmore complex, frequently ponded","Somewhat poorly drained","D",1.5,14,6.7]
["NE179","Wayne","Gibbon silty clay loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.4,7.9]
["NE179","Wayne","Hadar-Thurman complex, 6 to 11 percent slopes","Well drained","C",0.5,85.1,6.5]
["NE179","Wayne","Hadar-Thurman complex, 6 to 17 percent slopes","Well drained","C",0.5,82.1,6.5]
["NE179","Wayne","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE179","Wayne","Hord silt loam, rarely flooded","Well drained","B",0.75,9.3000000000000007,7]
["NE179","Wayne","Judson silt loam, 2 to 6 percent slopes","Well drained","C",2.5,7,6.5]
["NE179","Wayne","Kennebec silt loam, rarely flooded","Moderately well drained","B",3.5,9.9,6.6]
["NE179","Wayne","Kennebec silty clay loam, occasionally flooded","Moderately well drained","B",3.5,10.4,6.6]
["NE179","Wayne","Lamo silt loam, occasionally flooded","Somewhat poorly drained","C",1.375,9.9,7.9]
["NE179","Wayne","Lamo silty clay loam, occasionally flooded","Somewhat poorly drained","C",1.375,9.9,7.9]
["NE179","Wayne","Leisy fine sandy loam, 6 to 11 percent slopes","Well drained","C",0.75,39.200000000000003,6.5]
["NE179","Wayne","Leisy loam, 0 to 6 percent slopes","Well drained","B",0.75,39.200000000000003,6.5]
["NE179","Wayne","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.5,11.45,7.5]
["NE179","Wayne","Loretto fine sandy loam, 0 to 2 percent slopes","Well drained","A",1.5,37.200000000000003,6.5]
["NE179","Wayne","McPaul silt loam, occasionally flooded","Moderately well drained","B",1.5,28,7.9]
["NE179","Wayne","McPaul silt loam, wet, occasionally flooded","Somewhat poorly drained","C",0.25,14.2,7.9]
["NE179","Wayne","Moody silt loam, 2 to 6 percent slopes","Well drained","C",3,7,6.5]
["NE179","Wayne","Moody silty clay loam, 2 to 6 percent slopes","Well drained","C",3,7,6.5]
["NE179","Wayne","Moody silty clay loam, 6 to 11 percent slopes","Well drained","C",3,7,6.5]
["NE179","Wayne","Moody silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",3,7,6.5]
["NE179","Wayne","Muir silt loam, rarely flooded","Well drained","B",2.5,9.25,6.6]
["NE179","Wayne","Nora silt loam, 11 to 17 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE179","Wayne","Nora silt loam, 11 to 17 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE179","Wayne","Nora silt loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE179","Wayne","Nora silt loam, 6 to 11 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE179","Wayne","Nora silt loam, 6 to 11 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE179","Wayne","Nora silty clay loam, 11 to 17 percent slopes","Well drained","B",0.75,8.9,7]
["NE179","Wayne","Nora silty clay loam, 2 to 6 percent slopes, eroded","Well drained","C",1.25,6.9,6.5]
["NE179","Wayne","Nora silty clay loam, 6 to 11 percent slopes","Well drained","C",0.75,8.9,7]
["NE179","Wayne","Nora silty clay loam, 6 to 11 percent slopes, eroded","Well drained","C",0.75,8.9,7]
["NE179","Wayne","Nora-Crofton complex, 2 to 6 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE179","Wayne","Nora-Crofton complex, 6 to 11 percent slopes, eroded","Well drained","B",1.25,9.1,7.9]
["NE179","Wayne","Nora-Moody silty clay loams, 11 to 17 percent slopes","Well drained","C",1.875,7,6.85]
["NE179","Wayne","Nora-Moody silty clay loams, 6 to 11 percent slopes","Well drained","C",1.875,7,6.85]
["NE179","Wayne","Obert silt loam, frequently ponded","Very poorly drained","C/D",2.25,9.3000000000000007,7.9]
["NE179","Wayne","Obert silty clay loam, frequently ponded","Very poorly drained","C/D",1.5,7.3,7.9]
["NE179","Wayne","Ortello fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,68.5,6.7]
["NE179","Wayne","Ortello fine sandy loam, 6 to 11 percent slopes","Well drained","A",0.75,68.5,6.7]
["NE179","Wayne","Shell loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE179","Wayne","Shell silt loam, occasionally flooded","Well drained","B",0.75,9.1,6.5]
["NE179","Wayne","Shell silty clay loam, 0 to 1 percent slopes","Well drained","C",0.75,9.1,6.5]
["NE179","Wayne","Thurman fine sandy loam, 6 to 11 percent slopes","Somewhat excessively drained","A",0.25,84.9,6.5]
["NE179","Wayne","Thurman loamy fine sand, 2 to 6 percent slopes","Somewhat excessively drained","A",0.25,82.2,6.5]
["NE179","Wayne","Thurman loamy fine sand, 6 to 17 percent slopes","Somewhat excessively drained","A",0.25,82.2,6.5]
["NE179","Wayne","Thurman loamy fine sand, loamy subsoil, 2 to 6 percent slopes","Somewhat excessively drained","B",0.75,81.5,7]
["NE179","Wayne","Thurman-Valentine complex, undulating","Somewhat excessively drained","A",0.25,94,6.5]
["NE179","Wayne","Trent silty clay loam","Moderately well drained","B",2.5,6.9,6.7]
["NE179","Wayne","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.25,96.3,6.5]
["NE179","Wayne","Valentine loamy fine sand, rolling","Excessively drained","A",0.5,91.15,6.5]
["NE179","Wayne","Zook silty clay loam, occasionally flooded","Poorly drained","C/D",4.5,7.45,6.6]
["NE181","Webster",null,"",""]
["NE181","Webster","Coly silt loam, 3 to 11 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE181","Webster","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE181","Webster","Coly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",1.75,17.5,7.35]
["NE181","Webster","Coly-Uly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",0.75,11.3,7.25]
["NE181","Webster","Deroin soils, 3 to 6 percent slopes, severely eroded","Well drained","C",0.5,6.7,7]
["NE181","Webster","Deroin soils, 6 to 11 percent slopes, severely eroded","Well drained","C",0.5,6.7,7]
["NE181","Webster","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE181","Webster","Fluvaquents, frequently flooded","Very poorly drained","A/D",2.5,9.6,3.75]
["NE181","Webster","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.5,44.9,3.75]
["NE181","Webster","Geary and Hobbs soils","Well drained","C",1.75,15,6.95]
["NE181","Webster","Geary silt loam, 11 to 30 percent slopes","Well drained","C",0.65,17,6.8000000000000007]
["NE181","Webster","Geary silt loam, 3 to 7 percent slopes","Well drained","C",0.65,17,6.8000000000000007]
["NE181","Webster","Geary silt loam, 7 to 11 percent slopes","Well drained","C",0.65,17,6.8000000000000007]
["NE181","Webster","Geary-Hobbs silt loams, 0 to 30 percent slopes","Well drained","C",1.75,15,6.95]
["NE181","Webster","Geary-Uly complex, 11 to 30 percent slopes","Well drained","C",0.8,18,6.9]
["NE181","Webster","Gibbon silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,9.5,7.9]
["NE181","Webster","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE181","Webster","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE181","Webster","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE181","Webster","Hobbs silt loam, channeled, frequently flooded","Well drained","B",2,31,7.15]
["NE181","Webster","Hobbs silt loam, frequently flooded","Well drained","B",2,31,7.15]
["NE181","Webster","Hobbs silt loam, occasionally flooded","Well drained","B",2,31,7.15]
["NE181","Webster","Holdrege and Uly soils, 3 to 7 percent slopes, eroded","Well drained","C",0.75,9.4,7.2]
["NE181","Webster","Holdrege silt loam, 0 to 1 percent slopes","Well drained","C",1.25,7,7.2]
["NE181","Webster","Holdrege silt loam, 1 to 3 percent slopes","Well drained","C",1.25,7,7.2]
["NE181","Webster","Holdrege silt loam, 1 to 3 percent slopes, eroded","Well drained","C",0.8,11,7.4]
["NE181","Webster","Holdrege silt loam, 3 to 7 percent slopes, eroded","Well drained","C",1.25,7,7.2]
["NE181","Webster","Holdrege silt loam, 7 to 11 percent slopes","Well drained","C",1.25,7,7.2]
["NE181","Webster","Holdrege soils, 3 to 7 percent slopes, severely eroded","Well drained","C",0.75,6.3,7.2]
["NE181","Webster","Holdrege soils, 7 to 11 percent slopes, severely eroded","Well drained","C",0.75,6.3,7.2]
["NE181","Webster","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,7,7]
["NE181","Webster","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,11.2,7]
["NE181","Webster","Inavale fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,92.2,6.7]
["NE181","Webster","Inavale fine sandy loam, 0 to 3 percent slopes","Excessively drained","A",0.25,84.3,6.7]
["NE181","Webster","Inavale fine sandy loam, rarely flooded","Excessively drained","A",0.5,73.55,6.7]
["NE181","Webster","Inavale loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,84.3,6.7]
["NE181","Webster","Kipson complex, 7 to 30 percent slopes","Somewhat excessively drained","D",0.75,23.5,7.9]
["NE181","Webster","Kipson silt loam, 7 to 30 percent slopes","Somewhat excessively drained","D",1,13.15,3.95]
["NE181","Webster","Massie silty clay loam, frequently ponded","Very poorly drained","D",1.25,6,6.4]
["NE181","Webster","McCook silt loam, rarely flooded","Well drained","B",0.5,62.7,7.9]
["NE181","Webster","Meadin loam, 6 to 30 percent slopes","Excessively drained","B",0.75,65.7,6.2]
["NE181","Webster","Munjor fine sandy loam, rarely flooded","Well drained","A",0.25,70.900000000000006,7.9]
["NE181","Webster","Munjor loamy fine sand, rarely flooded","Well drained","A",0.25,78.599999999999994,7.9]
["NE181","Webster","Nuckolls and Holdrege silt loams, 3 to 6 percent slopes","Well drained","C",0.75,9.1,7.2]
["NE181","Webster","Nuckolls and Holdrege silt loams, 6 to 11 percent slopes","Well drained","C",0.75,9.1,7.2]
["NE181","Webster","Nuckolls-Hobbs complex, 11 to 30 percent slopes","Well drained","B",0.75,9.4499999999999993,7.2]
["NE181","Webster","Rock Outcrop-Kipson complex, 7 to 45 percent slopes","Somewhat excessively drained","D",0.375,9.6,3.95]
["NE181","Webster","Roxbury silt loam, rarely flooded","Well drained","B",1,9,7.9]
["NE181","Webster","Uly-Coly silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7.8]
["NE181","Webster","Uly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",1.5,24,7.4]
["NE181","Webster","McCook fine sandy loam, very rarely flooded","Well drained","B",0.5,70.099999999999994,7.9]
["NE181","Webster","Munjor fine sandy loam, slightly wet variant","Somewhat poorly drained","B",0.25,67.7,7.9]
["NE181","Webster","Holdrege silt loam, 0 to 1 percent slopes, plains and breaks","Well drained","C",1,10.5,7.25]
["NE181","Webster","Holdrege silt loam, 1 to 3 percent slopes, plains and breaks","Well drained","C",0.95000000000000007,10.5,7.25]
["NE181","Webster","Holdrege silt loam, 3 to 7 percent slopes, plains and breaks","Well drained","C",0.95000000000000007,10.5,7.25]
["NE181","Webster","Wakeen silt loam, 3 to 11 percent slopes","Well drained","B",0.75,7.2,7.9]
["NE181","Webster","Wakeen silt loam, 3 to 11 percent slopes, eroded","Well drained","C",0.75,6.8,7.9]
["NE181","Webster","Wakeen silt loam, 11 to 30 percent slopes","Well drained","C",0.75,6.8,7.9]
["NE181","Webster","Humbarger silt loam, very rarely flooded","Moderately well drained","C",1,30.15,7.9]
["NE181","Webster","Crete silt loam, 0 to 1 percent slopes, loess plains and breaks","Moderately well drained","C",1.1499999999999999,5,6.8]
["NE181","Webster","Gibbon silty clay loam, rarely flooded","Somewhat poorly drained","C",0.75,7,7.9]
["NE181","Webster","Ustorthents","Excessively drained","A",0.25,91.75,6.35]
["NE183","Wheeler",null,"",""]
["NE183","Wheeler","Almeria loamy fine sand, channeled, frequently flooded","Very poorly drained","A/D",1.25,75.349999999999994,6.9]
["NE183","Wheeler","Almeria-Calamus complex, channeled, frequently flooded","Poorly drained","A/D",0.25,92.2,6.2]
["NE183","Wheeler","Almeria-Inavale complex, channeled, frequently flooded","Poorly drained","A/D",0.25,89.5,6.7]
["NE183","Wheeler","Anselmo fine sandy loam, 0 to 1 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE183","Wheeler","Anselmo fine sandy loam, 1 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE183","Wheeler","Anselmo fine sandy loam, 3 to 6 percent slopes","Well drained","A",0.75,66.099999999999994,7]
["NE183","Wheeler","Blackloup loam, occasionally flooded","Very poorly drained","B/D",0.5,72.55,7.4]
["NE183","Wheeler","Boelus loamy sand, 0 to 3 percent slopes","Well drained","C",0.5,70.400000000000006,7]
["NE183","Wheeler","Boelus loamy sand, 3 to 6 percent slopes","Well drained","B",0.5,51.95,7]
["NE183","Wheeler","Coly silt loam, 17 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE183","Wheeler","Coly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",1.125,11.3,7.9]
["NE183","Wheeler","Coly-Hobbs silt loams, 3 to 60 percent slopes","Well drained","B",1.125,11.3,7.7]
["NE183","Wheeler","Coly-Uly silt loams, 11 to 17 percent slopes, eroded","Well drained","B",0.75,11.2,7.9]
["NE183","Wheeler","Dunday loamy fine sand, 0 to 3 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE183","Wheeler","Dunday loamy fine sand, 3 to 6 percent slopes","Somewhat excessively drained","A",0.875,90.85,6.85]
["NE183","Wheeler","Els loamy sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,84.3,6.7]
["NE183","Wheeler","Els-Ipage fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE183","Wheeler","Elsmere loamy fine sand, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,86.8,6.5]
["NE183","Wheeler","Elsmere-Ipage loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.25,94.9,6.5]
["NE183","Wheeler","Elsmere-Loup complex, 0 to 3 percent slopes","Somewhat poorly drained","A",0.75,86.8,6.5]
["NE183","Wheeler","Elsmere-Selia loamy fine sands, 0 to 3 percent slopes","Somewhat poorly drained","A",0.5,86.35,7.4]
["NE183","Wheeler","Fluvaquents, sandy, frequently flooded","Very poorly drained","A/D",2.75,90.15,7.5]
["NE183","Wheeler","Gates silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.5,12.95,7.7]
["NE183","Wheeler","Gates very fine sandy loam, 1 to 3 percent slopes","Well drained","B",0.5,58.6,7.5]
["NE183","Wheeler","Gates very fine sandy loam, 3 to 6 percent slopes","Well drained","B",0.5,58.6,7.5]
["NE183","Wheeler","Gates very fine sandy loam, 6 to 11 percent slopes, eroded","Well drained","B",0.5,58.6,7.5]
["NE183","Wheeler","Gates-Hersh complex, 0 to 3 percent slopes","Well drained","B",0.625,66.099999999999994,7.35]
["NE183","Wheeler","Gibbon loam, occasionally flooded","Somewhat poorly drained","C",0.75,41.5,7.9]
["NE183","Wheeler","Hall silt loam, 1 to 3 percent slopes","Well drained","C",1.125,10.4,7.1]
["NE183","Wheeler","Hersh fine sandy loam, 0 to 3 percent slopes","Well drained","A",0.75,66.099999999999994,6.7]
["NE183","Wheeler","Hobbs silt loam, occasionally flooded","Well drained","B",0.75,11.3,7]
["NE183","Wheeler","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE183","Wheeler","Ipage fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.5,95.199999999999989,6.2]
["NE183","Wheeler","Ipage loamy sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,89.199999999999989,6.2]
["NE183","Wheeler","Leshara silt loam, occasionally flooded","Somewhat poorly drained","C",0.75,11.6,7.5]
["NE183","Wheeler","Libory loamy fine sand, 0 to 3 percent slopes","Moderately well drained","A",0.75,86.4,6.5]
["NE183","Wheeler","Loretto loam, 0 to 2 percent slopes","Well drained","C",1.5,39.1,6.5]
["NE183","Wheeler","Loup fine sandy loam, 0 to 1 percent slopes","Poorly drained","A/D",0.75,63.5,7.5]
["NE183","Wheeler","Loup fine sandy loam, frequently ponded","Very poorly drained","A/D",3.375,79.2,6.6]
["NE183","Wheeler","Loup fine sandy loam, rarely flooded","Poorly drained","A/D",3.375,79.2,6.6]
["NE183","Wheeler","Marlake loamy fine sand, frequently ponded","Very poorly drained","A/D",0.75,86.8,7]
["NE183","Wheeler","Nimbro silt loam, 0 to 2 percent slopes","Well drained","B",1.75,30.900000000000002,7.9]
["NE183","Wheeler","Ord loam, rarely flooded","Somewhat poorly drained","C",0.75,62.5,7.5]
["NE183","Wheeler","Tryon loamy fine sand, 0 to 3 percent slopes","Poorly drained","A/D",3.375,91.1,7]
["NE183","Wheeler","Tryon loamy fine sand, frequently ponded","Very poorly drained","A/D",3.375,91.1,6.85]
["NE183","Wheeler","Tryon loamy fine sand, rarely flooded","Poorly drained","A/D",3.375,91.1,6.85]
["NE183","Wheeler","Uly silt loam, 3 to 6 percent slopes","Well drained","B",0.75,9.5,7]
["NE183","Wheeler","Uly silt loam, 6 to 11 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE183","Wheeler","Uly-Coly silt loams, 17 to 30 percent slopes, eroded","Well drained","B",1.125,10.35,7.45]
["NE183","Wheeler","Uly-Coly silt loams, 6 to 11 percent slopes, eroded","Well drained","B",1.125,10.35,7.45]
["NE183","Wheeler","Valentine fine sand, 0 to 3 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE183","Wheeler","Valentine fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,96.3,6.5]
["NE183","Wheeler","Valentine fine sand, rolling","Excessively drained","A",0.5,96.3,6.5]
["NE183","Wheeler","Valentine fine sand, rolling and hilly","Excessively drained","A",0.5,96.3,6.5]
["NE183","Wheeler","Valentine loamy fine sand, 0 to 3 percent slopes","Excessively drained","A",0.25,87.3,6.5]
["NE183","Wheeler","Valentine loamy fine sand, 3 to 9 percent slopes","Excessively drained","A",0.5,91.35,6.5]
["NE183","Wheeler","Valentine-Dunday loamy fine sands, 3 to 9 percent slopes","Somewhat excessively drained","A",0.25,92.7,6.5]
["NE183","Wheeler","Valentine-Els fine sands, 0 to 9 percent slopes","Somewhat poorly drained","A",0.25,95.4,6.5]
["NE185","York",null,"",""]
["NE185","York","Butler silt loam, 0 to 1 percent slopes","Somewhat poorly drained","C/D",1.5,6,7]
["NE185","York","Coly silt loam, 11 to 30 percent slopes","Well drained","B",1.125,11.3,7.9]
["NE185","York","Crete silt loam, 0 to 1 percent slopes","Moderately well drained","C",1.5,6,6.7]
["NE185","York","Crete silt loam, 1 to 3 percent slopes","Moderately well drained","C",1.625,13.2,6.25]
["NE185","York","Fillmore silt loam, frequently ponded","Somewhat poorly drained","D",1,6,7]
["NE185","York","Geary silty clay loam, 3 to 7 percent slopes, eroded","Well drained","B",1.5,7.1,7]
["NE185","York","Geary silty clay loam, 7 to 11 percent slopes, eroded","Well drained","B",1.5,7.1,7]
["NE185","York","Geary-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",2,11.3,7]
["NE185","York","Hall silt loam, 0 to 1 percent slopes","Well drained","C",1.5,9.5,7]
["NE185","York","Hastings silt loam, 0 to 1 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE185","York","Hastings silt loam, 1 to 3 percent slopes","Well drained","C",1.125,8.5,6.55]
["NE185","York","Hastings silt loam, 3 to 7 percent slopes","Well drained","C",0.625,6.95,7.0500000000000007]
["NE185","York","Hastings silt loam, 7 to 11 percent slopes","Well drained","C",0.5,20,6.5]
["NE185","York","Hastings silty clay loam, 3 to 7 percent slopes, eroded","Well drained","C",0.75,20,7.3]
["NE185","York","Hastings silty clay loam, 7 to 11 percent slopes, eroded","Well drained","C",0.75,20,7.3]
["NE185","York","Hobbs silt loam, channeled, frequently flooded","Well drained","B",0.75,11.3,7]
["NE185","York","Hobbs silt loam, frequently flooded","Well drained","B",0.75,11.3,7]
["NE185","York","Hobbs silt loam, occasionally flooded","Well drained","B",1.875,11.3,7]
["NE185","York","Hord silt loam, 0 to 1 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE185","York","Hord silt loam, 1 to 3 percent slopes","Well drained","B",0.75,9.3000000000000007,7]
["NE185","York","Hord silt loam, rarely flooded","Well drained","B",0.75,9.3000000000000007,7]
["NE185","York","Hord-Hastings complex, 3 to 6 percent slopes","Well drained","C",0.625,10.25,6.75]
["NE185","York","Massie silty clay loam, frequently ponded","Very poorly drained","D",1.25,6,6.4]
["NE185","York","Scott silt loam, frequently ponded","Poorly drained","D",1,6,6.8]
["NE185","York","Uly silt loam, 11 to 30 percent slopes, eroded","Well drained","B",0.75,9.5,7]
["NE185","York","Uly-Hobbs silt loams, 0 to 30 percent slopes","Well drained","B",0.75,10.35,7]
["NE185","York","Uly-Hobbs silt loams, 11 to 30 percent slopes","Well drained","B",0.75,11.2,7]

{"sheet":"NEapplicationTime","index":7,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":true,"merged":[]}
[null,"Default Application ","Default Application",null,"Season #","Time of Application"]
["Fertilizer","Time","Time List Number",null,1]
[null,null,1,null,2,"Fall"]
["Ammonium nitrate incorporated  ","Spring ",3,null,3,"Spring "]
["Ammonium nitrate surface applied","Spring ",3,null,4,"In-season (spilt)"]
["Ammonium sulfate incorporated","Spring ",3]
["Ammonium sulfate surface applied","Spring ",3]
["Anhydrous ammonia injected","Spring ",3]
["Other incorporated/injected","Spring ",3]
["UAN fertigation","In-season (spilt)",4]
["UAN incorporated/injected","Spring ",3]
["UAN sidedress surface","In-season (spilt)",4]
["UAN surface","Spring ",3]
["UAN sidedress injected","In-season (spilt)",4]
["Urea incorporated","Spring ",3]
["Urea surface","Spring ",3]

{"sheet":"NEcountyPrcp","index":8,"n_rows":94,"n_cols":3,"rows_kept":94,"cut":false,"hidden":true,"merged":[]}
["County","Out of Season","In Season"]
["Adams",12.29,15.620000000000001]
["Antelope",13.030000000000001,14.530000000000001]
["Arthur",7.99,11.61]
["Banner",6.9200000000000008,9.34]
["Blaine",10.430000000000001,13.27]
["Boone",12.639999999999999,14.96]
["Box Butte",6.7999999999999989,9.39]
["Boyd",12.13,13.15]
["Brown",10.14,13.38]
["Buffalo",10.87,14.870000000000001]
["Burt",14.82,15.990000000000002]
["Butler",13.53,15.959999999999999]
["Cass",16.72,17.45]
["Cedar",13.67,14.29]
["Chase",7.7400000000000011,11.68]
["Cherry",8.94,12]
["Cheyenne",7.17,10.62]
["Clay",12.66,15.93]
["Colfax",13.5,16.310000000000002]
["Cuming",13.990000000000002,16.010000000000002]
["Custer",10.479999999999999,13.629999999999999]
["Dakota",14.52,15.23]
["Dawes",7.8100000000000005,9.7099999999999991]
["Dawson",9.94,13.969999999999999]
["Deuel",7.66,11.02]
["Dixon",14.360000000000001,14.83]
["Dodge",14.250000000000002,16.350000000000001]
["Douglas",14.66,16.77]
["Dundy",8.02,11.219999999999999]
["Fillmore",13.15,15.89]
["Franklin",11.180000000000001,15.13]
["Frontier",9.17,12.97]
["Furnas",10.399999999999999,13.530000000000001]
["Gage",14.670000000000002,17.23]
["Garden",7.38,10.610000000000001]
["Garfield",11.850000000000001,14.270000000000001]
["Gosper",9.85,13.86]
["Grant",8.1800000000000015,11.690000000000001]
["Greeley",12.140000000000002,14.64]
["Hall",12.26,15.559999999999999]
["Hamilton",13.26,16.240000000000002]
["Harlan",10.479999999999999,14.47]
["Hayes",8.84,12.48]
["Hitchcock",8.9099999999999984,12.62]
["Holt",12.030000000000001,13.559999999999999]
["Hooker",9.4200000000000017,12.68]
["Howard",12.14,14.79]
["Jefferson",14.209999999999999,17.189999999999998]
["Johnson",15.21,17.190000000000001]
["Kearney",11.080000000000002,15.27]
["Keith",8.14,11.49]
["Keya Paha",10.25,13.41]
["Kimball",6.76,9.89]
["Knox",13.07,13.89]
["Lancaster",14.45,16.82]
["Lincoln",8.99,12.66]
["Logan",10.07,12.93]
["Loup",11.389999999999999,13.58]
["McPherson",8.98,12.33]
["Madison",13.089999999999998,15.32]
["Merrick",12.92,15.48]
["Morrill",7.12,9.879999999999999]
["Nance",12.77,15.1]
["Nemaha",15.969999999999999,18.510000000000002]
["Nuckolls",12.62,15.270000000000001]
["Otoe",15.320000000000002,17.700000000000003]
["Pawnee",15.809999999999999,17.47]
["Perkins",8.1300000000000008,11.93]
["Phelps",10.52,15.09]
["Pierce",13.52,14.48]
["Platte",13.469999999999999,15.94]
["Polk",13.11,15.520000000000001]
["Red Willow",9.120000000000001,12.889999999999999]
["Richardson",16.18,18.29]
["Rock",11.23,13.580000000000002]
["Saline",13.69,16.310000000000002]
["Sarpy",15.999999999999998,17.159999999999997]
["Saunders",14.370000000000001,16.66]
["Scotts Bluff",6.45,8.73]
["Seward",13.2,15.9]
["Sheridan",7.46,10.32]
["Sherman",11.75,14.73]
["Sioux",7.0600000000000005,8.92]
["Stanton",13.260000000000002,15.62]
["Thayer",13.68,16.389999999999997]
["Thomas",9.84,12.889999999999999]
["Thurston",14.34,15.459999999999999]
["Valley",11.770000000000001,14.04]
["Washington",14.89,16.43]
["Wayne",13.530000000000001,14.729999999999999]
["Webster",11.91,15.170000000000002]
["Wheeler",12.66,14.42]
["York",13.010000000000002,15.809999999999999]

{"sheet":"NEmanure","index":9,"n_rows":86,"n_cols":9,"rows_kept":86,"cut":false,"hidden":true,"merged":[[70,0,70,7],[15,0,15,8],[17,5,17,8],[62,0,62,7],[41,0,41,7],[51,1,51,5],[27,5,27,8],[36,5,36,8]]}
["Drop Down List","Unit for Application","Manure Type","Dry Matter Content","Conversion Factor\nUnit for App to t/ac","Ammonium-N\n(lbs of N per Unit)","Organic-N\n(lbs of N per Unit)","Ammonium-N\nAvailable","Organic-N\nAvailable"]
[{"$f":"IF(DropDownLists!H3<>\"\",DropDownLists!H3,\"\")","v":""}]
[{"$f":"IF(DropDownLists!H4<>\"\",DropDownLists!H4,\"\")","v":"Effluent Pond"},"acre-inch/acre","Effluent Pond",2.5000000000000001E-3,93.375,71,8,{"$f":"IF($B$74<>A77,0,1)*IFERROR(IF(AND($C$11>=0,$C$11<=7),VLOOKUP($C$11,$B$54:$C$61,2,FALSE),0),0)","v":0},{"$f":"IF($F$86=1,0.35,$F$86)","v":0}]
[{"$f":"IF(DropDownLists!H5<>\"\",DropDownLists!H5,\"\")","v":"Feedlot solid"},"ton/acre","Beef (dirt lot)",0.67,1,2,22,{"$f":"IF($B$74<>$A$77,0,1)*IFERROR(IF(AND($C$11>=0,$C$11<=7),VLOOKUP($C$11,$E$54:$F$61,2,FALSE),0),0)","v":0},{"$f":"IF($F$86=1,0.25,$F$86)","v":0}]
[{"$f":"IF(DropDownLists!H6<>\"\",DropDownLists!H6,\"\")","v":"Poultry solid"},"ton/acre","Broilers (litter from house)/Layer",{"$f":"AVERAGE(D33,D34)","v":0.55000000000000004},1,{"$f":"AVERAGE(F33,F34)","v":16.5},{"$f":"AVERAGE(G33,G34)","v":39.5},{"$f":"IF($B$74<>$A$77,0,1)*IFERROR(IF(AND($C$11>=0,$C$11<=7),VLOOKUP($C$11,$E$54:$F$61,2,FALSE),0),0)","v":0},{"$f":"IF($F$86=1,0.3,$F$86)","v":0}]
[{"$f":"IF(DropDownLists!H7<>\"\",DropDownLists!H7,\"\")","v":"Swine lagoon"},"acre-inch/acre","Swine (lagoon)",4.0000000000000001E-3,93.375,91,45,{"$f":"IF($B$74<>$A$77,0,1)*IFERROR(IF(AND($C$11>=0,$C$11<=7),VLOOKUP($C$11,$B$54:$C$61,2,FALSE),0),0)","v":0},{"$f":"IF($F$86=1,0.35,$F$86)","v":0}]
[{"$f":"IF(DropDownLists!H8<>\"\",DropDownLists!H8,\"\")","v":"Swine or dairy slurry"},"1,000 gallon/acre","Swine (Finish building)/Dairy",{"$f":"AVERAGE(D19,D23)","v":0.05},3.4583333333333335,{"$f":"AVERAGE(F19,F23)","v":12},{"$f":"AVERAGE(G19,G23)","v":9},{"$f":"IF($B$74<>$A$77,0,1)*IFERROR(IF(AND($C$11>=0,$C$11<=7),VLOOKUP($C$11,$B$54:$C$61,2,FALSE),0),0)","v":0},{"$f":"IF($F$86=1,0.5,$F$86)","v":0}]
[{"$f":"IF(DropDownLists!H9<>\"\",DropDownLists!H9,\"\")","v":"Swine or dairy solid"},"ton/acre","Dairy (scraped earthen lots)",0.46,1,3,14,{"$f":"IF($B$74<>$A$77,0,1)*IFERROR(IF(AND($C$11>=0,$C$11<=7),VLOOKUP($C$11,$E$54:$F$61,2,FALSE),0),0)","v":0},{"$f":"IF($F$86=1,0.25,$F$86)","v":0}]
[]
["Drop Down Application List","Days to Incorporation\nInterface Value","Days to Incorporation \nDefault Adjustment"]
[{"$f":"IF(NLossCalculations!J30<>0,NLossCalculations!J30,\"\")","v":""},{"$f":"IFERROR(VLOOKUP(A11,$B$66:$C$69,2,FALSE),\"\")","v":""},{"$f":"IFERROR(ROUND(VLOOKUP($A$11,$B$66:$D$69,3,FALSE),0),\"\")","v":""}]
[]
[]
[]
[]
["Reference List for Manure Properties"]
[null,null,null,null,"Conversion Factor","Ammonium-N","Organic-N","P2O5","K2O"]
[null,"Unit for Application","Slurry Manure","Dry Matter","Unit for App to t/ac","----------(lbs of nutrient per 1,000 gallons of manure)---------"]
["Swine or dairy slurry","1,000 gal/ac","Dairy",0.08,8300,12,13,25,40]
[null,"1,000 gal/ac","Beef",0.28999999999999998,8300,5,9,9,13]
[null,"1,000 gal/ac","Swine (finisher, wet-dry feeder)",0.09,8300,42,17,40,24]
[null,"1,000 gal/ac","Swine (slurry storage, dry feeder)",0.06,8300,28,11,34,24]
["Swine or dairy slurry","1,000 gal/ac","Swine (Finish building)",0.02,8300,12,5,13,17]
[null,"1,000 gal/ac","Layer",0.11,8300,37,20,51,33]
[null,"1,000 gal/ac","Dairy (lagoon sludge)",0.1,8300,4,17,20,16]
[null,"1,000 gal/ac","Swine (lagoon sludge)",0.1,8300,6,16,48,7]
[]
[null,null,"Solid Manure",null,null,"----------(lbs of nutrient per ton of manure)---------"]
["Feedlot solid","t/ac","Beef (dirt lot)",0.67,1,2,22,23,30]
[null,"t/ac","Beef (paved lot)",0.28999999999999998,1,5,9,9,13]
[null,"t/ac","Swine (hoop barns)",0.56999999999999995,1,4,13,20]
["Swine or dairy solid","t/ac","Dairy (scraped earthen lots)",0.46,1,3,14,11,16]
["Poultry solid","t/ac","Broilers (litter from house)",0.7,1,15,60,27,33]
["Poultry solid","t/ac","Layer",0.4,1,18,19,55,31]
[null,"t/ac","Turkey (grower house litter)",0.7,1,null,null,15,30]
[]
[null,null,"Liquid Effluent from lagoon or holding pond",null,null,"----------(lbs of nutrient per acre-inch)---------"]
["Feedlot holding pond","ac-in/ac","Beef (runoff holding pond) - - Effluent Pond",2.5000000000000001E-3,224100,71,8,47,92]
["Swine Lagoon","ac-in/ac","Swine (lagoon)",4.0000000000000001E-3,224100,91,45,104,189]
[null,"ac-in/ac","Dairy (lagoon)",0.02,224100,317,362,674,1082]
[]
["Reference List for Ammonium-N and Organic-N Availability"]
[]
["Manure List #","Type","Organic-N"]
[2,"Feedlot holding pond",0.35]
[3,"Feedlot solid",0.25]
[4,"Poultry solid",0.3]
[5,"Swine lagoon",0.35]
[6,"Swine or dairy slurry",0.5]
[7,"Swine or dairy solid",0.25]
[]
[null,"Ammonium-N"]
["Manure - Liquid List #","Days","Liquid","Manure - Solid List #","Days","Solid"]
[2,0,0.95,3,0,0.95]
[5,1,0.7,4,1,0.5]
[6,2,0.5,7,2,0.25]
[null,3,0.35,null,3,0.15]
[null,4,0.1,null,4,0.25]
[null,5,0.05,null,5,0.15]
[null,6,0,null,6,0.05]
[null,7,0,null,7,0]
[]
["Reference List for Application Method and Days to Incorporation"]
[]
["Drop Down List #","List Value","Number of Days for Application Default","Number of Days for \nApplication Adjusted"]
[1]
[2,{"$f":"DropDownLists!I4","v":"Injected"},"Skip",0]
[3,{"$f":"DropDownLists!I5","v":"Incorporated within 7 days"},"Enter Days",{"$f":"IF(NLossCalculations!J36=C68,0,IF(AND(NLossCalculations!J36>=0,NLossCalculations!J36<=7),NLossCalculations!J36,7))","v":7}]
[4,{"$f":"DropDownLists!I6","v":"Not incorporated within 7 days"},"Skip",7]
[]
["Reference List for Year of Application to Make Organic N Adjustment"]
[]
["Current Date","Crop Year"]
[{"$f":"NOW()","v":"2015-01-06T15:10:02.210"},{"$f":"IF(AND(MONTH(A74)>=6,MONTH(A74)<=12),YEAR(A74)+1,YEAR(A74))","v":2015}]
[]
["Manure Application Year","Season Applied","Season Applied ID Number"]
[{"$f":"NLossCalculations!I35","v":""},{"$f":"NLossCalculations!J31","v":0},{"$f":"NLossCalculations!I31","v":1}]
[]
[]
["Season","Year","Season","Year","Factors","Final Adj. Factor"]
["Fall - Current Crop Year",{"$f":"$B$74-1","v":2014},"Spring - Current Crop Year",{"$f":"$B$74","v":2015},1,{"$f":"IFERROR(IF(OR(AND($B$74-A77=1,$C$77=3),AND($B$74=D81,$C$77=2,SUM(F82:F84)=0)),E81,0),0)","v":0}]
["Fall - Prior Crop Year",{"$f":"$B$74-2","v":2013},"Spring - Prior Crop Year",{"$f":"$B$74-1","v":2014},0.15,{"$f":"IFERROR(IF(OR(AND($B$74-$A$77=2,$C$77=3),AND($B$74-$A$77=1,$C$77=2)),E82,0),0)","v":0}]
["Fall - Two Prior Crop Years",{"$f":"$B$74-3","v":2012},"Spring - Two Prior Crop Years",{"$f":"$B$74-2","v":2013},7.0000000000000007E-2,{"$f":"IFERROR(IF(OR(AND($B$74-$A$77=3,$C$77=3),AND($B$74-$A$77=2,$C$77=2)),E83,0),0)","v":0}]
["Fall - Three Prior Crop Years",{"$f":"$B$74-4","v":2011},"Spring - Three Prior Crop Years",{"$f":"$B$74-3","v":2012},0.04,{"$f":"IFERROR(IF(OR(AND($B$74-$A$77=4,$C$77=3),AND($B$74-$A$77=3,$C$77=2)),E84,0),0)","v":0}]
[]
[null,null,null,null,"Adjustment Factor",{"$f":"SUM(F81:F84)","v":0}]

{"sheet":"NEfertilizer","index":10,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":true,"merged":[]}
["Drop Down List","Urea N","Ammonium N","Nitrate ","AmN (Ammonium N\n+ Urea N)"]
[]
["Ammonium nitrate incorporated  ",0,0.5,0.5,{"$f":"C3+B3","v":0.5}]
["Ammonium nitrate surface applied",0,0.5,0.5,{"$f":"C4+B4","v":0.5}]
["Ammonium sulfate incorporated",0,1,0,1]
["Ammonium sulfate surface applied",0,1,0,1]
["Anhydrous ammonia injected",0,1,0,1]
["Other incorporated/injected",0,1,0,1]
["UAN fertigation",0.5,0.25,0.25,0.75]
["UAN incorporated/injected",0.5,0.25,0.25,0.75]
["UAN sidedress surface",0.5,0.25,0.25,0.75]
["UAN surface",0.5,0.25,0.25,0.75]
["UAN sidedress injected",0.5,0.25,0.25,0.75]
["Urea incorporated",1,0,0,1]
["Urea surface",1,0,0,1]